--- a/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-rock-3a.dts
@@ -15,6 +15,10 @@
 		ethernet0 = &gmac1;
 		mmc0 = &sdhci;
 		mmc1 = &sdmmc0;
+		led-boot = &led_blue;
+		led-failsafe = &led_blue;
+		led-running = &led_blue;
+		led-upgrade = &led_blue;
 	};
 
 	chosen: chosen {
@@ -42,11 +46,11 @@
 	leds {
 		compatible = "gpio-leds";
 
-		led_user: led-0 {
-			gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
-			function = LED_FUNCTION_HEARTBEAT;
+		led_blue: led-0 {
 			color = <LED_COLOR_ID_BLUE>;
-			linux,default-trigger = "heartbeat";
+			default-state = "on";
+			function = LED_FUNCTION_HEARTBEAT;
+			gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
 			pinctrl-names = "default";
 			pinctrl-0 = <&led_user_en>;
 		};
