From dd6dc0c4c1265129c229e26917bf4de1d97ff91f Mon Sep 17 00:00:00 2001
From: Benjamin Gaignard <benjamin.gaignard@collabora.com>
Date: Fri, 6 Oct 2023 08:53:34 +0200
Subject: [PATCH] arm64: dts: rockchip: Add AV1 decoder node to rk3588s

Add node for AV1 video decoder.

Signed-off-by: Benjamin Gaignard <benjamin.gaignard@collabora.com>
Reviewed-by: Sebastian Reichel <sebastian.reichel@collabora.com>
Link: https://lore.kernel.org/r/20231006065334.8117-1-benjamin.gaignard@collabora.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3588s.dtsi | 13 +++++++++++++
 1 file changed, 13 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3588s.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588s.dtsi
@@ -2314,6 +2314,19 @@
 			#interrupt-cells = <2>;
 		};
 	};
+
+	av1d: video-codec@fdc70000 {
+		compatible = "rockchip,rk3588-av1-vpu";
+		reg = <0x0 0xfdc70000 0x0 0x800>;
+		interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH 0>;
+		interrupt-names = "vdpu";
+		assigned-clocks = <&cru ACLK_AV1>, <&cru PCLK_AV1>;
+		assigned-clock-rates = <400000000>, <400000000>;
+		clocks = <&cru ACLK_AV1>, <&cru PCLK_AV1>;
+		clock-names = "aclk", "hclk";
+		power-domains = <&power RK3588_PD_AV1>;
+		resets = <&cru SRST_A_AV1>, <&cru SRST_P_AV1>, <&cru SRST_A_AV1_BIU>, <&cru SRST_P_AV1_BIU>;
+	};
 };
 
 #include "rk3588s-pinctrl.dtsi"
