From 7541089d40221a708e606bb0c05eb66dc136e105 Mon Sep 17 00:00:00 2001
From: Naushir Patuck <naush@raspberrypi.com>
Date: Tue, 21 Apr 2020 15:06:19 +0100
Subject: [PATCH 0208/1085] media: uapi: v4l-ctrls: Add CID base for the
 bcm2835-isp driver

We are reserving controls for the new bcm2835-isp driver.

Signed-off-by: Naushir Patuck <naush@raspberrypi.com>
---
 .../admin-guide/media/bcm2835-isp.rst         | 127 ++++++++++++++++++
 .../userspace-api/media/drivers/index.rst     |   1 +
 include/uapi/linux/v4l2-controls.h            |   4 +
 3 files changed, 132 insertions(+)
 create mode 100644 Documentation/admin-guide/media/bcm2835-isp.rst

--- /dev/null
+++ b/Documentation/admin-guide/media/bcm2835-isp.rst
@@ -0,0 +1,127 @@
+.. SPDX-License-Identifier: GPL-2.0
+
+BCM2835 ISP Driver
+==================
+
+Introduction
+------------
+
+The BCM2835 Image Sensor Pipeline (ISP) is a fixed function hardware pipeline
+for performing image processing operations.  Images are fed to the input
+of the ISP through memory frame buffers.  These images may be in various YUV,
+RGB, or Bayer formats.  A typical use case would have Bayer images obtained from
+an image sensor by the BCM2835 Unicam peripheral, written to a memory
+frame buffer, and finally fed into the input of the ISP.  Two concurrent output
+images may be generated in YUV or RGB format at different resolutions.
+Statistics output is also generated for Bayer input images.
+
+The bcm2835-isp driver exposes the following media pads as V4L2 device nodes:
+
+.. tabularcolumns:: |l|l|l|l|
+
+.. cssclass: longtable
+
+.. flat-table::
+
+    * - *Pad*
+      - *Direction*
+      - *Purpose*
+      - *Formats*
+
+    * - "bcm2835-isp0-output0"
+      - sink
+      - Accepts Bayer, RGB or YUV format frame buffers as input to the ISP HW
+        pipeline.
+      - :ref:`RAW8 <V4L2-PIX-FMT-SRGGB8>`,
+        :ref:`RAW10P <V4L2-PIX-FMT-SRGGB10P>`,
+        :ref:`RAW12P <V4L2-PIX-FMT-SRGGB12P>`,
+        :ref:`RAW14P <V4L2-PIX-FMT-SRGGB14P>`,
+        :ref:`RAW16 <V4L2-PIX-FMT-SRGGB16>`,
+        :ref:`RGB24/BGR24 <V4L2-PIX-FMT-RGB24>`,
+        :ref:`YUYV <V4L2-PIX-FMT-YUYV>`,
+        :ref:`YVYU <V4L2-PIX-FMT-YVYU>`,
+        :ref:`UYVY <V4L2-PIX-FMT-UYVY>`,
+        :ref:`VYUY <V4L2-PIX-FMT-VYUY>`,
+        :ref:`YUV420/YVU420 <V4L2-PIX-FMT-YUV420>`
+
+    * - "bcm2835-isp0-capture1"
+      - source
+      - High resolution YUV or RGB processed output from the ISP.
+      - :ref:`RGB565 <V4L2-PIX-FMT-RGB565>`,
+        :ref:`RGB24/BGR24 <V4L2-PIX-FMT-RGB24>`,
+        :ref:`ABGR32 <V4L2-PIX-FMT-ABGR32>`,
+        :ref:`YUYV <V4L2-PIX-FMT-YUYV>`,
+        :ref:`YVYU <V4L2-PIX-FMT-YVYU>`,
+        :ref:`UYVY <V4L2-PIX-FMT-UYVY>`,
+        :ref:`VYUY <V4L2-PIX-FMT-VYUY>`.
+        :ref:`YUV420/YVU420 <V4L2-PIX-FMT-YUV420>`,
+        :ref:`NV12/NV21 <V4L2-PIX-FMT-NV12>`,
+
+    * - "bcm2835-isp0-capture2"
+      - source
+      - Low resolution YUV processed output from the ISP. The output of
+        this pad cannot have a resolution larger than the "bcm2835-isp0-capture1" pad in any dimension.
+      - :ref:`YUYV <V4L2-PIX-FMT-YUYV>`,
+        :ref:`YVYU <V4L2-PIX-FMT-YVYU>`,
+        :ref:`UYVY <V4L2-PIX-FMT-UYVY>`,
+        :ref:`VYUY <V4L2-PIX-FMT-VYUY>`.
+        :ref:`YUV420/YVU420 <V4L2-PIX-FMT-YUV420>`,
+        :ref:`NV12/NV21 <V4L2-PIX-FMT-NV12>`,
+
+    * - "bcm2835-isp0-capture1"
+      - source
+      - Image statistics calculated from the input image provided on the
+        "bcm2835-isp0-output0" pad.  Statistics are only available for Bayer
+        format input images.
+      - :ref:`v4l2-meta-fmt-bcm2835-isp-stats`.
+
+Pipeline Configuration
+----------------------
+
+The ISP pipeline can be configure through user-space by calling
+:ref:`VIDIOC_S_EXT_CTRLS <VIDIOC_G_EXT_CTRLS>` on the “bcm2835-isp0-output0”
+node with the appropriate parameters as shown in the table below.
+
+.. tabularcolumns:: |p{2cm}|p{5.0cm}|
+
+.. cssclass: longtable
+
+.. flat-table::
+
+    * - *id*
+      - *Parameter*
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_CC_MATRIX``
+      - struct :c:type:`bcm2835_isp_custom_ccm`
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_LENS_SHADING``
+      - struct :c:type:`bcm2835_isp_lens_shading`
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_BLACK_LEVEL``
+      - struct :c:type:`bcm2835_isp_black_level`
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_GEQ``
+      - struct :c:type:`bcm2835_isp_geq`
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_GAMMA``
+      - struct :c:type:`bcm2835_isp_gamma`
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_DENOISE``
+      - struct :c:type:`bcm2835_isp_denoise`
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_SHARPEN``
+      - struct :c:type:`bcm2835_isp_sharpen`
+
+    * - ``V4L2_CID_USER_BCM2835_ISP_DPC``
+      - struct :c:type:`bcm2835_isp_dpc`
+
+++++++++++++++++++++++++
+Configuration Parameters
+++++++++++++++++++++++++
+
+.. kernel-doc:: include/uapi/linux/bcm2835-isp.h
+   :functions: bcm2835_isp_rational bcm2835_isp_ccm bcm2835_isp_custom_ccm
+                bcm2835_isp_gain_format bcm2835_isp_lens_shading
+                bcm2835_isp_black_level bcm2835_isp_geq bcm2835_isp_gamma
+                bcm2835_isp_denoise bcm2835_isp_sharpen
+                bcm2835_isp_dpc_mode bcm2835_isp_dpc
--- a/Documentation/userspace-api/media/drivers/index.rst
+++ b/Documentation/userspace-api/media/drivers/index.rst
@@ -36,6 +36,7 @@ For more details see the file COPYING in
 	cx2341x-uapi
 	dw100
 	imx-uapi
+	bcm2835-isp
 	max2175
 	omap3isp-uapi
 	st-vgxy61
--- a/include/uapi/linux/v4l2-controls.h
+++ b/include/uapi/linux/v4l2-controls.h
@@ -203,6 +203,10 @@ enum v4l2_colorfx {
  */
 #define V4L2_CID_USER_ASPEED_BASE		(V4L2_CID_USER_BASE + 0x11a0)
 
+/* The base for the bcm2835-isp driver controls.
+ * We reserve 16 controls for this driver. */
+#define V4L2_CID_USER_BCM2835_ISP_BASE		(V4L2_CID_USER_BASE + 0x10f0)
+
 /* MPEG-class control IDs */
 /* The MPEG controls are applicable to all codec controls
  * and the 'MPEG' part of the define is historical */
