From ed23e07bf7a1896b6eaa85b773bb43b1fad66d4b Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Sat, 21 Dec 2024 00:07:11 +0100
Subject: [PATCH] ARM: dts: ixp4xx: Fix up PCI on WG302

Looking at the board file for WG302 v2 was not a good idea
because the GPIO IRQ for slot 2 differs, and v1 uses GPIO
10 instead of GPIO 9. Fix it up.

Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
---
 .../dts/intel/ixp/intel-ixp42x-netgear-wg302v1.dts     | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

--- a/arch/arm/boot/dts/intel/ixp/intel-ixp42x-netgear-wg302v1.dts
+++ b/arch/arm/boot/dts/intel/ixp/intel-ixp42x-netgear-wg302v1.dts
@@ -57,7 +57,7 @@
 			status = "okay";
 
 			/*
-			 * Taken from WG302 v2 PCI boardfile (wg302v2-pci.c)
+			 * Taken from WG302 v1 PCI boardfile (wg302v1-pci.c)
 			 * We have slots (IDSEL) 1 and 2 with one assigned IRQ
 			 * each handling all IRQs.
 			 */
@@ -70,10 +70,10 @@
 			<0x0800 0 0 3 &gpio0 8 IRQ_TYPE_LEVEL_LOW>, /* INT C on slot 1 is irq 8 */
 			<0x0800 0 0 4 &gpio0 8 IRQ_TYPE_LEVEL_LOW>, /* INT D on slot 1 is irq 8 */
 			/* IDSEL 2 */
-			<0x1000 0 0 1 &gpio0 9 IRQ_TYPE_LEVEL_LOW>, /* INT A on slot 2 is irq 9 */
-			<0x1000 0 0 2 &gpio0 9 IRQ_TYPE_LEVEL_LOW>, /* INT B on slot 2 is irq 9 */
-			<0x1000 0 0 3 &gpio0 9 IRQ_TYPE_LEVEL_LOW>, /* INT C on slot 2 is irq 9 */
-			<0x1000 0 0 4 &gpio0 9 IRQ_TYPE_LEVEL_LOW>; /* INT D on slot 2 is irq 9 */
+			<0x1000 0 0 1 &gpio0 10 IRQ_TYPE_LEVEL_LOW>, /* INT A on slot 2 is irq 10 */
+			<0x1000 0 0 2 &gpio0 10 IRQ_TYPE_LEVEL_LOW>, /* INT B on slot 2 is irq 10 */
+			<0x1000 0 0 3 &gpio0 10 IRQ_TYPE_LEVEL_LOW>, /* INT C on slot 2 is irq 10 */
+			<0x1000 0 0 4 &gpio0 10 IRQ_TYPE_LEVEL_LOW>; /* INT D on slot 2 is irq 10 */
 		};
 
 		ethernet@c8009000 {
