From patchwork Wed Nov 20 09:15:04 2024
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
X-Patchwork-Submitter: Md Sadre Alam <quic_mdalam@quicinc.com>
X-Patchwork-Id: 2013501
Return-Path: 
 <linux-mtd-bounces+incoming=patchwork.ozlabs.org@lists.infradead.org>
X-Original-To: incoming@patchwork.ozlabs.org
Delivered-To: patchwork-incoming@legolas.ozlabs.org
Authentication-Results: legolas.ozlabs.org;
	dkim=pass (2048-bit key;
 secure) header.d=lists.infradead.org header.i=@lists.infradead.org
 header.a=rsa-sha256 header.s=bombadil.20210309 header.b=EI114Wyi;
	dkim=fail reason="signature verification failed" (2048-bit key;
 unprotected) header.d=quicinc.com header.i=@quicinc.com header.a=rsa-sha256
 header.s=qcppdkim1 header.b=WgJ5on5Q;
	dkim-atps=neutral
Authentication-Results: legolas.ozlabs.org;
 spf=none (no SPF record) smtp.mailfrom=lists.infradead.org
 (client-ip=2607:7c80:54:3::133; helo=bombadil.infradead.org;
 envelope-from=linux-mtd-bounces+incoming=patchwork.ozlabs.org@lists.infradead.org;
 receiver=patchwork.ozlabs.org)
Received: from bombadil.infradead.org (bombadil.infradead.org
 [IPv6:2607:7c80:54:3::133])
	(using TLSv1.3 with cipher TLS_AES_256_GCM_SHA384 (256/256 bits)
	 key-exchange X25519 server-signature ECDSA (secp384r1) server-digest SHA384)
	(No client certificate requested)
	by legolas.ozlabs.org (Postfix) with ESMTPS id 4XtbMW1JfFz1xyG
	for <incoming@patchwork.ozlabs.org>; Wed, 20 Nov 2024 20:16:23 +1100 (AEDT)
DKIM-Signature: v=1; a=rsa-sha256; q=dns/txt; c=relaxed/relaxed;
	d=lists.infradead.org; s=bombadil.20210309; h=Sender:
	Content-Transfer-Encoding:Content-Type:List-Subscribe:List-Help:List-Post:
	List-Archive:List-Unsubscribe:List-Id:MIME-Version:References:In-Reply-To:
	Message-ID:Date:Subject:CC:To:From:Reply-To:Content-ID:Content-Description:
	Resent-Date:Resent-From:Resent-Sender:Resent-To:Resent-Cc:Resent-Message-ID:
	List-Owner; bh=HhmgnJkVgny0u3hKiTd0ZM4cwdwqDHQn7f5raP0Z97Q=; b=EI114WyiL0woYU
	WPjsi5XhHUI2CGLrmf8w0ScC9Pq7PFPwTPGxLYcoSh0JNv/FIax+J93VC5zYRp68aD4mTdTjU6bra
	kTYGxoBj28Lwiy1jmYm0SWp8dPzX2hCg1lNWr9mP+JjnhuZpyt26qUJnshLyQbVgv8uoEiYGpJjIv
	GBwOKIvs0vkaJy2E1MBvCO2/+qlNpOlz83wg1tF8uS4MJF+fjWgmVHBrXfRoTlEk6CJumTvpluqNx
	nzaRMXONO/wYP03WjutalMhZJsQpInGIZhhKL8TOksrLF2q2b4gzF1JAucwPq78p0bWAcgS2ih8vP
	564SGleqnhz8GQTtUxog==;
Received: from localhost ([::1] helo=bombadil.infradead.org)
	by bombadil.infradead.org with esmtp (Exim 4.98 #2 (Red Hat Linux))
	id 1tDgom-0000000Esn9-19FP;
	Wed, 20 Nov 2024 09:16:12 +0000
Received: from mx0b-0031df01.pphosted.com ([205.220.180.131])
	by bombadil.infradead.org with esmtps (Exim 4.98 #2 (Red Hat Linux))
	id 1tDgoi-0000000EsiZ-1EXE
	for linux-mtd@lists.infradead.org;
	Wed, 20 Nov 2024 09:16:10 +0000
Received: from pps.filterd (m0279873.ppops.net [127.0.0.1])
	by mx0a-0031df01.pphosted.com (8.18.1.2/8.18.1.2) with ESMTP id
 4AK9FRJU010557;
	Wed, 20 Nov 2024 09:16:00 GMT
DKIM-Signature: v=1; a=rsa-sha256; c=relaxed/relaxed; d=quicinc.com; h=
	cc:content-transfer-encoding:content-type:date:from:in-reply-to
	:message-id:mime-version:references:subject:to; s=qcppdkim1; bh=
	5iRCp4ZP77j9GA9UB1rMArUv8juFZCi6KdJ0Pw/qPiM=; b=WgJ5on5QibUuTZPB
	Ps89rgba/1Sz4aAyNPfSD9p3o4Lkpefh8wQBsnNvyMAqm6bP9GqT4GsoLIWzh2iL
	f+NE+/ukvlaLa7P7MQHd14J0blNY2tD9ooc8NodYJJNu1Ul84oegXRuGSTvqh5h7
	Xm2jOZDpHs7GIB/opkfbaLyFkMdDmMo8zBjL338260tHaKQf5vc62PNv6I5roF2O
	QictV4vxOJvogxIcNrtAtGwkgsY8+UKYiK0Kf5J7JV7QpK1ejDCqv1NcNPu/87tp
	u1a5iWy5iFKPldKgO0B/sAvGc2y8tw3Td8lnu2+CQAdyNMVUnBcB71XGvkrINO+y
	vVURBw==
Received: from nasanppmta02.qualcomm.com (i-global254.qualcomm.com
 [199.106.103.254])
	by mx0a-0031df01.pphosted.com (PPS) with ESMTPS id 43091mda79-1
	(version=TLSv1.2 cipher=ECDHE-RSA-AES256-GCM-SHA384 bits=256 verify=NOT);
	Wed, 20 Nov 2024 09:15:59 +0000 (GMT)
Received: from nasanex01a.na.qualcomm.com (nasanex01a.na.qualcomm.com
 [10.52.223.231])
	by NASANPPMTA02.qualcomm.com (8.18.1.2/8.18.1.2) with ESMTPS id
 4AK9FwXk025630
	(version=TLSv1.2 cipher=ECDHE-RSA-AES256-GCM-SHA384 bits=256 verify=NOT);
	Wed, 20 Nov 2024 09:15:58 GMT
Received: from hu-mdalam-blr.qualcomm.com (10.80.80.8) by
 nasanex01a.na.qualcomm.com (10.52.223.231) with Microsoft SMTP Server
 (version=TLS1_2, cipher=TLS_ECDHE_RSA_WITH_AES_256_GCM_SHA384) id
 15.2.1544.9; Wed, 20 Nov 2024 01:15:53 -0800
From: Md Sadre Alam <quic_mdalam@quicinc.com>
To: <broonie@kernel.org>, <robh@kernel.org>, <krzk+dt@kernel.org>,
        <conor+dt@kernel.org>, <andersson@kernel.org>,
        <konradybcio@kernel.org>, <miquel.raynal@bootlin.com>,
        <richard@nod.at>, <vigneshr@ti.com>,
        <manivannan.sadhasivam@linaro.org>, <linux-arm-msm@vger.kernel.org>,
        <linux-spi@vger.kernel.org>, <devicetree@vger.kernel.org>,
        <linux-kernel@vger.kernel.org>, <linux-mtd@lists.infradead.org>
CC: <quic_srichara@quicinc.com>, <quic_varada@quicinc.com>,
        <quic_mdalam@quicinc.com>
Subject: [PATCH v14 6/8] spi: spi-qpic: add driver for QCOM SPI NAND flash
 Interface
Date: Wed, 20 Nov 2024 14:45:04 +0530
Message-ID: <20241120091507.1404368-7-quic_mdalam@quicinc.com>
X-Mailer: git-send-email 2.34.1
In-Reply-To: <20241120091507.1404368-1-quic_mdalam@quicinc.com>
References: <20241120091507.1404368-1-quic_mdalam@quicinc.com>
MIME-Version: 1.0
X-Originating-IP: [10.80.80.8]
X-ClientProxiedBy: nasanex01a.na.qualcomm.com (10.52.223.231) To
 nasanex01a.na.qualcomm.com (10.52.223.231)
X-QCInternal: smtphost
X-Proofpoint-Virus-Version: vendor=nai engine=6200 definitions=5800
 signatures=585085
X-Proofpoint-ORIG-GUID: Ma2z9oeQxcw35J8DzEJ64cF8a3mxAzPO
X-Proofpoint-GUID: Ma2z9oeQxcw35J8DzEJ64cF8a3mxAzPO
X-Proofpoint-Virus-Version: vendor=baseguard
 engine=ICAP:2.0.293,Aquarius:18.0.1039,Hydra:6.0.680,FMLib:17.12.60.29
 definitions=2024-09-06_09,2024-09-06_01,2024-09-02_01
X-Proofpoint-Spam-Details: rule=outbound_notspam policy=outbound score=0
 suspectscore=0
 impostorscore=0 spamscore=0 priorityscore=1501 phishscore=0 malwarescore=0
 clxscore=1015 bulkscore=0 mlxlogscore=999 lowpriorityscore=0 adultscore=0
 mlxscore=0 classifier=spam adjust=0 reason=mlx scancount=1
 engine=8.19.0-2409260000 definitions=main-2411200063
X-CRM114-Version: 20100106-BlameMichelson ( TRE 0.8.0 (BSD) ) MR-646709E3 
X-CRM114-CacheID: sfid-20241120_011608_535555_EC8A73C5 
X-CRM114-Status: GOOD (  24.86  )
X-Spam-Score: -2.8 (--)
X-Spam-Report: Spam detection software,
 running on the system "bombadil.infradead.org",
 has NOT identified this incoming email as spam.  The original
 message has been attached to this so you can view it or label
 similar future email.  If you have any questions, see
 the administrator of that system for details.
 Content preview:  This driver implements support for the SPI-NAND mode of
 QCOM
    NAND Flash Interface as a SPI-MEM controller with pipelined ECC
 capability.
    Co-developed-by: Sricharan Ramabadhran <quic_srichara@quicinc.com>
 Signed-off-by:
    Sricharan Ramabadhran <quic_srichara@quicinc.com> Co-developed-by:
 Varadarajan
    Narayanan <quic_varada@quicinc.com> Sig [...]
 Content analysis details:   (-2.8 points, 5.0 required)
  pts rule name              description
 ---- ----------------------
 --------------------------------------------------
  0.0 RCVD_IN_VALIDITY_RPBL_BLOCKED RBL: ADMINISTRATOR NOTICE: The query to
                              Validity was blocked.  See
                             https://knowledge.validity.com/hc/en-us/articles/20961730681243
                              for more information.
                           [205.220.180.131 listed in
 bl.score.senderscore.com]
  0.0 RCVD_IN_VALIDITY_SAFE_BLOCKED RBL: ADMINISTRATOR NOTICE: The query to
                              Validity was blocked.  See
                             https://knowledge.validity.com/hc/en-us/articles/20961730681243
                              for more information.
                             [205.220.180.131 listed in
 sa-accredit.habeas.com]
 -0.7 RCVD_IN_DNSWL_LOW      RBL: Sender listed at https://www.dnswl.org/, low
                             trust
                             [205.220.180.131 listed in list.dnswl.org]
  0.0 RCVD_IN_VALIDITY_CERTIFIED_BLOCKED RBL: ADMINISTRATOR NOTICE: The
                             query to Validity was blocked.  See
                             https://knowledge.validity.com/hc/en-us/articles/20961730681243
                              for more information.
                        [205.220.180.131 listed in
 sa-trusted.bondedsender.org]
 -0.0 SPF_PASS               SPF: sender matches SPF record
  0.0 SPF_HELO_NONE          SPF: HELO does not publish an SPF Record
 -0.1 DKIM_VALID             Message has at least one valid DKIM or DK
 signature
 -0.1 DKIM_VALID_EF          Message has a valid DKIM or DK signature from
                             envelope-from domain
 -0.1 DKIM_VALID_AU          Message has a valid DKIM or DK signature from
 author's
                             domain
  0.1 DKIM_SIGNED            Message has a DKIM or DK signature,
 not necessarily valid
 -1.9 BAYES_00               BODY: Bayes spam probability is 0 to 1%
                             [score: 0.0000]
X-BeenThere: linux-mtd@lists.infradead.org
X-Mailman-Version: 2.1.34
Precedence: list
List-Id: Linux MTD discussion mailing list <linux-mtd.lists.infradead.org>
List-Unsubscribe: <http://lists.infradead.org/mailman/options/linux-mtd>,
 <mailto:linux-mtd-request@lists.infradead.org?subject=unsubscribe>
List-Archive: <http://lists.infradead.org/pipermail/linux-mtd/>
List-Post: <mailto:linux-mtd@lists.infradead.org>
List-Help: <mailto:linux-mtd-request@lists.infradead.org?subject=help>
List-Subscribe: <http://lists.infradead.org/mailman/listinfo/linux-mtd>,
 <mailto:linux-mtd-request@lists.infradead.org?subject=subscribe>
Sender: "linux-mtd" <linux-mtd-bounces@lists.infradead.org>
Errors-To: linux-mtd-bounces+incoming=patchwork.ozlabs.org@lists.infradead.org

This driver implements support for the SPI-NAND mode of QCOM NAND Flash
Interface as a SPI-MEM controller with pipelined ECC capability.

Co-developed-by: Sricharan Ramabadhran <quic_srichara@quicinc.com>
Signed-off-by: Sricharan Ramabadhran <quic_srichara@quicinc.com>
Co-developed-by: Varadarajan Narayanan <quic_varada@quicinc.com>
Signed-off-by: Varadarajan Narayanan <quic_varada@quicinc.com>
Signed-off-by: Md Sadre Alam <quic_mdalam@quicinc.com>
---

Change in [v14]

* No Change 

Change in [v13]

* Changed return type of qcom_spi_cmd_mapping() from u32 to
  int to fix the kernel test bot warning
* Changed type of variable cmd in qcom_spi_write_page() from u32
  to int
* Removed unused variable s_op from qcom_spi_write_page()
* Updated return value variable type from u32 to int in
  qcom_spi_send_cmdaddr() 

Change in [v12]

* Added obj-$(CONFIG_SPI_QPIC_SNAND) += qpic_common.o in Makefile
  to build qpic_common.c based on CONFIG_SPI_QPIC_SNAND

Change in [v11]

* Fixed build error reported by kernel test bot
* Changed "depends on MTD" to "select MTD" in
  drivers/spi/Kconfig file

Change in [v10]

* Fixed compilation warnings reported by kernel test robot.
* Added depends on CONFIG_MTD
* removed extra bracket from statement if (i == (num_cw - 1)) in 
  qcom_spi_program_raw() api.

Change in [v9]

* Changed data type of addr1, addr2, cmd, to __le32 in qpic_spi_nand
  structure
* In qcom_spi_set_read_loc_first() api added cpu_to_le32() macro to fix
  compilation warning
* In qcom_spi_set_read_loc_last() api added cpu_to_le32() macro to fix
  compilation warning
* In qcom_spi_init() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_ecc_init_ctx_pipelined() api removed unused variables
  reqs, user, step_size, strength and added cpu_to_le32() macro as well
  to fix compilation warning
* In qcom_spi_read_last_cw() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_check_error() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_read_page_ecc() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_read_page_oob() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_program_raw() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_program_ecc() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_program_oob() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_send_cmdaddr() api added cpu_to_le32() macro to fix compilation
  warning
* In qcom_spi_io_op() api added cpu_to_le32() macro to fix compilation
  warning

Change in [v8]

* Included "bitfield.h" file to /spi-qpic-snand.c
  to fix compilation warning reported by kernel test robot
* Removed unused variable "steps" in 
  qcom_spi_ecc_init_ctx_pipelined() to fix compilation warning

Change in [v7]

* Added read_oob() and write_oob() api

* Handled offset value for oob layout

* Made CONFIG_SPI_QPIC_SNAND as bool

* Added macro ecceng_to_qspi()

* Added FIELD_PREP() Macro in spi init

* Added else condition in 
  qcom_spi_ecc_finish_io_req_pipelined()
  for corrected ecc

* Handled multiple error condition for api
  qcom_spi_cmd_mapping()

* Fix typo for printing debug message
  
Change in [v6]

* Added separate qpic_spi_nand{...} struct

* moved qpic_ecc and qcom_ecc_stats struct to
  spi-qpic-snand.c file, since its spi nand
  specific

* Added FIELD_PREP() and GENMASK() macro

* Removed rawnand.h and partition.h from 
  spi-qpic-snand.c

* Removed oob_buff assignment form
  qcom_spi_write_page_cache

* Added qcom_nand_unalloc() in remove() path

* Fixes all all comments

Change in [v5]

* Added raw_read() and raw_write() api

* Updated commit message

* Removed register indirection

* Added qcom_spi_ prefix to all the api

* Removed snand_set_reg() api.

* Fixed nandbiterr issue

* Removed hardcoded num_cw and made it variable

* Removed hardcoded value for mtd pagesize

* Added -ENOSUPPORT in cmd mapping for unsupported
  commands

* Replace if..else with switch..case statement

Change in [v4]

* No change

Change in [v3]

* Set SPI_QPIC_SNAND to n and added COMPILE_TEST in Kconfig

* Made driver name sorted in Make file

* Made comment like c++

* Changed macro to functions, snandc_set_read_loc_last()
  and snandc_set_read_loc_first()

* Added error handling in snandc_set_reg()

* Changed into normal conditional statement for
  return snandc->ecc_stats.failed ? -EBADMSG :
  snandc->ecc_stats.bitflips;

* Remove cast of wbuf in qpic_snand_program_execute()
  function

* Made num_cw variable instead hardcoded value

* changed if..else condition of function qpic_snand_io_op()
  to switch..case statement

* Added __devm_spi_alloc_controller() api instead of
  devm_spi_alloc_master()

* Disabling clock in remove path

Change in [v2]

* Added initial support for SPI-NAND driver

Change in [v1]

* Added RFC patch for design review

 drivers/mtd/nand/Makefile            |    4 +
 drivers/spi/Kconfig                  |    9 +
 drivers/spi/Makefile                 |    1 +
 drivers/spi/spi-qpic-snand.c         | 1633 ++++++++++++++++++++++++++
 include/linux/mtd/nand-qpic-common.h |    7 +
 5 files changed, 1654 insertions(+)
 create mode 100644 drivers/spi/spi-qpic-snand.c

--- a/drivers/mtd/nand/Makefile
+++ b/drivers/mtd/nand/Makefile
@@ -4,7 +4,11 @@ nandcore-objs := core.o bbt.o
 obj-$(CONFIG_MTD_NAND_CORE) += nandcore.o
 obj-$(CONFIG_MTD_NAND_ECC_MEDIATEK) += ecc-mtk.o
 obj-$(CONFIG_MTD_NAND_MTK_BMT)	+= mtk_bmt.o mtk_bmt_v2.o mtk_bmt_bbt.o mtk_bmt_nmbm.o
+ifeq ($(CONFIG_SPI_QPIC_SNAND),y)
+obj-$(CONFIG_SPI_QPIC_SNAND) += qpic_common.o
+else
 obj-$(CONFIG_MTD_NAND_QCOM) += qpic_common.o
+endif
 obj-y	+= onenand/
 obj-y	+= raw/
 obj-y	+= spi/
--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -870,6 +870,15 @@ config SPI_QCOM_QSPI
 	help
 	  QSPI(Quad SPI) driver for Qualcomm QSPI controller.
 
+config SPI_QPIC_SNAND
+	bool "QPIC SNAND controller"
+	depends on ARCH_QCOM || COMPILE_TEST
+	select MTD
+	help
+	  QPIC_SNAND (QPIC SPI NAND) driver for Qualcomm QPIC controller.
+	  QPIC controller supports both parallel nand and serial nand.
+	  This config will enable serial nand driver for QPIC controller.
+
 config SPI_QUP
 	tristate "Qualcomm SPI controller with QUP interface"
 	depends on ARCH_QCOM || COMPILE_TEST
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -110,6 +110,7 @@ obj-$(CONFIG_SPI_PXA2XX)		+= spi-pxa2xx-
 obj-$(CONFIG_SPI_PXA2XX_PCI)		+= spi-pxa2xx-pci.o
 obj-$(CONFIG_SPI_QCOM_GENI)		+= spi-geni-qcom.o
 obj-$(CONFIG_SPI_QCOM_QSPI)		+= spi-qcom-qspi.o
+obj-$(CONFIG_SPI_QPIC_SNAND)            += spi-qpic-snand.o
 obj-$(CONFIG_SPI_QUP)			+= spi-qup.o
 obj-$(CONFIG_SPI_ROCKCHIP)		+= spi-rockchip.o
 obj-$(CONFIG_SPI_ROCKCHIP_SFC)		+= spi-rockchip-sfc.o
--- /dev/null
+++ b/drivers/spi/spi-qpic-snand.c
@@ -0,0 +1,1633 @@
+/*
+ * SPDX-License-Identifier: GPL-2.0
+ *
+ * Copyright (c) 2023, Qualcomm Innovation Center, Inc. All rights reserved.
+ *
+ * Authors:
+ *	Md Sadre Alam <quic_mdalam@quicinc.com>
+ *	Sricharan R <quic_srichara@quicinc.com>
+ *	Varadarajan Narayanan <quic_varada@quicinc.com>
+ */
+#include <linux/bitops.h>
+#include <linux/clk.h>
+#include <linux/delay.h>
+#include <linux/dmaengine.h>
+#include <linux/dma-mapping.h>
+#include <linux/dma/qcom_adm.h>
+#include <linux/dma/qcom_bam_dma.h>
+#include <linux/module.h>
+#include <linux/of.h>
+#include <linux/platform_device.h>
+#include <linux/slab.h>
+#include <linux/mtd/nand-qpic-common.h>
+#include <linux/mtd/spinand.h>
+#include <linux/bitfield.h>
+
+#define NAND_FLASH_SPI_CFG		0xc0
+#define NAND_NUM_ADDR_CYCLES		0xc4
+#define NAND_BUSY_CHECK_WAIT_CNT	0xc8
+#define NAND_FLASH_FEATURES		0xf64
+
+/* QSPI NAND config reg bits */
+#define LOAD_CLK_CNTR_INIT_EN		BIT(28)
+#define CLK_CNTR_INIT_VAL_VEC		0x924
+#define CLK_CNTR_INIT_VAL_VEC_MASK	GENMASK(27, 16)
+#define FEA_STATUS_DEV_ADDR		0xc0
+#define FEA_STATUS_DEV_ADDR_MASK	GENMASK(15, 8)
+#define SPI_CFG				BIT(0)
+#define SPI_NUM_ADDR			0xDA4DB
+#define SPI_WAIT_CNT			0x10
+#define QPIC_QSPI_NUM_CS		1
+#define SPI_TRANSFER_MODE_x1		BIT(29)
+#define SPI_TRANSFER_MODE_x4		(3 << 29)
+#define SPI_WP				BIT(28)
+#define SPI_HOLD			BIT(27)
+#define QPIC_SET_FEATURE		BIT(31)
+
+#define SPINAND_RESET			0xff
+#define SPINAND_READID			0x9f
+#define SPINAND_GET_FEATURE		0x0f
+#define SPINAND_SET_FEATURE		0x1f
+#define SPINAND_READ			0x13
+#define SPINAND_ERASE			0xd8
+#define SPINAND_WRITE_EN		0x06
+#define SPINAND_PROGRAM_EXECUTE		0x10
+#define SPINAND_PROGRAM_LOAD		0x84
+
+#define ACC_FEATURE			0xe
+#define BAD_BLOCK_MARKER_SIZE		0x2
+#define OOB_BUF_SIZE			128
+#define ecceng_to_qspi(eng)		container_of(eng, struct qpic_spi_nand, ecc_eng)
+struct qpic_snand_op {
+	u32 cmd_reg;
+	u32 addr1_reg;
+	u32 addr2_reg;
+};
+
+struct snandc_read_status {
+	__le32 snandc_flash;
+	__le32 snandc_buffer;
+	__le32 snandc_erased_cw;
+};
+
+/*
+ * ECC state struct
+ * @corrected:		ECC corrected
+ * @bitflips:		Max bit flip
+ * @failed:		ECC failed
+ */
+struct qcom_ecc_stats {
+	u32 corrected;
+	u32 bitflips;
+	u32 failed;
+};
+
+struct qpic_ecc {
+	struct device *dev;
+	int ecc_bytes_hw;
+	int spare_bytes;
+	int bbm_size;
+	int ecc_mode;
+	int bytes;
+	int steps;
+	int step_size;
+	int strength;
+	int cw_size;
+	int cw_data;
+	u32 cfg0;
+	u32 cfg1;
+	u32 cfg0_raw;
+	u32 cfg1_raw;
+	u32 ecc_buf_cfg;
+	u32 ecc_bch_cfg;
+	u32 clrflashstatus;
+	u32 clrreadstatus;
+	bool bch_enabled;
+};
+
+struct qpic_spi_nand {
+	struct qcom_nand_controller *snandc;
+	struct spi_controller *ctlr;
+	struct mtd_info *mtd;
+	struct clk *iomacro_clk;
+	struct qpic_ecc *ecc;
+	struct qcom_ecc_stats ecc_stats;
+	struct nand_ecc_engine ecc_eng;
+	u8 *data_buf;
+	u8 *oob_buf;
+	u32 wlen;
+	__le32 addr1;
+	__le32 addr2;
+	__le32 cmd;
+	u32 num_cw;
+	bool oob_rw;
+	bool page_rw;
+	bool raw_rw;
+};
+
+static void qcom_spi_set_read_loc_first(struct qcom_nand_controller *snandc,
+					int reg, int cw_offset, int read_size,
+					int is_last_read_loc)
+{
+	__le32 locreg_val;
+	u32 val = (((cw_offset) << READ_LOCATION_OFFSET) |
+		  ((read_size) << READ_LOCATION_SIZE) | ((is_last_read_loc)
+		  << READ_LOCATION_LAST));
+
+	locreg_val = cpu_to_le32(val);
+
+	if (reg == NAND_READ_LOCATION_0)
+		snandc->regs->read_location0 = locreg_val;
+	else if (reg == NAND_READ_LOCATION_1)
+		snandc->regs->read_location1 = locreg_val;
+	else if (reg == NAND_READ_LOCATION_2)
+		snandc->regs->read_location1 = locreg_val;
+	else if (reg == NAND_READ_LOCATION_3)
+		snandc->regs->read_location3 = locreg_val;
+}
+
+static void qcom_spi_set_read_loc_last(struct qcom_nand_controller *snandc,
+				       int reg, int cw_offset, int read_size,
+				       int is_last_read_loc)
+{
+	__le32 locreg_val;
+	u32 val = (((cw_offset) << READ_LOCATION_OFFSET) |
+		  ((read_size) << READ_LOCATION_SIZE) | ((is_last_read_loc)
+		  << READ_LOCATION_LAST));
+
+	locreg_val = cpu_to_le32(val);
+
+	if (reg == NAND_READ_LOCATION_LAST_CW_0)
+		snandc->regs->read_location_last0 = locreg_val;
+	else if (reg == NAND_READ_LOCATION_LAST_CW_1)
+		snandc->regs->read_location_last1 = locreg_val;
+	else if (reg == NAND_READ_LOCATION_LAST_CW_2)
+		snandc->regs->read_location_last2 = locreg_val;
+	else if (reg == NAND_READ_LOCATION_LAST_CW_3)
+		snandc->regs->read_location_last3 = locreg_val;
+}
+
+static struct qcom_nand_controller *nand_to_qcom_snand(struct nand_device *nand)
+{
+	struct nand_ecc_engine *eng = nand->ecc.engine;
+	struct qpic_spi_nand *qspi = ecceng_to_qspi(eng);
+
+	return qspi->snandc;
+}
+
+static int qcom_spi_init(struct qcom_nand_controller *snandc)
+{
+	u32 snand_cfg_val = 0x0;
+	int ret;
+
+	snand_cfg_val = FIELD_PREP(CLK_CNTR_INIT_VAL_VEC_MASK, CLK_CNTR_INIT_VAL_VEC) |
+			FIELD_PREP(LOAD_CLK_CNTR_INIT_EN, 0) |
+			FIELD_PREP(FEA_STATUS_DEV_ADDR_MASK, FEA_STATUS_DEV_ADDR) |
+			FIELD_PREP(SPI_CFG, 0);
+
+	snandc->regs->spi_cfg = cpu_to_le32(snand_cfg_val);
+	snandc->regs->num_addr_cycle = cpu_to_le32(SPI_NUM_ADDR);
+	snandc->regs->busy_wait_cnt = cpu_to_le32(SPI_WAIT_CNT);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->spi_cfg, NAND_FLASH_SPI_CFG, 1, 0);
+
+	snand_cfg_val &= ~LOAD_CLK_CNTR_INIT_EN;
+	snandc->regs->spi_cfg = cpu_to_le32(snand_cfg_val);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->spi_cfg, NAND_FLASH_SPI_CFG, 1, 0);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->num_addr_cycle, NAND_NUM_ADDR_CYCLES, 1, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->busy_wait_cnt, NAND_BUSY_CHECK_WAIT_CNT, 1,
+			   NAND_BAM_NEXT_SGL);
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure in submitting spi init descriptor\n");
+		return ret;
+	}
+
+	return ret;
+}
+
+static int qcom_spi_ooblayout_ecc(struct mtd_info *mtd, int section,
+				  struct mtd_oob_region *oobregion)
+{
+	struct nand_device *nand = mtd_to_nanddev(mtd);
+	struct qcom_nand_controller *snandc = nand_to_qcom_snand(nand);
+	struct qpic_ecc *qecc = snandc->qspi->ecc;
+
+	if (section > 1)
+		return -ERANGE;
+
+	oobregion->length = qecc->ecc_bytes_hw + qecc->spare_bytes;
+	oobregion->offset = mtd->oobsize - oobregion->length;
+
+	return 0;
+}
+
+static int qcom_spi_ooblayout_free(struct mtd_info *mtd, int section,
+				   struct mtd_oob_region *oobregion)
+{
+	struct nand_device *nand = mtd_to_nanddev(mtd);
+	struct qcom_nand_controller *snandc = nand_to_qcom_snand(nand);
+	struct qpic_ecc *qecc = snandc->qspi->ecc;
+
+	if (section)
+		return -ERANGE;
+
+	oobregion->length = qecc->steps * 4;
+	oobregion->offset = ((qecc->steps - 1) * qecc->bytes) + qecc->bbm_size;
+
+	return 0;
+}
+
+static const struct mtd_ooblayout_ops qcom_spi_ooblayout = {
+	.ecc = qcom_spi_ooblayout_ecc,
+	.free = qcom_spi_ooblayout_free,
+};
+
+static int qcom_spi_ecc_init_ctx_pipelined(struct nand_device *nand)
+{
+	struct qcom_nand_controller *snandc = nand_to_qcom_snand(nand);
+	struct nand_ecc_props *conf = &nand->ecc.ctx.conf;
+	struct mtd_info *mtd = nanddev_to_mtd(nand);
+	int cwperpage, bad_block_byte;
+	struct qpic_ecc *ecc_cfg;
+
+	cwperpage = mtd->writesize / NANDC_STEP_SIZE;
+	snandc->qspi->num_cw = cwperpage;
+
+	ecc_cfg = kzalloc(sizeof(*ecc_cfg), GFP_KERNEL);
+	if (!ecc_cfg)
+		return -ENOMEM;
+	snandc->qspi->oob_buf = kzalloc(mtd->writesize + mtd->oobsize,
+					GFP_KERNEL);
+	if (!snandc->qspi->oob_buf)
+		return -ENOMEM;
+
+	memset(snandc->qspi->oob_buf, 0xff, mtd->writesize + mtd->oobsize);
+
+	nand->ecc.ctx.priv = ecc_cfg;
+	snandc->qspi->mtd = mtd;
+
+	ecc_cfg->ecc_bytes_hw = 7;
+	ecc_cfg->spare_bytes = 4;
+	ecc_cfg->bbm_size = 1;
+	ecc_cfg->bch_enabled = true;
+	ecc_cfg->bytes = ecc_cfg->ecc_bytes_hw + ecc_cfg->spare_bytes + ecc_cfg->bbm_size;
+
+	ecc_cfg->steps = 4;
+	ecc_cfg->strength = 4;
+	ecc_cfg->step_size = 512;
+	ecc_cfg->cw_data = 516;
+	ecc_cfg->cw_size = ecc_cfg->cw_data + ecc_cfg->bytes;
+	bad_block_byte = mtd->writesize - ecc_cfg->cw_size * (cwperpage - 1) + 1;
+
+	mtd_set_ooblayout(mtd, &qcom_spi_ooblayout);
+
+	ecc_cfg->cfg0 = FIELD_PREP(CW_PER_PAGE_MASK, (cwperpage - 1)) |
+			FIELD_PREP(UD_SIZE_BYTES_MASK, ecc_cfg->cw_data) |
+			FIELD_PREP(DISABLE_STATUS_AFTER_WRITE, 1) |
+			FIELD_PREP(NUM_ADDR_CYCLES_MASK, 3) |
+			FIELD_PREP(ECC_PARITY_SIZE_BYTES_RS, ecc_cfg->ecc_bytes_hw) |
+			FIELD_PREP(STATUS_BFR_READ, 0) |
+			FIELD_PREP(SET_RD_MODE_AFTER_STATUS, 1) |
+			FIELD_PREP(SPARE_SIZE_BYTES_MASK, ecc_cfg->spare_bytes);
+
+	ecc_cfg->cfg1 = FIELD_PREP(NAND_RECOVERY_CYCLES_MASK, 0) |
+			FIELD_PREP(CS_ACTIVE_BSY, 0) |
+			FIELD_PREP(BAD_BLOCK_BYTE_NUM_MASK, bad_block_byte) |
+			FIELD_PREP(BAD_BLOCK_IN_SPARE_AREA, 0) |
+			FIELD_PREP(WR_RD_BSY_GAP_MASK, 20) |
+			FIELD_PREP(WIDE_FLASH, 0) |
+			FIELD_PREP(ENABLE_BCH_ECC, ecc_cfg->bch_enabled);
+
+	ecc_cfg->cfg0_raw = FIELD_PREP(CW_PER_PAGE_MASK, (cwperpage - 1)) |
+			    FIELD_PREP(NUM_ADDR_CYCLES_MASK, 3) |
+			    FIELD_PREP(UD_SIZE_BYTES_MASK, ecc_cfg->cw_size) |
+			    FIELD_PREP(SPARE_SIZE_BYTES_MASK, 0);
+
+	ecc_cfg->cfg1_raw = FIELD_PREP(NAND_RECOVERY_CYCLES_MASK, 0) |
+			    FIELD_PREP(CS_ACTIVE_BSY, 0) |
+			    FIELD_PREP(BAD_BLOCK_BYTE_NUM_MASK, 17) |
+			    FIELD_PREP(BAD_BLOCK_IN_SPARE_AREA, 1) |
+			    FIELD_PREP(WR_RD_BSY_GAP_MASK, 20) |
+			    FIELD_PREP(WIDE_FLASH, 0) |
+			    FIELD_PREP(DEV0_CFG1_ECC_DISABLE, 1);
+
+	ecc_cfg->ecc_bch_cfg = FIELD_PREP(ECC_CFG_ECC_DISABLE, !ecc_cfg->bch_enabled) |
+			       FIELD_PREP(ECC_SW_RESET, 0) |
+			       FIELD_PREP(ECC_NUM_DATA_BYTES_MASK, ecc_cfg->cw_data) |
+			       FIELD_PREP(ECC_FORCE_CLK_OPEN, 1) |
+			       FIELD_PREP(ECC_MODE_MASK, 0) |
+			       FIELD_PREP(ECC_PARITY_SIZE_BYTES_BCH_MASK, ecc_cfg->ecc_bytes_hw);
+
+	ecc_cfg->ecc_buf_cfg = 0x203 << NUM_STEPS;
+	ecc_cfg->clrflashstatus = FS_READY_BSY_N;
+	ecc_cfg->clrreadstatus = 0xc0;
+
+	conf->step_size = ecc_cfg->step_size;
+	conf->strength = ecc_cfg->strength;
+
+	snandc->regs->erased_cw_detect_cfg_clr = cpu_to_le32(CLR_ERASED_PAGE_DET);
+	snandc->regs->erased_cw_detect_cfg_set = cpu_to_le32(SET_ERASED_PAGE_DET);
+
+	dev_dbg(snandc->dev, "ECC strength: %u bits per %u bytes\n",
+		ecc_cfg->strength, ecc_cfg->step_size);
+
+	return 0;
+}
+
+static void qcom_spi_ecc_cleanup_ctx_pipelined(struct nand_device *nand)
+{
+	struct qpic_ecc *ecc_cfg = nand_to_ecc_ctx(nand);
+
+	kfree(ecc_cfg);
+}
+
+static int qcom_spi_ecc_prepare_io_req_pipelined(struct nand_device *nand,
+						 struct nand_page_io_req *req)
+{
+	struct qcom_nand_controller *snandc = nand_to_qcom_snand(nand);
+	struct qpic_ecc *ecc_cfg = nand_to_ecc_ctx(nand);
+
+	snandc->qspi->ecc = ecc_cfg;
+	snandc->qspi->raw_rw = false;
+	snandc->qspi->oob_rw = false;
+	snandc->qspi->page_rw = false;
+
+	if (req->datalen)
+		snandc->qspi->page_rw = true;
+
+	if (req->ooblen)
+		snandc->qspi->oob_rw = true;
+
+	if (req->mode == MTD_OPS_RAW)
+		snandc->qspi->raw_rw = true;
+
+	return 0;
+}
+
+static int qcom_spi_ecc_finish_io_req_pipelined(struct nand_device *nand,
+						struct nand_page_io_req *req)
+{
+	struct qcom_nand_controller *snandc = nand_to_qcom_snand(nand);
+	struct mtd_info *mtd = nanddev_to_mtd(nand);
+
+	if (req->mode == MTD_OPS_RAW || req->type != NAND_PAGE_READ)
+		return 0;
+
+	if (snandc->qspi->ecc_stats.failed)
+		mtd->ecc_stats.failed += snandc->qspi->ecc_stats.failed;
+	else
+		mtd->ecc_stats.corrected += snandc->qspi->ecc_stats.corrected;
+
+	if (snandc->qspi->ecc_stats.failed)
+		return -EBADMSG;
+	else
+		return snandc->qspi->ecc_stats.bitflips;
+}
+
+static struct nand_ecc_engine_ops qcom_spi_ecc_engine_ops_pipelined = {
+	.init_ctx = qcom_spi_ecc_init_ctx_pipelined,
+	.cleanup_ctx = qcom_spi_ecc_cleanup_ctx_pipelined,
+	.prepare_io_req = qcom_spi_ecc_prepare_io_req_pipelined,
+	.finish_io_req = qcom_spi_ecc_finish_io_req_pipelined,
+};
+
+/* helper to configure location register values */
+static void qcom_spi_set_read_loc(struct qcom_nand_controller *snandc, int cw, int reg,
+				  int cw_offset, int read_size, int is_last_read_loc)
+{
+	int reg_base = NAND_READ_LOCATION_0;
+	int num_cw = snandc->qspi->num_cw;
+
+	if (cw == (num_cw - 1))
+		reg_base = NAND_READ_LOCATION_LAST_CW_0;
+
+	reg_base += reg * 4;
+
+	if (cw == (num_cw - 1))
+		return qcom_spi_set_read_loc_last(snandc, reg_base, cw_offset,
+						  read_size, is_last_read_loc);
+	else
+		return qcom_spi_set_read_loc_first(snandc, reg_base, cw_offset,
+						   read_size, is_last_read_loc);
+}
+
+static void
+qcom_spi_config_cw_read(struct qcom_nand_controller *snandc, bool use_ecc, int cw)
+{
+	__le32 *reg = &snandc->regs->read_location0;
+	int num_cw = snandc->qspi->num_cw;
+
+	qcom_write_reg_dma(snandc, reg, NAND_READ_LOCATION_0, 4, NAND_BAM_NEXT_SGL);
+	if (cw == (num_cw - 1)) {
+		reg = &snandc->regs->read_location_last0;
+		qcom_write_reg_dma(snandc, reg, NAND_READ_LOCATION_LAST_CW_0, 4,
+				   NAND_BAM_NEXT_SGL);
+	}
+
+	qcom_write_reg_dma(snandc, &snandc->regs->cmd, NAND_FLASH_CMD, 1, NAND_BAM_NEXT_SGL);
+	qcom_write_reg_dma(snandc, &snandc->regs->exec, NAND_EXEC_CMD, 1, NAND_BAM_NEXT_SGL);
+
+	qcom_read_reg_dma(snandc, NAND_FLASH_STATUS, 2, 0);
+	qcom_read_reg_dma(snandc, NAND_ERASED_CW_DETECT_STATUS, 1,
+			  NAND_BAM_NEXT_SGL);
+}
+
+static int qcom_spi_block_erase(struct qcom_nand_controller *snandc)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	int ret;
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->addr0 = snandc->qspi->addr1;
+	snandc->regs->addr1 = snandc->qspi->addr2;
+	snandc->regs->cfg0 = cpu_to_le32(ecc_cfg->cfg0_raw & ~(7 << CW_PER_PAGE));
+	snandc->regs->cfg1 = cpu_to_le32(ecc_cfg->cfg1_raw);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->cmd, NAND_FLASH_CMD, 3, NAND_BAM_NEXT_SGL);
+	qcom_write_reg_dma(snandc, &snandc->regs->cfg0, NAND_DEV0_CFG0, 2, NAND_BAM_NEXT_SGL);
+	qcom_write_reg_dma(snandc, &snandc->regs->exec, NAND_EXEC_CMD, 1, NAND_BAM_NEXT_SGL);
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure to erase block\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static void qcom_spi_config_single_cw_page_read(struct qcom_nand_controller *snandc,
+						bool use_ecc, int cw)
+{
+	__le32 *reg = &snandc->regs->read_location0;
+	int num_cw = snandc->qspi->num_cw;
+
+	qcom_write_reg_dma(snandc, &snandc->regs->addr0, NAND_ADDR0, 2, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->cfg0, NAND_DEV0_CFG0, 3, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_clr,
+			   NAND_ERASED_CW_DETECT_CFG, 1, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_set,
+			   NAND_ERASED_CW_DETECT_CFG, 1,
+			   NAND_ERASED_CW_SET | NAND_BAM_NEXT_SGL);
+
+	if (cw == (num_cw - 1)) {
+		reg = &snandc->regs->read_location_last0;
+		qcom_write_reg_dma(snandc, reg, NAND_READ_LOCATION_LAST_CW_0, 4, NAND_BAM_NEXT_SGL);
+	}
+	qcom_write_reg_dma(snandc, &snandc->regs->cmd, NAND_FLASH_CMD, 1, NAND_BAM_NEXT_SGL);
+	qcom_write_reg_dma(snandc, &snandc->regs->exec, NAND_EXEC_CMD, 1, NAND_BAM_NEXT_SGL);
+
+	qcom_read_reg_dma(snandc, NAND_FLASH_STATUS, 1, 0);
+}
+
+static int qcom_spi_read_last_cw(struct qcom_nand_controller *snandc,
+				 const struct spi_mem_op *op)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	struct mtd_info *mtd = snandc->qspi->mtd;
+	int size, ret = 0;
+	int col,  bbpos;
+	u32 cfg0, cfg1, ecc_bch_cfg;
+	u32 num_cw = snandc->qspi->num_cw;
+
+	qcom_clear_bam_transaction(snandc);
+	qcom_clear_read_regs(snandc);
+
+	size = ecc_cfg->cw_size;
+	col = ecc_cfg->cw_size * (num_cw - 1);
+
+	memset(snandc->data_buffer, 0xff, size);
+	snandc->regs->addr0 = (snandc->qspi->addr1 | cpu_to_le32(col));
+	snandc->regs->addr1 = snandc->qspi->addr2;
+
+	cfg0 = (ecc_cfg->cfg0_raw & ~(7U << CW_PER_PAGE)) |
+		0 << CW_PER_PAGE;
+	cfg1 = ecc_cfg->cfg1_raw;
+	ecc_bch_cfg = 1 << ECC_CFG_ECC_DISABLE;
+
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->cfg0 = cpu_to_le32(cfg0);
+	snandc->regs->cfg1 = cpu_to_le32(cfg1);
+	snandc->regs->ecc_bch_cfg = cpu_to_le32(ecc_bch_cfg);
+	snandc->regs->clrflashstatus = cpu_to_le32(ecc_cfg->clrflashstatus);
+	snandc->regs->clrreadstatus = cpu_to_le32(ecc_cfg->clrreadstatus);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	qcom_spi_set_read_loc(snandc, num_cw - 1, 0, 0, ecc_cfg->cw_size, 1);
+
+	qcom_spi_config_single_cw_page_read(snandc, false, num_cw - 1);
+
+	qcom_read_data_dma(snandc, FLASH_BUF_ACC, snandc->data_buffer, size, 0);
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failed to read last cw\n");
+		return ret;
+	}
+
+	qcom_nandc_dev_to_mem(snandc, true);
+	u32 flash = le32_to_cpu(snandc->reg_read_buf[0]);
+
+	if (flash & (FS_OP_ERR | FS_MPU_ERR))
+		return -EIO;
+
+	bbpos = mtd->writesize - ecc_cfg->cw_size * (num_cw - 1);
+
+	if (snandc->data_buffer[bbpos] == 0xff)
+		snandc->data_buffer[bbpos + 1] = 0xff;
+	if (snandc->data_buffer[bbpos] != 0xff)
+		snandc->data_buffer[bbpos + 1] = snandc->data_buffer[bbpos];
+
+	memcpy(op->data.buf.in, snandc->data_buffer + bbpos, op->data.nbytes);
+
+	return ret;
+}
+
+static int qcom_spi_check_error(struct qcom_nand_controller *snandc, u8 *data_buf, u8 *oob_buf)
+{
+	struct snandc_read_status *buf;
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	int i, num_cw = snandc->qspi->num_cw;
+	bool flash_op_err = false, erased;
+	unsigned int max_bitflips = 0;
+	unsigned int uncorrectable_cws = 0;
+
+	snandc->qspi->ecc_stats.failed = 0;
+	snandc->qspi->ecc_stats.corrected = 0;
+
+	qcom_nandc_dev_to_mem(snandc, true);
+	buf = (struct snandc_read_status *)snandc->reg_read_buf;
+
+	for (i = 0; i < num_cw; i++, buf++) {
+		u32 flash, buffer, erased_cw;
+		int data_len, oob_len;
+
+		if (i == (num_cw - 1)) {
+			data_len = NANDC_STEP_SIZE - ((num_cw - 1) << 2);
+			oob_len = num_cw << 2;
+		} else {
+			data_len = ecc_cfg->cw_data;
+			oob_len = 0;
+		}
+
+		flash = le32_to_cpu(buf->snandc_flash);
+		buffer = le32_to_cpu(buf->snandc_buffer);
+		erased_cw = le32_to_cpu(buf->snandc_erased_cw);
+
+		if ((flash & FS_OP_ERR) && (buffer & BS_UNCORRECTABLE_BIT)) {
+			if (ecc_cfg->bch_enabled)
+				erased = (erased_cw & ERASED_CW) == ERASED_CW;
+			else
+				erased = false;
+
+			if (!erased)
+				uncorrectable_cws |= BIT(i);
+
+		} else if (flash & (FS_OP_ERR | FS_MPU_ERR)) {
+			flash_op_err = true;
+		} else {
+			unsigned int stat;
+
+			stat = buffer & BS_CORRECTABLE_ERR_MSK;
+			snandc->qspi->ecc_stats.corrected += stat;
+			max_bitflips = max(max_bitflips, stat);
+		}
+
+		if (data_buf)
+			data_buf += data_len;
+		if (oob_buf)
+			oob_buf += oob_len + ecc_cfg->bytes;
+	}
+
+	if (flash_op_err)
+		return -EIO;
+
+	if (!uncorrectable_cws)
+		snandc->qspi->ecc_stats.bitflips = max_bitflips;
+	else
+		snandc->qspi->ecc_stats.failed++;
+
+	return 0;
+}
+
+static int qcom_spi_check_raw_flash_errors(struct qcom_nand_controller *snandc, int cw_cnt)
+{
+	int i;
+
+	qcom_nandc_dev_to_mem(snandc, true);
+
+	for (i = 0; i < cw_cnt; i++) {
+		u32 flash = le32_to_cpu(snandc->reg_read_buf[i]);
+
+		if (flash & (FS_OP_ERR | FS_MPU_ERR))
+			return -EIO;
+	}
+
+	return 0;
+}
+
+static int qcom_spi_read_cw_raw(struct qcom_nand_controller *snandc, u8 *data_buf,
+				u8 *oob_buf, int cw)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	struct mtd_info *mtd = snandc->qspi->mtd;
+	int data_size1, data_size2, oob_size1, oob_size2;
+	int ret, reg_off = FLASH_BUF_ACC, read_loc = 0;
+	int raw_cw = cw;
+	u32 cfg0, cfg1, ecc_bch_cfg, num_cw = snandc->qspi->num_cw;
+	int col;
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+	raw_cw = num_cw - 1;
+
+	cfg0 = (ecc_cfg->cfg0_raw & ~(7U << CW_PER_PAGE)) |
+				0 << CW_PER_PAGE;
+	cfg1 = ecc_cfg->cfg1_raw;
+	ecc_bch_cfg = ECC_CFG_ECC_DISABLE;
+
+	col = ecc_cfg->cw_size * cw;
+
+	snandc->regs->addr0 = (snandc->qspi->addr1 | cpu_to_le32(col));
+	snandc->regs->addr1 = snandc->qspi->addr2;
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->cfg0 = cpu_to_le32(cfg0);
+	snandc->regs->cfg1 = cpu_to_le32(cfg1);
+	snandc->regs->ecc_bch_cfg = cpu_to_le32(ecc_bch_cfg);
+	snandc->regs->clrflashstatus = cpu_to_le32(ecc_cfg->clrflashstatus);
+	snandc->regs->clrreadstatus = cpu_to_le32(ecc_cfg->clrreadstatus);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	qcom_spi_set_read_loc(snandc, raw_cw, 0, 0, ecc_cfg->cw_size, 1);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->addr0, NAND_ADDR0, 2, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->cfg0, NAND_DEV0_CFG0, 3, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->ecc_buf_cfg, NAND_EBI2_ECC_BUF_CFG, 1, 0);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_clr,
+			   NAND_ERASED_CW_DETECT_CFG, 1, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_set,
+			   NAND_ERASED_CW_DETECT_CFG, 1,
+			   NAND_ERASED_CW_SET | NAND_BAM_NEXT_SGL);
+
+	data_size1 = mtd->writesize - ecc_cfg->cw_size * (num_cw - 1);
+	oob_size1 = ecc_cfg->bbm_size;
+
+	if (cw == (num_cw - 1)) {
+		data_size2 = NANDC_STEP_SIZE - data_size1 -
+			     ((num_cw - 1) * 4);
+		oob_size2 = (num_cw * 4) + ecc_cfg->ecc_bytes_hw +
+			    ecc_cfg->spare_bytes;
+	} else {
+		data_size2 = ecc_cfg->cw_data - data_size1;
+		oob_size2 = ecc_cfg->ecc_bytes_hw + ecc_cfg->spare_bytes;
+	}
+
+	qcom_spi_set_read_loc(snandc, cw, 0, read_loc, data_size1, 0);
+	read_loc += data_size1;
+
+	qcom_spi_set_read_loc(snandc, cw, 1, read_loc, oob_size1, 0);
+	read_loc += oob_size1;
+
+	qcom_spi_set_read_loc(snandc, cw, 2, read_loc, data_size2, 0);
+	read_loc += data_size2;
+
+	qcom_spi_set_read_loc(snandc, cw, 3, read_loc, oob_size2, 1);
+
+	qcom_spi_config_cw_read(snandc, false, raw_cw);
+
+	qcom_read_data_dma(snandc, reg_off, data_buf, data_size1, 0);
+	reg_off += data_size1;
+
+	qcom_read_data_dma(snandc, reg_off, oob_buf, oob_size1, 0);
+	reg_off += oob_size1;
+
+	qcom_read_data_dma(snandc, reg_off, data_buf + data_size1, data_size2, 0);
+	reg_off += data_size2;
+
+	qcom_read_data_dma(snandc, reg_off, oob_buf + oob_size1, oob_size2, 0);
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure to read raw cw %d\n", cw);
+		return ret;
+	}
+
+	return qcom_spi_check_raw_flash_errors(snandc, 1);
+}
+
+static int qcom_spi_read_page_raw(struct qcom_nand_controller *snandc,
+				  const struct spi_mem_op *op)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	u8 *data_buf = NULL, *oob_buf = NULL;
+	int ret, cw;
+	u32 num_cw = snandc->qspi->num_cw;
+
+	if (snandc->qspi->page_rw)
+		data_buf = op->data.buf.in;
+
+	oob_buf = snandc->qspi->oob_buf;
+	memset(oob_buf, 0xff, OOB_BUF_SIZE);
+
+	for (cw = 0; cw < num_cw; cw++) {
+		ret = qcom_spi_read_cw_raw(snandc, data_buf, oob_buf, cw);
+		if (ret)
+			return ret;
+
+		if (data_buf)
+			data_buf += ecc_cfg->cw_data;
+		if (oob_buf)
+			oob_buf += ecc_cfg->bytes;
+	}
+
+	return 0;
+}
+
+static int qcom_spi_read_page_ecc(struct qcom_nand_controller *snandc,
+				  const struct spi_mem_op *op)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	u8 *data_buf = NULL, *data_buf_start, *oob_buf = NULL, *oob_buf_start;
+	int ret, i;
+	u32 cfg0, cfg1, ecc_bch_cfg, num_cw = snandc->qspi->num_cw;
+
+	data_buf = op->data.buf.in;
+	data_buf_start = data_buf;
+
+	oob_buf = snandc->qspi->oob_buf;
+	oob_buf_start = oob_buf;
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+
+	cfg0 = (ecc_cfg->cfg0 & ~(7U << CW_PER_PAGE)) |
+				(num_cw - 1) << CW_PER_PAGE;
+	cfg1 = ecc_cfg->cfg1;
+	ecc_bch_cfg = ecc_cfg->ecc_bch_cfg;
+
+	snandc->regs->addr0 = snandc->qspi->addr1;
+	snandc->regs->addr1 = snandc->qspi->addr2;
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->cfg0 = cpu_to_le32(cfg0);
+	snandc->regs->cfg1 = cpu_to_le32(cfg1);
+	snandc->regs->ecc_bch_cfg = cpu_to_le32(ecc_bch_cfg);
+	snandc->regs->clrflashstatus = cpu_to_le32(ecc_cfg->clrflashstatus);
+	snandc->regs->clrreadstatus = cpu_to_le32(ecc_cfg->clrreadstatus);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	qcom_spi_set_read_loc(snandc, 0, 0, 0, ecc_cfg->cw_data, 1);
+
+	qcom_clear_bam_transaction(snandc);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->addr0, NAND_ADDR0, 2, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->cfg0, NAND_DEV0_CFG0, 3, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_clr,
+			   NAND_ERASED_CW_DETECT_CFG, 1, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_set,
+			   NAND_ERASED_CW_DETECT_CFG, 1,
+			   NAND_ERASED_CW_SET | NAND_BAM_NEXT_SGL);
+
+	for (i = 0; i < num_cw; i++) {
+		int data_size, oob_size;
+
+		if (i == (num_cw - 1)) {
+			data_size = 512 - ((num_cw - 1) << 2);
+			oob_size = (num_cw << 2) + ecc_cfg->ecc_bytes_hw +
+				    ecc_cfg->spare_bytes;
+		} else {
+			data_size = ecc_cfg->cw_data;
+			oob_size = ecc_cfg->ecc_bytes_hw + ecc_cfg->spare_bytes;
+		}
+
+		if (data_buf && oob_buf) {
+			qcom_spi_set_read_loc(snandc, i, 0, 0, data_size, 0);
+			qcom_spi_set_read_loc(snandc, i, 1, data_size, oob_size, 1);
+		} else if (data_buf) {
+			qcom_spi_set_read_loc(snandc, i, 0, 0, data_size, 1);
+		} else {
+			qcom_spi_set_read_loc(snandc, i, 0, data_size, oob_size, 1);
+		}
+
+		qcom_spi_config_cw_read(snandc, true, i);
+
+		if (data_buf)
+			qcom_read_data_dma(snandc, FLASH_BUF_ACC, data_buf,
+					   data_size, 0);
+		if (oob_buf) {
+			int j;
+
+			for (j = 0; j < ecc_cfg->bbm_size; j++)
+				*oob_buf++ = 0xff;
+
+			qcom_read_data_dma(snandc, FLASH_BUF_ACC + data_size,
+					   oob_buf, oob_size, 0);
+		}
+
+		if (data_buf)
+			data_buf += data_size;
+		if (oob_buf)
+			oob_buf += oob_size;
+	}
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure to read page\n");
+		return ret;
+	}
+
+	return qcom_spi_check_error(snandc, data_buf_start, oob_buf_start);
+}
+
+static int qcom_spi_read_page_oob(struct qcom_nand_controller *snandc,
+				  const struct spi_mem_op *op)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	u8 *data_buf = NULL, *data_buf_start, *oob_buf = NULL, *oob_buf_start;
+	int ret, i;
+	u32 cfg0, cfg1, ecc_bch_cfg, num_cw = snandc->qspi->num_cw;
+
+	oob_buf = op->data.buf.in;
+	oob_buf_start = oob_buf;
+
+	data_buf_start = data_buf;
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+
+	cfg0 = (ecc_cfg->cfg0 & ~(7U << CW_PER_PAGE)) |
+				(num_cw - 1) << CW_PER_PAGE;
+	cfg1 = ecc_cfg->cfg1;
+	ecc_bch_cfg = ecc_cfg->ecc_bch_cfg;
+
+	snandc->regs->addr0 = snandc->qspi->addr1;
+	snandc->regs->addr1 = snandc->qspi->addr2;
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->cfg0 = cpu_to_le32(cfg0);
+	snandc->regs->cfg1 = cpu_to_le32(cfg1);
+	snandc->regs->ecc_bch_cfg = cpu_to_le32(ecc_bch_cfg);
+	snandc->regs->clrflashstatus = cpu_to_le32(ecc_cfg->clrflashstatus);
+	snandc->regs->clrreadstatus = cpu_to_le32(ecc_cfg->clrreadstatus);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	qcom_spi_set_read_loc(snandc, 0, 0, 0, ecc_cfg->cw_data, 1);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->addr0, NAND_ADDR0, 2, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->cfg0, NAND_DEV0_CFG0, 3, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_clr,
+			   NAND_ERASED_CW_DETECT_CFG, 1, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->erased_cw_detect_cfg_set,
+			   NAND_ERASED_CW_DETECT_CFG, 1,
+			   NAND_ERASED_CW_SET | NAND_BAM_NEXT_SGL);
+
+	for (i = 0; i < num_cw; i++) {
+		int data_size, oob_size;
+
+		if (i == (num_cw - 1)) {
+			data_size = NANDC_STEP_SIZE - ((num_cw - 1) << 2);
+			oob_size = (num_cw << 2) + ecc_cfg->ecc_bytes_hw +
+				    ecc_cfg->spare_bytes;
+		} else {
+			data_size = ecc_cfg->cw_data;
+			oob_size = ecc_cfg->ecc_bytes_hw + ecc_cfg->spare_bytes;
+		}
+
+		qcom_spi_set_read_loc(snandc, i, 0, data_size, oob_size, 1);
+
+		qcom_spi_config_cw_read(snandc, true, i);
+
+		if (oob_buf) {
+			int j;
+
+			for (j = 0; j < ecc_cfg->bbm_size; j++)
+				*oob_buf++ = 0xff;
+
+			qcom_read_data_dma(snandc, FLASH_BUF_ACC + data_size,
+					   oob_buf, oob_size, 0);
+		}
+
+		if (oob_buf)
+			oob_buf += oob_size;
+	}
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure to read oob\n");
+		return ret;
+	}
+
+	return qcom_spi_check_error(snandc, data_buf_start, oob_buf_start);
+}
+
+static int qcom_spi_read_page(struct qcom_nand_controller *snandc,
+			      const struct spi_mem_op *op)
+{
+	if (snandc->qspi->page_rw && snandc->qspi->raw_rw)
+		return qcom_spi_read_page_raw(snandc, op);
+
+	if (snandc->qspi->page_rw)
+		return qcom_spi_read_page_ecc(snandc, op);
+
+	if (snandc->qspi->oob_rw && snandc->qspi->raw_rw)
+		return qcom_spi_read_last_cw(snandc, op);
+
+	if (snandc->qspi->oob_rw)
+		return qcom_spi_read_page_oob(snandc, op);
+
+	return 0;
+}
+
+static void qcom_spi_config_page_write(struct qcom_nand_controller *snandc)
+{
+	qcom_write_reg_dma(snandc, &snandc->regs->addr0, NAND_ADDR0, 2, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->cfg0, NAND_DEV0_CFG0, 3, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->ecc_buf_cfg, NAND_EBI2_ECC_BUF_CFG,
+			   1, NAND_BAM_NEXT_SGL);
+}
+
+static void qcom_spi_config_cw_write(struct qcom_nand_controller *snandc)
+{
+	qcom_write_reg_dma(snandc, &snandc->regs->cmd, NAND_FLASH_CMD, 1, NAND_BAM_NEXT_SGL);
+	qcom_write_reg_dma(snandc, &snandc->regs->exec, NAND_EXEC_CMD, 1, NAND_BAM_NEXT_SGL);
+	qcom_read_reg_dma(snandc, NAND_FLASH_STATUS, 1, NAND_BAM_NEXT_SGL);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->clrflashstatus, NAND_FLASH_STATUS, 1, 0);
+	qcom_write_reg_dma(snandc, &snandc->regs->clrreadstatus, NAND_READ_STATUS, 1,
+			   NAND_BAM_NEXT_SGL);
+}
+
+static int qcom_spi_program_raw(struct qcom_nand_controller *snandc,
+				const struct spi_mem_op *op)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	struct mtd_info *mtd = snandc->qspi->mtd;
+	u8 *data_buf = NULL, *oob_buf = NULL;
+	int i, ret;
+	int num_cw = snandc->qspi->num_cw;
+	u32 cfg0, cfg1, ecc_bch_cfg;
+
+	cfg0 = (ecc_cfg->cfg0_raw & ~(7U << CW_PER_PAGE)) |
+			(num_cw - 1) << CW_PER_PAGE;
+	cfg1 = ecc_cfg->cfg1_raw;
+	ecc_bch_cfg = ECC_CFG_ECC_DISABLE;
+
+	data_buf = snandc->qspi->data_buf;
+
+	oob_buf = snandc->qspi->oob_buf;
+	memset(oob_buf, 0xff, OOB_BUF_SIZE);
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+
+	snandc->regs->addr0 = snandc->qspi->addr1;
+	snandc->regs->addr1 = snandc->qspi->addr2;
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->cfg0 = cpu_to_le32(cfg0);
+	snandc->regs->cfg1 = cpu_to_le32(cfg1);
+	snandc->regs->ecc_bch_cfg = cpu_to_le32(ecc_bch_cfg);
+	snandc->regs->clrflashstatus = cpu_to_le32(ecc_cfg->clrflashstatus);
+	snandc->regs->clrreadstatus = cpu_to_le32(ecc_cfg->clrreadstatus);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	qcom_spi_config_page_write(snandc);
+
+	for (i = 0; i < num_cw; i++) {
+		int data_size1, data_size2, oob_size1, oob_size2;
+		int reg_off = FLASH_BUF_ACC;
+
+		data_size1 = mtd->writesize - ecc_cfg->cw_size * (num_cw - 1);
+		oob_size1 = ecc_cfg->bbm_size;
+
+		if (i == (num_cw - 1)) {
+			data_size2 = NANDC_STEP_SIZE - data_size1 -
+				     ((num_cw - 1) << 2);
+			oob_size2 = (num_cw << 2) + ecc_cfg->ecc_bytes_hw +
+				    ecc_cfg->spare_bytes;
+		} else {
+			data_size2 = ecc_cfg->cw_data - data_size1;
+			oob_size2 = ecc_cfg->ecc_bytes_hw + ecc_cfg->spare_bytes;
+		}
+
+		qcom_write_data_dma(snandc, reg_off, data_buf, data_size1,
+				    NAND_BAM_NO_EOT);
+		reg_off += data_size1;
+		data_buf += data_size1;
+
+		qcom_write_data_dma(snandc, reg_off, oob_buf, oob_size1,
+				    NAND_BAM_NO_EOT);
+		oob_buf += oob_size1;
+		reg_off += oob_size1;
+
+		qcom_write_data_dma(snandc, reg_off, data_buf, data_size2,
+				    NAND_BAM_NO_EOT);
+		reg_off += data_size2;
+		data_buf += data_size2;
+
+		qcom_write_data_dma(snandc, reg_off, oob_buf, oob_size2, 0);
+		oob_buf += oob_size2;
+
+		qcom_spi_config_cw_write(snandc);
+	}
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure to write raw page\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static int qcom_spi_program_ecc(struct qcom_nand_controller *snandc,
+				const struct spi_mem_op *op)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	u8 *data_buf = NULL, *oob_buf = NULL;
+	int i, ret;
+	int num_cw = snandc->qspi->num_cw;
+	u32 cfg0, cfg1, ecc_bch_cfg, ecc_buf_cfg;
+
+	cfg0 = (ecc_cfg->cfg0 & ~(7U << CW_PER_PAGE)) |
+				(num_cw - 1) << CW_PER_PAGE;
+	cfg1 = ecc_cfg->cfg1;
+	ecc_bch_cfg = ecc_cfg->ecc_bch_cfg;
+	ecc_buf_cfg = ecc_cfg->ecc_buf_cfg;
+
+	if (snandc->qspi->data_buf)
+		data_buf = snandc->qspi->data_buf;
+
+	oob_buf = snandc->qspi->oob_buf;
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+
+	snandc->regs->addr0 = snandc->qspi->addr1;
+	snandc->regs->addr1 = snandc->qspi->addr2;
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->cfg0 = cpu_to_le32(cfg0);
+	snandc->regs->cfg1 = cpu_to_le32(cfg1);
+	snandc->regs->ecc_bch_cfg = cpu_to_le32(ecc_bch_cfg);
+	snandc->regs->ecc_buf_cfg = cpu_to_le32(ecc_buf_cfg);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	qcom_spi_config_page_write(snandc);
+
+	for (i = 0; i < num_cw; i++) {
+		int data_size, oob_size;
+
+		if (i == (num_cw - 1)) {
+			data_size = NANDC_STEP_SIZE - ((num_cw - 1) << 2);
+			oob_size = (num_cw << 2) + ecc_cfg->ecc_bytes_hw +
+				    ecc_cfg->spare_bytes;
+		} else {
+			data_size = ecc_cfg->cw_data;
+			oob_size = ecc_cfg->bytes;
+		}
+
+		if (data_buf)
+			qcom_write_data_dma(snandc, FLASH_BUF_ACC, data_buf, data_size,
+					    i == (num_cw - 1) ? NAND_BAM_NO_EOT : 0);
+
+		if (i == (num_cw - 1)) {
+			if (oob_buf) {
+				oob_buf += ecc_cfg->bbm_size;
+				qcom_write_data_dma(snandc, FLASH_BUF_ACC + data_size,
+						    oob_buf, oob_size, 0);
+			}
+		}
+
+		qcom_spi_config_cw_write(snandc);
+
+		if (data_buf)
+			data_buf += data_size;
+		if (oob_buf)
+			oob_buf += oob_size;
+	}
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure to write page\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static int qcom_spi_program_oob(struct qcom_nand_controller *snandc,
+				const struct spi_mem_op *op)
+{
+	struct qpic_ecc *ecc_cfg = snandc->qspi->ecc;
+	u8 *oob_buf = NULL;
+	int ret, col, data_size, oob_size;
+	int num_cw = snandc->qspi->num_cw;
+	u32 cfg0, cfg1, ecc_bch_cfg, ecc_buf_cfg;
+
+	cfg0 = (ecc_cfg->cfg0 & ~(7U << CW_PER_PAGE)) |
+				(num_cw - 1) << CW_PER_PAGE;
+	cfg1 = ecc_cfg->cfg1;
+	ecc_bch_cfg = ecc_cfg->ecc_bch_cfg;
+	ecc_buf_cfg = ecc_cfg->ecc_buf_cfg;
+
+	col = ecc_cfg->cw_size * (num_cw - 1);
+
+	oob_buf = snandc->qspi->data_buf;
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+	snandc->regs->addr0 = (snandc->qspi->addr1 | cpu_to_le32(col));
+	snandc->regs->addr1 = snandc->qspi->addr2;
+	snandc->regs->cmd = snandc->qspi->cmd;
+	snandc->regs->cfg0 = cpu_to_le32(cfg0);
+	snandc->regs->cfg1 = cpu_to_le32(cfg1);
+	snandc->regs->ecc_bch_cfg = cpu_to_le32(ecc_bch_cfg);
+	snandc->regs->ecc_buf_cfg = cpu_to_le32(ecc_buf_cfg);
+	snandc->regs->exec = cpu_to_le32(1);
+
+	/* calculate the data and oob size for the last codeword/step */
+	data_size = NANDC_STEP_SIZE - ((num_cw - 1) << 2);
+	oob_size = snandc->qspi->mtd->oobavail;
+
+	memset(snandc->data_buffer, 0xff, ecc_cfg->cw_data);
+	/* override new oob content to last codeword */
+	mtd_ooblayout_get_databytes(snandc->qspi->mtd, snandc->data_buffer + data_size,
+				    oob_buf, 0, snandc->qspi->mtd->oobavail);
+	qcom_spi_config_page_write(snandc);
+	qcom_write_data_dma(snandc, FLASH_BUF_ACC, snandc->data_buffer, data_size + oob_size, 0);
+	qcom_spi_config_cw_write(snandc);
+
+	ret = qcom_submit_descs(snandc);
+	if (ret) {
+		dev_err(snandc->dev, "failure to write oob\n");
+		return ret;
+	}
+
+	return 0;
+}
+
+static int qcom_spi_program_execute(struct qcom_nand_controller *snandc,
+				    const struct spi_mem_op *op)
+{
+	if (snandc->qspi->page_rw && snandc->qspi->raw_rw)
+		return qcom_spi_program_raw(snandc, op);
+
+	if (snandc->qspi->page_rw)
+		return qcom_spi_program_ecc(snandc, op);
+
+	if (snandc->qspi->oob_rw)
+		return qcom_spi_program_oob(snandc, op);
+
+	return 0;
+}
+
+static int qcom_spi_cmd_mapping(struct qcom_nand_controller *snandc, u32 opcode)
+{
+	int cmd = 0x0;
+
+	switch (opcode) {
+	case SPINAND_RESET:
+		cmd = (SPI_WP | SPI_HOLD | SPI_TRANSFER_MODE_x1 | OP_RESET_DEVICE);
+		break;
+	case SPINAND_READID:
+		cmd = (SPI_WP | SPI_HOLD | SPI_TRANSFER_MODE_x1 | OP_FETCH_ID);
+		break;
+	case SPINAND_GET_FEATURE:
+		cmd = (SPI_TRANSFER_MODE_x1 | SPI_WP | SPI_HOLD | ACC_FEATURE);
+		break;
+	case SPINAND_SET_FEATURE:
+		cmd = (SPI_TRANSFER_MODE_x1 | SPI_WP | SPI_HOLD | ACC_FEATURE |
+			QPIC_SET_FEATURE);
+		break;
+	case SPINAND_READ:
+		if (snandc->qspi->raw_rw) {
+			cmd = (PAGE_ACC | LAST_PAGE | SPI_TRANSFER_MODE_x1 |
+					SPI_WP | SPI_HOLD | OP_PAGE_READ);
+		} else {
+			cmd = (PAGE_ACC | LAST_PAGE | SPI_TRANSFER_MODE_x1 |
+					SPI_WP | SPI_HOLD | OP_PAGE_READ_WITH_ECC);
+		}
+
+		break;
+	case SPINAND_ERASE:
+		cmd = OP_BLOCK_ERASE | PAGE_ACC | LAST_PAGE | SPI_WP |
+			SPI_HOLD | SPI_TRANSFER_MODE_x1;
+		break;
+	case SPINAND_WRITE_EN:
+		cmd = SPINAND_WRITE_EN;
+		break;
+	case SPINAND_PROGRAM_EXECUTE:
+		cmd = (PAGE_ACC | LAST_PAGE | SPI_TRANSFER_MODE_x1 |
+				SPI_WP | SPI_HOLD | OP_PROGRAM_PAGE);
+		break;
+	case SPINAND_PROGRAM_LOAD:
+		cmd = SPINAND_PROGRAM_LOAD;
+		break;
+	default:
+		dev_err(snandc->dev, "Opcode not supported: %u\n", opcode);
+		return -EOPNOTSUPP;
+	}
+
+	return cmd;
+}
+
+static int qcom_spi_write_page(struct qcom_nand_controller *snandc,
+			       const struct spi_mem_op *op)
+{
+	int cmd;
+
+	cmd = qcom_spi_cmd_mapping(snandc, op->cmd.opcode);
+	if (cmd < 0)
+		return cmd;
+
+	if (op->cmd.opcode == SPINAND_PROGRAM_LOAD)
+		snandc->qspi->data_buf = (u8 *)op->data.buf.out;
+
+	return 0;
+}
+
+static int qcom_spi_send_cmdaddr(struct qcom_nand_controller *snandc,
+				 const struct spi_mem_op *op)
+{
+	struct qpic_snand_op s_op = {};
+	u32 cmd;
+	int ret, opcode;
+
+	ret = qcom_spi_cmd_mapping(snandc, op->cmd.opcode);
+	if (ret < 0)
+		return ret;
+
+	cmd = ret;
+
+	s_op.cmd_reg = cmd;
+	s_op.addr1_reg = op->addr.val;
+	s_op.addr2_reg = 0;
+
+	opcode = op->cmd.opcode;
+
+	switch (opcode) {
+	case SPINAND_WRITE_EN:
+		return 0;
+	case SPINAND_PROGRAM_EXECUTE:
+		s_op.addr1_reg = op->addr.val << 16;
+		s_op.addr2_reg = op->addr.val >> 16 & 0xff;
+		snandc->qspi->addr1 = cpu_to_le32(s_op.addr1_reg);
+		snandc->qspi->addr2 = cpu_to_le32(s_op.addr2_reg);
+		snandc->qspi->cmd = cpu_to_le32(cmd);
+		return qcom_spi_program_execute(snandc, op);
+	case SPINAND_READ:
+		s_op.addr1_reg = (op->addr.val << 16);
+		s_op.addr2_reg = op->addr.val >> 16 & 0xff;
+		snandc->qspi->addr1 = cpu_to_le32(s_op.addr1_reg);
+		snandc->qspi->addr2 = cpu_to_le32(s_op.addr2_reg);
+		snandc->qspi->cmd = cpu_to_le32(cmd);
+		return 0;
+	case SPINAND_ERASE:
+		s_op.addr2_reg = (op->addr.val >> 16) & 0xffff;
+		s_op.addr1_reg = op->addr.val;
+		snandc->qspi->addr1 = cpu_to_le32(s_op.addr1_reg << 16);
+		snandc->qspi->addr2 = cpu_to_le32(s_op.addr2_reg);
+		snandc->qspi->cmd = cpu_to_le32(cmd);
+		qcom_spi_block_erase(snandc);
+		return 0;
+	default:
+		break;
+	}
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+
+	snandc->regs->cmd = cpu_to_le32(s_op.cmd_reg);
+	snandc->regs->exec = cpu_to_le32(1);
+	snandc->regs->addr0 = cpu_to_le32(s_op.addr1_reg);
+	snandc->regs->addr1 = cpu_to_le32(s_op.addr2_reg);
+
+	qcom_write_reg_dma(snandc, &snandc->regs->cmd, NAND_FLASH_CMD, 3, NAND_BAM_NEXT_SGL);
+	qcom_write_reg_dma(snandc, &snandc->regs->exec, NAND_EXEC_CMD, 1, NAND_BAM_NEXT_SGL);
+
+	ret = qcom_submit_descs(snandc);
+	if (ret)
+		dev_err(snandc->dev, "failure in submitting cmd descriptor\n");
+
+	return ret;
+}
+
+static int qcom_spi_io_op(struct qcom_nand_controller *snandc, const struct spi_mem_op *op)
+{
+	int ret, val, opcode;
+	bool copy = false, copy_ftr = false;
+
+	ret = qcom_spi_send_cmdaddr(snandc, op);
+	if (ret)
+		return ret;
+
+	snandc->buf_count = 0;
+	snandc->buf_start = 0;
+	qcom_clear_read_regs(snandc);
+	qcom_clear_bam_transaction(snandc);
+	opcode = op->cmd.opcode;
+
+	switch (opcode) {
+	case SPINAND_READID:
+		snandc->buf_count = 4;
+		qcom_read_reg_dma(snandc, NAND_READ_ID, 1, NAND_BAM_NEXT_SGL);
+		copy = true;
+		break;
+	case SPINAND_GET_FEATURE:
+		snandc->buf_count = 4;
+		qcom_read_reg_dma(snandc, NAND_FLASH_FEATURES, 1, NAND_BAM_NEXT_SGL);
+		copy_ftr = true;
+		break;
+	case SPINAND_SET_FEATURE:
+		snandc->regs->flash_feature = cpu_to_le32(*(u32 *)op->data.buf.out);
+		qcom_write_reg_dma(snandc, &snandc->regs->flash_feature,
+				   NAND_FLASH_FEATURES, 1, NAND_BAM_NEXT_SGL);
+		break;
+	case SPINAND_PROGRAM_EXECUTE:
+	case SPINAND_WRITE_EN:
+	case SPINAND_RESET:
+	case SPINAND_ERASE:
+	case SPINAND_READ:
+		return 0;
+	default:
+		return -EOPNOTSUPP;
+	}
+
+	ret = qcom_submit_descs(snandc);
+	if (ret)
+		dev_err(snandc->dev, "failure in submitting descriptor for:%d\n", opcode);
+
+	if (copy) {
+		qcom_nandc_dev_to_mem(snandc, true);
+		memcpy(op->data.buf.in, snandc->reg_read_buf, snandc->buf_count);
+	}
+
+	if (copy_ftr) {
+		qcom_nandc_dev_to_mem(snandc, true);
+		val = le32_to_cpu(*(__le32 *)snandc->reg_read_buf);
+		val >>= 8;
+		memcpy(op->data.buf.in, &val, snandc->buf_count);
+	}
+
+	return ret;
+}
+
+static bool qcom_spi_is_page_op(const struct spi_mem_op *op)
+{
+	if (op->addr.buswidth != 1 && op->addr.buswidth != 2 && op->addr.buswidth != 4)
+		return false;
+
+	if (op->data.dir == SPI_MEM_DATA_IN) {
+		if (op->addr.buswidth == 4 && op->data.buswidth == 4)
+			return true;
+
+		if (op->addr.nbytes == 2 && op->addr.buswidth == 1)
+			return true;
+
+	} else if (op->data.dir == SPI_MEM_DATA_OUT) {
+		if (op->data.buswidth == 4)
+			return true;
+		if (op->addr.nbytes == 2 && op->addr.buswidth == 1)
+			return true;
+	}
+
+	return false;
+}
+
+static bool qcom_spi_supports_op(struct spi_mem *mem, const struct spi_mem_op *op)
+{
+	if (!spi_mem_default_supports_op(mem, op))
+		return false;
+
+	if (op->cmd.nbytes != 1 || op->cmd.buswidth != 1)
+		return false;
+
+	if (qcom_spi_is_page_op(op))
+		return true;
+
+	return ((!op->addr.nbytes || op->addr.buswidth == 1) &&
+		(!op->dummy.nbytes || op->dummy.buswidth == 1) &&
+		(!op->data.nbytes || op->data.buswidth == 1));
+}
+
+static int qcom_spi_exec_op(struct spi_mem *mem, const struct spi_mem_op *op)
+{
+	struct qcom_nand_controller *snandc = spi_controller_get_devdata(mem->spi->controller);
+
+	dev_dbg(snandc->dev, "OP %02x ADDR %08llX@%d:%u DATA %d:%u", op->cmd.opcode,
+		op->addr.val, op->addr.buswidth, op->addr.nbytes,
+		op->data.buswidth, op->data.nbytes);
+
+	if (qcom_spi_is_page_op(op)) {
+		if (op->data.dir == SPI_MEM_DATA_IN)
+			return qcom_spi_read_page(snandc, op);
+		if (op->data.dir == SPI_MEM_DATA_OUT)
+			return qcom_spi_write_page(snandc, op);
+	} else {
+		return qcom_spi_io_op(snandc, op);
+	}
+
+	return 0;
+}
+
+static const struct spi_controller_mem_ops qcom_spi_mem_ops = {
+	.supports_op = qcom_spi_supports_op,
+	.exec_op = qcom_spi_exec_op,
+};
+
+static const struct spi_controller_mem_caps qcom_spi_mem_caps = {
+	.ecc = true,
+};
+
+static int qcom_spi_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct spi_controller *ctlr;
+	struct qcom_nand_controller *snandc;
+	struct qpic_spi_nand *qspi;
+	struct qpic_ecc *ecc;
+	struct resource *res;
+	const void *dev_data;
+	int ret;
+
+	ecc = devm_kzalloc(dev, sizeof(*ecc), GFP_KERNEL);
+	if (!ecc)
+		return -ENOMEM;
+
+	qspi = devm_kzalloc(dev, sizeof(*qspi), GFP_KERNEL);
+	if (!qspi)
+		return -ENOMEM;
+
+	ctlr = __devm_spi_alloc_controller(dev, sizeof(*snandc), false);
+	if (!ctlr)
+		return -ENOMEM;
+
+	platform_set_drvdata(pdev, ctlr);
+
+	snandc = spi_controller_get_devdata(ctlr);
+	qspi->snandc = snandc;
+
+	snandc->dev = dev;
+	snandc->qspi = qspi;
+	snandc->qspi->ctlr = ctlr;
+	snandc->qspi->ecc = ecc;
+
+	dev_data = of_device_get_match_data(dev);
+	if (!dev_data) {
+		dev_err(&pdev->dev, "failed to get device data\n");
+		return -ENODEV;
+	}
+
+	snandc->props = dev_data;
+	snandc->dev = &pdev->dev;
+
+	snandc->core_clk = devm_clk_get(dev, "core");
+	if (IS_ERR(snandc->core_clk))
+		return PTR_ERR(snandc->core_clk);
+
+	snandc->aon_clk = devm_clk_get(dev, "aon");
+	if (IS_ERR(snandc->aon_clk))
+		return PTR_ERR(snandc->aon_clk);
+
+	snandc->qspi->iomacro_clk = devm_clk_get(dev, "iom");
+	if (IS_ERR(snandc->qspi->iomacro_clk))
+		return PTR_ERR(snandc->qspi->iomacro_clk);
+
+	snandc->base = devm_platform_get_and_ioremap_resource(pdev, 0, &res);
+	if (IS_ERR(snandc->base))
+		return PTR_ERR(snandc->base);
+
+	snandc->base_phys = res->start;
+	snandc->base_dma = dma_map_resource(dev, res->start, resource_size(res),
+					    DMA_BIDIRECTIONAL, 0);
+	if (dma_mapping_error(dev, snandc->base_dma))
+		return -ENXIO;
+
+	ret = clk_prepare_enable(snandc->core_clk);
+	if (ret)
+		goto err_dis_core_clk;
+
+	ret = clk_prepare_enable(snandc->aon_clk);
+	if (ret)
+		goto err_dis_aon_clk;
+
+	ret = clk_prepare_enable(snandc->qspi->iomacro_clk);
+	if (ret)
+		goto err_dis_iom_clk;
+
+	ret = qcom_nandc_alloc(snandc);
+	if (ret)
+		goto err_snand_alloc;
+
+	ret = qcom_spi_init(snandc);
+	if (ret)
+		goto err_spi_init;
+
+	/* setup ECC engine */
+	snandc->qspi->ecc_eng.dev = &pdev->dev;
+	snandc->qspi->ecc_eng.integration = NAND_ECC_ENGINE_INTEGRATION_PIPELINED;
+	snandc->qspi->ecc_eng.ops = &qcom_spi_ecc_engine_ops_pipelined;
+	snandc->qspi->ecc_eng.priv = snandc;
+
+	ret = nand_ecc_register_on_host_hw_engine(&snandc->qspi->ecc_eng);
+	if (ret) {
+		dev_err(&pdev->dev, "failed to register ecc engine:%d\n", ret);
+		goto err_spi_init;
+	}
+
+	ctlr->num_chipselect = QPIC_QSPI_NUM_CS;
+	ctlr->mem_ops = &qcom_spi_mem_ops;
+	ctlr->mem_caps = &qcom_spi_mem_caps;
+	ctlr->dev.of_node = pdev->dev.of_node;
+	ctlr->mode_bits = SPI_TX_DUAL | SPI_RX_DUAL |
+			    SPI_TX_QUAD | SPI_RX_QUAD;
+
+	ret = spi_register_controller(ctlr);
+	if (ret) {
+		dev_err(&pdev->dev, "spi_register_controller failed.\n");
+		goto err_spi_init;
+	}
+
+	return 0;
+
+err_spi_init:
+	qcom_nandc_unalloc(snandc);
+err_snand_alloc:
+	clk_disable_unprepare(snandc->qspi->iomacro_clk);
+err_dis_iom_clk:
+	clk_disable_unprepare(snandc->aon_clk);
+err_dis_aon_clk:
+	clk_disable_unprepare(snandc->core_clk);
+err_dis_core_clk:
+	dma_unmap_resource(dev, res->start, resource_size(res),
+			   DMA_BIDIRECTIONAL, 0);
+	return ret;
+}
+
+static void qcom_spi_remove(struct platform_device *pdev)
+{
+	struct spi_controller *ctlr = platform_get_drvdata(pdev);
+	struct qcom_nand_controller *snandc = spi_controller_get_devdata(ctlr);
+	struct resource *res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+
+	spi_unregister_controller(ctlr);
+
+	qcom_nandc_unalloc(snandc);
+
+	clk_disable_unprepare(snandc->aon_clk);
+	clk_disable_unprepare(snandc->core_clk);
+	clk_disable_unprepare(snandc->qspi->iomacro_clk);
+
+	dma_unmap_resource(&pdev->dev, snandc->base_dma, resource_size(res),
+			   DMA_BIDIRECTIONAL, 0);
+}
+
+static const struct qcom_nandc_props ipq9574_snandc_props = {
+	.dev_cmd_reg_start = 0x7000,
+	.supports_bam = true,
+};
+
+static const struct of_device_id qcom_snandc_of_match[] = {
+	{
+		.compatible = "qcom,ipq9574-snand",
+		.data = &ipq9574_snandc_props,
+	},
+	{}
+}
+MODULE_DEVICE_TABLE(of, qcom_snandc_of_match);
+
+static struct platform_driver qcom_spi_driver = {
+	.driver = {
+		.name		= "qcom_snand",
+		.of_match_table = qcom_snandc_of_match,
+	},
+	.probe = qcom_spi_probe,
+	.remove_new = qcom_spi_remove,
+};
+module_platform_driver(qcom_spi_driver);
+
+MODULE_DESCRIPTION("SPI driver for QPIC QSPI cores");
+MODULE_AUTHOR("Md Sadre Alam <quic_mdalam@quicinc.com>");
+MODULE_LICENSE("GPL");
+
--- a/include/linux/mtd/nand-qpic-common.h
+++ b/include/linux/mtd/nand-qpic-common.h
@@ -325,6 +325,10 @@ struct nandc_regs {
 	__le32 read_location_last1;
 	__le32 read_location_last2;
 	__le32 read_location_last3;
+	__le32 spi_cfg;
+	__le32 num_addr_cycle;
+	__le32 busy_wait_cnt;
+	__le32 flash_feature;
 
 	__le32 erased_cw_detect_cfg_clr;
 	__le32 erased_cw_detect_cfg_set;
@@ -339,6 +343,7 @@ struct nandc_regs {
  *
  * @core_clk:			controller clock
  * @aon_clk:			another controller clock
+ * @iomacro_clk:		io macro clock
  *
  * @regs:			a contiguous chunk of memory for DMA register
  *				writes. contains the register values to be
@@ -348,6 +353,7 @@ struct nandc_regs {
  *				initialized via DT match data
  *
  * @controller:			base controller structure
+ * @qspi:			qpic spi structure
  * @host_list:			list containing all the chips attached to the
  *				controller
  *
@@ -392,6 +398,7 @@ struct qcom_nand_controller {
 	const struct qcom_nandc_props *props;
 
 	struct nand_controller *controller;
+	struct qpic_spi_nand *qspi;
 	struct list_head host_list;
 
 	union {
