// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include "armada-385.dtsi"

/ {
	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_red;
		led-running = &led_status_green;
		led-upgrade = &led_status_green;
		label-mac-device = &eth0;
	};

	chosen {
		stdout-path = "serial0:9600n8";
	};

	soc {
		ranges = <MBUS_ID(0xf0, 0x01) 0 0xf1000000 0x100000
			  MBUS_ID(0x01, 0x1d) 0 0xfff00000 0x100000
			  MBUS_ID(0x09, 0x19) 0 0xf1100000 0x10000
			  MBUS_ID(0x09, 0x15) 0 0xf1110000 0x10000
			  MBUS_ID(0x0c, 0x04) 0 0xf1200000 0x100000>;
	};

	gpio-keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&pmx_gpio_keys_pins>;

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio1 22 GPIO_ACTIVE_LOW>;
		};
	};

	gpio_leds: gpio-leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&pmx_gpio_leds_pins>;

		led-0 {
			gpios = <&gpio0 30 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_ALARM;
		};

		led-1 {
			gpios = <&gpio1 0 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = "ha";
		};

		led_status_green: led-2 {
			gpios = <&gpio1 1 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
		};

		led-3 {
			gpios = <&gpio1 3 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = "ha";
		};

		led-4 {
			gpios = <&gpio1 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_ALARM;
		};

		led_status_red: led-5 {
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
		};

		led-6 {
			gpios = <&gpio2 4 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <4>;
			linux,default-trigger = "mv88e6xxx-0:01:1Gbps";
		};

		led-7 {
			gpios = <&gpio2 5 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <4>;
			linux,default-trigger = "mv88e6xxx-0:01:100Mbps";
		};

		led-8 {
			gpios = <&gpio2 6 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <3>;
			linux,default-trigger = "mv88e6xxx-0:02:100Mbps";
		};

		led-9 {
			gpios = <&gpio2 7 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <3>;
			linux,default-trigger = "mv88e6xxx-0:02:1Gbps";
		};

		led-10 {
			gpios = <&gpio2 12 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <1>;
			linux,default-trigger = "mv88e6xxx-0:04:1Gbps";
		};

		led-11 {
			gpios = <&gpio2 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <1>;
			linux,default-trigger = "mv88e6xxx-0:04:100Mbps";
		};

		led-12 {
			gpios = <&gpio2 14 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <2>;
			linux,default-trigger = "mv88e6xxx-0:03:1Gbps";
		};

		led-13 {
			gpios = <&gpio2 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_AMBER>;
			function = LED_FUNCTION_SPEED_LAN;
			function-enumerator = <2>;
			linux,default-trigger = "mv88e6xxx-0:03:100Mbps";
		};
	};

	reg_usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb-vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpios = <&gpio1 21 GPIO_ACTIVE_LOW>;
		regulator-always-on;
	};
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins>;
	status = "okay";

	gpio2: gpio@24 {
		compatible = "nxp,pca9555";
		reg = <0x24>;
		gpio-controller;
		#gpio-cells = <0x2>;
	};

	hwmon@28 {
		compatible = "nuvoton,nct7802";
		reg = <0x28>;
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins>;
	status = "okay";
};

&pinctrl {
	pmx_gpio_leds_pins: gpio-leds-pins {
		marvell,pins = "mpp30", "mpp32", "mpp33", "mpp35",
			       "mpp45", "mpp47";
		marvell,function = "gpio";
	};

	pmx_usb_pins: usb-pins {
		marvell,pins = "mpp53";
		marvell,function = "gpio";
	};

	pmx_gpio_keys_pins: gpio-keys-pins {
		marvell,pins = "mpp54";
		marvell,function = "gpio";
	};
};

&bm {
	status = "okay";
};

&bm_bppi {
	status = "okay";
};

&eth0 {
	pinctrl-names = "default";
	pinctrl-0 = <&ge0_rgmii_pins>;
	status = "okay";

	phy-connection-type = "rgmii-id";
	buffer-manager = <&bm>;
	bm,pool-long = <0>;
	bm,pool-short = <1>;
	nvmem-cells = <&macaddr_bdinfo_d880 0>;
	nvmem-cell-names = "mac-address";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&usb3_0 {
	pinctrl-names = "default";
	pinctrl-0 = <&pmx_usb_pins>;
	status = "okay";

	vbus-supply = <&reg_usb_vbus>;
};

&spi1 {
	pinctrl-names = "default";
	pinctrl-0 = <&spi1_pins>;
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x1c0000>;
				label = "u-boot";
				read-only;
			};

			partition@1c0000 {
				reg = <0x1c0000 0x10000>;
				label = "firmware-info";

				/*
				 *  0x10 - 0x2f : image name (image1)
				 *  0x30 - 0x4f : image name (image2)
				 * 0x170 (1byte): active image (0x0/0x1)
				 * 0x184 - 0x185: kernel block count (image1)
				 * 0x18c - 0x18d: rootfs block count (image1)
				 * 0x194 - 0x195: kernel block count (image2)
				 * 0x19c - 0x19d: rootfs block count (image2)
				 * 0x1be (1byte): bit7 -> active flag (image1)?
				 * 0x1ce (1byte): bit7 -> active flag (image2)?
				 *
				 * Note: block size --> 0x200 (512 bytes)
				 */
			};

			partition@1d0000 {
				reg = <0x1d0000 0x10000>;
				label = "dtb";
				read-only;
			};

			partition@1e0000 {
				reg = <0x1e0000 0x10000>;
				label = "u-boot-env";
				read-only;
			};

			partition@1f0000 {
				reg = <0x1f0000 0x10000>;
				label = "board-info";
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_bdinfo_d880: macaddr@d880 {
						compatible = "mac-base";
						reg = <0xd880 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@200000 {
				reg = <0x200000 0x600000>;
				label = "kernel";
			};

			partition@800000 {
				reg = <0x800000 0x1800000>;
				label = "rootfs";
			};

			partition@2000000 {
				reg = <0x2000000 0x600000>;
				label = "kn2";
				read-only;
			};

			partition@2600000 {
				reg = <0x2600000 0x1800000>;
				label = "rfs2";
				read-only;
			};

			partition@3e00000 {
				reg = <0x3e00000 0x1200000>;
				label = "part1";
				read-only;
			};

			partition@5000000 {
				reg = <0x5000000 0x1200000>;
				label = "part2";
				read-only;
			};

			partition@6200000 {
				reg = <0x6200000 0x1e00000>;
				label = "config";
				read-only;
			};
		};
	};
};
