From edd35490f2c99fa62a2514a7cb3a9afe483ee31b Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Thu, 27 Apr 2023 11:26:10 +0200
Subject: [PATCH 0618/1085] drm/vc4: txp: Move the encoder type in the variant
 structure

We'll have multiple TXP instances in the BCM2712, so we can't use a
single encoder type anymore. Let's tie the encoder type to the
compatible.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_drv.h | 1 +
 drivers/gpu/drm/vc4/vc4_txp.c | 3 ++-
 2 files changed, 3 insertions(+), 1 deletion(-)

--- a/drivers/gpu/drm/vc4/vc4_drv.h
+++ b/drivers/gpu/drm/vc4/vc4_drv.h
@@ -548,6 +548,7 @@ struct vc4_crtc_data {
 
 struct vc4_txp_data {
 	struct vc4_crtc_data	base;
+	enum vc4_encoder_type encoder_type;
 	unsigned int has_byte_enable:1;
 	unsigned int size_minus_one:1;
 	unsigned int supports_40bit_addresses:1;
--- a/drivers/gpu/drm/vc4/vc4_txp.c
+++ b/drivers/gpu/drm/vc4/vc4_txp.c
@@ -513,6 +513,7 @@ const struct vc4_txp_data bcm2835_txp_da
 		.hvs_available_channels = BIT(2),
 		.hvs_output = 2,
 	},
+	.encoder_type = VC4_ENCODER_TYPE_TXP,
 	.has_byte_enable = true,
 };
 
@@ -556,7 +557,7 @@ static int vc4_txp_bind(struct device *d
 		return ret;
 
 	vc4_encoder = &txp->encoder;
-	txp->encoder.type = VC4_ENCODER_TYPE_TXP;
+	txp->encoder.type = txp_data->encoder_type;
 
 	encoder = &vc4_encoder->base;
 	encoder->possible_crtcs = drm_crtc_mask(&vc4_crtc->base);
