From 0773a4a199aabb60afe50f5a19a6772abf4ad0bf Mon Sep 17 00:00:00 2001
From: Sebastian Reichel <sebastian.reichel@collabora.com>
Date: Mon, 6 Nov 2023 16:54:32 +0100
Subject: [PATCH] arm64: dts: rockchip: add USB3 host to rock-5a

Enable USB3 host controller for the Radxa ROCK 5 Model A. This adds
USB3 for the lower USB3 port (the one closer to the PCB).

The upper USB3 port uses the RK3588 USB TypeC host controller, which
use a different PHY without upstream support.

Signed-off-by: Sebastian Reichel <sebastian.reichel@collabora.com>
Link: https://lore.kernel.org/r/20231106155934.80838-2-sebastian.reichel@collabora.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3588s-rock-5a.dts | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/arch/arm64/boot/dts/rockchip/rk3588s-rock-5a.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588s-rock-5a.dts
@@ -113,6 +113,10 @@
 	};
 };
 
+&combphy2_psu {
+	status = "okay";
+};
+
 &cpu_b0 {
 	cpu-supply = <&vdd_cpu_big0_s0>;
 };
@@ -734,3 +738,7 @@
 &usb_host1_ohci {
 	status = "okay";
 };
+
+&usb_host2_xhci {
+	status = "okay";
+};
