// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca953x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "tplink,archer-d50-v1", "qca,qca9531";
	model = "TP-Link Archer D50 v1";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &wmac;
	};

	leds {
		compatible = "gpio-leds";

		wlan2g {
			label = "white:wlan2g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "white:wlan5g";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		qss {
			label = "white:qss";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};

		wan {
			function = LED_FUNCTION_WAN;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		lan {
			function = LED_FUNCTION_LAN;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		usb {
			function = LED_FUNCTION_USB;
			color = <LED_COLOR_ID_WHITE>;
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port0>;
			linux,default-trigger = "usbport";
		};

		internet {
			label = "white:internet";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led_system: system {
			label = "white:system";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		rfkill {
			label = "RFKILL button";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x020000>;
				read-only;
			};

			partition@20000 {
				compatible = "tplink,firmware";
				label = "firmware";
				reg = <0x020000 0x7a0000>;
			};

			partition@7c0000 {
				label = "config";
				reg = <0x7c0000 0x010000>;
				read-only;
			};

			partition@7d0000 {
				label = "romfile";
				reg = <0x7d0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_romfile_f100: macaddr@f100 {
						compatible = "mac-base";
						reg = <0xf100 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@7e0000 {
				label = "rom";
				reg = <0x7e0000 0x010000>;
				read-only;
			};

			partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					cal_art_1000: calibration@1000 {
						reg = <0x1000 0x440>;
					};

					cal_art_5000: calibration@5000 {
						reg = <0x5000 0x844>;
					};
				};
			};
		};
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy4>;

	nvmem-cells = <&macaddr_romfile_f100 1>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	nvmem-cells = <&macaddr_romfile_f100 0>;
	nvmem-cell-names = "mac-address";
};

&wmac {
	status = "okay";

	nvmem-cells = <&macaddr_romfile_f100 0>, <&cal_art_1000>;
	nvmem-cell-names = "mac-address", "calibration";
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,003c";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&cal_art_5000>, <&macaddr_romfile_f100 2>;
		nvmem-cell-names = "calibration", "mac-address";
	};
};

&usb_phy {
	status = "okay";
};

&usb0 {
	status = "okay";
};
