From 97b384a6321493008599f5c68e7c610e377cb8e6 Mon Sep 17 00:00:00 2001
From: Jonathan Bell <jonathan@raspberrypi.com>
Date: Wed, 26 Oct 2022 17:46:44 +0100
Subject: [PATCH 0393/1085] drivers: dwc_otg: stop GCC from patching FIQ
 functions

Configuring GCC to use task stack protector canaries means it will
insert calls to check functions in FIQ code. This is bad, as a) the
FIQ's stack is banked and b) the failure invokes __stack_chk_fail which
eventually tries to call printk(). Printing to the console inside the
FIQ is generally fatal.

Add CFLAGS to stop this happening in FIQ code.

Also catch one function where notrace wasn't specified.

Signed-off-by: Jonathan Bell <jonathan@raspberrypi.com>
---
 drivers/usb/host/dwc_otg/Makefile          | 1 +
 drivers/usb/host/dwc_otg/dwc_otg_fiq_fsm.c | 2 +-
 2 files changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/usb/host/dwc_otg/Makefile
+++ b/drivers/usb/host/dwc_otg/Makefile
@@ -28,6 +28,7 @@ ccflags-y   	+= -DDWC_LINUX
 ccflags-y   	+= $(CFI)
 ccflags-y	+= $(BUS_INTERFACE)
 #ccflags-y	+= -DDWC_DEV_SRPCAP
+CFLAGS_dwc_otg_fiq_fsm.o += -fno-stack-protector
 
 obj-$(CONFIG_USB_DWCOTG) += dwc_otg.o
 
--- a/drivers/usb/host/dwc_otg/dwc_otg_fiq_fsm.c
+++ b/drivers/usb/host/dwc_otg/dwc_otg_fiq_fsm.c
@@ -142,7 +142,7 @@ inline void fiq_fsm_spin_unlock(fiq_lock
  * fiq_fsm_restart_channel() - Poke channel enable bit for a split transaction
  * @channel: channel to re-enable
  */
-static void fiq_fsm_restart_channel(struct fiq_state *st, int n, int force)
+static void notrace fiq_fsm_restart_channel(struct fiq_state *st, int n, int force)
 {
 	hcchar_data_t hcchar = { .d32 = FIQ_READ(st->dwc_regs_base + HC_START + (HC_OFFSET * n) + HCCHAR) };
 
