From: George Moussalem <george.moussalem@outlook.com>
Date: Wed, 27 Oct 2024 16:34:11 +0400
Subject: [PATCH] wifi: ath11k: add hw ring mask for QCN6122

Add ring mask for QCN6122 and register them in hw params.

Signed-off-by: George Moussalem <george.moussalem@outlook.com>
---
--- a/drivers/net/wireless/ath/ath11k/core.c
+++ b/drivers/net/wireless/ath/ath11k/core.c
@@ -821,6 +821,7 @@ static struct ath11k_hw_params ath11k_hw
 		.max_radios = MAX_RADIOS_5018,
 		.bdf_addr = 0x4D200000,
 		.hw_ops = &ipq5018_ops,
+		.ring_mask = &ath11k_hw_ring_mask_qcn6122,
 		.hal_desc_sz = sizeof(struct hal_rx_desc_qcn9074),
 		.regs = &qcn6122_regs,
 		.qmi_service_ins_id = ATH11K_QMI_WLFW_SERVICE_INS_ID_V01_QCN6122,
--- a/drivers/net/wireless/ath/ath11k/hw.c
+++ b/drivers/net/wireless/ath/ath11k/hw.c
@@ -2070,6 +2070,43 @@ const struct ath11k_hw_ring_mask ath11k_
 	},
 };
 
+const struct ath11k_hw_ring_mask ath11k_hw_ring_mask_qcn6122 = {
+	.tx  = {
+		ATH11K_TX_RING_MASK_0,
+		ATH11K_TX_RING_MASK_1,
+		ATH11K_TX_RING_MASK_2,
+	},
+	.rx_mon_status = {
+		0, 0, 0,
+		ATH11K_RX_MON_STATUS_RING_MASK_0,
+	},
+	.rx = {
+		0, 0, 0, 0,
+		ATH11K_RX_RING_MASK_0,
+		ATH11K_RX_RING_MASK_1,
+		ATH11K_RX_RING_MASK_2,
+		ATH11K_RX_RING_MASK_3,
+	},
+	.rx_err = {
+		0, 0, 0, 0, 0, 0, 0, 0,
+		ATH11K_RX_ERR_RING_MASK_0,
+	},
+	.rx_wbm_rel = {
+		0, 0, 0, 0, 0, 0, 0, 0, 0,
+		ATH11K_RX_WBM_REL_RING_MASK_0,
+	},
+       .reo_status = {
+		0, 0, 0,
+		ATH11K_REO_STATUS_RING_MASK_0,
+	},
+	.rxdma2host = {
+		ATH11K_RXDMA2HOST_RING_MASK_0,
+	},
+	.host2rxdma = {
+		ATH11K_HOST2RXDMA_RING_MASK_0,
+	},
+};
+
 /* Target firmware's Copy Engine configuration for IPQ5018 */
 const struct ce_pipe_config ath11k_target_ce_config_wlan_ipq5018[] = {
 	/* CE0: host->target HTC control and raw streams */
--- a/drivers/net/wireless/ath/ath11k/hw.h
+++ b/drivers/net/wireless/ath/ath11k/hw.h
@@ -289,6 +289,7 @@ extern const struct ath11k_hw_ring_mask
 extern const struct ath11k_hw_ring_mask ath11k_hw_ring_mask_qca6390;
 extern const struct ath11k_hw_ring_mask ath11k_hw_ring_mask_qcn9074;
 extern const struct ath11k_hw_ring_mask ath11k_hw_ring_mask_wcn6750;
+extern const struct ath11k_hw_ring_mask ath11k_hw_ring_mask_qcn6122;
 
 extern const struct ce_ie_addr ath11k_ce_ie_addr_ipq8074;
 extern const struct ce_ie_addr ath11k_ce_ie_addr_ipq5018;
