From 4e07a95f7402de092cd71b2cb96c69f85c98f251 Mon Sep 17 00:00:00 2001
From: Sebastian Reichel <sebastian.reichel@collabora.com>
Date: Tue, 9 Apr 2024 00:50:31 +0200
Subject: [PATCH] arm64: dts: rockchip: fix usb2phy nodename for rk3588

usb2-phy should be named usb2phy according to the DT binding,
so let's fix it up accordingly.

Signed-off-by: Sebastian Reichel <sebastian.reichel@collabora.com>
Link: https://lore.kernel.org/r/20240408225109.128953-5-sebastian.reichel@collabora.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3588s.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/rockchip/rk3588s.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588s.dtsi
@@ -599,7 +599,7 @@
 		#address-cells = <1>;
 		#size-cells = <1>;
 
-		u2phy2: usb2-phy@8000 {
+		u2phy2: usb2phy@8000 {
 			compatible = "rockchip,rk3588-usb2phy";
 			reg = <0x8000 0x10>;
 			interrupts = <GIC_SPI 391 IRQ_TYPE_LEVEL_HIGH 0>;
@@ -624,7 +624,7 @@
 		#address-cells = <1>;
 		#size-cells = <1>;
 
-		u2phy3: usb2-phy@c000 {
+		u2phy3: usb2phy@c000 {
 			compatible = "rockchip,rk3588-usb2phy";
 			reg = <0xc000 0x10>;
 			interrupts = <GIC_SPI 392 IRQ_TYPE_LEVEL_HIGH 0>;
