#继承4.18.0-425.el8，并分支，添加4.18.0-425.el8-4.18.0-477.el8、4.18.0-477.1.1.el8-4.18.0-477.10.1.el8

* Wed Apr 05 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.10.1.el8_8]
- dm: fix __send_duplicate_bios() to always allow for splitting IO (Benjamin Marzinski) [2184429]
- dm: fix improper splitting for abnormal bios (Benjamin Marzinski) [2184429]

* Tue Apr 04 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.9.1.el8_8]
- ovl: fail on invalid uid/gid mapping at copy up (Miklos Szeredi) [2165342] {CVE-2023-0386}

* Mon Apr 03 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.8.1.el8_8]
- redhat/configs: Put CONFIG_SFC_* to a proper location (Vladis Dronov)
- redhat/configs: Put CONFIG_SEV_GUEST to a proper location (Vladis Dronov)
- Reinstate "GFS2: free disk inode which is deleted by remote node -V2" (Bob Peterson) [2181343]

* Thu Mar 30 2023 Patrick Talbert <ptalbert@redhat.com> [4.18.0-477.7.1.el8_8]
- iavf: fix hang on reboot with ice (Stefan Assmann) [2181811]
- iavf: Fix race condition between iavf_shutdown and iavf_remove (Stefan Assmann) [2181811]
- net/ulp: use consistent error code when blocking ULP (Sabrina Dubroca) [2176955 2176956] {CVE-2023-0461}
- net/ulp: prevent ULP without clone op from entering the LISTEN status (Sabrina Dubroca) [2176955 2176956] {CVE-2023-0461}
- lockd: lockd server-side shouldn't set fl_ops (Jeffrey Layton) [2179329]
- NFS: Correct timing for assigning access cache timestamp (Benjamin Coddington) [2180851]
- Switch to z-stream for 8.8 for CKI pipelines (Michael Hofmann)

* Wed Mar 22 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.6.1.el8_8]
- KVM: VMX: Execute IBPB on emulated VM-exit when guest has IBRS (Jon Maloy) [2160033] {CVE-2022-2196}

* Mon Mar 20 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.5.1.el8_8]
- Revert "GFS2: free disk inode which is deleted by remote node -V2" (Bob Peterson) [2109600]
- gfs2: Evict inodes cooperatively (Andreas Gruenbacher) [2109600]
- gfs2: Flush delete work before shrinking inode cache (Andreas Gruenbacher) [2109600]
- gfs2: Add SDF_DEACTIVATING super block flag (Bob Peterson) [2109600]
- gfs2: check gl_object in rgrp glops (Bob Peterson) [2109600]
- gfs2: Split the two kinds of glock "delete" work (Andreas Gruenbacher) [2109600]
- gfs2: Move delete workqueue into super block (Andreas Gruenbacher) [2109600]
- gfs2: Use container_of() for gfs2_glock(aspace) (Andreas Gruenbacher) [2109600]
- gfs2: Get rid of GLF_PENDING_DELETE flag (Andreas Gruenbacher) [2109600]
- gfs2: Make glock lru list scanning safer (Andreas Gruenbacher) [2109600]
- gfs2: Fix use-after-free in gfs2_glock_shrink_scan (Andreas Gruenbacher) [2109600]
- gfs2: Clean up gfs2_scan_glock_lru (Andreas Gruenbacher) [2109600]
- gfs2: gl_object races fix (Andreas Gruenbacher) [2109600]
- iomap/gfs2: Unlock and put folio in page_done handler (Andreas Gruenbacher) [2109600]
- iomap: Add __iomap_put_folio helper (Andreas Gruenbacher) [2109600]
- gfs2: Remove support for glock holder auto-demotion (2) (Andreas Gruenbacher) [2109600]
- gfs2: Remove support for glock holder auto-demotion (Andreas Gruenbacher) [2109600]
- gfs2: Minor gfs2_try_evict cleanup (Andreas Gruenbacher) [2109600]
- gfs2: Partially revert gfs2_inode_lookup change (Andreas Gruenbacher) [2109600]
- gfs2: Add gfs2_inode_lookup comment (Andreas Gruenbacher) [2109600]
- gfs2: Uninline and improve glock_{set,clear}_object (Andreas Gruenbacher) [2109600]
- gfs2: Simply dequeue iopen glock in gfs2_evict_inode (Andreas Gruenbacher) [2109600]
- gfs2: Clean up after gfs2_create_inode rework (Andreas Gruenbacher) [2109600]
- gfs2: Avoid dequeuing GL_ASYNC glock holders twice (Andreas Gruenbacher) [2109600]
- gfs2: Handle -EBUSY result of insert_inode_locked4 (Andreas Gruenbacher) [2109600]
- gfs2: Fix and clean up create / evict interaction (Andreas Gruenbacher) [2109600]
- gfs2: Clean up initialization of "ip" in gfs2_create_inode (Andreas Gruenbacher) [2109600]
- gfs2: Get rid of ghs[] in gfs2_create_inode (Andreas Gruenbacher) [2109600]
- gfs2: Dequeue waiters when withdrawn (Bob Peterson) [2109600]
- gfs2: Prevent double iput for journal on error (Bob Peterson) [2109600]
- Revert "gfs2: stop using generic_writepages in gfs2_ail1_start_one" (Andreas Gruenbacher) [2109600]
- gfs2: remove ->writepage (Andreas Gruenbacher) [2109600]
- gfs2: stop using generic_writepages in gfs2_ail1_start_one (Andreas Gruenbacher) [2109600]
- gfs2: List traversal in do_promote is safe (Andreas Gruenbacher) [2109600]
- gfs2: do_promote glock holder stealing fix (Bob Peterson) [2109600]
- gfs2: Use better variable name (Andreas Gruenbacher) [2109600]
- gfs2: Make go_instantiate take a glock (Andreas Gruenbacher) [2109600]
- gfs2: Add new go_held glock operation (Andreas Gruenbacher) [2109600]
- gfs2: Revert 'Fix "truncate in progress" hang' (Andreas Gruenbacher) [2109600]
- gfs2: Instantiate glocks ouside of glock state engine (Andreas Gruenbacher) [2109600]
- gfs2: Fix up gfs2_glock_async_wait (Andreas Gruenbacher) [2109600]
- gfs2: Add GL_NOPID flag for process-independent glock holders (Andreas Gruenbacher) [2109600]
- gfs2: dump inode object for iopen glocks (Bob Peterson) [2109600]
- gfs2: convert to use DEFINE_SEQ_ATTRIBUTE macro (Andreas Gruenbacher) [2109600]
- gfs2: Use TRY lock in gfs2_inode_lookup for UNLINKED inodes (Bob Peterson) [2109600]

* Fri Mar 17 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.4.1.el8_8]
- Updated dist tag to el8_8 (Lucas Zampieri)
- Revert "net/mlx5: Don't perform lookup after already known sec_path" (Amir Tzin) [2176349]
- KVM: x86: do not report a vCPU as preempted outside instruction boundaries (Jon Maloy) [2124800] {CVE-2022-39189}
- Drivers: vmbus: Check for channel allocation before looking up relids (Mohammed Gamal) [2178622]

* Mon Mar 13 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.3.1.el8]
- drm/nouveau/fb/tu102-: fix register used to determine scrub status (Karol Herbst) [2168648]
- drm/nouveau/devinit/tu102-: wait for GFW_BOOT_PROGRESS == COMPLETED (Karol Herbst) [2168648]
- fs/proc: task_mmu.c: don't read mapcount for migration entry (Jay Shin) [2174623]
- perf/core: Fix cgroup event list management (Michael Petlan) [2162525]

* Wed Mar 08 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.2.1.el8]
- net: mana: Fix IRQ name - add PCI and queue number (Mohammed Gamal) [2166787]
- crypto: des - disallow des3 in FIPS mode (Vladis Dronov) [2175234]
- self-tests: more rps self tests (Paolo Abeni) [2168878]
- net: make default_rps_mask a per netns attribute (Paolo Abeni) [2168878]
- self-tests: introduce self-tests for RPS default mask (Paolo Abeni) [2168878]
- net: introduce default_rps_mask netns attribute (Paolo Abeni) [2168878]
- net-sysctl: factor-out rpm mask manipulation helpers (Paolo Abeni) [2168878]
- net-sysctl: factor out cpumask parsing helper (Paolo Abeni) [2168878]
- txhash: Make rethinking txhash behavior configurable via sysctl (Paolo Abeni) [2168878]
- net-sysfs: Call dev_hold always in rx_queue_add_kobject (Paolo Abeni) [2168878]
- net-sysfs: Call dev_hold always in netdev_queue_add_kobject (Paolo Abeni) [2168878]
- net-sysfs: fix netdev_queue_add_kobject() breakage (Paolo Abeni) [2168878]
- net-sysfs: Fix reference count leak in rx|netdev_queue_add_kobject (Paolo Abeni) [2168878]

* Mon Mar 06 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.1.1.el8]
- ice/ptp: fix the PTP worker retrying indefinitely if the link went down (Petr Oros) [2166392]
- ice: reschedule ice_ptp_wait_for_offset_valid during reset (Petr Oros) [2166392]
- ice: make Tx and Rx vernier offset calibration independent (Petr Oros) [2166392]
- ice: only check set bits in ice_ptp_flush_tx_tracker (Petr Oros) [2166392]
- ice: handle flushing stale Tx timestamps in ice_ptp_tx_tstamp (Petr Oros) [2166392]
- ice: cleanup allocations in ice_ptp_alloc_tx_tracker (Petr Oros) [2166392]
- ice: protect init and calibrating check in ice_ptp_request_ts (Petr Oros) [2166392]
- ice: check Tx timestamp memory register for ready timestamps (Petr Oros) [2166392]
- ice: handle discarding old Tx requests in ice_ptp_tx_tstamp (Petr Oros) [2166392]
- ice: always call ice_ptp_link_change and make it void (Petr Oros) [2166392]
- ice: fix misuse of "link err" with "link status" (Petr Oros) [2166392]
- ice: Reset TS memory for all quads (Petr Oros) [2166392]
- ice: Remove the E822 vernier "bypass" logic (Petr Oros) [2166392]
- ice: Use more generic names for ice_ptp_tx fields (Petr Oros) [2166392]
- ice: Merge pin initialization of E810 and E810T adapters (Petr Oros) [2166392]
- ice: Check if reset in progress while waiting for offsets (Petr Oros) [2166392]
- NFS: Judge the file access cache's timestamp in rcu path (Benjamin Coddington) [2161321]
- redhat: switch to z-stream for 8.8 (Lucas Zampieri)

* Thu Feb 23 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-477.el8]
- cpufreq: intel_pstate: Add Sapphire Rapids support in no-HWP mode (Prarit Bhargava) [2170564]

* Thu Feb 23 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-476.el8]
- igb: Initialize mailbox message for VF reset (Corinna Vinschen) [2103948]
- igb: Allocate MSI-X vector when testing (Corinna Vinschen) [2103948]
- igb: Proactively round up to kmalloc bucket size (Corinna Vinschen) [2103948]
- igb: Do not free q_vector unless new one was allocated (Corinna Vinschen) [2103948]
- ptp: introduce helpers to adjust by scaled parts per million (Corinna Vinschen) [2103948]
- net: Remove the obsolte u64_stats_fetch_*_irq() users (drivers). (Corinna Vinschen) [2103948]
- net: ethernet: move from strlcpy with unused retval to strscpy (Corinna Vinschen) [2103948]
- igb: convert .adjfreq to .adjfine (Corinna Vinschen) [2103948]
- ASoC: Intel: soc-acpi: add configuration for variant of 0C11 product (Jaroslav Kysela) [2100582]
- ASoC: Intel: soc-acpi: add configuration for variant of 0C40 product (Jaroslav Kysela) [2100582]
- ASoC: Intel: sof_sdw: use common helpers for all Realtek amps (Jaroslav Kysela) [2100582]
- ASoC: Intel: sof_sdw: Add support for SKU 0C11 product (Jaroslav Kysela) [2100582]
- ASoC: Intel: sof_sdw: Add support for SKU 0C4F product (Jaroslav Kysela) [2100582]
- ASoC: Intel: sof_sdw: Add support for SKU 0C40 product (Jaroslav Kysela) [2100582]
- ASoC: Intel: sof_sdw: Add support for SKU 0C10 product (Jaroslav Kysela) [2100582]
- ASoC: Intel: sof_sdw_rt1316: add BQ params for the Dell models (Jaroslav Kysela) [2100582]
- ASoC: Intel: sof_sdw_rt1308: add BQ params for the Dell models (Jaroslav Kysela) [2100582]
- ASoC: intel: sof_sdw: add rt1318 codec support. (Jaroslav Kysela) [2100582]
- ASoC: rt1318: Add RT1318 SDCA vendor-specific driver (Jaroslav Kysela) [2100582]
- ASoC: Intel: soc-acpi: update codec addr on 0C11/0C4F product (Jaroslav Kysela) [2100582]
- ASoC: Intel: soc-acpi: add SKU 0C11 SoundWire configuration (Jaroslav Kysela) [2100582]
- ASoC: Intel: soc-acpi: add SKU 0C40 SoundWire configuration (Jaroslav Kysela) [2100582]
- ASoC: Intel: soc-acpi: add SKU 0C10 SoundWire configuration (Jaroslav Kysela) [2100582]
- ASoC: Intel: soc-acpi-intel-rpl-match: add rpl_sdca_3_in_1 support (Jaroslav Kysela) [2100582]

* Wed Feb 22 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-475.el8]
- net: ena: Update NUMA TPH hint register upon NUMA node update (Petr Oros) [2167316]
- net: ena: Set default value for RX interrupt moderation (Petr Oros) [2167316]
- net: ena: Fix rx_copybreak value update (Petr Oros) [2167316]
- net: ena: Use bitmask to indicate packet redirection (Petr Oros) [2167316]
- net: ena: Account for the number of processed bytes in XDP (Petr Oros) [2167316]
- net: ena: Don't register memory info on XDP exchange (Petr Oros) [2167316]
- net: ena: Fix toeplitz initial hash value (Petr Oros) [2167316]
- net: ena: Fix error handling in ena_init() (Petr Oros) [2167316]
- net: sched: disallow noqueue for qdisc classes (Xin Long) [2168282] {CVE-2022-47929}
- net: sched: cbq: dont intepret cls results when asked to drop (Xin Long) [2168327] {CVE-2023-23454}
- sctp: do not check hb_timer.expires when resetting hb_timer (Xin Long) [2133092]
- arm64: Add AMPERE1 to the Spectre-BHB affected list (Mark Salter) [2140727]
- net: mana: Fix accessing freed irq affinity_hint (Emanuele Giuseppe Esposito) [2168969]
- net: mana: Assign interrupts to CPUs based on NUMA nodes (Emanuele Giuseppe Esposito) [2168969]
- Revert "RDMA/irdma: Report the correct link speed" (Kamal Heib) [2143088]
- Documentation/sysctl: document page_lock_unfairness (Nico Pache) [2165737] {CVE-2022-3623}
- mm: allow a controlled amount of unfairness in the page lock (Nico Pache) [2165737] {CVE-2022-3623}
- mm/hugetlb: fix races when looking up a CONT-PTE/PMD size hugetlb page (Nico Pache) [2165737] {CVE-2022-3623}
- mm/migration: fix potential pte_unmap on an not mapped pte (Nico Pache) [2165737] {CVE-2022-3623}
- mm/migrate.c: rework migration_entry_wait() to not take a pageref (Nico Pache) [2165737] {CVE-2022-3623}
- mm: make wait_on_page_writeback() wait for multiple pending writebacks (Nico Pache) [2165737] {CVE-2022-3623}
- mm: rewrite wait_on_page_bit_common() logic (Nico Pache) [2165737] {CVE-2022-3623}
- mm/gup.c: use is_vm_hugetlb_page() to check whether to follow huge (Nico Pache) [2165737] {CVE-2022-3623}

* Mon Feb 20 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-474.el8]
- perf/x86/amd: Fix crash due to race between amd_pmu_enable_all, perf NMI and throttling (Michael Petlan) [2085282]
- x86/perf: Fix snapshot_branch_stack warning in VM (Michael Petlan) [2085282]
- perf/x86/amd/core: Fix reloading events for SVM (Michael Petlan) [2085282 2086722]
- perf/x86/amd: Run AMD BRS code only on supported hw (Michael Petlan) [2085282]
- perf/x86/amd: Fix AMD BRS period adjustment (Michael Petlan) [2085282]
- perf/x86/amd: Remove unused variable 'hwc' (Michael Petlan) [2085282]
- perf/ibs: Fix comment (Michael Petlan) [2085282]
- perf report: Add tools/arch/x86/include/asm/amd-ibs.h (Michael Petlan) [2085282]
- perf/amd/ibs: Advertise zen4_ibs_extensions as pmu capability attribute (Michael Petlan) [2085282]
- perf/amd/ibs: Add support for L3 miss filtering (Michael Petlan) [2085282]
- perf/amd/ibs: Use ->is_visible callback for dynamic attributes (Michael Petlan) [2085282]
- perf/amd/ibs: Cascade pmu init functions' return value (Michael Petlan) [2085282]
- perf/amd/ibs: Use interrupt regs ip for stack unwinding (Michael Petlan) [2085282]
- perf/x86/amd/core: Add PerfMonV2 overflow handling (Michael Petlan) [2085282 2086722]
- perf/x86/amd/core: Add PerfMonV2 counter control (Michael Petlan) [2085282 2086722]
- perf/x86/amd/core: Detect available counters (Michael Petlan) [2085282 2086722]
- perf/x86/amd/core: Detect PerfMonV2 support (Michael Petlan) [2085282 2086722]
- x86/msr: Add PerfCntrGlobal* registers (Michael Petlan) [2085282 2086722]
- x86/cpufeatures: Add PerfMonV2 feature bit (Michael Petlan) [2085282 2086722]
- perf/x86: Unify format of events sysfs show (Michael Petlan) [2085282]
- perf/x86/amd: Add idle hooks for branch sampling (Michael Petlan) [2085282]
- perf: Enable branch record for software events (Michael Petlan) [2085282]
- redhat/configs: Enable AMD Zen3 branch sampling by default (Michael Petlan) [2085282]
- perf/x86/amd: Make Zen3 branch sampling opt-in (Michael Petlan) [2085282]
- perf/x86/amd: Add AMD branch sampling period adjustment (Michael Petlan) [2085282]
- perf/x86/amd: Enable branch sampling priv level filtering (Michael Petlan) [2085282]
- perf/x86/amd: Add branch-brs helper event for Fam19h BRS (Michael Petlan) [2085282]
- perf/x86/amd: Add AMD Fam19h Branch Sampling support (Michael Petlan) [2085282]
- perf/x86/amd/ibs: Add bitfield definitions in new <asm/amd-ibs.h> header (Michael Petlan) [2085282]
- perf/amd/uncore: Allow the driver to be built as a module (Michael Petlan) [2085282]
- perf/amd/uncore: Clean up header use, use <linux/ include paths instead of <asm/ (Michael Petlan) [2085282]
- perf/amd/uncore: Simplify code, use free_percpu()'s built-in check for NULL (Michael Petlan) [2085282]
- x86/cpufeatures: Add AMD Fam19h Branch Sampling feature (Michael Petlan) [2085282]
- perf/core: Add perf_clear_branch_entry_bitfields() helper (Michael Petlan) [2085282]

* Fri Feb 17 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-473.el8]
- ice: fix lost multicast packets in promisc mode (Ken Cox) [2138215]
- RDMA/irdma: Cap MSIX used to online CPUs + 1 (Kamal Heib) [2118548]
- usb: mon: make mmapped memory read only (Desnes Nunes) [2157697] {CVE-2022-43750}
- blk-cgroup: don't update io stat for root cgroup (Ming Lei) [2167547]
- x86/hyperv: Remove unregister syscore call from Hyper-V cleanup (Mohammed Gamal) [1865745]
- perf test: Skip watchpoint tests if no watchpoints available (Michael Petlan) [2148337]
- powercap: intel_rapl: Add support for RAPTORLAKE_P (Prarit Bhargava) [2076726]
- crypto: hmac - disallow keys < 112 bits in FIPS mode (Vladis Dronov) [2166715]
- crypto: hmac - add fips_skip support (Vladis Dronov) [2166715]
- crypto: dh - limit key size to 2048 in FIPS mode (Vladis Dronov) [2166715]
- crypto: rsa - limit key size to 2048 in FIPS mode (Vladis Dronov) [2166715]

* Wed Feb 15 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-472.el8]
- netfilter: flowtable_offload: add missing locking (Florian Westphal) [2134371]
- netfilter: ipset: Rework long task execution when adding/deleting entries (Florian Westphal) [2134371]
- netfilter: ipset: fix hash:net,port,net hang with /0 subnet (Florian Westphal) [2134371]
- netfilter: ipset: regression in ip_set_hash_ip.c (Florian Westphal) [2134371]
- netfilter: ipset: Limit the maximal range of consecutive elements to add/delete (Florian Westphal) [2134371]
- netfilter: flowtable: really fix NAT IPv6 offload (Florian Westphal) [2134371]
- netfilter: nft_set_pipapo: Actually validate intervals in fields after the first one (Florian Westphal) [2134371]
- netfilter: Cleanup nft_net->module_list from nf_tables_exit_net() (Florian Westphal) [2134371]
- netfilter: nf_tables: fix nft_counters_enabled underflow at nf_tables_addchain() (Florian Westphal) [2134371]
- netfilter: nf_tables: do not leave chain stats enabled on error (Florian Westphal) [2134371]
- ipvs: use explicitly signed chars (Florian Westphal) [2134371]
- netfilter: nf_tables: release flow rule object from commit path (Florian Westphal) [2134371]
- netfilter: nf_tables: fix percpu memory leak at nf_tables_addchain() (Florian Westphal) [2134371]
- netfilter: nf_tables: clean up hook list when offload flags check fails (Florian Westphal) [2134371]
- netfilter: br_netfilter: Drop dst references before setting. (Florian Westphal) [2134371]
- netfilter: nft_tproxy: restrict to prerouting hook (Florian Westphal) [2134371]
- netfilter: ebtables: fix memory leak when blob is malformed (Florian Westphal) [2134371]
- netfilter: ebtables: reject blobs that don't provide all entry points (Florian Westphal) [2134371]
- netfilter: nf_tables: check NFT_SET_CONCAT flag if field_count is specified (Florian Westphal) [2134371]
- netfilter: nf_tables: relax NFTA_SET_ELEM_KEY_END set flags requirements (Florian Westphal) [2134371]
- netfilter: nf_tables: NFTA_SET_ELEM_KEY_END requires concat and interval flags (Florian Westphal) [2134371]
- netfilter: nf_tables: validate NFTA_SET_ELEM_OBJREF based on NFT_SET_OBJECT flag (Florian Westphal) [2134371]
- netfilter: nf_tables: possible module reference underflow in error path (Florian Westphal) [2134371]
- netfilter: nf_tables: disallow NFTA_SET_ELEM_KEY_END with NFT_SET_ELEM_INTERVAL_END flag (Florian Westphal) [2134371]
- netfilter: nf_tables: use READ_ONCE and WRITE_ONCE for shared generation id access (Florian Westphal) [2134371]
- netfilter: nf_tables: fix null deref due to zeroed list head (Florian Westphal) [2134371]

* Wed Feb 15 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-471.el8]
- bnxt_en: fix memory leak in bnxt_nvm_test() (Ken Cox) [2112186]
- bnxt_en: Fix HDS and jumbo thresholds for RX packets (Ken Cox) [2112186]
- bnxt_en: Fix first buffer size calculations for XDP multi-buffer (Ken Cox) [2112186]
- bnxt_en: Fix XDP RX path (Ken Cox) [2112186]
- bnxt_en: Simplify bnxt_xdp_buff_init() (Ken Cox) [2112186]
- bnxt: prevent skb UAF after handing over to PTP worker (Ken Cox) [2112186]
- bnxt_en: fix flags to check for supported fw version (Ken Cox) [2112186]
- net: ethernet: move from strlcpy with unused retval to strscpy (Ken Cox) [2112186]
- bnxt_en: fix NQ resource accounting during vf creation on 57500 chips (Ken Cox) [2112186]
- bnxt_en: set missing reload flag in devlink features (Ken Cox) [2112186]
- bnxt_en: Use PAGE_SIZE to init buffer when multi buffer XDP is not in use (Ken Cox) [2112186]
- bnxt_en: Remove duplicated include bnxt_devlink.c (Ken Cox) [2112186]
- bnxt_en: implement callbacks for devlink selftests (Ken Cox) [2112186]
- bnxt_en: Fix bnxt_refclk_read() (Ken Cox) [2112186]
- bnxt_en: fix livepatch query (Ken Cox) [2112186]
- bnxt_en: Fix bnxt_reinit_after_abort() code path (Ken Cox) [2112186]
- bnxt_en: reclaim max resources if sriov enable fails (Ken Cox) [2112186]
- bnxt: Use the bitmap API to allocate bitmaps (Ken Cox) [2112186]
- bnxt: Fix typo in comments (Ken Cox) [2112186]
- eth: bnxt: make ulp_id unsigned to make GCC 12 happy (Ken Cox) [2112186]
- bnxt_en: Enable packet timestamping for all RX packets (Ken Cox) [2112186]
- bnxt_en: Configure ptp filters during bnxt open (Ken Cox) [2112186]
- bnxt_en: Update firmware interface to 1.10.2.95 (Ken Cox) [2112186]
- bnxt: add page_pool support for aggregation ring when using xdp (Ken Cox) [2112186]
- bnxt: change receive ring space parameters (Ken Cox) [2112186]
- bnxt: rename bnxt_rx_pages to bnxt_rx_agg_pages_skb (Ken Cox) [2112186]
- bnxt: refactor bnxt_rx_pages operate on skb_shared_info (Ken Cox) [2112186]
- bnxt: add flag to denote that an xdp program is currently attached (Ken Cox) [2112186]
- bnxt: refactor bnxt_rx_xdp to separate xdp_init_buff/xdp_prepare_buff (Ken Cox) [2112186]
- bnxt: report header-data split state (Ken Cox) [2112186]
- net: Don't include filter.h from net/sock.h (Ken Cox) [2112186]
- ethernet: constify references to netdev->dev_addr in drivers (Ken Cox) [2112186]
- ethernet: use eth_hw_addr_set() for dev->addr_len cases (Ken Cox) [2112186]
- ethernet: use eth_hw_addr_set() instead of ether_addr_copy() (Ken Cox) [2112186]
- bnxt_en: Use struct_group_attr() for memcpy() region (Ken Cox) [2112186]
- net: don't include ethtool.h from netdevice.h (Ken Cox) [2112186]
- treewide: Use fallthrough pseudo-keyword (Ken Cox) [2112186]
- net: Use skb_frag_off accessors (Ken Cox) [2112186]
- net: Use skb accessors in network drivers (Ken Cox) [2112186]
- ethernet: remove redundant memset (Ken Cox) [2112186]
- treewide: Add SPDX license identifier - Makefile/Kconfig (Ken Cox) [2112186]

* Wed Feb 15 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-470.el8]
- ASoC: amd: renoir: Add a module parameter to influence pdm_gain (Jaroslav Kysela) [2169761]
- ASoC: amd: renoir: Adjust the gain for PDM DMIC (Jaroslav Kysela) [2169761]
- ASoC: amd: yc: Add a module parameter to influence pdm_gain (Jaroslav Kysela) [2169761]
- ASoC: amd: yc: Adjust the gain for PDM DMIC (Jaroslav Kysela) [2169761]
- genirq: Fix reference leaks on irq affinity notifiers (Ricardo Robaina) [2154842]
- genirq: Prevent use-after-free and work list corruption (Ricardo Robaina) [2154842]
- perf/x86/uncore: Don't WARN_ON_ONCE() for a broken discovery table (Michael Petlan) [2154044]
- perf/x86/uncore: Add a quirk for UPI on SPR (Michael Petlan) [2154044]
- perf/x86/uncore: Ignore broken units in discovery table (Michael Petlan) [2154044]
- perf/x86/uncore: Fix potential NULL pointer in uncore_get_alias_name (Michael Petlan) [2154044]
- perf/x86/uncore: Factor out uncore_device_to_die() (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Support extra IMC channel on Ice Lake server (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix CAS_COUNT_WRITE issue for ICX (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix IIO event constraints for Snowridge (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix IIO event constraints for Skylake Server (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix filter_tid mask for CHA events on Skylake Server (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix Intel ICX IIO event constraints (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix reference count leak in __uncore_imc_init_box() (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix reference count leak in snr_uncore_mmio_map() (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix reference count leak in hswep_has_limit_sbox() (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Fix reference count leak in sad_cfg_iio_topology() (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Make set_mapping() procedure void (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Update sysfs-devices-mapping file (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Enable UPI topology discovery for Sapphire Rapids (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Enable UPI topology discovery for Icelake Server (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Get UPI NodeID and GroupID (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Enable UPI topology discovery for Skylake Server (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Generalize get_topology() for SKX PMUs (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Disable I/O stacks to PMU mapping on ICX-D (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Clear attr_update properly (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Introduce UPI topology type (Michael Petlan) [2154044]
- perf/x86/intel/uncore: Generalize IIO topology support (Michael Petlan) [2154044]

* Wed Feb 15 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-469.el8]
- net/mlx4: Check retval of mlx4_bitmap_init (Amir Tzin) [2150787]
- net/mlx4: Fix error check for dma_map_sg (Amir Tzin) [2150787]
- net/mlx4_en: Fix wrong return value on ioctl EEPROM query failure (Amir Tzin) [2150787]
- RDMA/mlx4: Avoid flush_scheduled_work() usage (Amir Tzin) [2150787]
- net: mellanox: fix open-coded for_each_set_bit() (Amir Tzin) [2150787]
- tracing: Add linear buckets to histogram logic (Jerome Marchand) [2161509]
- configs/generic: enable CONFIG_RTC_SYSTOHC (Marcelo Tosatti) [2135417]
- watchdog: fix UAF in reboot notifier handling in watchdog core code (Wander Lairson Costa) [2131308]

* Tue Feb 14 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-468.el8]
- drm/i915/fbdev: do not create fbdev if HPD is suspended (Jocelyn Falempe) [2156006]
- drm/i915/fbdev: suspend HPD before fbdev unregistration (Jocelyn Falempe) [2156006]
- drm/i915/hpd: suspend MST at the end of intel_modeset_driver_remove (Jocelyn Falempe) [2156006]
- drm/i915/gvt: fix vgpu debugfs clean in remove (Jocelyn Falempe) [2115903]
- drm/i915/gvt: fix gvt debugfs destroy (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix kernel warning during topology setup (Jocelyn Falempe) [2115903]
- Revert "drm/amd/display: Enable Freesync Video Mode by default" (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix double release compute pasid (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix kfd_process_device_init_vm error handling (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix size validation for non-exclusive domains (v4) (Jocelyn Falempe) [2115903]
- drm/i915/gvt: fix double free bug in split_2MB_gtt_entry (Jocelyn Falempe) [2115903]
- drm/i915: unpin on error in intel_vgpu_shadow_mm_pin() (Jocelyn Falempe) [2115903]
- drm/amd/pm: correct the fan speed retrieving in PWM for some SMU13 asics (Jocelyn Falempe) [2115903]
- drm/amd/pm: bump SMU13.0.0 driver_if header to version 0x34 (Jocelyn Falempe) [2115903]
- drm/amd/pm: add missing SMU13.0.7 mm_dpm feature mapping (Jocelyn Falempe) [2115903]
- drm/amd/pm: add missing SMU13.0.0 mm_dpm feature mapping (Jocelyn Falempe) [2115903]
- drm/i915/migrate: Account for the reserved_space (Jocelyn Falempe) [2115903]
- drm/i915: improve the catch-all evict to handle lock contention (Jocelyn Falempe) [2115903]
- drm/amdgpu: make display pinning more flexible (v2) (Jocelyn Falempe) [2115903]
- drm/amdgpu: handle polaris10/11 overlap asics (v2) (Jocelyn Falempe) [2115903]
- drm/amd/display: Add DCN314 display SG Support (Jocelyn Falempe) [2115903]
- drm/i915/ttm: consider CCS for backup objects (Jocelyn Falempe) [2115903]
- drm/i915/dsi: fix VBT send packet port selection for dual link DSI (Jocelyn Falempe) [2115903]
- drm/vmwgfx: Validate the box size for the snooped cursor (Jocelyn Falempe) [2115903]
- drm/connector: send hotplug uevent on connector cleanup (Jocelyn Falempe) [2115903]
- drm/amdgpu: fix mmhub register base coding error (Jocelyn Falempe) [2115903]
- drm/amd/pm: correct SMU13.0.0 pstate profiling clock settings (Jocelyn Falempe) [2115903]
- drm/amd/pm: update SMU13.0.0 reported maximum shader clock (Jocelyn Falempe) [2115903]
- drm/amdgpu: skip MES for S0ix as well since it's part of GFX (Jocelyn Falempe) [2115903]
- drm/amd/display: revert Disable DRR actions during state commit (Jocelyn Falempe) [2115903]
- drm/amd/pm: avoid large variable on kernel stack (Jocelyn Falempe) [2115903]
- drm/i915/display: Don't disable DDI/Transcoder when setting phy test pattern (Jocelyn Falempe) [2115903]
- drm/sti: Fix return type of sti_{dvo,hda,hdmi}_connector_mode_valid() (Jocelyn Falempe) [2115903]
- drm/fsl-dcu: Fix return type of fsl_dcu_drm_connector_mode_valid() (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix DTBCLK disable requests and SRC_SEL programming (Jocelyn Falempe) [2115903]
- drm/amd/display: Use the largest vready_offset in pipe group (Jocelyn Falempe) [2115903]
- drm/amd/display: fix array index out of bound error in bios parser (Jocelyn Falempe) [2115903]
- drm/amd/display: Workaround to increase phantom pipe vactive in pipesplit (Jocelyn Falempe) [2115903]
- drm/sti: Use drm_mode_copy() (Jocelyn Falempe) [2115903]
- drm/amd/display: Disable DRR actions during state commit (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix type of second parameter in odn_edit_dpm_table() callback (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix type of second parameter in trans_msg() callback (Jocelyn Falempe) [2115903]
- Revert "drm/amd/display: Limit max DSC target bpp for specific monitors" (Jocelyn Falempe) [2115903]
- drm/edid: add a quirk for two LG monitors to get them to work on 10bpc (Jocelyn Falempe) [2115903]
- drm/amd/display: prevent memory leak (Jocelyn Falempe) [2115903]
- drm/i915/bios: fix a memory leak in generate_lfp_data_ptrs (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix memory leakage (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix PCI device refcount leak in amdgpu_atrm_get_bios() (Jocelyn Falempe) [2115903]
- drm/radeon: Fix PCI device refcount leak in radeon_atrm_get_bios() (Jocelyn Falempe) [2115903]
- amdgpu/nv.c: Corrected typo in the video capabilities resolution (Jocelyn Falempe) [2115903]
- drm/amd/pm/smu11: BACO is supported when it's in BACO state (Jocelyn Falempe) [2115903]
- drm/tegra: Add missing clk_disable_unprepare() in tegra_dc_probe() (Jocelyn Falempe) [2115903]
- drm/i915/guc: make default_lists const data (Jocelyn Falempe) [2115903]
- drm/amdgpu: fix pci device refcount leak (Jocelyn Falempe) [2115903]
- drm/fourcc: Fix vsub/hsub for Q410 and Q401 (Jocelyn Falempe) [2115903]
- amdgpu/pm: prevent array underflow in vega20_odn_edit_dpm_table() (Jocelyn Falempe) [2115903]
- drm/radeon: Add the missed acpi_put_table() to fix memory leak (Jocelyn Falempe) [2115903]
- drm/ttm: fix undefined behavior in bit shift for TTM_TT_FLAG_PRIV_POPULATED (Jocelyn Falempe) [2115903]
- drm/panel/panel-sitronix-st7701: Remove panel on DSI attach failure (Jocelyn Falempe) [2115903]
- drm/amd/display: wait for vblank during pipe programming (Jocelyn Falempe) [2115903]
- drm/i915/guc: Fix GuC error capture sizing estimation and reporting (Jocelyn Falempe) [2115903]
- drm/i915/guc: Add error-capture init warnings when needed (Jocelyn Falempe) [2115903]
- drm/i915/guc: Make GuC log sizes runtime configurable (Jocelyn Falempe) [2115903]
- drm/i915/guc: Fix capture size warning and bump the size (Jocelyn Falempe) [2115903]
- drm/i915/guc: Add a helper for log buffer size (Jocelyn Falempe) [2115903]
- drm/i915: Fix compute pre-emption w/a to apply to compute engines (Jocelyn Falempe) [2115903]
- drm/i915/guc: Limit scheduling properties to avoid overflow (Jocelyn Falempe) [2115903]
- drm/bridge: it6505: Initialize AUX channel in it6505_i2c_probe (Jocelyn Falempe) [2115903]
- drm/amdgpu/powerplay/psm: Fix memory leak in power state init (Jocelyn Falempe) [2115903]
- drm/bridge: adv7533: remove dynamic lane switching from adv7533 bridge (Jocelyn Falempe) [2115903]
- drm/atomic-helper: Don't allocate new plane state in CRTC check (Jocelyn Falempe) [2115903]
- drm/amdgpu/vcn: update vcn4 fw shared data structure (Jocelyn Falempe) [2115903]
- drm: bridge: dw_hdmi: fix preference of RGB modes over YUV420 (Jocelyn Falempe) [2115903]
- drm/bridge: ti-sn65dsi86: Fix output polarity setting bug (Jocelyn Falempe) [2115903]
- drm/vmwgfx: Fix race issue calling pin_user_pages (Jocelyn Falempe) [2115903]
- drm/shmem-helper: Avoid vm_open error paths (Jocelyn Falempe) [2115903]
- drm/shmem-helper: Remove errant put in error path (Jocelyn Falempe) [2115903]
- drm/amd/display: fix array index out of bound error in DCN32 DML (Jocelyn Falempe) [2115903]
- drm/amdgpu/sdma_v4_0: turn off SDMA ring buffer in the s2idle suspend (Jocelyn Falempe) [2115903]
- drm/vmwgfx: Don't use screen objects when SEV is active (Jocelyn Falempe) [2115903]
- drm/amdgpu: fix use-after-free during gpu recovery (Jocelyn Falempe) [2115903]
- drm/amd/display: Use new num clk levels struct for max mclk index (Jocelyn Falempe) [2115903]
- drm/amd/display: Avoid setting pixel rate divider to N/A (Jocelyn Falempe) [2115903]
- drm/amd/display: Use viewport height for subvp mall allocation size (Jocelyn Falempe) [2115903]
- drm/i915: Remove non-existent pipes from bigjoiner pipe mask (Jocelyn Falempe) [2115903]
- drm/i915: Never return 0 if not all requests retired (Jocelyn Falempe) [2115903]
- drm/i915: Fix negative value passed as remaining time (Jocelyn Falempe) [2115903]
- drm/amdgpu: enable Vangogh VCN indirect sram mode (Jocelyn Falempe) [2115903]
- drm/amdgpu: temporarily disable broken Clang builds due to blown stack-frame (Jocelyn Falempe) [2115903]
- drm/amd/pm: update driver if header for smu_13_0_7 (Jocelyn Falempe) [2115903]
- drm/amd/pm: update driver-if header for smu_v13_0_10 (Jocelyn Falempe) [2115903]
- drm/amd/pm: add smu_v13_0_10 driver if version (Jocelyn Falempe) [2115903]
- drm/amdgpu: fix userptr HMM range handling v2 (Jocelyn Falempe) [2115903]
- drm/amdgpu: cleanup error handling in amdgpu_cs_parser_bos (Jocelyn Falempe) [2115903]
- drm/amdgpu: move setting the job resources (Jocelyn Falempe) [2115903]
- drm/amdgpu: Partially revert "drm/amdgpu: update drm_display_info correctly when the edid is read" (Jocelyn Falempe) [2115903]
- drm/amdgpu: always register an MMU notifier for userptr (Jocelyn Falempe) [2115903]
- drm/amd/display: Update soc bounding box for dcn32/dcn321 (Jocelyn Falempe) [2115903]
- drm/amd/amdgpu: reserve vm invalidation engine for firmware (Jocelyn Falempe) [2115903]
- drm/amdgpu: Enable Aldebaran devices to report CU Occupancy (Jocelyn Falempe) [2115903]
- drm/amdgpu/psp: don't free PSP buffers on suspend (Jocelyn Falempe) [2115903]
- drm/amd/display: No display after resume from WB/CB (Jocelyn Falempe) [2115903]
- drm/amd/dc/dce120: Fix audio register mapping, stop triggering KASAN (Jocelyn Falempe) [2115903]
- drm/display/dp_mst: Fix drm_dp_mst_add_affected_dsc_crtcs() return code (Jocelyn Falempe) [2115903]
- drm/i915/ttm: never purge busy objects (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix a memory limit issue (Jocelyn Falempe) [2115903]
- drm/amdgpu: disable BACO support on more cards (Jocelyn Falempe) [2115903]
- drm/amd/display: use uclk pstate latency for fw assisted mclk validation dcn32 (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix calculation for cursor CAB allocation (Jocelyn Falempe) [2115903]
- drm/amd/display: Update MALL SS NumWays calculation (Jocelyn Falempe) [2115903]
- drm/amd/display: Add debug option for allocating extra way for cursor (Jocelyn Falempe) [2115903]
- drm/amd/display: Added debug option for forcing subvp num ways (Jocelyn Falempe) [2115903]
- drm/amdkfd: update GFX11 CWSR trap handler (Jocelyn Falempe) [2115903]
- drm/amdgpu: Enable SA software trap. (Jocelyn Falempe) [2115903]
- dma-buf: Use dma_fence_unwrap_for_each when importing fences (Jocelyn Falempe) [2115903]
- dma-buf: fix racing conflict of dma_heap_add() (Jocelyn Falempe) [2115903]
- drm/i915: Fix warn in intel_display_power_*_domain() functions (Jocelyn Falempe) [2115903]
- drm/amd/display: only fill dirty rectangles when PSR is enabled (Jocelyn Falempe) [2115903]
- drm/amdgpu: Drop eviction lock when allocating PT BO (Jocelyn Falempe) [2115903]
- Revert "drm/amdgpu: Revert "drm/amdgpu: getting fan speed pwm for vega10 properly"" (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix gpio port mapping issue (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix FCLK deviation and tool compile issues (Jocelyn Falempe) [2115903]
- drm/amd/display: Zeromem mypipe heap struct before using it (Jocelyn Falempe) [2115903]
- drm: panel-orientation-quirks: Add quirk for Acer Switch V 10 (SW5-017) (Jocelyn Falempe) [2115903]
- drm: panel-orientation-quirks: Add quirk for Nanote UMPC-01 (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix prefetch calculations for dcn32 (Jocelyn Falempe) [2115903]
- drm/amd/display: don't enable DRM CRTC degamma property for DCE (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix optc2_configure warning on dcn314 (Jocelyn Falempe) [2115903]
- drm/amd/display: Support parsing VRAM info v3.0 from VBIOS (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix access timeout to DPIA AUX at boot time (Jocelyn Falempe) [2115903]
- drm/amd/display: Add HUBP surface flip interrupt handler (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix invalid DPIA AUX reply causing system hang (Jocelyn Falempe) [2115903]
- drm/display: Don't assume dual mode adaptors support i2c sub-addressing (Jocelyn Falempe) [2115903]
- drm/amd/pm: fix SMU13 runpm hang due to unintentional workaround (Jocelyn Falempe) [2115903]
- drm/amd/pm: enable runpm support over BACO for SMU13.0.0 (Jocelyn Falempe) [2115903]
- drm/amd/pm: enable runpm support over BACO for SMU13.0.7 (Jocelyn Falempe) [2115903]
- drm: Fix potential null-ptr-deref in drm_vblank_destroy_worker() (Jocelyn Falempe) [2115903]
- drm/drv: Fix potential memory leak in drm_dev_init() (Jocelyn Falempe) [2115903]
- drm/panel: simple: set bpc field for logic technologies displays (Jocelyn Falempe) [2115903]
- drm/amd/display: Investigate tool reported FCLK P-state deviations (Jocelyn Falempe) [2115903]
- drm/amd/display: Round up DST_after_scaler to nearest int (Jocelyn Falempe) [2115903]
- drm/amd/display: Use forced DSC bpp in DML (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix DCN32 DSC delay calculation (Jocelyn Falempe) [2115903]
- drm/amd: Fail the suspend if resources can't be evicted (Jocelyn Falempe) [2115903]
- drm/amdgpu: set fb_modifiers_not_supported in vkms (Jocelyn Falempe) [2115903]
- drm/amd/display: Enable timing sync on DCN32 (Jocelyn Falempe) [2115903]
- drm/amd/display: Ignore Cable ID Feature (Jocelyn Falempe) [2115903]
- drm/imx: imx-tve: Fix return type of imx_tve_connector_mode_valid (Jocelyn Falempe) [2115903]
- drm/scheduler: fix fence ref counting (Jocelyn Falempe) [2115903]
- drm/amd/display: Don't return false if no stream (Jocelyn Falempe) [2115903]
- drm/amd/display: Remove wrong pipe control lock (Jocelyn Falempe) [2115903]
- drm/amdgpu: Adjust MES polling timeout for sriov (Jocelyn Falempe) [2115903]
- drm/amdkfd: Migrate in CPU page fault use current mm (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix error handling in kfd_criu_restore_events (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix error handling in criu_checkpoint (Jocelyn Falempe) [2115903]
- drm/amdgpu: disable BACO on special BEIGE_GOBY card (Jocelyn Falempe) [2115903]
- drm/amdgpu: workaround for TLB seq race (Jocelyn Falempe) [2115903]
- drm/amd/display: Update SR watermarks for DCN314 (Jocelyn Falempe) [2115903]
- drm/amd/pm: update SMU IP v13.0.4 msg interface header (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix reg timeout in enc314_enable_fifo (Jocelyn Falempe) [2115903]
- drm/i915/dmabuf: fix sg_table handling in map_dma_buf (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix the lpfn checking condition in drm buddy (Jocelyn Falempe) [2115903]
- drm/i915: Do not set cache_dirty for DGFX (Jocelyn Falempe) [2115903]
- drm/i915/psr: Send update also on invalidate (Jocelyn Falempe) [2115903]
- drm/vc4: Fix missing platform_unregister_drivers() call in vc4_drm_register() (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix NULL pointer dereference in svm_migrate_to_ram() (Jocelyn Falempe) [2115903]
- drm/amdkfd: handle CPU fault on COW mapping (Jocelyn Falempe) [2115903]
- drm/amd/display: Set memclk levels to be at least 1 for dcn32 (Jocelyn Falempe) [2115903]
- drm/amd/display: Limit dcn32 to 1950Mhz display clock (Jocelyn Falempe) [2115903]
- drm/amd/display: Acquire FCLK DPM levels on DCN32 (Jocelyn Falempe) [2115903]
- drm/i915/sdvo: Grab mode_config.mutex during LVDS init to avoid WARNs (Jocelyn Falempe) [2115903]
- drm/i915: Simplify intel_panel_add_edid_alt_fixed_modes() (Jocelyn Falempe) [2115903]
- drm/i915: Allow more varied alternate fixed modes for panels (Jocelyn Falempe) [2115903]
- drm/i915/sdvo: Setup DDC fully before output init (Jocelyn Falempe) [2115903]
- drm/i915/sdvo: Filter out invalid outputs more sensibly (Jocelyn Falempe) [2115903]
- drm/amd/display: Update DSC capabilitie for DCN314 (Jocelyn Falempe) [2115903]
- drm/amd/display: Update latencies on DCN321 (Jocelyn Falempe) [2115903]
- drm/amdgpu: disable GFXOFF during compute for GFX11 (Jocelyn Falempe) [2115903]
- drm/i915: stop abusing swiotlb_max_segment (Jocelyn Falempe) [2115903]
- drm/rockchip: fix fbdev on non-IOMMU devices (Jocelyn Falempe) [2115903]
- drm/rockchip: dw_hdmi: filter regulator -EPROBE_DEFER error messages (Jocelyn Falempe) [2115903]
- drm/amdgpu: dequeue mes scheduler during fini (Jocelyn Falempe) [2115903]
- drm/amdgpu: Program GC registers through RLCG interface in gfx_v11/gmc_v11 (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix type of reset_type parameter in hqd_destroy() callback (Jocelyn Falempe) [2115903]
- drm/amd/pm: skip loading pptable from driver on secure board for smu_v13_0_10 (Jocelyn Falempe) [2115903]
- drm/amdgpu: set vm_update_mode=0 as default for Sienna Cichlid in SRIOV case (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix memory leak in kfd_mem_dmamap_userptr() (Jocelyn Falempe) [2115903]
- drm/i915/dp: Reset frl trained flag before restarting FRL training (Jocelyn Falempe) [2115903]
- drm/i915/dgfx: Keep PCI autosuspend control 'on' by default on all dGPU (Jocelyn Falempe) [2115903]
- drm/bridge: ps8640: Add back the 50 ms mystery delay after HPD (Jocelyn Falempe) [2115903]
- drm/msm: Fix return type of mdp4_lvds_connector_mode_valid (Jocelyn Falempe) [2115903]
- drm/msm/hdmi: fix memory corruption with too many bridges (Jocelyn Falempe) [2115903]
- drm/msm/dsi: fix memory corruption with too many bridges (Jocelyn Falempe) [2115903]
- drm/amdkfd: correct the cache info for gfx1036 (Jocelyn Falempe) [2115903]
- drm/amdkfd: update gfx1037 Lx cache setting (Jocelyn Falempe) [2115903]
- drm/amd/display: Revert logic for plane modifiers (Jocelyn Falempe) [2115903]
- drm/amdgpu: fix pstate setting issue (Jocelyn Falempe) [2115903]
- drm/amdgpu: disallow gfxoff until GC IP blocks complete s2idle resume (Jocelyn Falempe) [2115903]
- drm/amdgpu: Remove ATC L2 access for MMHUB 2.1.x (Jocelyn Falempe) [2115903]
- drm/i915: Extend Wa_1607297627 to Alderlake-P (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix for BO move issue (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix VRAM BO swap issue (Jocelyn Falempe) [2115903]
- drm/vc4: Add module dependency on hdmi-codec (Jocelyn Falempe) [2115903]
- drm/amdgpu: fix sdma doorbell init ordering on APUs (Jocelyn Falempe) [2115903]
- drm/amd/pm: update SMU IP v13.0.4 driver interface version (Jocelyn Falempe) [2115903]
- drm/amd/pm: fulfill SMU13.0.0 cstate control interface (Jocelyn Falempe) [2115903]
- drm/amd/pm: disable cstate feature for gpu reset scenario (Jocelyn Falempe) [2115903]
- drm/amd/pm: add SMU IP v13.0.4 IF version define to V7 (Jocelyn Falempe) [2115903]
- drm/amd/pm: fulfill SMU13.0.7 cstate control interface (Jocelyn Falempe) [2115903]
- drm/i915/bios: Use hardcoded fp_timing size for generating LFP data pointers (Jocelyn Falempe) [2115903]
- drm/i915/bios: Validate fp_timing terminator presence (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix build breakage with CONFIG_DEBUG_FS=n (Jocelyn Falempe) [2115903]
- Revert "drm/amd/display: correct hostvm flag" (Jocelyn Falempe) [2115903]
- drm/amdkfd: Fix UBSAN shift-out-of-bounds warning (Jocelyn Falempe) [2115903]
- drm/amd/display: polling vid stream status in hpo dp blank (Jocelyn Falempe) [2115903]
- drm/amd/display: Remove interface for periodic interrupt 1 (Jocelyn Falempe) [2115903]
- drm/dp: Don't rewrite link config when setting phy test pattern (Jocelyn Falempe) [2115903]
- drm/amdgpu: fix initial connector audio value (Jocelyn Falempe) [2115903]
- drm/amd/display: correct hostvm flag (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix urgent latency override for DCN32/DCN321 (Jocelyn Falempe) [2115903]
- drm/amdgpu: SDMA update use unlocked iterator (Jocelyn Falempe) [2115903]
- drm: panel-orientation-quirks: Add quirk for Aya Neo Air (Jocelyn Falempe) [2115903]
- drm: panel-orientation-quirks: Add quirk for Anbernic Win600 (Jocelyn Falempe) [2115903]
- drm/vc4: vec: Fix timings for VEC modes (Jocelyn Falempe) [2115903]
- drm/admgpu: Skip CG/PG on SOC21 under SRIOV VF (Jocelyn Falempe) [2115903]
- drm/amdgpu: Skip the program of MMMC_VM_AGP_* in SRIOV on MMHUB v3_0_0 (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix variable dereferenced before check (Jocelyn Falempe) [2115903]
- drm: bridge: dw_hdmi: only trigger hotplug event on link change (Jocelyn Falempe) [2115903]
- drm/amd: fix potential memory leak (Jocelyn Falempe) [2115903]
- udmabuf: Set ubuf->sg = NULL if the creation of sg table fails (Jocelyn Falempe) [2115903]
- drm/amd/display: fix overflow on MIN_I64 definition (Jocelyn Falempe) [2115903]
- gpu: lontium-lt9611: Fix NULL pointer dereference in lt9611_connector_init() (Jocelyn Falempe) [2115903]
- drm: Prevent drm_copy_field() to attempt copying a NULL pointer (Jocelyn Falempe) [2115903]
- drm: Use size_t type for len variable in drm_copy_field() (Jocelyn Falempe) [2115903]
- drm/nouveau/nouveau_bo: fix potential memory leak in nouveau_bo_alloc() (Jocelyn Falempe) [2115903]
- virtio-gpu: fix shift wrapping bug in virtio_gpu_fence_event_create() (Jocelyn Falempe) [2115903]
- drm/vmwgfx: Fix memory leak in vmw_mksstat_add_ioctl() (Jocelyn Falempe) [2115903]
- drm/amdgpu: Fix memory leak in hpd_rx_irq_create_workqueue() (Jocelyn Falempe) [2115903]
- drm/bochs: fix blanking (Jocelyn Falempe) [2115903]
- drm/virtio: set fb_modifiers_not_supported (Jocelyn Falempe) [2115903]
- drm/bridge: it6505: Fix the order of DP_SET_POWER commands (Jocelyn Falempe) [2115903]
- drm/bridge: megachips: Fix a null pointer dereference bug (Jocelyn Falempe) [2115903]
- drm/amdgpu: add missing pci_disable_device() in amdgpu_pmops_runtime_resume() (Jocelyn Falempe) [2115903]
- drm: fix drm_mipi_dbi build errors (Jocelyn Falempe) [2115903]
- drm/panel: use 'select' for Ili9341 panel driver helpers (Jocelyn Falempe) [2115903]
- drm/virtio: Fix same-context optimization (Jocelyn Falempe) [2115903]
- drm/i915/dg2: Bump up CDCLK for DG2 (Jocelyn Falempe) [2115903]
- drm/dp_mst: fix drm_dp_dpcd_read return value checks (Jocelyn Falempe) [2115903]
- drm/format-helper: Fix test on big endian architectures (Jocelyn Falempe) [2115903]
- drm/bridge: parade-ps8640: Fix regulator supply order (Jocelyn Falempe) [2115903]
- drm/bridge: tc358767: Add of_node_put() when breaking out of loop (Jocelyn Falempe) [2115903]
- drm/bridge: anx7625: Fix refcount bug in anx7625_parse_dt() (Jocelyn Falempe) [2115903]
- drm/virtio: Correct drm_gem_shmem_get_sg_table() error handling (Jocelyn Falempe) [2115903]
- drm/bridge: it6505: Power on downstream device in .atomic_enable (Jocelyn Falempe) [2115903]
- drm/mipi-dsi: Detach devices when removing the host (Jocelyn Falempe) [2115903]
- drm/bridge: Avoid uninitialized variable warning (Jocelyn Falempe) [2115903]
- drm: bridge: adv7511: unregister cec i2c device after cec adapter (Jocelyn Falempe) [2115903]
- drm: bridge: adv7511: fix CEC power down control register offset (Jocelyn Falempe) [2115903]
- drm/amdgpu: Enable F32_WPTR_POLL_ENABLE in mqd (Jocelyn Falempe) [2115903]
- drm/amdgpu: Enable VCN PG on GC11_0_1 (Jocelyn Falempe) [2115903]
- drm/amd/display: explicitly disable psr_feature_enable appropriately (Jocelyn Falempe) [2115903]
- drm/amd/display: Add HUBP surface flip interrupt handler (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix vblank refcount in vrr transition (Jocelyn Falempe) [2115903]
- drm/amd/display: Enable 2 to 1 ODM policy if supported (Jocelyn Falempe) [2115903]
- drm/amd/display: Enable dpia support for dcn314 (Jocelyn Falempe) [2115903]
- drm/amd/display: Validate DSC After Enable All New CRTCs (Jocelyn Falempe) [2115903]
- drm/amd/display: zeromem mypipe heap struct before using it (Jocelyn Falempe) [2115903]
- drm/amd/display: Update PMFW z-state interface for DCN314 (Jocelyn Falempe) [2115903]
- drm/amd/display: Fix watermark calculation (Jocelyn Falempe) [2115903]
- drm/i915: Fix display problems after resume (Jocelyn Falempe) [2115903]
- drm/i915/guc: Fix revocation of non-persistent contexts (Jocelyn Falempe) [2115903]
- drm/i915/gt: Use i915_vm_put on ppgtt_create error paths (Jocelyn Falempe) [2115903]
- drm/nouveau: fix a use-after-free in nouveau_gem_prime_import_sg_table() (Jocelyn Falempe) [2115903]
- drm/udl: Restore display mode on resume (Jocelyn Falempe) [2115903]
- drm/virtio: Use appropriate atomic state in virtio_gpu_plane_cleanup_fb() (Jocelyn Falempe) [2115903]
- drm/virtio: Unlock reservations on dma_resv_reserve_fences() error (Jocelyn Falempe) [2115903]
- drm/virtio: Unlock reservations on virtio_gpu_object_shmem_init() error (Jocelyn Falempe) [2115903]
- drm/virtio: Check whether transferred 2D BO is shmem (Jocelyn Falempe) [2115903]
- Revert "drm/amdgpu: use dirty framebuffer helper" (Jocelyn Falempe) [2115903]

* Mon Feb 13 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-467.el8]
- nvme: fix SRCU protection of nvme_ns_head list (Ewan D. Milne) [2113865]
- perf vendor events power10: Fix hv-24x7 metric events (Mamatha Inamdar) [2149192]
- perf tests: Fix 'perf probe' error log check in skip_if_no_debuginfo (Mamatha Inamdar) [2149192]
- perf tests: Fix *probe_vfs_getname.sh test failures (Mamatha Inamdar) [2149192]
- blk-cgroup: Optimize blkcg_rstat_flush() (Waiman Long) [2162173]
- blk-cgroup: Return -ENOMEM directly in blkcg_css_alloc() error path (Waiman Long) [2162173]
- blk-cgroup: factor out blkcg_iostat_update() (Waiman Long) [2162173]
- mm/memcg: Free percpu stats memory of dying memcg's again (Waiman Long) [2162173]
- memcg: sync flush only if periodic flush is delayed (Waiman Long) [2162173]
- memcg: better bounds on the memcg stats updates (Waiman Long) [2162173]
- memcg: unify memcg stat flushing (Waiman Long) [2162173]
- memcg: flush stats only if updated (Waiman Long) [2162173]
- memcg: flush lruvec stats in the refault (Waiman Long) [2162173]
- memcg: infrastructure to flush memcg stats (Waiman Long) [2162173]
- memcg: switch lruvec stats to rstat (Waiman Long) [2162173]
- mm/memcg: Remove mem_cgroup_per_node from being kABI protected (Waiman Long) [2162173]
- mm/memcg: Revert "Free percpu stats memory of dying memcg's" (Waiman Long) [2162173]

* Mon Feb 13 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-466.el8]
- virt/sev-guest: Prevent IV reuse in the SNP guest driver (John Allen) [2087262]
- virt/sev-guest: Add a MODULE_ALIAS (John Allen) [2087262]
- virt/sev-guest: Remove unnecessary free in init_crypto() (John Allen) [2087262]
- x86/sev: Don't use cc_platform_has() for early SEV-SNP calls (John Allen) [2087262]
- x86/boot: Don't propagate uninitialized boot_params->cc_blob_address (John Allen) [2087262]
- x86/idt: Rework IDT setup for boot CPU (John Allen) [2087262]
- x86/cpu: Init AP exception handling from cpu_init_secondary() (John Allen) [2087262]
- x86/idt: Cleanup trap_init() (John Allen) [2087262]
- x86/idt: Annotate alloc_intr_gate() with __init (John Allen) [2087262]
- redhat/configs: enable CONFIG_SEV_GUEST (John Allen) [2087262]
- virt: sev-guest: Pass the appropriate argument type to iounmap() (John Allen) [2087262]
- x86/compressed/64: Add identity mappings for setup_data entries (John Allen) [2087262]
- x86/sev: Mark the code returning to user space as syscall gap (John Allen) [2087262]
- x86/sev: Annotate stack change in the #VC handler (John Allen) [2087262]
- x86/sev: Remove duplicated assignment to variable info (John Allen) [2087262]
- x86/sev: Fix address space sparse warning (John Allen) [2087262]
- x86/sev: Get the AP jump table address from secrets page (John Allen) [2087262]
- x86/sev: Add missing __init annotations to SEV init routines (John Allen) [2087262]
- virt: sevguest: Rename the sevguest dir and files to sev-guest (John Allen) [2087262]
- virt: sevguest: Change driver name to reflect generic SEV support (John Allen) [2087262]
- x86/boot: Put globals that are accessed early into the .data section (John Allen) [2087262]
- x86/boot: Add an efi.h header for the decompressor (John Allen) [2087262]
- virt: sevguest: Fix bool function returning negative value (John Allen) [2087262]
- virt: sevguest: Fix return value check in alloc_shared_pages() (John Allen) [2087262]
- x86/sev: Unroll string mmio with CC_ATTR_GUEST_UNROLL_STRING_IO (John Allen) [2087262]
- x86/sev-es: Replace open-coded hlt-loop with sev_es_terminate() (John Allen) [2087262]
- virt: sevguest: Add documentation for SEV-SNP CPUID Enforcement (John Allen) [2087262]
- virt: sevguest: Add support to get extended report (John Allen) [2087262]
- virt: sevguest: Add support to derive key (John Allen) [2087262]
- virt: Add SEV-SNP guest driver (John Allen) [2087262]
- x86/sev: Register SEV-SNP guest request platform device (John Allen) [2087262]
- x86/sev: Provide support for SNP guest request NAEs (John Allen) [2087262]
- x86/sev: Add a sev= cmdline option (John Allen) [2087262]
- x86/sev: Use firmware-validated CPUID for SEV-SNP guests (John Allen) [2087262]
- x86/sev: Add SEV-SNP feature detection/setup (John Allen) [2087262]
- x86/sev: Check SME/SEV support in CPUID first (John Allen) [2087262]
- x86/compressed/64: Add identity mapping for Confidential Computing blob (John Allen) [2087262]
- x86/compressed: Export and rename add_identity_map() (John Allen) [2087262]
- x86/compressed: Use firmware-validated CPUID leaves for SEV-SNP guests (John Allen) [2087262]
- x86/compressed: Add SEV-SNP feature detection/setup (John Allen) [2087262]
- x86/boot: Add a pointer to Confidential Computing blob in bootparams (John Allen) [2087262]
- x86/boot: Preserve boot_params.secure_boot from sanitizing (John Allen) [2087262]
- x86/boot: Fix boot regression caused by bootparam sanitizing (John Allen) [2087262]
- x86/boot: Save fields explicitly, zero out everything else (John Allen) [2087262]
- x86/compressed/64: Add support for SEV-SNP CPUID table in #VC handlers (John Allen) [2087262]
- x86/sev: Move MSR-based VMGEXITs for CPUID to helper (John Allen) [2087262]
- KVM: x86: Move lookup of indexed CPUID leafs to helper (John Allen) [2087262]
- x86/boot: Add Confidential Computing type to setup_data (John Allen) [2087262]
- x86/compressed/acpi: Move EFI kexec handling into common code (John Allen) [2087262]
- x86/compressed/acpi: Move EFI vendor table lookup to helper (John Allen) [2087262]
- x86/compressed/acpi: Move EFI config table lookup to helper (John Allen) [2087262]
- x86/compressed/acpi: Move EFI system table lookup to helper (John Allen) [2087262]
- x86/compressed/acpi: Move EFI detection to helper (John Allen) [2087262]
- x86/head/64: Re-enable stack protection (John Allen) [2087262]
- x86/sev: Use SEV-SNP AP creation to start secondary CPUs (John Allen) [2087262]
- x86/apic/of: Fix CPU devicetree-node lookups (John Allen) [2087262]
- x86/mm: Validate memory when changing the C-bit (John Allen) [2087262]
- x86/kernel: Validate ROM memory before accessing when SEV-SNP is active (John Allen) [2087262]
- x86/kernel: Mark the .bss..decrypted section as shared in the RMP table (John Allen) [2087262]
- x86/sev: Add helper for validating pages in early enc attribute changes (John Allen) [2087262]
- x86/sev: Register GHCB memory when SEV-SNP is active (John Allen) [2087262]
- x86/compressed: Register GHCB memory when SEV-SNP is active (John Allen) [2087262]
- x86/compressed: Add helper for validating pages in the decompression stage (John Allen) [2087262]
- x86/sev: Check the VMPL level (John Allen) [2087262]
- x86/sev: Add a helper for the PVALIDATE instruction (John Allen) [2087262]
- x86/sev: Check SEV-SNP features support (John Allen) [2087262]
- x86/mm: Extend cc_attr to include AMD SEV-SNP (John Allen) [2087262]
- x86/sev: Detect/setup SEV/SME features earlier in boot (John Allen) [2087262]
- x86/compressed/64: Detect/setup SEV/SME features earlier during boot (John Allen) [2087262]
- x86/boot: Use MSR read/write helpers instead of inline assembly (John Allen) [2087262]
- x86/boot: Introduce helpers for MSR reads/writes (John Allen) [2087262]
- KVM: SVM: Update the SEV-ES save area mapping (John Allen) [2087262]
- KVM: SVM: Create a separate mapping for the GHCB save area (John Allen) [2087262]
- KVM: SVM: Create a separate mapping for the SEV-ES save area (John Allen) [2087262]
- KVM: SVM: Define sev_features and VMPL field in the VMSA (John Allen) [2087262]
- x86/sev: Remove do_early_exception() forward declarations (John Allen) [2087262]
- x86/sev: Make the #VC exception stacks part of the default stacks storage (John Allen) [2087262]
- x86: Increase exception stack sizes (John Allen) [2087262]
- x86/head64: Carve out the guest encryption postprocessing into a helper (John Allen) [2087262]
- x86/sev: Get rid of excessive use of defines (John Allen) [2087262]
- x86/sev: Add defines for GHCB version 2 MSR protocol requests (John Allen) [2087262]
- x86/sev: Make sure IRQs are disabled while GHCB is active (John Allen) [2087262]
- x86/sev: Propagate #GP if getting linear instruction address failed (John Allen) [2087262]
- x86/insn: Extend error reporting from insn_fetch_from_user[_inatomic]() (John Allen) [2087262]
- x86/sev-es: Convert to insn_decode() (John Allen) [2087262]
- x86/sev-es: Split vc_decode_insn() (John Allen) [2087262]
- x86/insn-eval: Make 0 a valid RIP for insn_get_effective_ip() (John Allen) [2087262]
- x86/sev: Fix error message in runtime #VC handler (John Allen) [2087262]
- x86/sev-es: Optimize __sev_es_ist_enter() for better readability (John Allen) [2087262]
- x86/sev: Do not require Hypervisor CPUID bit for SEV guests (John Allen) [2087262]
- x86/boot/compressed/64: Cleanup exception handling before booting kernel (John Allen) [2087262]
- x86/sev-es: Remove subtraction of res variable (John Allen) [2087262]

* Thu Feb 09 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-465.el8]
- net: mlx5: eliminate anonymous module_init & module_exit (Amir Tzin) [2157750]
- net/mlx5: E-switch, Fix switchdev mode after devlink reload (Amir Tzin) [2157750]
- net/mlx5e: Set decap action based on attr for sample (Amir Tzin) [2157750]
- net/mlx5e: QoS, Fix wrongfully setting parent_element_id on MODIFY_SCHEDULING_ELEMENT (Amir Tzin) [2157750]
- net/mlx5: E-switch, Fix setting of reserved fields on MODIFY_SCHEDULING_ELEMENT (Amir Tzin) [2157750]
- net/mlx5e: Avoid false lock dependency warning on tc_ht even more (Amir Tzin) [2157750]
- net/mlx5: fix missing mutex_unlock in mlx5_fw_fatal_reporter_err_work() (Amir Tzin) [2157750]
- net/mlx5: Fix ptp max frequency adjustment range (Amir Tzin) [2157750]
- net/mlx5e: IPoIB, Fix child PKEY interface stats on rx path (Amir Tzin) [2157750]
- net/mlx5e: IPoIB, Block PKEY interfaces with less rx queues than parent (Amir Tzin) [2157750]
- net/mlx5e: IPoIB, Block queue count configuration when sub interfaces are present (Amir Tzin) [2157750]
- net/mlx5e: Verify dev is present for fix features ndo (Amir Tzin) [2157750]
- net/mlx5: Fix command stats access after free (Amir Tzin) [2157750]
- net/mlx5e: TC, Keep mod hdr actions after mod hdr alloc (Amir Tzin) [2157750]
- net/mlx5: check attr pointer validity before dereferencing it (Amir Tzin) [2157750]
- RDMA/mlx5: Fix validation of max_rd_atomic caps for DC (Amir Tzin) [2157750]
- RDMA/mlx5: Fix mlx5_ib_get_hw_stats when used for device (Amir Tzin) [2157750]
- net/mlx5e: Set geneve_tlv_option_0_exist when matching on geneve option (Amir Tzin) [2157750]
- net/mlx5e: Fix hw mtu initializing at XDP SQ allocation (Amir Tzin) [2157750]
- net/mlx5e: Always clear dest encap in neigh-update-del (Amir Tzin) [2157750]
- net/mlx5e: CT: Fix ct debugfs folder name (Amir Tzin) [2157750]
- net/mlx5e: IPoIB, Don't allow CQE compression to be turned on by default (Amir Tzin) [2157750]
- net/mlx5: Fix RoCE setting at HCA level (Amir Tzin) [2157750]
- net/mlx5: Avoid recovery in probe flows (Amir Tzin) [2157750]
- net/mlx5: Fix io_eq_size and event_eq_size params validation (Amir Tzin) [2157750]
- net/mlx5: Add forgotten cleanup calls into mlx5_init_once() error path (Amir Tzin) [2157750]
- net/mlx5: E-Switch, properly handle ingress tagged packets on VST (Amir Tzin) [2157750 2096109]
- dm thin: Use last transaction's pmd->root when commit failed (Benjamin Marzinski) [2162537]
- dm thin: resume even if in FAIL mode (Benjamin Marzinski) [2162537]
- dm cache: set needs_check flag after aborting metadata (Benjamin Marzinski) [2162537]
- dm cache: Fix ABBA deadlock between shrink_slab and dm_cache_metadata_abort (Benjamin Marzinski) [2162537]
- dm thin: Fix ABBA deadlock between shrink_slab and dm_pool_abort_metadata (Benjamin Marzinski) [2162537]
- dm integrity: Fix UAF in dm_integrity_dtr() (Benjamin Marzinski) [2162537]
- dm cache: Fix UAF in destroy() (Benjamin Marzinski) [2162537]
- dm thin: Fix UAF in run_timer_softirq() (Benjamin Marzinski) [2162537]
- dm integrity: clear the journal on suspend (Benjamin Marzinski) [2162537]
- dm integrity: flush the journal on suspend (Benjamin Marzinski) [2162537]
- dm bufio: Fix missing decrement of no_sleep_enabled if dm_bufio_client_create failed (Benjamin Marzinski) [2162537]
- dm ioctl: fix misbehavior if list_versions races with module loading (Benjamin Marzinski) [2162537]

* Thu Feb 09 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-464.el8]
- net: gso: fix panic on frag_list with mixed head alloc types (Jiri Benc) [2136229]
- futex: Resend potentially swallowed owner death notification (Rafael Aquini) [2161526]
- Bluetooth: L2CAP: Fix memory leak in vhci_write (Wander Lairson Costa) [2155872] {CVE-2022-3619}
- net: Use this_cpu_inc() to increment net->core_stats (Antoine Tenart) [2152542]
- vlan: fix memory leak in vlan_newlink() (Xin Long) [2051415]
- vlan: move dev_put into vlan_dev_uninit (Xin Long) [2051415]
- vlan: introduce vlan_dev_free_egress_priority (Xin Long) [2051415]
- vlan: fix memory leak in vlan_dev_set_egress_priority (Xin Long) [2051415]
- net: ethernet: move from strlcpy with unused retval to strscpy (Ken Cox) [2103956]
- intel/ixgbevf:fix repeated words in comments (Ken Cox) [2103956]
- intel: remove unused macros (Ken Cox) [2103956]
- ixgbe: propagate XFRM offload state direction instead of flags (Ken Cox) [2103956]
- ixgbevf: add disable link state (Ken Cox) [2103956]
- ixgbevf: clean up some inconsistent indenting (Ken Cox) [2103956]
- ethernet: use eth_hw_addr_set() instead of ether_addr_copy() (Ken Cox) [2103956]
- intel: Remove rcu_read_lock() around XDP program invocation (Ken Cox) [2103956]

* Thu Feb 09 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-463.el8]
- RDMA/siw: Always consume all skbuf data in sk_data_ready() upcall. (Kamal Heib) [2141420]
- cifs: fix use-after-free caused by invalid pointer `hostname` (Ronnie Sahlberg) [2154172]
- ceph: blocklist the kclient when receiving corrupted snap trace (Xiubo Li) [2162414]
- ceph: move mount state enum to super.h (Xiubo Li) [2162414]
- xfs: estimate post-merge refcounts correctly (Bill O'Donnell) [2161678]
- xfs: hoist refcount record merge predicates (Bill O'Donnell) [2161678]
- NFS: Fix revalidation of empty readdir pages (Benjamin Coddington) [2166364]
- NFS: Don't deadlock when cookie hashes collide (Benjamin Coddington) [2166364]
- locking/rwsem: Disable preemption in all down_read*() and up_read() code paths (Waiman Long) [2162139]
- locking/rwsem: Prevent non-first waiter from spinning in down_write() slowpath (Waiman Long) [2162139]
- locking/rwsem: Allow slowpath writer to ignore handoff bit if not set by first waiter (Waiman Long) [2162139]
- locking/rwsem: Always try to wake waiters in out_nolock path (Waiman Long) [2162139]
- locking/rwsem: No need to check for handoff bit if wait queue empty (Waiman Long) [2162139]
- locking/rwsem: Make handoff bit handling more consistent (Waiman Long) [2162139]
- dax: fix ENOMEM handling in grab_mapping_entry() (Andrey Albershteyn) [2128474]
- crypto: ccp - Failure on re-initialization due to duplicate sysfs filename (Vladis Dronov) [2130714]
- crypto: ccp - Avoid page allocation failure warning for SEV_GET_ID2 (Vladis Dronov) [2130714]
- crypto: ccp - Add support for TEE for PCI ID 0x14CA (Vladis Dronov) [2130714]
- crypto: ccp - Remove unused struct ccp_crypto_cpu (Vladis Dronov) [2130714]
- crypto: ccp - Add __init/__exit annotations to module init/exit funcs (Vladis Dronov) [2130714]
- i40e: Fix the inability to attach XDP program on downed interface (Ivan Vecera) [2121511]
- mm, compaction: fix fast_isolate_around() to stay within boundaries (Daniel Vacek) [2149309]

* Wed Feb 08 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-462.el8]
- aio: fix mremap after fork null-deref (Jeff Moyer) [2166088]
- mm/hugetlb: use hugetlb_pte_stable in migration race check (Rafael Aquini) [2158120] {CVE-2022-3522}
- mm/hugetlb: fix race condition of uffd missing/minor handling (Rafael Aquini) [2158120] {CVE-2022-3522}
- mm/hugetlb: simplify the code when alloc_huge_page() failed in hugetlb_no_page() (Rafael Aquini) [2158120] {CVE-2022-3522}
- mm/hugetlb: pass the old pte entry value to hugetlb_no_page() (Rafael Aquini) [2158120] {CVE-2022-3522}
- perf/arm-cmn: Add more bits to child node address offset field (Charles Mirabile) [2122267]
- perf/arm-cmn: Decode CAL devices properly in debugfs (Charles Mirabile) [2122267]
- perf/arm-cmn: Fix filter_sel lookup (Charles Mirabile) [2122267]
- drivers/perf: arm_spe: Expose saturating counter to 16-bit (Charles Mirabile) [2122267]
- perf/arm-cmn: Add CMN-700 support (Charles Mirabile) [2122267]
- perf/arm-cmn: Refactor occupancy filter selector (Charles Mirabile) [2122267]
- perf/arm-cmn: Add CMN-650 support (Charles Mirabile) [2122267]
- perf: check return value of armpmu_request_irq() (Charles Mirabile) [2122267]
- arm_pmu: Validate single/group leader events (Charles Mirabile) [2122267]
- perf: qcom_l2_pmu: fix an incorrect NULL check on list iterator (Charles Mirabile) [2122267]
- drivers/perf: arm_pmu: Handle 47 bit counters (Charles Mirabile) [2122267]
- perf/arm-cmn: Update watchpoint format (Charles Mirabile) [2122267]
- perf/arm-cmn: Hide XP PUB events for CMN-600 (Charles Mirabile) [2122267]
- perf: replace bitmap_weight with bitmap_empty where appropriate (Charles Mirabile) [2122267]
- perf: Replace acpi_bus_get_device() (Charles Mirabile) [2122267]
- perf/arm-cmn: Make arm_cmn_debugfs static (Charles Mirabile) [2122267]
- perf/arm-ccn: Use platform_get_irq() to get the interrupt (Charles Mirabile) [2122267]
- perf/smmuv3: Don't cast parameter in bit operations (Charles Mirabile) [2122267]
- perf/smmuv3: Use msi_get_virq() (Charles Mirabile) [2122267]
- perf/smmuv3: Synthesize IIDR from CoreSight ID registers (Charles Mirabile) [2122267]
- perf/arm-cmn: Add debugfs topology info (Charles Mirabile) [2122267]
- perf/arm-cmn: Add CI-700 Support (Charles Mirabile) [2122267]
- perf/arm-cmn: Support new IP features (Charles Mirabile) [2122267]
- devres: provide devm_krealloc() (Charles Mirabile) [2122267]
- devres: move the size check from alloc_dr() into a separate function (Charles Mirabile) [2122267]
- perf/arm-cmn: Demarcate CMN-600 specifics (Charles Mirabile) [2122267]
- perf/arm-cmn: Move group validation data off-stack (Charles Mirabile) [2122267]
- perf/arm-cmn: Optimise DTC counter accesses (Charles Mirabile) [2122267]
- perf/arm-cmn: Optimise DTM counter reads (Charles Mirabile) [2122267]
- perf/arm-cmn: Refactor DTM handling (Charles Mirabile) [2122267]
- perf/arm-cmn: Streamline node iteration (Charles Mirabile) [2122267]
- perf/arm-cmn: Refactor node ID handling (Charles Mirabile) [2122267]
- perf/arm-cmn: Drop compile-test restriction (Charles Mirabile) [2122267]
- perf/arm-cmn: Account for NUMA affinity (Charles Mirabile) [2122267]
- perf/arm-cmn: Fix CPU hotplug unregistration (Charles Mirabile) [2122267]
- drivers/perf: thunderx2_pmu: Change data in size tx2_uncore_event_update() (Charles Mirabile) [2122267]
- perf: qcom_l2_pmu: move to use request_irq by IRQF_NO_AUTOEN flag (Charles Mirabile) [2122267]
- arm_pmu: move to use request_irq by IRQF_NO_AUTOEN flag (Charles Mirabile) [2122267]
- arm64: perf: Fix 64-bit event counter read truncation (Charles Mirabile) [2122267]
- drivers/perf: Replace spin_lock_irqsave to spin_lock (Charles Mirabile) [2122267]
- arm_pmu: arm64: Use NMIs for PMU (Charles Mirabile) [2122267]
- arm_pmu: Introduce pmu_irq_ops (Charles Mirabile) [2122267]
- arm64: perf: Defer irq_work to IPI_IRQ_WORK (Charles Mirabile) [2122267]
- arm64: perf: Remove PMU locking (Charles Mirabile) [2122267]
- arm64: perf: Avoid PMXEV* indirection (Charles Mirabile) [2122267]
- arm64: perf: Add missing ISB in armv8pmu_enable_counter() (Charles Mirabile) [2122267]
- perf: arm_spe: Remove unnecessary zero check on 'nr_pages' (Charles Mirabile) [2122267]
- drivers/perf: arm_pmu_acpi: Fix incorrect checking of gicc pointer (Charles Mirabile) [2122267]
- perf/smmuv3: Use platform_get_irq_optional() for wired interrupt (Charles Mirabile) [2122267]

* Wed Feb 08 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-461.el8]
- wifi: rtw89: Add missing check for alloc_workqueue (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: fix potential leak in rtw89_append_probe_req_ie() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix initialization of rx->link and rx->link_sta (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: Drop stations iterator where the iterator function may sleep (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath9k: use proper statements in conditionals (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix MLO + AP_VLAN check (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: fix coverity uninit_use_in_call in mt76_connac2_reverse_frag0_hdr_trans() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: nl80211: Add checks for nla_nest_start() in nl80211_send_iface() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: Add missing __packed annotation of struct mt7921_clc (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: do not send firmware FW_FEATURE_NON_DL region (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: Fix use after rcu_read_unlock in rtl8xxxu_bss_info_changed (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: fix physts IE page check (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: fix wrong power after multiple SAR set (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: Fix some error handling path in rtw89_core_sta_assoc() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: use u32_encode_bits() to fill MAC quota value (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: fix reporting of TX AGGR histogram (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix ifdef symbol name (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: fix firmware assert during bandwidth change for peer sta (Jose Ignacio Tornos Martinez) [2136125]
- Revert "mt76: use IEEE80211_OFFLOAD_ENCAP_ENABLED instead of MT_DRV_AMSDU_OFFLOAD" (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: gen2: Turn on the rate control (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: fix warning in dma_free_coherent() of memory chunks while recovery (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: check link ID in auth/assoc continuation (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: mlme: fix null-ptr deref on failed assoc (Jose Ignacio Tornos Martinez) [2136125]
- wifi: fix multi-link element subelement iteration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: fix antenna signal are way off in monitor mode (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac8021: fix possible oob access in ieee80211_get_rate_duration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: don't allow multi-BSSID in S1G (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: fix buffer overflow in elem comparison (Jose Ignacio Tornos Martinez) [2136125]
- net: mhi: Fix memory leak in mhi_net_dellink() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Fix QCN9074 firmware boot on x86 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: Set TWT Information Frame Disabled bit as 1 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: Fix ack frame idr leak when mesh has no route (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix general-protection-fault in ieee80211_subif_start_xmit() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: fix debugfs attribute ps with rc table support (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: Fix bitrates overflow issue (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: fix memory leak in query_regdb_file() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix memory free error when registering wiphy fail (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: silence a sparse RCU warning (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: use explicitly signed or unsigned types (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: mac: fix reading 16 bytes from a region of size 0 warning (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: fix rx checksum offload on mt7615/mt7915/mt7921 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: fix receiving LLC packets on mt7615/mt7915 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: update hidden BSSes to avoid WARN_ON (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix crash in beacon protection for P2P-device (Jose Ignacio Tornos Martinez) [2136125 2134582] {CVE-2022-42722}
- wifi: mac80211_hwsim: avoid mac80211 warning on bad rate (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: avoid nontransmitted BSS list corruption (Jose Ignacio Tornos Martinez) [2136125 2134511] {CVE-2022-42721}
- wifi: cfg80211: fix BSS refcounting bugs (Jose Ignacio Tornos Martinez) [2136125 2134460] {CVE-2022-42720}
- wifi: cfg80211: ensure length byte is present before access (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix MBSSID parsing use-after-free (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211/mac80211: reject bad MBSSID elements (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: fix u8 overflow in cfg80211_update_notlisted_nontrans() (Jose Ignacio Tornos Martinez) [2136125 2134385] {CVE-2022-41674}
- wifi: nl80211: Split memcpy() of struct nl80211_wowlan_tcp_data_token flexible array (Jose Ignacio Tornos Martinez) [2136125]
- wifi: wext: use flex array destination for memcpy() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: fix ieee80211_data_to_8023_exthdr handling of small packets (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: netdev compatible TX stop for iTXQ drivers (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix decap offload for stations on AP_VLAN interfaces (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: unlock on error in ieee80211_can_powered_addr_change() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: remove/avoid misleading prints (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix probe req HE capabilities access (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: do not drop packets smaller than the LLC-SNAP header on fast-rx (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: fix rate reporting / throughput regression on mt7915 and newer (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: Improve rtl8xxxu_queue_select (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: Fix AIFS written to REG_EDCA_*_PARAM (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: gen2: Enable 40 MHz channel width (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852b: configure DLE mem (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: check DLE FIFO size with reserved size (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: mac: correct register of report IMR (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: set power cut closed for 8852be (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: add to do PCI auto calibration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852b: implement chip_ops::{enable,disable}_bb_rf (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: add DMA busy checking bits to chip info (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: mac: define DMA channel mask to avoid unsupported channels (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: mask out unsupported TX channels (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: Track scan_cmd allocation size explicitly (Jose Ignacio Tornos Martinez) [2136125]
- brcmfmac: Remove the call to "dtim_assoc" IOVAR (Jose Ignacio Tornos Martinez) [2136125]
- brcmfmac: increase dcmd maximum buffer size (Jose Ignacio Tornos Martinez) [2136125]
- brcmfmac: Support 89459 pcie (Jose Ignacio Tornos Martinez) [2136125]
- brcmfmac: increase default max WOWL patterns to 16 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Fix deadlock during WoWLAN suspend (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Remove redundant ath11k_mac_drain_tx (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Add spectral scan support for 160 MHz (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Add support to get power save duration for each client (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: fix peer addition/deletion error on sta band migration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support for enable/disable MSDU aggregation (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: disable 26-tone RU HE TB PPDU transmissions (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support for processing P2P power saving (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support WMM-PS in P2P GO mode (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: set wifi_role of P2P (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: send OFDM rate only in P2P mode (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support P2P (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: correctly set BBP register 86 for MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: set SoC wmac clock register (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: set VGC gain for both chains of MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: set correct TX_SW_CFG1 MAC register for MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: fix HT20/HT40 bandwidth switch on MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: move helper functions up in file (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: add TX LOFT calibration for MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: don't run Rt5592 IQ calibration on MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: add RXIQ calibration for MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: add RXDCOC calibration for MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: add r calibration for MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: add RF self TXDC calibration for MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: move up and reuse busy wait functions (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: add support for external PA on MT7620 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: add throughput LED trigger (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: define RF5592 in init_eeprom routine (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: fix number of VHT beamformee spatial streams (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: retrieve MAC address from system firmware if provided (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: add get_txpower mac ops (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: move firmware stats out of debugfs (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath9k: fix repeated the words in a comment (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath9k: fix repeated to words in a comment (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath10k: reset pointer after memory free to avoid potential use-after-free (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: fix failed to find the peer with peer_id 0 when disconnected (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: change complete() to complete_all() for scan.completed (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: update coexistence to 6.3.0 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: add logic to control BT scan priority (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: summarize Wi-Fi to BT scoreboard and inform BT one time a cycle (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: modify LNA2 setting to avoid BT destroyed Wi-Fi aggregation (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: add WL_S0 hardware TX/RX mask to allow WL_S0 TX/RX during GNT_BT (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: add v1 Wi-Fi firmware steps report (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: add v1 summary info to parse the traffic status from firmware (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: translate slot ID to readable name (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: add v1 cycle report to parsing Bluetooth A2DP status (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mwifiex: fix array of flexible structures warnings (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rndis_wlan: fix array of flexible structures warning (Jose Ignacio Tornos Martinez) [2136125]
- mwifiex: fix sleep in atomic context bugs caused by dev_coredumpv (Jose Ignacio Tornos Martinez) [2136125]
- bus: mhi: host: pci_generic: Add a secondary AT port to Telit FN990 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Add WoW support for WCN6750 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Include STA_KEEPALIVE_ARP_RESPONSE TLV header by default (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rt2x00: Fix "Error - Attempt to send packet over invalid queue 2" (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: add multi-port ID to TX descriptor (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: fix rx filter after scan (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: free unused skb to prevent memory leak (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: reset halt registers before turn on wifi CPU (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: update LTR settings (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: mac: set NAV upper to 25ms (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: initialize DMA of CMAC (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support SER L1 simulation (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: support fw crash simulation (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: introudce functions to drop packets (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: unify use of rtw89_h2c_tx() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: concentrate control function of TX DMA channel (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: correct enable functions of HCI/PCI DMA (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: L1 DMA reset has offloaded to FW (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support for setting TID specific configuration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support for setting HE GI and LTF (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: show connecting state in debug message (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: Combine set grant WL/BT and correct the debug log (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: Remove trace_step at COEX-MECH control structure for RTL8852C (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: Parsing Wi-Fi firmware TDMA info from reports (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: Parsing Wi-Fi firmware error message from reports (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: Move coexistence firmware buffer size parameter to chip info (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: Add v1 Wi-Fi firmware power-saving null data report (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: coex: use void pointer as temporal type to copy report (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: pcie: Add IDs/properties for BCM4378 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: pcie: Support PCIe core revisions >= 64 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: msgbuf: Increase RX ring sizes to 1024 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: firmware: Allow platform to override macaddr (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: pcie: Perform firmware selection for Apple platforms (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: of: Fetch Apple properties (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: pcie: Read Apple OTP information (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: firmware: Support passing in multiple board_types (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: pcie/sdio/usb: Get CLM blob via standard firmware mechanism (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: firmware: Handle per-board clm_blob files (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: d3: parse keys from wowlan info notification (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: iterate over interfaces after an assert in d3 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: trigger resume flow before wait for notifications (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: Add handling for scan offload match info notification (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: enable resume based on notifications (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: Add support for d3 end notification (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: Add support for wowlan wake packet notification (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: Add support for wowlan info notification (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: don't check D0I3 version (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: cfg: remove IWL_DEVICE_BZ_COMMON macro (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: refactor iwl_mvm_set_sta_rate() a bit (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: rxmq: further unify some VHT/HE code (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: rxmq: refactor mac80211 rx_status setting (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: mvm: fix typo in struct iwl_rx_no_data API (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: pcie: add support for BZ devices (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Fix kernel-doc issues (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Fix miscellaneous spelling errors (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath10k: Fix miscellaneous spelling errors (Jose Ignacio Tornos Martinez) [2136125]
- bus: mhi: host: always print detected modem name (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921s: Switch to DEFINE_SIMPLE_DEV_PM_OPS() and pm_sleep_ptr() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7663s: Switch to DEFINE_SIMPLE_DEV_PM_OPS() and pm_sleep_ptr() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921e: fix random fw download fail (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: introduce Country Location Control support (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921e: fix rmmod crash in driver reload test (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: reset msta->airtime_ac while clearing up hw value (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7915: do not check state before configuring implicit beamform (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: fix uninitialized pointer in mt7921_mac_fill_rx (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7915: fix mcs value in ht mode (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: get rid of the false positive reset (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: connac: fix in comment (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: add PPDU based TxS support for WED device (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: move move mt76_sta_stats to mt76_wcid (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: fix the firmware version report (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: add mt7921_mutex_acquire at mt7921_sta_set_decap_offload (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: add mt7921_mutex_acquire at mt7921_[start, stop]_ap (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt76_usb.mt76u_mcu.burst is always false remove related code (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7663s: add rx_check callback (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: connac: fix possible unaligned access in mt76_connac_mcu_add_nested_tlv (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7915: fix possible unaligned access in mt7915_mac_add_twt_setup (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7615: add mt7615_mutex_acquire/release in mt7615_sta_set_decap_offload (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: sdio: fix transmitting packet hangs (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: sdio: add rx_check callback for sdio devices (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: delete stray if statement (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: fix use after free in mt7921_acpi_read() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7915: fix an uninitialized variable bug (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: sdio: poll sta stat when device transmits data (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: sdio: fix the deadlock caused by sdio->stat_work (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921: move mt7921_rx_check and mt7921_queue_rx_skb in mac.c (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921u: remove unnecessary MT76_STATE_SUSPEND (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921u: fix race issue between reset and suspend/resume (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921s: fix race issue between reset and suspend/resume (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: mt7921e: fix race issue between reset and suspend/resume (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: add rx_check callback for usb devices (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: testmode: use random payload for tx packets (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mt76: connac: introduce mt76_connac_reg_map structure (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: Remove copy-paste leftover in gen2_update_rate_mask (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: gen2: Fix mistake in path B IQ calibration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: split scan including lots of channels (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: support hw_scan (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: call tx_wake notify for 8852c in deep ps mode (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support deep ps mode for rtw8852c (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: set response rate selection (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: set TX to single path TX on path B in 6GHz band (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: enlarge polling timeout of RX DCK (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: enable the interference cancellation of MU-MIMO on 6GHz (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: add DIG register struct to share common algorithm (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: support TX diversity for 1T2R chipset (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: record signal strength per RF path (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: configure TX path via H2C command (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: parse phycap of TX/RX antenna number (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: use u32_get_bits to access C2H content of PHY capability (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Increase TCL data ring size for WCN6750 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Add multi TX ring support for WCN6750 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Enable threaded NAPI (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: mhi: fix potential memory leak in ath11k_mhi_register() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: implement SRAM dump debugfs interface (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Split PCI write/read functions (Jose Ignacio Tornos Martinez) [2136125]
- ath11k: Enable remain-on-channel support on WCN6750 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mwifiex: fix endian annotations in casts (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mwifiex: fix endian conversion (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mwifiex: mark a variable unused (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: Fix skb misuse in TX queue selection (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: remove redundant variable err (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: add 43439 SDIO ids and initialization (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: Simplify the error handling code (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mwifiex: Fix comment typo (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: Add DMI nvram filename quirk for Chuwi Hi8 Pro tablet (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: Use ISO3166 country code and rev 0 as fallback on 43430 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: fix use-after-free bug in brcmf_netdev_start_xmit() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: iwlwifi: calib: Refactor iwl_calib_result usage for clarity (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: always activate all links (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: implement link switching (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: keep A-MSDU data in sta and per-link (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: set up beacon timing config on links (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: add vif/sta link RCU dereference macros (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: send NDP for link (de)activation (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: extend ieee80211_nullfunc_get() for MLO (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: track active STA links (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: skip inactive links on TX (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: add ieee80211_find_sta_by_link_addrs API (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: isolate driver from inactive links (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: make smps_mode per-link (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: use correct rx link_sta instead of default (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: set link_sta in reorder timeout (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: fix multi-channel handling in netlink RX (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: call drv_sta_state() under sdata_lock() in reconfig (Jose Ignacio Tornos Martinez) [2136125]
- wifi: nl80211: add MLD address to assoc BSS entries (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: mlme: refactor QoS settings code (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: warn on invalid link address (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix double SW scan stop (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: mlme: assign link address correctly (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: move link code to a new file (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: refactor RX a bit (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: check STA magic in change_sta_links (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: remove unused arg to ieee80211_chandef_eht_oper (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: remove multicast workaround (Jose Ignacio Tornos Martinez) [2136125]
- wifi: nl80211: remove redundant err variable (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: Support POWERED_ADDR_CHANGE feature (Jose Ignacio Tornos Martinez) [2136125]
- wifi: nl80211: Add POWERED_ADDR_CHANGE feature (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: prevent 4-addr use on MLDs (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: prevent VLANs on MLDs (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Add support to connect to non-transmit MBSSID profiles (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Fix hardware restart failure due to twt debugfs failure (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Add TWT debugfs support for STA interface (Jose Ignacio Tornos Martinez) [2136125]
- wifi: move from strlcpy with unused retval to strscpy (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: add missing destroy_workqueue() on error path in rtw_core_init() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtl8xxxu: tighten bounds checking in rtl8xxxu_read_efuse() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: declare to support beamformee above bandwidth 80MHz (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: correct polling address of address CAM (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: no HTC field if TX rate might fallback to legacy (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: correct TX resource checking in low power mode (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: fix interrupt stuck after leaving low power mode (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: enlarge the CFO tracking boundary (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: correct suspend/resume setting for variant chips (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: enable CLK_REQ, ASPM, L1 and L1ss for 8852c (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: pci: fix PCI PHY auto adaption by using software restore (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: set TBTT shift configuration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: add retry to change power_mode state (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: correct BA CAM allocation (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: initialize and correct BA CAM content (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: declare correct BA CAM number (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: update TX power tables to R49 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852c: update RF radio A/B parameters to R49 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: TX power limit/limit_ru consider negative (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: Update Wi-Fi driver/firmware TDMA cycle report for RTL8852c (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: Add v1 Wi-Fi SCC coexistence policy (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: Move _set_policy to chip_ops (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: update WL role info v1 for RTL8852C branch using (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: Add v1 version TDMA format and parameters (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: Define BT B1 slot length (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: Add logic to parsing rtl8852c firmware type ctrl report (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: Move Wi-Fi firmware coexistence matching version to chip (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: coex: update radio state for RTL8852A/RTL8852C (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: 8852c: adjust mactxen delay of mac/phy interface (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: 8852c: modify PCIE prebkf time (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: ser: leave lps with mutex (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: declare support HE HTC always (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: 8852a: update HW setting on BB (Jose Ignacio Tornos Martinez) [2136125]
- rtw89: 8852c: disable dma during mac init (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: declare support for mac80211 chanctx ops by chip (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: add skeleton of mac80211 chanctx ops support (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: introduce entity mode and its recalculated prototype (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: initialize entity and configure default chandef (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: concentrate chandef setting to stack callback (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: concentrate parameter control for setting channel callback (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: rfk: concentrate parameter control while set_channel() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: txpwr: concentrate channel related control to top (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: create rtw89_chan centrally to avoid breakage (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: re-arrange channel related stuffs under HAL (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: introduce rtw89_chan for channel stuffs (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: rewrite decision on channel by entity state (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Add cold boot calibration support on WCN6750 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Fix incorrect QMI message ID mappings (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath11k: Register shutdown handler for WCN6750 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath9k: avoid uninit memory read in ath9k_htc_rx_msg() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix potential deadlock in ieee80211_key_link() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: fix uninitialized use of primary channel index (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: use full 'unsigned int' type (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: move from strlcpy with unused retval to strscpy (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: read ethtool's sta_stats from sinfo (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: correct SMPS mode in HE 6 GHz capability (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: Add link_id to cfg80211_ch_switch_started_notify() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: nl80211: send MLO links channel info in GET_INTERFACE (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: allow bw change during channel switch in mesh (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: clean up a needless assignment in ieee80211_sta_activate_link() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: allow link address A2 in TXQ dequeue (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix control port frame addressing (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: set link ID in TX info for beacons (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: fix link change handling (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: maintain link_id in link_sta (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211/mac80211: check EHT capability size correctly (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211_hwsim: split iftype data into AP/non-AP (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: mlme: don't add empty EML capabilities (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: use link ID for MLO in queued frames (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: use the corresponding link for stats update (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: add link information in ieee80211_rx_status (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: properly implement MLO key handling (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: Add link_id parameter to various key operations for MLO (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: Prevent cfg80211_wext_siwencodeext() on MLD (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: reject connect response with MLO params for WEP (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: fix use-after-free (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: use link in TXQ parameter configuration (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: add link id to txq params (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: set link BSSID (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: get correct AP link chandef (Jose Ignacio Tornos Martinez) [2136125]
- wifi: cfg80211: Update RNR parsing to align with Draft P802.11be_D2.0 (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: properly set old_links when removing a link (Jose Ignacio Tornos Martinez) [2136125]
- wifi: mac80211: accept STA changes without link changes (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: prohibit enter IPS during HW scan (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: add flag check before enter or leave IPS (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: add flushing queue before HW scan (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: fix WARNING:rtw_get_tx_power_params() during HW scan (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: add the update channel flow to support setting by parameters (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: add mutex when set regulatory and get Tx power table (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: add mutex when set SAR (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: Fix to add skb free for TIM update info when tx is completed (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: Fix to add brcmf_clear_assoc_ies when rmmod (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: fix invalid address access when enabling SCAN log level (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: fix scheduling while atomic issue when deleting flowring (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmfmac: fix continuous 802.1x tx pending timeout error (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath10k: add peer map clean up for peer delete in ath10k_sta_state() (Jose Ignacio Tornos Martinez) [2136125]
- wifi: ath10k: Set tx credit to one for WCN3990 snoc based devices (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: 8852a: correct WDE IMR settings (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw89: refine leaving LPS function (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtlwifi: 8192de: correct checking of IQK reload (Jose Ignacio Tornos Martinez) [2136125]
- wifi: brcmsmac: remove duplicate words (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: access chip_info by const pointer (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: phy: fix warning of possible buffer overflow (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: fix store OP channel info timing when HW scan (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: fix stopping queues in wrong timing when HW scan (Jose Ignacio Tornos Martinez) [2136125]
- wifi: rtw88: 8822c: extend supported probe request size (Jose Ignacio Tornos Martinez) [2136125]

* Tue Feb 07 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-459.el8]
- ALSA: pcm: Move rwsem lock inside snd_ctl_elem_read to prevent UAF (Jaroslav Kysela) [2125548] {CVE-2023-0266}
- ALSA: usb-audio: Remove redundant workaround for Roland quirk (Jaroslav Kysela) [2125548]
- ASoC: jz4740-i2s: Handle independent FIFO flush bits (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Apply dual codec fixup for Dell Latitude laptops (Jaroslav Kysela) [2125548]
- ALSA: patch_realtek: Fix Dell Inspiron Plus 16 (Jaroslav Kysela) [2125548]
- ALSA: hda/hdmi: Static PCM mapping again with AMD HDMI codecs (Jaroslav Kysela) [2125548]
- ALSA: line6: fix stack overflow in line6_midi_transmit (Jaroslav Kysela) [2125548]
- ALSA: line6: correct midi status byte when receiving data from podxt (Jaroslav Kysela) [2125548]
- ALSA: hda/hdmi: Add HP Device 0x8711 to force connect list (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add quirk for Lenovo TianYi510Pro-14IOB (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: add the quirk for KT0206 device (Jaroslav Kysela) [2125548]
- ASoC: rt5670: Remove unbalanced pm_runtime_put() (Jaroslav Kysela) [2125548]
- ASoC: rockchip: spdif: Add missing clk_disable_unprepare() in rk_spdif_runtime_resume() (Jaroslav Kysela) [2125548]
- ASoC: wm8994: Fix potential deadlock (Jaroslav Kysela) [2125548]
- ALSA: hda/hdmi: fix stream-id config keep-alive for rt suspend (Jaroslav Kysela) [2125548]
- ALSA: hda/hdmi: set default audio parameters for KAE silent-stream (Jaroslav Kysela) [2125548]
- ALSA: hda/hdmi: fix i915 silent stream programming flow (Jaroslav Kysela) [2125548]
- ASoC: rockchip: pdm: Add missing clk_disable_unprepare() in rockchip_pdm_runtime_resume() (Jaroslav Kysela) [2125548]
- ASoC: audio-graph-card: fix refcount leak of cpu_ep in __graph_for_each_link() (Jaroslav Kysela) [2125548]
- ASoC: mediatek: mt8173-rt5650-rt5514: fix refcount leak in mt8173_rt5650_rt5514_dev_probe() (Jaroslav Kysela) [2125548]
- ASoC: Intel: Skylake: Fix driver hang during shutdown (Jaroslav Kysela) [2125548]
- ALSA: hda: add snd_hdac_stop_streams() helper (Jaroslav Kysela) [2125548]
- ASoC: sof_es8336: fix possible use-after-free in sof_es8336_remove() (Jaroslav Kysela) [2125548]
- ASoC: amd: yc: Add Xiaomi Redmi Book Pro 14 2022 into DMI table (Jaroslav Kysela) [2125548]
- ASoC: Intel: avs: Add quirk for KBL-R RVP platform (Jaroslav Kysela) [2125548]
- ASoC: codecs: rt298: Add quirk for KBL-R RVP platform (Jaroslav Kysela) [2125548]
- ALSA: mts64: fix possible null-ptr-defer in snd_mts64_interrupt (Jaroslav Kysela) [2125548]
- ALSA: pcm: Set missing stop_operating flag at undoing trigger start (Jaroslav Kysela) [2125548]
- ASoC: pcm512x: Fix PM disable depth imbalance in pcm512x_probe (Jaroslav Kysela) [2125548]
- ALSA: asihpi: fix missing pci_disable_device() (Jaroslav Kysela) [2125548]
- ASoC: mediatek: mtk-btcvsd: Add checks for write and read of mtk_btcvsd_snd (Jaroslav Kysela) [2125548]
- ASoC: qcom: Add checks for devm_kcalloc (Jaroslav Kysela) [2125548]
- ASoC: Intel: avs: Lock substream before snd_pcm_stop() (Jaroslav Kysela) [2125548]
- ASoC: pxa: fix null-pointer dereference in filter() (Jaroslav Kysela) [2125548]
- ASoC: Intel: avs: Fix potential RX buffer overflow (Jaroslav Kysela) [2125548]
- ASoC: Intel: avs: Fix DMA mask assignment (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: fix mute/micmute LEDs for a HP ProBook (Jaroslav Kysela) [2125548]
- ASoC: ops: Correct bounds check for second channel on SX controls (Jaroslav Kysela) [2125548]
- ASoC: cs42l51: Correct PGA Volume minimum value (Jaroslav Kysela) [2125548]
- ASoC: ops: Check bounds for second channel in snd_soc_put_volsw_sx() (Jaroslav Kysela) [2125548]
- ASoC: fsl_micfil: explicitly clear CHnF flags (Jaroslav Kysela) [2125548]
- ASoC: fsl_micfil: explicitly clear software reset bit (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: More robust component matching for CS35L41 (Jaroslav Kysela) [2125548]
- ASoC: soc-pcm: Add NULL check in BE reparenting (Jaroslav Kysela) [2125548]
- ALSA: seq: Fix function prototype mismatch in snd_seq_expand_var_event (Jaroslav Kysela) [2125548]
- ASoC: rt711-sdca: fix the latency time of clock stop prepare state machine transitions (Jaroslav Kysela) [2125548]
- ASoC: wm8962: Wait for updated value of WM8962_CLOCKING1 register (Jaroslav Kysela) [2125548]
- ASoC: ops: Fix bounds check for _sx controls (Jaroslav Kysela) [2125548]
- ALSA: dice: fix regression for Lexicon I-ONIX FW810S (Jaroslav Kysela) [2125548]
- ASoC: sof_es8336: reduce pop noise on speaker (Jaroslav Kysela) [2125548]
- ASoC: SOF: ipc3-topology: use old pipeline teardown flow with SOF2.1 and older (Jaroslav Kysela) [2125548]
- ASoC: hda: intel-dsp-config: add ES83x6 quirk for IceLake (Jaroslav Kysela) [2125548]
- ASoC: Intel: soc-acpi: add ES83x6 support to IceLake (Jaroslav Kysela) [2125548]
- ASoC: Intel: bytcht_es8316: Add quirk for the Nanote UMPC-01 (Jaroslav Kysela) [2125548]
- ASoC: amd: yc: Add Alienware m17 R5 AMD into DMI table (Jaroslav Kysela) [2125548]
- ASoC: max98373: Add checks for devm_kcalloc (Jaroslav Kysela) [2125548]
- ASoC: soc-pcm: Don't zero TDM masks in __soc_pcm_open() (Jaroslav Kysela) [2125548]
- ASoC: sgtl5000: Reset the CHIP_CLK_CTRL reg on remove (Jaroslav Kysela) [2125548]
- ASoC: hdac_hda: fix hda pcm buffer overflow issue (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: add quirk to fix Hamedal C20 disconnect issue (Jaroslav Kysela) [2125548]
- ASoC: SOF: topology: No need to assign core ID if token parsing failed (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Fix the speaker output on Samsung Galaxy Book Pro 360 (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: fix speakers for Samsung Galaxy Book Pro (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Drop snd_BUG_ON() from snd_usbmidi_output_open() (Jaroslav Kysela) [2125548]
- ASoC: soc-utils: Remove __exit for snd_soc_util_exit() (Jaroslav Kysela) [2125548]
- ASoC: rt5677: fix legacy dai naming (Jaroslav Kysela) [2125548]
- ASoC: rt5514: fix legacy dai naming (Jaroslav Kysela) [2125548]
- ASoC: tas2764: Fix set_tdm_slot in case of single slot (Jaroslav Kysela) [2125548]
- ASoC: tas2770: Fix set_tdm_slot in case of single slot (Jaroslav Kysela) [2125548]
- ASoC: core: Fix use-after-free in snd_soc_exit() (Jaroslav Kysela) [2125548]
- ASoC: codecs: jz4725b: Fix spelling mistake "Sourc" -> "Source", "Routee" -> "Route" (Jaroslav Kysela) [2125548]
- ASoC: amd: yc: Add Lenovo Thinkbook 14+ 2022 21D0 to quirks table (Jaroslav Kysela) [2125548]
- ASoC: amd: yc: Adding Lenovo ThinkBook 14 Gen 4+ ARA and Lenovo ThinkBook 16 Gen 4+ ARA to the Quirks List (Jaroslav Kysela) [2125548]
- ASoC: rt1308-sdw: add the default value of some registers (Jaroslav Kysela) [2125548]
- ASoC: Intel: sof_rt5682: Add quirk for Rex board (Jaroslav Kysela) [2125548]
- ASoC: Intel: sof_sdw: add quirk variant for LAPBC710 NUC15 (Jaroslav Kysela) [2125548]
- ASoC: codecs: jz4725b: fix capture selector naming (Jaroslav Kysela) [2125548]
- ASoC: codecs: jz4725b: use right control for Capture Volume (Jaroslav Kysela) [2125548]
- ASoC: codecs: jz4725b: fix reported volume for Master ctl (Jaroslav Kysela) [2125548]
- ASoC: codecs: jz4725b: add missed Line In power control bit (Jaroslav Kysela) [2125548]
- ASoC: wm8962: Add an event handler for TEMP_HP and TEMP_SPK (Jaroslav Kysela) [2125548]
- ASoC: rt1019: Fix the TDM settings (Jaroslav Kysela) [2125548]
- ASoC: rt5682s: Fix the TDM Tx settings (Jaroslav Kysela) [2125548]
- ASoC: mt6660: Keep the pm_runtime enables before component stuff in mt6660_i2c_probe (Jaroslav Kysela) [2125548]
- ASoC: wm8997: Revert "ASoC: wm8997: Fix PM disable depth imbalance in wm8997_probe" (Jaroslav Kysela) [2125548]
- ASoC: wm5110: Revert "ASoC: wm5110: Fix PM disable depth imbalance in wm5110_probe" (Jaroslav Kysela) [2125548]
- ASoC: wm5102: Revert "ASoC: wm5102: Fix PM disable depth imbalance in wm5102_probe" (Jaroslav Kysela) [2125548]
- ALSA: memalloc: Try dma_alloc_noncontiguous() at first (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Add DSD support for Accuphase DAC-60 (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Add quirk entry for M-Audio Micro (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Yet more regression for for the delayed card registration (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add Positivo C6300 model quirk (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add quirk for ASUS Zenbook using CS35L41 (Jaroslav Kysela) [2125548]
- ALSA: hda: fix potential memleak in 'add_widget_node' (Jaroslav Kysela) [2125548]
- ALSA: hda/ca0132: add quirk for EVGA Z390 DARK (Jaroslav Kysela) [2125548]
- ALSA: hda/hdmi - enable runtime pm for more AMD display audio (Jaroslav Kysela) [2125548]
- ALSA: memalloc: Don't fall back for SG-buffer with IOMMU (Jaroslav Kysela) [2125548]
- ALSA: aoa: Fix I2S device accounting (Jaroslav Kysela) [2125548]
- ALSA: aoa: i2sbus: fix possible memory leak in i2sbus_add_dev() (Jaroslav Kysela) [2125548]
- ALSA: ac97: fix possible memory leak in snd_ac97_dev_register() (Jaroslav Kysela) [2125548]
- ASoC: SOF: Intel: pci-tgl: fix ADL-N descriptor (Jaroslav Kysela) [2125548]
- ASoC: SOF: Intel: pci-tgl: use RPL specific firmware definitions (Jaroslav Kysela) [2125548]
- ASoC: Intel: common: add ACPI matching tables for Raptor Lake (Jaroslav Kysela) [2125548]
- ALSA: rme9652: use explicitly signed char (Jaroslav Kysela) [2125548]
- ALSA: au88x0: use explicitly signed char (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add another HP ZBook G9 model quirks (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Add quirks for M-Audio Fast Track C400/600 (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add quirk for ASUS Zenbook using CS35L41 (Jaroslav Kysela) [2125548]
- ALSA: Use del_timer_sync() before freeing timer (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Fix last interface check for registration (Jaroslav Kysela) [2125548]
- ASoC: amd: yc: Add Lenovo Yoga Slim 7 Pro X to quirks table (Jaroslav Kysela) [2125548]
- ASoC: amd: yc: Add ASUS UM5302TA into DMI table (Jaroslav Kysela) [2125548]
- ASoC: SOF: add quirk to override topology mclk_id (Jaroslav Kysela) [2125548]
- ASoC: SOF: pci: Change DMI match info to support all Chrome platforms (Jaroslav Kysela) [2125548]
- ALSA: intel-dspconfig: add ES8336 support for AlderLake-PS (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Register card at the last interface (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Add quirk to enable Avid Mbox 3 support (Jaroslav Kysela) [2125548]
- ASoC: mt6660: Fix PM disable depth imbalance in mt6660_i2c_probe (Jaroslav Kysela) [2125548]
- ASoC: wm5102: Fix PM disable depth imbalance in wm5102_probe (Jaroslav Kysela) [2125548]
- ASoC: wm5110: Fix PM disable depth imbalance in wm5110_probe (Jaroslav Kysela) [2125548]
- ASoC: wm8997: Fix PM disable depth imbalance in wm8997_probe (Jaroslav Kysela) [2125548]
- ASoC: stm: Fix PM disable depth imbalance in stm32_i2s_probe (Jaroslav Kysela) [2125548]
- ASoC: stm32: spdifrx: Fix PM disable depth imbalance in stm32_spdifrx_probe (Jaroslav Kysela) [2125548]
- ASoC: stm32: dfsdm: Fix PM disable depth imbalance in stm32_adfsdm_probe (Jaroslav Kysela) [2125548]
- ALSA: dmaengine: increment buffer pointer atomically (Jaroslav Kysela) [2125548]
- ASoC: da7219: Fix an error handling path in da7219_register_dai_clks() (Jaroslav Kysela) [2125548]
- ASoC: eureka-tlv320: Hold reference returned from of_find_xxx API (Jaroslav Kysela) [2125548]
- ASoC: wm_adsp: Handle optional legacy support (Jaroslav Kysela) [2125548]
- ASoC: rsnd: Add check for rsnd_mod_power_on (Jaroslav Kysela) [2125548]
- ASoC: soc-pcm.c: call __soc_pcm_close() in soc_pcm_close() (Jaroslav Kysela) [2125548]
- ASoC: mt6359: fix tests for platform_get_irq() failure (Jaroslav Kysela) [2125548]
- ASoC: wcd934x: fix order of Slimbus unprepare/disable (Jaroslav Kysela) [2125548]
- ASoC: wcd9335: fix order of Slimbus unprepare/disable (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add Intel Reference SSID to support headset keys (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add quirk for ASUS GV601R laptop (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Fix NULL dererence at error path (Jaroslav Kysela) [2125548]
- ALSA: usb-audio: Fix potential memory leaks (Jaroslav Kysela) [2125548]
- ALSA: rawmidi: Drop register_mutex in snd_rawmidi_free() (Jaroslav Kysela) [2125548]
- ALSA: oss: Fix potential deadlock at unregistration (Jaroslav Kysela) [2125548]
- ALSA: hda/realtek: Add quirk for HP Zbook Firefly 14 G9 model (Jaroslav Kysela) [2125548]
- ALSA: hda: Fix position reporting on Poulsbo (Jaroslav Kysela) [2125548]

* Mon Feb 06 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-458.el8]
- KVM: x86: smm: preserve interrupt shadow in SMRAM (Maxim Levitsky) [2097144]
- KVM: x86: SVM: don't save SVM state to SMRAM when VM is not long mode capable (Maxim Levitsky) [2097144]
- KVM: x86: SVM: use smram structs (Maxim Levitsky) [2097144]
- KVM: svm: drop explicit return value of kvm_vcpu_map (Maxim Levitsky) [2097144]
- KVM: x86: smm: use smram struct for 64 bit smram load/restore (Maxim Levitsky) [2097144]
- KVM: x86: smm: use smram struct for 32 bit smram load/restore (Maxim Levitsky) [2097144]
- KVM: x86: smm: use smram structs in the common code (Maxim Levitsky) [2097144]
- KVM: x86: smm: add structs for KVM's smram layout (Maxim Levitsky) [2097144]
- KVM: x86: smm: check for failures on smm entry (Maxim Levitsky) [2097144]
- KVM: x86: do not go through ctxt->ops when emulating rsm (Maxim Levitsky) [2097144]
- KVM: x86: move SMM exit to a new file (Maxim Levitsky) [2097144]
- KVM: x86: move SMM entry to a new file (Maxim Levitsky) [2097144]
- KVM: x86: start moving SMM-related functions to new files (Maxim Levitsky) [2097144]
- bug: introduce ASSERT_STRUCT_OFFSET (Maxim Levitsky) [2097144]
- KVM: x86: Rename and expose helper to detect if INIT/SIPI are allowed (Maxim Levitsky) [2097144]
- KVM: x86: smm: number of GPRs in the SMRAM image depends on the image format (Maxim Levitsky) [2097144]
- KVM: x86: emulator: update the emulation mode after CR0 write (Maxim Levitsky) [2097144]
- KVM: x86: emulator: update the emulation mode after rsm (Maxim Levitsky) [2097144]
- KVM: x86: emulator: introduce emulator_recalc_and_set_mode (Maxim Levitsky) [2097144]
- KVM: x86: emulator: em_sysexit should update ctxt->mode (Maxim Levitsky) [2097144]
- KVM: x86: Bug the VM if the emulator accesses a non-existent GPR (Maxim Levitsky) [2097144]
- KVM: x86: Reduce the number of emulator GPRs to '8' for 32-bit KVM (Maxim Levitsky) [2097144]
- KVM: x86: Use 16-bit fields to track dirty/valid emulator GPRs (Maxim Levitsky) [2097144]
- KVM: x86: Omit VCPU_REGS_RIP from emulator's _regs array (Maxim Levitsky) [2097144]
- KVM: x86: Harden _regs accesses to guard against buggy input (Maxim Levitsky) [2097144]
- KVM: x86: Grab regs_dirty in local 'unsigned long' (Maxim Levitsky) [2097144]

* Fri Feb 03 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-457.el8]
- RDMA/bnxt_re: Fix endianness warning for req.pkey (Kamal Heib) [2142690]
- RDMA/bnxt_re: Use bitmap_zalloc() when applicable (Kamal Heib) [2142690]
- RDMA/bnxt_re: Remove dynamic pkey table (Kamal Heib) [2142690]
- RDMA/bnxt_re: Scan the whole bitmap when checking if "disabling RCFW with pending cmd-bit" (Kamal Heib) [2142690]
- RDMA/bnxt_re: Remove unneeded variable (Kamal Heib) [2142690]
- RDMA/bnxt_re: Remove unsupported bnxt_re_modify_ah callback (Kamal Heib) [2142690]
- RDMA/bnxt_re: Use helper function to set GUIDs (Kamal Heib) [2142690]
- RDMA/bnxt_re: Check if the vlan is valid before reporting (Kamal Heib) [2142690]
- RDMA/bnxt_re: Correct FRMR size calculation (Kamal Heib) [2142690]
- RDMA/bnxt_re: Use GFP_KERNEL in non atomic context (Kamal Heib) [2142690]
- RDMA/bnxt_re: Fix FRMR issue with single page MR allocation (Kamal Heib) [2142690]
- RDMA/bnxt_re: Fix query SRQ failure (Kamal Heib) [2142690]
- RDMA/bnxt_re: Suppress unwanted error messages (Kamal Heib) [2142690]
- RDMA/bnxt_re: Support multiple page sizes (Kamal Heib) [2142690]
- RDMA/bnxt_re: Reduce the delay in polling for hwrm command completion (Kamal Heib) [2142690]
- RDMA/bnxt_re: Use separate response buffer for stat_ctx_free (Kamal Heib) [2142690]
- net/mlx5: Lag, Fix for loop when checking lag (Amir Tzin) [2112917]
- net/mlx5e: Fix use-after-free when reverting termination table (Amir Tzin) [2112927]
- net/mlx5: Fix uninitialized variable bug in outlen_write() (Amir Tzin) [2112927]
- net/mlx5: E-switch, Fix duplicate lag creation (Amir Tzin) [2112927 2112917]
- net/mlx5: E-switch, Destroy legacy fdb table when needed (Amir Tzin) [2112927 2112917]
- net/mlx5: DR, Fix uninitialized var warning (Amir Tzin) [2112927]
- net/mlx5e: Offload rule only when all encaps are valid (Amir Tzin) [2112927]
- net/mlx5: Fix sync reset event handler error flow (Amir Tzin) [2112927]
- net/mlx5: E-Switch, Set correctly vport destination (Amir Tzin) [2112927]
- net/mlx5: Fix handling of entry refcount when command is not issued to FW (Amir Tzin) [2112927]
- net/mlx5: cmdif, Print info on any firmware cmd failure to tracepoint (Amir Tzin) [2112927]
- net/mlx5: SF: Fix probing active SFs during driver probe phase (Amir Tzin) [2112927]
- net/mlx5: Fix FW tracer timestamp calculation (Amir Tzin) [2112927]
- net/mlx5: Do not query pci info while pci disabled (Amir Tzin) [2112927 2129249]
- net/mlx5e: TC, Fix slab-out-of-bounds in parse_tc_actions (Amir Tzin) [2112927]
- net/mlx5e: Clean up and fix error flows in mlx5e_alloc_rq (Amir Tzin) [2112927]
- net/mlx5: DR, Fix the SMFS sync_steering for fast teardown (Amir Tzin) [2112927]
- net/mlx5e: E-Switch, Fix comparing termination table instance (Amir Tzin) [2112927]
- net/mlx5e: TC, Fix wrong rejection of packet-per-second policing (Amir Tzin) [2112927 2049622]
- net/mlx5e: Fix tc acts array not to be dependent on enum order (Amir Tzin) [2112927]
- net/mlx5e: Add missing sanity checks for max TX WQE size (Amir Tzin) [2112927]
- net/mlx5: fw_reset: Don't try to load device in case PCI isn't working (Amir Tzin) [2112927]
- net/mlx5: E-switch, Set to legacy mode if failed to change switchdev mode (Amir Tzin) [2112927 2112917]
- net/mlx5: Allow async trigger completion execution on single CPU systems (Amir Tzin) [2112927]
- net/mlx5: Bridge, verify LAG state when adding bond to bridge (Amir Tzin) [2112927]
- net/mlx5: Fix crash during sync firmware reset (Amir Tzin) [2112927]
- net/mlx5e: TC, Fix cloned flow attr instance dests are not zeroed (Amir Tzin) [2112927]
- net/mlx5: Fix possible use-after-free in async command interface (Amir Tzin) [2112927]
- net/mlx5: ASO, Create the ASO SQ with the correct timestamp format (Amir Tzin) [2112927 2049622]
- net/mlx5e: Update restore chain id for slow path packets (Amir Tzin) [2112927]
- net/mlx5e: Extend SKB room check to include PTP-SQ (Amir Tzin) [2112927]
- net/mlx5: DR, Fix matcher disconnect error flow (Amir Tzin) [2112927]
- net/mlx5: Wait for firmware to enable CRS before pci_restore_state (Amir Tzin) [2112927]
- net/mlx5e: Do not increment ESN when updating IPsec ESN state (Amir Tzin) [2112927]
- net/mlx5e: Fix calculations for ICOSQ size (Amir Tzin) [2112927]
- net/mlx5: Fix spelling mistake "syndrom" -> "syndrome" (Amir Tzin) [2112927]
- net/mlx5e: Fix a typo in mlx5e_xdp_mpwqe_is_full (Amir Tzin) [2112927]
- RDMA/mlx5: Don't compare mkey tags in DEVX indirect mkey (Amir Tzin) [2112927]
- RDMA/mlx5: Fix UMR cleanup on error flow of driver init (Amir Tzin) [2112927]
- RDMA/mlx5: Rely on RoCE fw cap instead of devlink when setting profile (Amir Tzin) [2112927]
- net/mlx5: Unlock on error in mlx5_sriov_enable() (Amir Tzin) [2112927]
- net/mlx5e: Fix use after free in mlx5e_fs_init() (Amir Tzin) [2112927]
- net/mlx5e: kTLS, Use _safe() iterator in mlx5e_tls_priv_tx_list_cleanup() (Amir Tzin) [2112927]
- net/mlx5: unlock on error path in esw_vfs_changed_event_handler() (Amir Tzin) [2112927 2150647]
- net/mlx5e: Fix wrong tc flag used when set hw-tc-offload off (Amir Tzin) [2112927]
- net/mlx5e: TC, Add missing policer validation (Amir Tzin) [2112927]
- net/mlx5e: Fix wrong application of the LRO state (Amir Tzin) [2112927]
- net/mlx5: Avoid false positive lockdep warning by adding lock_class_key (Amir Tzin) [2112927]
- net/mlx5: Fix cmd error logging for manage pages cmd (Amir Tzin) [2112927]
- net/mlx5: Disable irq when locking lag_lock (Amir Tzin) [2112927]
- net/mlx5: Eswitch, Fix forwarding decision to uplink (Amir Tzin) [2112927 2150647]
- net/mlx5: LAG, fix logic over MLX5_LAG_FLAG_NDEVS_READY (Amir Tzin) [2112927]
- net/mlx5e: Properly disable vlan strip on non-UL reps (Amir Tzin) [2112927]
- net/mlx5e: Allocate flow steering storage during uplink initialization (Amir Tzin) [2112927]
- RDMA/mlx5: Use the proper number of ports (Amir Tzin) [2112927]
- mlx5: do not use RT_TOS for IPv6 flowlabel (Amir Tzin) [2112927]
- RDMA/mlx5: Add missing check for return value in get namespace flow (Amir Tzin) [2112927]
- net/mlx5e: xsk: Discard unaligned XSK frames on striding RQ (Amir Tzin) [2112927]
- net: devlink: convert reload command to take implicit devlink->lock (mlx5 hunk only) (Amir Tzin) [2112927]
- devlink: Hold the instance lock in health callbacks (mlx5 hunk only) (Amir Tzin) [2112927]
- net/mlx5: Lock mlx5 devlink health recovery callback (Amir Tzin) [2112927]
- net/mlx5: Lock mlx5 devlink reload callbacks (Amir Tzin) [2112927]
- net/mlx5: Move fw reset unload to mlx5_fw_reset_complete_reload (Amir Tzin) [2112927]
- net/mlx5e: kTLS, Dynamically re-size TX recycling pool (Amir Tzin) [2112927]
- net/mlx5e: kTLS, Recycle objects of device-offloaded TLS TX connections (Amir Tzin) [2112927]
- net/mlx5e: kTLS, Take stats out of OOO handler (Amir Tzin) [2112927]
- net/mlx5e: kTLS, Introduce TLS-specific create TIS (Amir Tzin) [2112927]
- net/mlx5e: Move mlx5e_init_l2_addr to en_main (Amir Tzin) [2112927]
- net/mlx5e: Split en_fs ndo's and move to en_main (Amir Tzin) [2112927]
- net/mlx5e: Separate mlx5e_set_rx_mode_work and move caller to en_main (Amir Tzin) [2112927]
- net/mlx5e: Add mdev to flow_steering struct (Amir Tzin) [2112927]
- net/mlx5e: Report flow steering errors with mdev err report API (Amir Tzin) [2112927]
- net/mlx5e: Convert mlx5e_flow_steering member of mlx5e_priv to pointer (Amir Tzin) [2112927]
- net/mlx5e: Allocate VLAN and TC for featured profiles only (Amir Tzin) [2112927]
- net/mlx5e: Make mlx5e_tc_table private (Amir Tzin) [2112927]
- net/mlx5e: Convert mlx5e_tc_table member of mlx5e_flow_steering to pointer (Amir Tzin) [2112927]
- net/mlx5e: TC, Support tc action api for police (Amir Tzin) [2112927]
- net/mlx5e: TC, Separate get/update/replace meter functions (Amir Tzin) [2112927]
- net/mlx5e: Add red and green counters for metering (Amir Tzin) [2112927]
- net/mlx5e: TC, Allocate post meter ft per rule (Amir Tzin) [2112927]
- net/mlx5: DR, Add support for flow metering ASO (Amir Tzin) [2112927]
- net/mlx5: Fix driver use of uninitialized timeout (Amir Tzin) [2112927]
- net/mlx5: DR, Fix SMFS steering info dump format (Amir Tzin) [2112927]
- net/mlx5: Adjust log_max_qp to be 18 at most (Amir Tzin) [2112927]
- net/mlx5e: Modify slow path rules to go to slow fdb (Amir Tzin) [2112927 2150647]
- net/mlx5e: Fix calculations related to max MPWQE size (Amir Tzin) [2112927]
- net/mlx5e: xsk: Account for XSK RQ UMRs when calculating ICOSQ size (Amir Tzin) [2112927]
- net/mlx5e: Fix the value of MLX5E_MAX_RQ_NUM_MTTS (Amir Tzin) [2112927]
- net/mlx5e: TC, Fix post_act to not match on in_port metadata (Amir Tzin) [2112927]
- net/mlx5e: Remove WARN_ON when trying to offload an unsupported TLS cipher/version (Amir Tzin) [2112927]
- RDMA/mlx5: Rename the mkey cache variables and functions (Amir Tzin) [2112927]
- RDMA/mlx5: Store in the cache mkeys instead of mrs (Amir Tzin) [2112927]
- RDMA/mlx5: Store the number of in_use cache mkeys instead of total_mrs (Amir Tzin) [2112927]
- RDMA/mlx5: Replace cache list with Xarray (Amir Tzin) [2112927]
- RDMA/mlx5: Replace ent->lock with xa_lock (Amir Tzin) [2112927]
- net/mlx5: CT: Remove warning of ignore_flow_level support for non PF (Amir Tzin) [2112927]
- net/mlx5e: Add resiliency for PTP TX port timestamp (Amir Tzin) [2112927]
- net/mlx5: Expose ts_cqe_metadata_size2wqe_counter (Amir Tzin) [2112927]
- net/mlx5e: HTB, move htb functions to a new file (Amir Tzin) [2112927]
- net/mlx5e: HTB, change functions name to follow convention (Amir Tzin) [2112927]
- net/mlx5e: HTB, remove priv from htb function calls (Amir Tzin) [2112927]
- net/mlx5e: HTB, hide and dynamically allocate mlx5e_htb structure (Amir Tzin) [2112927]
- net/mlx5e: HTB, move stats and max_sqs to priv (Amir Tzin) [2112927]
- net/mlx5e: HTB, move section comment to the right place (Amir Tzin) [2112927]
- net/mlx5e: HTB, move ids to selq_params struct (Amir Tzin) [2112927]
- net/mlx5e: HTB, reduce visibility of htb functions (Amir Tzin) [2112927]
- net/mlx5e: Fix mqprio_rl handling on devlink reload (Amir Tzin) [2112927]
- net/mlx5e: Report header-data split state through ethtool (Amir Tzin) [2112927]
- RDMA/mlx5: Expose steering anchor to userspace (Amir Tzin) [2112927]
- RDMA/mlx5: Refactor get flow table function (Amir Tzin) [2112927]
- net/mlx5: fs, allow flow table creation with a UID (Amir Tzin) [2112927]
- net/mlx5: fs, expose flow table ID to users (Amir Tzin) [2112927]
- net/mlx5: Expose the ability to point to any UID from shared UID (Amir Tzin) [2112927]
- net/mlx5e: Remove the duplicating check for striding RQ when enabling LRO (Amir Tzin) [2112927]
- net/mlx5e: Move the LRO-XSK check to mlx5e_fix_features (Amir Tzin) [2112927]
- net/mlx5e: Extend flower police validation (Amir Tzin) [2112927]
- net/mlx5e: configure meter in flow action (Amir Tzin) [2112927 2150647 2049622]
- net/mlx5e: Removed useless code in function (Amir Tzin) [2112927]
- net/mlx5: Bridge, implement QinQ support (Amir Tzin) [2112927]
- net/mlx5: Bridge, implement infrastructure for VLAN protocol change (Amir Tzin) [2112927]
- net/mlx5: Bridge, extract VLAN push/pop actions creation (Amir Tzin) [2112927]
- net/mlx5: Bridge, rename filter fg to vlan_filter (Amir Tzin) [2112927]
- net/mlx5: Bridge, refactor groups sizes and indices (Amir Tzin) [2112927]
- net/mlx5: debugfs, Add num of in-use FW command interface slots (Amir Tzin) [2112927]
- net/mlx5: Expose vnic diagnostic counters for eswitch managed vports (Amir Tzin) [2112927 2150647 2049881]
- net/mlx5: Use software VHCA id when it's supported (Amir Tzin) [2112927]
- net/mlx5: Introduce ifc bits for using software vhca id (Amir Tzin) [2112927]
- net/mlx5: Use the bitmap API to allocate bitmaps (Amir Tzin) [2112927]
- devlink: Hold the instance lock in port_new / port_del callbacks (mlx5 hunks only) (Amir Tzin) [2112925]
- net/mlx5: Remove devl_unlock from mlx5_devlink_eswitch_mode_set (Amir Tzin) [2112927 2150647]
- net/mlx5: Use devl_ API in mlx5e_devlink_port_register (Amir Tzin) [2112927 2150647]
- net/mlx5: Use devl_ API in mlx5_esw_devlink_sf_port_register (Amir Tzin) [2112927]
- net/mlx5: Use devl_ API in mlx5_esw_offloads_devlink_port_register (Amir Tzin) [2112927 2150647]
- net/mlx5: Use devl_ API for rate nodes destroy (Amir Tzin) [2112927 2150647]
- net/mlx5: Remove devl_unlock from mlx5_eswtich_mode_callback_enter (Amir Tzin) [2112927 2150647]
- net/mlx5: fix 32bit build (Amir Tzin) [2112927 2049622]
- net/mlx5e: TC, Support offloading police action (Amir Tzin) [2112927 2049622]
- net/mlx5e: Add flow_action to parse state (Amir Tzin) [2112927 2049622]
- net/mlx5e: Add post meter table for flow metering (Amir Tzin) [2112927 2049622]
- net/mlx5e: Add generic macros to use metadata register mapping (Amir Tzin) [2112927 2049622]
- net/mlx5e: Get or put meter by the index of tc police action (Amir Tzin) [2112927 2049622]
- net/mlx5e: Add support to modify hardware flow meter parameters (Amir Tzin) [2112927 2049622]
- net/mlx5e: Prepare for flow meter offload if hardware supports it (Amir Tzin) [2112927 2049622]
- net/mlx5: Implement interfaces to control ASO SQ and CQ (Amir Tzin) [2112927 2049622]
- net/mlx5: Add support to create SQ and CQ for ASO (Amir Tzin) [2112927 2049622]
- net/mlx5: E-switch: Change eswitch mode only via devlink command (Amir Tzin) [2112927 2150647 2112917]
- net/mlx5: E-switch, Remove dependency between sriov and eswitch mode (Amir Tzin) [2112927 2150647 2112917]
- net/mlx5: E-switch, Introduce flag to indicate if fdb table is created (Amir Tzin) [2112927 2112917]
- net/mlx5: E-switch, Introduce flag to indicate if vport acl namespace is created (Amir Tzin) [2112927 2112917]
- net/mlx5: delete dead code in mlx5_esw_unlock() (Amir Tzin) [2112927]
- net/mlx5: Delete ipsec_fs header file as not used (Amir Tzin) [2112927]
- net/mlx5: Add bits and fields to support enhanced CQE compression (Amir Tzin) [2112927]
- net/mlx5: Remove not used MLX5_CAP_BITS_RW_MASK (Amir Tzin) [2112927]
- net/mlx5: group fdb cleanup to single function (Amir Tzin) [2112927]
- net/mlx5: Add support EXECUTE_ASO action for flow entry (Amir Tzin) [2112927 2049622]
- net/mlx5: Add HW definitions of vport debug counters (Amir Tzin) [2112927]
- net/mlx5: Add IFC bits and enums for flow meter (Amir Tzin) [2112927 2049622]
- RDMA/mlx5: Support handling of modify-header pattern ICM area (Amir Tzin) [2112927]
- net/mlx5: Manage ICM of type modify-header pattern (Amir Tzin) [2112927]
- net/mlx5: Introduce header-modify-pattern ICM properties (Amir Tzin) [2112927]
- RDMA/mlx5: Add a umr recovery flow (Amir Tzin) [2112927]
- net/mlx5e: Ring the TX doorbell on DMA errors (Amir Tzin) [2112925]
- net/mlx5e: Fix capability check for updating vnic env counters (Amir Tzin) [2112925]
- net/mlx5: Lag, correct get the port select mode str (Amir Tzin) [2112925]
- net/mlx5e: Fix enabling sriov while tc nic rules are offloaded (Amir Tzin) [2112925]
- net/mlx5e: kTLS, Fix build time constant test in RX (Amir Tzin) [2112925]
- net/mlx5e: kTLS, Fix build time constant test in TX (Amir Tzin) [2112925]
- net/mlx5: Lag, decouple FDB selection and shared FDB (Amir Tzin) [2112925]
- net/mlx5: TC, allow offload from uplink to other PF's VF (Amir Tzin) [2112925]
- mellanox: mlx5: avoid uninitialized variable warning with gcc-12 (Amir Tzin) [2112925]
- net/mlx5: E-Switch, pair only capable devices (Amir Tzin) [2112925 2150647]
- Revert "net/mlx5e: Allow relaxed ordering over VFs" (Amir Tzin) [2112925]
- net/mlx5: Fix mlx5_get_next_dev() peer device matching (Amir Tzin) [2112925]
- RDMA/mlx5: Remove duplicate pointer assignment in mlx5_ib_alloc_implicit_mr() (Amir Tzin) [2112925]
- net/mlx5: fix multiple definitions of mlx5_lag_mpesw_init / mlx5_lag_mpesw_cleanup (Amir Tzin) [2112925]
- net/mlx5: Support multiport eswitch mode (Amir Tzin) [2112925 2150647]
- net/mlx5: Remove unused argument (Amir Tzin) [2112925]
- net/mlx5: Lag, refactor lag state machine (Amir Tzin) [2112925]
- net/mlx5e: Add XDP SQs to uplink representors steering tables (Amir Tzin) [2112925]
- net/mlx5e: Allow relaxed ordering over VFs (Amir Tzin) [2112925]
- net/mlx5e: Support partial GSO for tunnels over vlans (Amir Tzin) [2112925]
- net/mlx5e: IPoIB, Improve ethtool rxnfc callback structure in IPoIB (Amir Tzin) [2112925]
- net/mlx5e: Allocate virtually contiguous memory for reps structures (Amir Tzin) [2112925]
- net/mlx5e: Allocate virtually contiguous memory for VLANs list (Amir Tzin) [2112925]
- net/mlx5: Allocate virtually contiguous memory in pci_irq.c (Amir Tzin) [2112925]
- net/mlx5: Allocate virtually contiguous memory in vport.c (Amir Tzin) [2112925]
- net/mlx5: Inline db alloc API function (Amir Tzin) [2112925]
- net/mlx5: Add last command failure syndrome to debugfs (Amir Tzin) [2112925]
- net/mlx5: sparse: error: context imbalance in 'mlx5_vf_get_core_dev' (Amir Tzin) [2112925]
- net/mlx5: Expose mlx5_sriov_blocking_notifier_register / unregister APIs (Amir Tzin) [2112925]
- net/mlx5: Lag, add debugfs to query hardware lag state (Amir Tzin) [2112925]
- net/mlx5: Lag, use buckets in hash mode (Amir Tzin) [2112925]
- net/mlx5: Lag, refactor dmesg print (Amir Tzin) [2112925]
- net/mlx5: Support devices with more than 2 ports (Amir Tzin) [2112925]
- net/mlx5: Lag, use actual number of lag ports (Amir Tzin) [2112925]
- net/mlx5: Lag, use hash when in roce lag on 4 ports (Amir Tzin) [2112925]
- net/mlx5: Lag, support single FDB only on 2 ports (Amir Tzin) [2112925]
- net/mlx5: Lag, store number of ports inside lag object (Amir Tzin) [2112925]
- net/mlx5: Lag, filter non compatible devices (Amir Tzin) [2112925]
- net/mlx5: Lag, use lag lock (Amir Tzin) [2112925]
- net/mlx5: Lag, move E-Switch prerequisite check into lag code (Amir Tzin) [2112925]
- net/mlx5: devcom only supports 2 ports (Amir Tzin) [2112925]
- net/mlx5: Lag, expose number of lag ports (Amir Tzin) [2112925]
- net/mlx5: Increase FW pre-init timeout for health recovery (Amir Tzin) [2112925]
- net/mlx5: Add exit route when waiting for FW (Amir Tzin) [2112925]
- net/mlx5e: Use XFRM state direction instead of flags (Amir Tzin) [2112925]
- net/mlx5: Allow future addition of IPsec object modifiers (Amir Tzin) [2112925]
- net/mlx5: Don't perform lookup after already known sec_path (Amir Tzin) [2112925]
- net/mlx5: Cleanup XFRM attributes struct (Amir Tzin) [2112925]
- net/mlx5: Remove not-supported ICV length (Amir Tzin) [2112925]
- net/mlx5: Simplify IPsec capabilities logic (Amir Tzin) [2112925]
- net/mlx5: Don't advertise IPsec netdev support for non-IPsec device (Amir Tzin) [2112925]
- net/mlx5: Make sure that no dangling IPsec FS pointers exist (Amir Tzin) [2112925]
- net/mlx5: Clean IPsec FS add/delete rules (Amir Tzin) [2112925]
- net/mlx5: Simplify HW context interfaces by using SA entry (Amir Tzin) [2112925]
- net/mlx5: Remove indirections from esp functions (Amir Tzin) [2112925]
- net/mlx5: Merge various control path IPsec headers into one file (Amir Tzin) [2112925]
- net/mlx5: Remove useless validity check (Amir Tzin) [2112925]
- net/mlx5: Store IPsec ESN update work in XFRM state (Amir Tzin) [2112925]
- net/mlx5: Reduce useless indirection in IPsec FS add/delete flows (Amir Tzin) [2112925]
- net/mlx5: Don't hide fallback to software IPsec in FS code (Amir Tzin) [2112925]
- net/mlx5: Check IPsec TX flow steering namespace in advance (Amir Tzin) [2112925]
- net/mlx5: Simplify IPsec flow steering init/cleanup functions (Amir Tzin) [2112925]
- net/mlx5: fs, an FTE should have no dests when deleted (Amir Tzin) [2112925]
- net/mlx5: fs, call the deletion function of the node (Amir Tzin) [2112925]
- net/mlx5: fs, delete the FTE when there are no rules attached to it (Amir Tzin) [2112925]
- net/mlx5: fs, do proper bookkeeping for forward destinations (Amir Tzin) [2112925]
- net/mlx5: fs, add unused destination type (Amir Tzin) [2112925]
- net/mlx5: fs, jump to exit point and don't fall through (Amir Tzin) [2112925]
- net/mlx5: fs, refactor software deletion rule (Amir Tzin) [2112925]
- net/mlx5: fs, split software and IFC flow destination definitions (Amir Tzin) [2112925]
- net/mlx5e: TC, set proper dest type (Amir Tzin) [2112925]
- net/mlx5e: Remove unused mlx5e_dcbnl_build_rep_netdev function (Amir Tzin) [2112925]
- net/mlx5e: Drop error CQE handling from the XSK RX handler (Amir Tzin) [2112925]
- net/mlx5: Print initializing field in case of timeout (Amir Tzin) [2112925]
- net/mlx5: Delete redundant default assignment of runtime devlink params (Amir Tzin) [2112925]
- net/mlx5: Remove useless kfree (Amir Tzin) [2112925]
- net/mlx5: use kvfree() for kvzalloc() in mlx5_ct_fs_smfs_matcher_create (Amir Tzin) [2112925]
- RDMA/mlx5: Clean UMR QP type flow from mlx5_ib_post_send() (Amir Tzin) [2112925]
- RDMA/mlx5: Use mlx5_umr_post_send_wait() to update xlt (Amir Tzin) [2112925]
- RDMA/mlx5: Use mlx5_umr_post_send_wait() to update MR pas (Amir Tzin) [2112925]
- RDMA/mlx5: Move creation and free of translation tables to umr.c (Amir Tzin) [2112925]
- RDMA/mlx5: Use mlx5_umr_post_send_wait() to rereg pd access (Amir Tzin) [2112925]
- RDMA/mlx5: Use mlx5_umr_post_send_wait() to revoke MRs (Amir Tzin) [2112925]
- RDMA/mlx5: Introduce mlx5_umr_post_send_wait() (Amir Tzin) [2112925]
- RDMA/mlx5: Expose wqe posting helpers outside of wr.c (Amir Tzin) [2112925]
- RDMA/mlx5: Simplify get_umr_update_access_mask() (Amir Tzin) [2112925]
- RDMA/mlx5: Move mkey ctrl segment logic to umr.c (Amir Tzin) [2112925]
- RDMA/mlx5: Move umr checks to umr.h (Amir Tzin) [2112925]
- RDMA/mlx5: Move init and cleanup of UMR to umr.c (Amir Tzin) [2112925]
- RDMA/mlx5: Fix flow steering egress flow (Amir Tzin) [2112925]
- mlx5, xsk: Diversify return values from xsk_wakeup call paths (Amir Tzin) [2112925]
- net/mlx5: Remove not-implemented IPsec capabilities (Amir Tzin) [2112925]
- net/mlx5: Remove ipsec_ops function table (Amir Tzin) [2112925]
- net/mlx5: Reduce kconfig complexity while building crypto support (Amir Tzin) [2112925]
- net/mlx5: Move IPsec file to relevant directory (Amir Tzin) [2112925]
- net/mlx5: Remove not-needed IPsec config (Amir Tzin) [2112925]
- net/mlx5: Align flow steering allocation namespace to common style (Amir Tzin) [2112925]
- net/mlx5: Unify device IPsec capabilities check (Amir Tzin) [2112925]
- net/mlx5: Remove useless IPsec device checks (Amir Tzin) [2112925]
- net/mlx5: Remove ipsec vs. ipsec offload file separation (Amir Tzin) [2112925]
- RDMA/mlx5: Drop crypto flow steering API (Amir Tzin) [2112925]
- RDMA/mlx5: Delete never supported IPsec flow action (Amir Tzin) [2112925]
- net/mlx5: Remove FPGA ipsec specific statistics (Amir Tzin) [2112925]
- net/mlx5: Remove XFRM no_trailer flag (Amir Tzin) [2112925]
- net/mlx5: Remove not-used IDA field from IPsec struct (Amir Tzin) [2112925]
- net/mlx5: Delete metadata handling logic (Amir Tzin) [2112925]
- net/mlx5_fpga: Drop INNOVA IPsec support (Amir Tzin) [2112925]
- net/mlx5: Cleanup kTLS function names and their exposure (Amir Tzin) [2112925]
- net/mlx5: Remove tls vs. ktls separation as it is the same (Amir Tzin) [2112925]
- net/mlx5: Remove indirection in TLS build (Amir Tzin) [2112925]
- net/mlx5: Reliably return TLS device capabilities (Amir Tzin) [2112925]
- net/mlx5_fpga: Drop INNOVA TLS support (Amir Tzin) [2112925]
- ipv6: Use ipv6_only_sock() helper in condition (mlx5 hunk only). (Amir Tzin) [2112925]
- Revert "stmmac/intel: mark driver as tech preview" (Mark Salter) [2122230]
- net: stmmac: Fix queue statistics reading (Mark Salter) [2122230]
- stmmac: intel: Update PCH PTP clock rate from 200MHz to 204.8MHz (Mark Salter) [2122230]
- net: stmmac: power up/down serdes in stmmac_open/release (Mark Salter) [2122230]
- stmmac: intel: Simplify intel_eth_pci_remove() (Mark Salter) [2122230]
- net: stmmac: work around sporadic tx issue on link-up (Mark Salter) [2122230]
- stmmac: intel: Add a missing clk_disable_unprepare() call in intel_eth_pci_remove() (Mark Salter) [2122230]
- net: phylink: fix SGMII inband autoneg enable (Mark Salter) [2122230]
- net: phylink: fix NULL pl->pcs dereference during phylink_pcs_poll_start (Mark Salter) [2122230]
- net: phylink: disable PCS polling over major configuration (Mark Salter) [2122230]
- net: phylink: remove pcs_ops member (Mark Salter) [2122230]
- net: pcs: xpcs: depends on PHYLINK in Kconfig (Mark Salter) [2122230]
- net: phylink: add QSGMII support to phylink_mii_c22_pcs_encode_advertisement() (Mark Salter) [2122230]
- net: stmmac: make mdio register skips PHY scanning for fixed-link (Mark Salter) [2122230]
- stmmac: intel: add phy-mode and fixed-link ACPI _DSD setting support (Mark Salter) [2122230]
- net: pcs: xpcs: add CL37 1000BASE-X AN support (Mark Salter) [2122230]
- stmmac: intel: prepare to support 1000BASE-X phy interface setting (Mark Salter) [2122230]
- net: make xpcs_do_config to accept advertising for pcs-xpcs and sja1105 (Mark Salter) [2122230]
- net: pcs: xpcs: propagate xpcs_read error to xpcs_get_state_c37_sgmii (Mark Salter) [2122230]
- net: stmmac: remove redunctant disable xPCS EEE call (Mark Salter) [2122230]
- net: stmmac: fix dma queue left shift overflow issue (Mark Salter) [2122230]
- net: stmmac: switch to use interrupt for hw crosstimestamping (Mark Salter) [2122230]
- net: stmmac: fix unbalanced ptp clock issue in suspend/resume flow (Mark Salter) [2122230]
- net: stmmac: fix pm runtime issue in stmmac_dvr_remove() (Mark Salter) [2122230]
- net: stmmac: dwc-qos: Disable split header for Tegra194 (Mark Salter) [2122230]
- stmmac: intel: Fix an error handling path in intel_eth_pci_probe() (Mark Salter) [2122230]
- stmmac: intel: Add RPL-P PCI ID (Mark Salter) [2122230]
- net: stmmac: use dev_err_probe() for reporting mdio bus registration failure (Mark Salter) [2122230]
- net: stmmac: remove unused get_addr() callback (Mark Salter) [2122230]
- net: pcs: pcs-xpcs: Convert to mdiobus_c45_read (Mark Salter) [2122230]
- net: phylink: Convert to mdiobus_c45_{read|write} (Mark Salter) [2122230]
- net: stmmac: stmmac_main: using pm_runtime_resume_and_get instead of pm_runtime_get_sync (Mark Salter) [2122230]
- net: phylink: remove phylink_helper_basex_speed() (Mark Salter) [2122230]
- net: phylink: remove phylink_set_10g_modes() (Mark Salter) [2122230]
- net: stmmac: using pm_runtime_resume_and_get instead of pm_runtime_get_sync (Mark Salter) [2122230]
- net: stmmac: fix missing pci_disable_device() on error in stmmac_pci_probe() (Mark Salter) [2122230]
- net: stmmac: disable Split Header (SPH) for Intel platforms (Mark Salter) [2122230]
- net: stmmac: Use readl_poll_timeout_atomic() in atomic state (Mark Salter) [2122230]
- net: stmmac: Fix unset max_speed difference between DT and non-DT platforms (Mark Salter) [2122230]
- stmmac: intel: Add ADL-N PCI ID (Mark Salter) [2122230]
- net: stmmac: switch no PTP HW support message to info level (Mark Salter) [2122230]
- net: phylink: remove phylink_set_pcs() (Mark Salter) [2122230]
- stmmac: intel: Enable 2.5Gbps for Intel AlderLake-S (Mark Salter) [2122230]
- net: phylink: remove phylink_config's pcs_poll (Mark Salter) [2122230]
- net: phylink: use legacy_pre_march2020 (Mark Salter) [2122230]
- net: phylink: add legacy_pre_march2020 indicator (Mark Salter) [2122230]
- net: stmmac: optimize locking around PTP clock reads (Mark Salter) [2122230]
- net: stmmac: use .mac_select_pcs() interface (Mark Salter) [2122230]
- net: stmmac: convert to phylink_generic_validate() (Mark Salter) [2122230]
- net: stmmac: remove phylink_config.pcs_poll usage (Mark Salter) [2122230]
- net: stmmac/xpcs: convert to pcs_validate() (Mark Salter) [2122230]
- net: convert users of bitmap_foo() to linkmode_foo() (Mark Salter) [2122230]
- net: phylink: add pcs_validate() method (Mark Salter) [2122230]
- net: phylink: add mac_select_pcs() method to phylink_mac_ops (Mark Salter) [2122230]
- net: phylink: tidy up disable bit clearing (Mark Salter) [2122230]
- net: phylink: handle NA interface mode in phylink_fwnode_phy_connect() (Mark Salter) [2122230]
- net: phylink: Add helpers for c22 registers without MDIO (Mark Salter) [2122230]
- net: phylink: add 1000base-KX to phylink_caps_to_linkmodes() (Mark Salter) [2122230]
- net: phylink: add generic validate implementation (Mark Salter) [2122230]
- net: phylink: use supported_interfaces for phylink validation (Mark Salter) [2122230]
- net: phylink: add MAC phy_interface_t bitmap (Mark Salter) [2122230]
- net: phy: add phy_interface_t bitmap support (Mark Salter) [2122230]
- net: phylink: Convert some users of mdiobus_* to mdiodev_* (Mark Salter) [2122230]
- net: phylink: use mdiobus_modify_changed() helper (Mark Salter) [2122230]
- net: mdio: add mdiobus_modify_changed() (Mark Salter) [2122230]
- net: phylink: add phylink_set_10g_modes() helper (Mark Salter) [2122230]
- net: stmmac: fill in supported_interfaces (Mark Salter) [2122230]
- net: stmmac: convert to phylink_get_linkmodes() (Mark Salter) [2122230]
- net: xpcs: add support for retrieving supported interface modes (Mark Salter) [2122230]
- net: mdio: Add helper functions for accessing MDIO devices (Mark Salter) [2122230]
- net: stmmac: fix return value of __setup handler (Mark Salter) [2122230]
- net: stmmac: only enable DMA interrupts when ready (Mark Salter) [2122230]
- net: stmmac: ensure PTP time register reads are consistent (Mark Salter) [2122230]
- net: stmmac: dump gmac4 DMA registers correctly (Mark Salter) [2122230]
- net: stmmac: properly handle with runtime pm in stmmac_dvr_remove() (Mark Salter) [2122230]
- net: stmmac: skip only stmmac_ptp_register when resume from suspend (Mark Salter) [2122230]
- drivers/net/ethernet: clean up mis-targeted comments (Mark Salter) [2122230]
- net: stmmac: configure PTP clock source prior to PTP initialization (Mark Salter) [2122230]
- net: stmmac: reduce unnecessary wakeups from eee sw timer (Mark Salter) [2122230]
- net: stmmac: remove unused members in struct stmmac_priv (Mark Salter) [2122230]
- net: stmmac: Fix "Unbalanced pm_runtime_enable!" warning (Mark Salter) [2122230]
- net: stmmac: add tc flower filter for EtherType matching (Mark Salter) [2122230]
- net: stmmac: bump tc when get underflow error from DMA descriptor (Mark Salter) [2122230]
- stmmac: remove ethtool driver version info (Mark Salter) [2122230]
- net: stmmac: Calculate CDC error only once (Mark Salter) [2122230]
- net: stmmac: ptp: fix potentially overflowing expression (Mark Salter) [2122230]
- net: stmmac: fix tc flower deletion for VLAN priority Rx steering (Mark Salter) [2122230]
- net: stmmac: Avoid DMA_CHAN_CONTROL write if no Split Header support (Mark Salter) [2122230]
- net: stmmac: Disable Tx queues when reconfiguring the interface (Mark Salter) [2122230]
- net: phylink: Force retrigger in case of latched link-fail indicator (Mark Salter) [2122230]
- net: phylink: Force link down and retrigger resolve on interface change (Mark Salter) [2122230]
- net: stmmac: retain PTP clock time during SIOCSHWTSTAMP ioctls (Mark Salter) [2122230]
- stmmac_pci: Fix underflow size in stmmac_rx (Mark Salter) [2122230]
- net: stmmac: Fix signed/unsigned wreckage (Mark Salter) [2122230]
- net: stmmac: allow a tc-taprio base-time of zero (Mark Salter) [2122230]
- ethernet: stmmac: use eth_hw_addr_set() (Mark Salter) [2122230]
- net: phylink: Support disabling autonegotiation for PCS (Mark Salter) [2122230]
- net: stmmac: fix off-by-one error in sanity check (Mark Salter) [2122230]
- net: stmmac: fix gcc-10 -Wrestrict warning (Mark Salter) [2122230]
- net: phylink: don't call netif_carrier_off() with NULL netdev (Mark Salter) [2122230]
- net: stmmac: Fix E2E delay mechanism (Mark Salter) [2122230]
- net: stmmac: add support for dwmac 3.40a (Mark Salter) [2122230]
- net: stmmac: fix get_hw_feature() on old hardware (Mark Salter) [2122230]
- net: stmmac: trigger PCS EEE to turn off on link down (Mark Salter) [2122230]
- net: pcs: xpcs: fix incorrect steps on disable EEE (Mark Salter) [2122230]
- net: pcs: xpcs: fix incorrect CL37 AN sequence (Mark Salter) [2122230]
- net: stmmac: fix EEE init issue when paired with EEE capable PHYs (Mark Salter) [2122230]
- net: stmmac: allow CSR clock of 300MHz (Mark Salter) [2122230]
- net: stmmac: platform: fix build warning when with !CONFIG_PM_SLEEP (Mark Salter) [2122230]
- net: stmmac: fix system hang caused by eee_ctrl_timer during suspend/resume (Mark Salter) [2122230]
- net: stmmac: fix MAC not working when system resume back with WoL active (Mark Salter) [2122230]
- net: phylink: add suspend/resume support (Mark Salter) [2122230]
- net: stmmac: add ethtool per-queue irq statistic support (Mark Salter) [2122230]
- net: stmmac: add ethtool per-queue statistic framework (Mark Salter) [2122230]
- net: stmmac: fix INTR TBU status affecting irq count statistic (Mark Salter) [2122230]
- net: pcs: xpcs: Add Pause Mode support for SGMII and 2500BaseX (Mark Salter) [2122230]
- net: stmmac: fix kernel panic due to NULL pointer dereference of plat->est (Mark Salter) [2122230]
- net: pcs: xpcs: fix error handling on failed to allocate memory (Mark Salter) [2122230]
- net: stmmac: add est_irq_status callback function for GMAC 4.10 and 5.10 (Mark Salter) [2122230]
- net: stmmac: ptp: update tas basetime after ptp adjust (Mark Salter) [2122230]
- net: stmmac: add mutex lock to protect est parameters (Mark Salter) [2122230]
- net: stmmac: separate the tas basetime calculation function (Mark Salter) [2122230]
- net: stmmac: Terminate FPE workqueue in suspend (Mark Salter) [2122230]
- stmmac: intel: set PCI_D3hot in suspend (Mark Salter) [2122230]
- stmmac: intel: Enable PHY WOL option in EHL (Mark Salter) [2122230]
- net: stmmac: option to enable PHY WOL with PMT enabled (Mark Salter) [2122230]
- net: stmmac: remove redundant continue statement (Mark Salter) [2122230]
- stmmac: intel: fix wrong kernel-doc (Mark Salter) [2122230]
- stmmac: intel: move definitions to dwmac-intel header file (Mark Salter) [2122230]
- net: pcs: xpcs: export xpcs_do_config and xpcs_link_up (Mark Salter) [2122230]
- net: pcs: xpcs: also ignore phy id if it's all ones (Mark Salter) [2122230]
- net: pcs: xpcs: add support for sgmii with no inband AN (Mark Salter) [2122230]
- net: pcs: xpcs: move register bit descriptions to a header file (Mark Salter) [2122230]
- net: stmmac: reduce indentation when calling stmmac_xpcs_setup (Mark Salter) [2122230]
- net: stmmac: reverse Christmas tree notation in stmmac_xpcs_setup (Mark Salter) [2122230]
- net: pcs: xpcs: rename mdio_xpcs_args to dw_xpcs (Mark Salter) [2122230]
- net: phylink: Refactor phylink_of_phy_connect() (Mark Salter) [2122230]
- net: phylink: introduce phylink_fwnode_phy_connect() (Mark Salter) [2122230]
- net: phy: Introduce phy related fwnode functions (Mark Salter) [2122230]
- net: phy: Introduce fwnode_mdio_find_device() (Mark Salter) [2122230]
- net: stmmac: Fix unused values warnings (Mark Salter) [2122230]
- net: stmmac: Fix mixed enum type warning (Mark Salter) [2122230]
- net: stmmac: Fix missing { } around two statements in an if statement (Mark Salter) [2122230]
- net: stmmac: explicitly deassert GMAC_AHB_RESET (Mark Salter) [2122230]
- net: stmmac: platform: use optional clk/reset get APIs (Mark Salter) [2122230]
- net: stmmac: fix NPD with phylink_set_pcs if there is no MDIO bus (Mark Salter) [2122230]
- net: stmmac: enable Intel mGbE 2.5Gbps link speed (Mark Salter) [2122230]
- net: pcs: add 2500BASEX support for Intel mGbE controller (Mark Salter) [2122230]
- net: stmmac: split xPCS setup from mdio register (Mark Salter) [2122230]
- net: pcs: xpcs: convert to phylink_pcs_ops (Mark Salter) [2122230]
- net: pcs: xpcs: convert to mdio_device (Mark Salter) [2122230]
- net: pcs: xpcs: use mdiobus_c45_addr in xpcs_{read,write} (Mark Salter) [2122230]
- net: pcs: xpcs: export xpcs_probe (Mark Salter) [2122230]
- net: pcs: xpcs: export xpcs_config_eee (Mark Salter) [2122230]
- net: pcs: xpcs: export xpcs_validate (Mark Salter) [2122230]
- net: pcs: xpcs: make the checks related to the PHY interface mode stateless (Mark Salter) [2122230]
- net: pcs: xpcs: delete shim definition for mdio_xpcs_get_ops() (Mark Salter) [2122230]
- net: pcs: xpcs: there is only one PHY ID (Mark Salter) [2122230]
- net: stmmac: enable platform specific safety features (Mark Salter) [2122230]
- net: stmmac: the XPCS obscures a potential "PHY not found" error (Mark Salter) [2122230]
- net: stmmac: Add callbacks for DWC xpcs Energy Efficient Ethernet (Mark Salter) [2122230]
- net: pcs: Introducing support for DWC xpcs Energy Efficient Ethernet (Mark Salter) [2122230]

* Thu Feb 02 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-456.el8]
- xfs: reserve quota for dir expansion when linking/unlinking files (Bill O'Donnell) [2086880]
- scsi: storvsc: Fix swiotlb bounce buffer leak in confidential VM (Emanuele Giuseppe Esposito) [2150659]
- ACPICA: Fix operand resolution (Mark Langsdorf) [2156144]
- driver core: Add missing kernel doc for device::msi_lock (Myron Stowe) [2158839]
- PCI/MSI: Protect msi_desc::masked for multi-MSI (Myron Stowe) [2158839]
- KVM: arm64: Don't retrieve memory slot again in page fault handler (Gavin Shan) [2161161]
- fs: allow cross-vfsmount reflink/dedupe (Andrey Albershteyn) [2086200]
- powerpc/hv-gpci: Fix hv_gpci event list (Mamatha Inamdar) [2161258]
- powerpc: declare unmodified attribute_group usages const (Mamatha Inamdar) [2161258]
- drm/amd: Delay removal of the firmware framebuffer (Michel Dänzer) [2162039]
- cpuidle: Add cpu_idle_miss trace event (Mark Langsdorf) [2122312]
- cpuidle: haltpoll: Add trace points for guest_halt_poll_ns grow/shrink (Mark Langsdorf) [2122312]
- efi/cper, cxl: Decode CXL Error Log (Lenny Szubowicz) [2143733]
- efi/cper, cxl: Decode CXL Protocol Error Section (Lenny Szubowicz) [2143733]
- efi: cper: Add support for printing Firmware Error Record Reference (Lenny Szubowicz) [2143733]
- Bluetooth: L2CAP: Fix use-after-free caused by l2cap_reassemble_sdu (Wander Lairson Costa) [2152927] {CVE-2022-3564}
- drm/i915: Fix CFI violations in gt_sysfs (Jocelyn Falempe) [2154880]
- NFS: Clear the file access cache upon login (Benjamin Coddington) [2050832]
- NFS: don't store 'struct cred *' in struct nfs_access_entry (Benjamin Coddington) [2050832]
- NFS: pass cred explicitly for access tests (Benjamin Coddington) [2050832]
- NFS: change nfs_access_get_cached to only report the mask (Benjamin Coddington) [2050832]
- init: Initialize noop_backing_dev_info early (Nico Pache) [2160228]
- mm: vmscan: make rotations a secondary factor in balancing anon vs file (Nico Pache) [2160228]
- writeback: Fix inode->i_io_list not be protected by inode->i_lock error (Nico Pache) [2160228]
- mm: vmscan: fix extreme overreclaim and swap floods (Nico Pache) [2160228]
- mm/page_alloc: ensure kswapd doesn't accidentally go to sleep (Nico Pache) [2160228]
- mm/page_io: count submission time as thrashing delay for delayacct (Nico Pache) [2160228]
- delayacct: support re-entrance detection of thrashing accounting (Nico Pache) [2160228]
- filemap: make the accounting of thrashing more consistent (Nico Pache) [2160228]
- writeback: don't warn on an unregistered BDI in __mark_inode_dirty (Nico Pache) [2160228]
- s390/dasd: fix no record found for raw_track_access (Tobias Huschle) [2161270]
- crypto: testmgr - disallow certain DRBG hash functions in FIPS mode (Vladis Dronov) [2152133]
- dmaengine: idxd: Fix crc_val field for completion record (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Make read buffer sysfs attributes invisible for Intel IAA (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Make max batch size attributes in sysfs invisible for Intel IAA (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Do not call DMX TX callbacks during workqueue disable (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Prevent use after free on completion memory (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Let probe fail when workqueue cannot be enabled (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Fix max batch size for Intel IAA (Jerry Snitselaar) [2144375]
- dmaengine: idxd: add configuration for concurrent batch descriptor processing (Jerry Snitselaar) [2144375]
- dmanegine: idxd: reformat opcap output to match bitmap_parse() input (Jerry Snitselaar) [2144375]
- dmaengine: idxd: add configuration for concurrent work descriptor processing (Jerry Snitselaar) [2144375]
- dmaengine: idxd: add WQ operation cap restriction support (Jerry Snitselaar) [2144375]
- dmaengine: idxd: convert ats_dis to a wq flag (Jerry Snitselaar) [2144375]
- dmaengine: idxd: track enabled workqueues in bitmap (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Set wq state to disabled in idxd_wq_disable_cleanup() (Jerry Snitselaar) [2144375]
- dmaengine: idxd: Do not enable user type Work Queue without Shared Virtual Addressing (Jerry Snitselaar) [2144375]
- dmaengine: idxd: fix RO device state error after been disabled/reset (Jerry Snitselaar) [2144375]
- dmaengine: idxd: avoid deadlock in process_misc_interrupts() (Jerry Snitselaar) [2144375]
- KVM: x86: nSVM: implement nested LBR virtualization (Emanuele Giuseppe Esposito) [2155149]
- KVM: x86: nSVM: correctly virtualize LBR msrs when L2 is running (Emanuele Giuseppe Esposito) [2155149]
- kvm: x86: SVM: use vmcb* instead of svm->vmcb where it makes sense (Emanuele Giuseppe Esposito) [2155149]
- KVM: x86: nSVM: implement nested VMLOAD/VMSAVE (Emanuele Giuseppe Esposito) [2155149]
- eth: octeon: fix build after netif_napi_add() changes (Íñigo Huguet) [2152918]
- net: drop the weight argument from netif_napi_add (Íñigo Huguet) [2152918]
- net: remove netif_tx_napi_add() (Íñigo Huguet) [2152918]
- ipoib: switch to netif_napi_add_weight() (Íñigo Huguet) [2152918]
- IB/hfi1: switch to netif_napi_add_weight() (Íñigo Huguet) [2152918]
- IB/hfi1: switch to netif_napi_add_tx() (Íñigo Huguet) [2152918]
- crypto: caam/qi2 - switch to netif_napi_add_tx_weight() (Íñigo Huguet) [2152918]
- can: can-dev: move to netif_napi_add_weight() (Íñigo Huguet) [2152918]
- net: virtio: switch to netif_napi_add_weight() (Íñigo Huguet) [2152918]
- r8152: switch to netif_napi_add_weight() (Íñigo Huguet) [2152918]
- eth: switch to netif_napi_add_weight() (Íñigo Huguet) [2152918]
- mt76: switch to netif_napi_add_tx() (Íñigo Huguet) [2152918]
- net: move snowflake callers to netif_napi_add_tx_weight() (Íñigo Huguet) [2152918]
- net: switch to netif_napi_add_tx() (Íñigo Huguet) [2152918]
- can: m_can: remove a copy of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2152918]
- eth: remove remaining copies of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2152918]
- eth: benet: remove a copy of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2152918]
- eth: atlantic: remove a copy of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2152918]
- eth: smsc: remove a copy of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2152918]
- eth: remove copies of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2152918]
- netdev: reshuffle netif_napi_add() APIs to allow dropping weight (Íñigo Huguet) [2152918]
- ipv6: raw: Deduct extension header length in rawv6_push_pending_frames (Hangbin Liu) [2162124] {CVE-2023-0394}
- netfilter: conntrack: handle tcp challenge acks during connection reuse (Florian Westphal) [2158726]
- act_mirred: use the backlog for nested calls to mirred ingress (Davide Caratti) [2131339] {CVE-2022-4269}
- net/sched: act_mirred: better wording on protection against excessive stack growth (Davide Caratti) [2131339]
- xfs: add selinux labels to whiteout inodes (Andrey Albershteyn) [2094060]
- tdx: enable TDX attestation driver (Wander Lairson Costa) [2076748]
- selftests/tdx: Test TDX attestation GetReport support (Wander Lairson Costa) [2076748]
- virt: Add TDX guest driver (Wander Lairson Costa) [2076748]
- x86/tdx: Add a wrapper to get TDREPORT0 from the TDX Module (Wander Lairson Costa) [2076748]
- proc: proc_skip_spaces() shouldn't think it is working on C strings (Wander Lairson Costa) [2152572] {CVE-2022-4378}
- proc: avoid integer type confusion in get_proc_long (Wander Lairson Costa) [2152572] {CVE-2022-4378}
- NFSv4.2: Update mode bits after ALLOCATE and DEALLOCATE (Jeffrey Layton) [2127153]
- NFS: nfsiod should not block forever in mempool_alloc() (Jeffrey Layton) [2127153]
- NFSv4.1: Handle NFS4ERR_DELAY replies to OP_SEQUENCE correctly (Benjamin Coddington) [2061259]
- NFSv4.1: Don't decrease the value of seq_nr_highest_sent (Benjamin Coddington) [2061259]

* Wed Feb 01 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-455.el8]
- uas: ignore UAS for Thinkplus chips (Torez Smith) [2113004]
- usb-storage: Add Hiksemi USB3-FW to IGNORE_UAS (Torez Smith) [2113004]
- thunderbolt: Explicitly reset plug events delay back to USB4 spec value (Torez Smith) [2113004]
- USB: serial: option: add Quectel BG95 0x0203 composition (Torez Smith) [2113004]
- thunderbolt: Add support for Intel Maple Ridge single port controller (Torez Smith) [2113004]
- USB: core: Fix RST error in hub.c (Torez Smith) [2113004]
- kunit: fix Kconfig for build-in tests USB4 and Nitro Enclaves (Torez Smith) [2113004]
- usb: storage: Add ASUS <0x0b05:0x1932> to IGNORE_UAS (Torez Smith) [2113004]
- USB: serial: cp210x: add Decagon UCA device id (Torez Smith) [2113004]
- USB: core: Prevent nested device-reset calls (Torez Smith) [2113004]
- usb: typec: Remove retimers properly (Torez Smith) [2113004]
- USB: serial: ftdi_sio: add Omron CS1W-CIF31 device id (Torez Smith) [2113004]
- USB: serial: option: add support for OPPO R11 diag port (Torez Smith) [2113004]
- xhci: Add grace period after xHC start to prevent premature runtime suspend. (Torez Smith) [2113004]
- xhci: Fix null pointer dereference in remove if xHC has only one roothub (Torez Smith) [2113004]
- USB: cdc-acm: Add Icom PMR F3400 support (0c26:0020) (Torez Smith) [2113004]
- usb: xhci-mtk: fix bandwidth release issue (Torez Smith) [2113004]
- usb: xhci-mtk: relax TT periodic bandwidth allocation (Torez Smith) [2113004]
- usb: typec: altmodes/displayport: correct pin assignment for UFP receptacles (Torez Smith) [2113004]
- usb: typec: intel_pmc_mux: Add new ACPI ID for Meteor Lake IOM device (Torez Smith) [2113004]
- usb-storage: Add ignore-residue quirk for NXP PN7462AU (Torez Smith) [2113004]
- usb: typec: tcpm: Return ENOTSUPP for power supply prop writes (Torez Smith) [2113004]
- thunderbolt: Check router generation before connecting xHCI (Torez Smith) [2113004]
- thunderbolt: Use the actual buffer in tb_async_error() (Torez Smith) [2113004]
- USB: usbsevseg: convert sysfs snprintf to sysfs_emit (Torez Smith) [2113004]
- dt-bindings: usb: Add binding for TI USB8041 hub controller (Torez Smith) [2113004]
- usb: typec: ucsi: stm32g0: add bootloader support (Torez Smith) [2113004]
- usb: typec: ucsi: stm32g0: add support for stm32g0 controller (Torez Smith) [2113004]
- dt-bindings: usb: typec: add bindings for stm32g0 controller (Torez Smith) [2113004]
- usb: typec: ucsi: Acknowledge the GET_ERROR_STATUS command completion (Torez Smith) [2113004]
- usb: typec: retimer: Add missing id check in match callback (Torez Smith) [2113004]
- USB: xhci: Fix comment typo (Torez Smith) [2113004]
- usb/typec/tcpm: fix repeated words in comments (Torez Smith) [2113004]
- usb/misc: fix repeated words in comments (Torez Smith) [2113004]
- usb/image: fix repeated words in comments (Torez Smith) [2113004]
- usb/host: fix repeated words in comments (Torez Smith) [2113004]
- usb/core: fix repeated words in comments (Torez Smith) [2113004]
- usb/atm: fix repeated words in comments (Torez Smith) [2113004]
- USB: HCD: Fix URB giveback issue in tasklet function (Torez Smith) [2113004]
- usb: xhci_plat_remove: avoid NULL dereference (Torez Smith) [2113004]
- USB: serial: fix tty-port initialized comments (Torez Smith) [2113004]
- USB: serial: usb_wwan: replace DTR/RTS magic numbers with macros (Torez Smith) [2113004]
- USB: cdc-acm: use CDC serial-state defines (Torez Smith) [2113004]
- USB: cdc-acm: use CDC control-line defines (Torez Smith) [2113004]
- USB: cdc: add serial-state defines (Torez Smith) [2113004]
- USB: cdc: add control-signal defines (Torez Smith) [2113004]
- net/cdc_ncm: Increase NTB max RX/TX values to 64kb (Torez Smith) [2113004]
- usb: typec: Add retimer handle to port (Torez Smith) [2113004]
- usb: typec: Add support for retimers (Torez Smith) [2113004]
- dt-bindings: usb: Add analogix anx7411 PD binding (Torez Smith) [2113004]
- usb: ldusb: replace ternary operator with max_t() (Torez Smith) [2113004]
- USB: serial: fix repeated word "the" in comments (Torez Smith) [2113004]
- USB: serial: io_edgeport: fix spelling mistakes (Torez Smith) [2113004]
- USB: serial: ftdi_sio: add Belimo device ids (Torez Smith) [2113004]
- thunderbolt: test: Use kunit_test_suite() macro (Torez Smith) [2113004]
- media: pvrusb2: drop unexpected word 'a' in comments (Torez Smith) [2113004]
- media: gspca: drop unexpected word 'is' in the comments (Torez Smith) [2113004]
- usb: typec: add missing uevent when partner support PD (Torez Smith) [2113004]
- tools: usb: testusb: Add super-plus speed reporting (Torez Smith) [2113004]
- tools: usb: testusb: Add super speed reporting (Torez Smith) [2113004]
- tools: usb: testusb: Add wireless speed reporting (Torez Smith) [2113004]
- usb: typec: tcpci: move tcpci.h to include/linux/usb/ (Torez Smith) [2113004]
- ARM: sa1100/assabet: move dmabounce hack to ohci driver (Torez Smith) [2113004]
- usb: host: xhci: use snprintf() in xhci_decode_trb() (Torez Smith) [2113004]
- USB: cdc-acm: use define for timeout (Torez Smith) [2113004]
- usb: typec_altmode: add a missing "@" at a kernel-doc parameter (Torez Smith) [2113004]
- usb: core: sysfs: convert sysfs snprintf to sysfs_emit (Torez Smith) [2113004]
- media: usb: gspca: aligned '*' each line (Torez Smith) [2113004]
- media: hdpvr: fix error value returns in hdpvr_read (Torez Smith) [2113004]
- media: em28xx: Remove useless license text when SPDX-License-Identifier is already used (Torez Smith) [2113004]
- USB: serial: use kmemdup instead of kmalloc + memcpy (Torez Smith) [2113004]
- usb: host: ehci-q: Fix ehci_submit_single_step_set_feature annotation typo (Torez Smith) [2113004]
- USB: storage: Fix typo in comment (Torez Smith) [2113004]
- usb: typec: mux: Add CONFIG guards for functions (Torez Smith) [2113004]
- usb: typec: mux: Allow muxes to specify mode-switch (Torez Smith) [2113004]
- usb: musb: Add support for PolarFire SoC's musb controller (Torez Smith) [2113004]
- media: pvrusb2: fix memory leak in pvr_probe (Torez Smith) [2113004]
- media: airspy: respect the DMA coherency rules (Torez Smith) [2113004]
- media: usbtv: Add PAL-Nc standard (Torez Smith) [2113004]
- thunderbolt: Fix typo in comment (Torez Smith) [2113004]
- dt-bindings: usb: add documentation for aspeed udc (Torez Smith) [2113004]
- usb: Avoid extra usb SET_SEL requests when enabling link power management (Torez Smith) [2113004]
- usb: typec: tcpm: Register USB Power Delivery Capabilities (Torez Smith) [2113004]
- usb: typec: USB Power Delivery helpers for ports and partners (Torez Smith) [2113004]
- usb: typec: Separate USB Power Delivery from USB Type-C (Torez Smith) [2113004]
- usb: hub: port: add sysfs entry to switch port power (Torez Smith) [2113004]
- ucsi_ccg: ACPI based I2c client enumeration for AMD ASICs (Torez Smith) [2113004]
- ucsi_ccg: Do not hardcode interrupt polarity and type (Torez Smith) [2113004]
- usb: xhci-mtk: add support optional controller reset (Torez Smith) [2113004]
- usb: typec: tcpm: fix typo in comment (Torez Smith) [2113004]
- usb: xhci: tegra: Fix error check (Torez Smith) [2113004]
- usb: common: usb-conn-gpio: Allow wakeup from system suspend (Torez Smith) [2113004]
- usbip: vudc: Don't enable IRQs prematurely (Torez Smith) [2113004]
- USB: usbip: clean up mixed use of _irq() and _irqsave() (Torez Smith) [2113004]
- USB: Follow-up to SPDX identifiers addition - remove now useless comments (Torez Smith) [2113004]
- thunderbolt: Fix some kernel-doc comments (Torez Smith) [2113004]
- usb: hub: Simplify error and success path in port_over_current_notify (Torez Smith) [2113004]
- usb: remove Link Powermanagement (LPM) disable before port reset. (Torez Smith) [2113004]
- thunderbolt: Change TMU mode to HiFi uni-directional once DisplayPort tunneled (Torez Smith) [2113004]
- usb: core: Bail out when port is stuck in reset loop (Torez Smith) [2113004]
- thunderbolt: Add CL1 support for USB4 and Titan Ridge routers (Torez Smith) [2113004]
- thunderbolt: Change downstream router's TMU rate in both TMU uni/bidir mode (Torez Smith) [2113004]
- USB: core: Fix bug in resuming hub's handling of wakeup requests (Torez Smith) [2113004]
- thunderbolt: Fix typos in CLx enabling (Torez Smith) [2113004]
- usb: hub: Add delay for SuperSpeed hub resume to let links transit to U0 (Torez Smith) [2113004]
- usb: hub: make wait_for_connected() take an int instead of a pointer to int (Torez Smith) [2113004]
- thunderbolt: CLx disable before system suspend only if previously enabled (Torez Smith) [2113004]
- usb: hub: avoid warm port reset during USB3 disconnect (Torez Smith) [2113004]
- thunderbolt: Silently ignore CLx enabling in case CLx is not supported (Torez Smith) [2113004]

* Mon Jan 30 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-454.el8]
- config: Enable Security Path (Ricardo Robaina) [2161309]
- tcp: Fix build break when CONFIG_IPV6=n (Jamie Bainbridge) [2143849]
- tcp: annotate data-race around queue->synflood_warned (Jamie Bainbridge) [2143849]
- tcp: Add listening address to SYN flood message (Jamie Bainbridge) [2143849]
- tcp: Fix data-races around sysctl_tcp_syncookies. (Jamie Bainbridge) [2143849]
- firmware_loader: Fix memory leak in firmware upload (Mark Langsdorf) [2122319]
- firmware_loader: Fix use-after-free during unregister (Mark Langsdorf) [2122319]
- firmware_loader: fix memory leak for paged buffer (Mark Langsdorf) [2122319]
- firmware_loader: describe 'module' parameter of firmware_upload_register() (Mark Langsdorf) [2122319]
- firmware_loader: Move definitions from sysfs_upload.h to sysfs.h (Mark Langsdorf) [2122319]
- firmware_loader: Add sysfs nodes to monitor fw_upload (Mark Langsdorf) [2122319]
- firmware_loader: Add firmware-upload support (Mark Langsdorf) [2122319]
- firmware_loader: Split sysfs support from fallback (Mark Langsdorf) [2122319]
- firmware_loader: Clear data and size in fw_free_paged_buf (Mark Langsdorf) [2122319]
- firmware: Use kvmalloc for page tables (Mark Langsdorf) [2122319]
- firmware: Unify the paged buffer release helper (Mark Langsdorf) [2122319]
- firmware: Free temporary page table after vmapping (Mark Langsdorf) [2122319]
- arch_topology: Make cluster topology span at least SMT CPUs (Mark Langsdorf) [2122319]
- driver core: fix driver_set_override() issue with empty strings (Mark Langsdorf) [2122319]
- arch_topology: Silence early cacheinfo errors when non-existent (Mark Langsdorf) [2122319]
- driver core: Don't probe devices after bus_type.match() probe deferral (Mark Langsdorf) [2122319]
- regmap: spi: Reserve space for register address/padding (Mark Langsdorf) [2122319]
- arch_topology: Fix cache attributes detection in the CPU hotplug path (Mark Langsdorf) [2122319]
- cacheinfo: Use atomic allocation for percpu cache attributes (Mark Langsdorf) [2122319]
- regmap: permit to set reg_update_bits with bulk implementation (Mark Langsdorf) [2122319]
- PM: domains: Ensure genpd_debugfs_dir exists before remove (Mark Langsdorf) [2122319]
- PM: runtime: Extend support for wakeirq for force_suspend|resume (Mark Langsdorf) [2122319]
- regmap: add WARN_ONCE when invalid mask is provided to regmap_field_init() (Mark Langsdorf) [2122319]
- PM: wakeup: Unify device_init_wakeup() for PM_SLEEP and !PM_SLEEP (Mark Langsdorf) [2122319]
- arch_topology: Warn that topology for nested clusters is not supported (Mark Langsdorf) [2122319]
- arch_topology: Add support for parsing sockets in /cpu-map (Mark Langsdorf) [2122319]
- arch_topology: Set cluster identifier in each core/thread from /cpu-map (Mark Langsdorf) [2122319]
- arch_topology: Limit span of cpu_clustergroup_mask() (Mark Langsdorf) [2122319]
- arch_topology: Don't set cluster identifier as physical package identifier (Mark Langsdorf) [2122319]
- arch_topology: Avoid parsing through all the CPUs once a outlier CPU is found (Mark Langsdorf) [2122319]
- arch_topology: Check for non-negative value rather than -1 for IDs validity (Mark Langsdorf) [2122319]
- arch_topology: Set thread sibling cpumask only within the cluster (Mark Langsdorf) [2122319]
- arch_topology: Drop LLC identifier stash from the CPU topology (Mark Langsdorf) [2122319]
- arm64: topology: Remove redundant setting of llc_id in CPU topology (Mark Langsdorf) [2122319]
- arch_topology: Use the last level cache information from the cacheinfo (Mark Langsdorf) [2122319]
- arch_topology: Add support to parse and detect cache attributes (Mark Langsdorf) [2122319]
- cacheinfo: Align checks in cache_shared_cpu_map_{setup,remove} for readability (Mark Langsdorf) [2122319]
- cacheinfo: Use cache identifiers to check if the caches are shared if available (Mark Langsdorf) [2122319]
- cacheinfo: Allow early detection and population of cache attributes (Mark Langsdorf) [2122319]
- cacheinfo: Add support to check if last level cache(LLC) is valid or shared (Mark Langsdorf) [2122319]
- cacheinfo: Move cache_leaves_are_shared out of CONFIG_OF (Mark Langsdorf) [2122319]
- cacheinfo: Add helper to access any cache index for a given CPU (Mark Langsdorf) [2122319]
- cacheinfo: Use of_cpu_device_node_get instead cpu_dev->of_node (Mark Langsdorf) [2122319]
- regmap: cache: Add extra parameter check in regcache_init (Mark Langsdorf) [2122319]
- regmap-irq: Refactor checks for status bulk read support (Mark Langsdorf) [2122319]
- regmap-irq: Remove mask_writeonly and regmap_irq_update_bits() (Mark Langsdorf) [2122319]
- regmap-irq: Remove inappropriate uses of regmap_irq_update_bits() (Mark Langsdorf) [2122319]
- driver core: fix potential deadlock in __driver_attach (Mark Langsdorf) [2122319]
- devtmpfs: fix the dangling pointer of global devtmpfsd thread (Mark Langsdorf) [2122319]
- regmap: Don't warn about cache only mode for devices with no cache (Mark Langsdorf) [2122319]
- regmap: Wire up regmap_config provided bulk write in missed functions (Mark Langsdorf) [2122319]
- regmap: Make regmap_noinc_read() return -ENOTSUPP if map->read isn't set (Mark Langsdorf) [2122319]
- regmap: Re-introduce bulk read support check in regmap_bulk_read() (Mark Langsdorf) [2122319]
- init: Initialize noop_backing_dev_info early (Mark Langsdorf) [2122319]
- driver core: Introduce device_find_any_child() helper (Mark Langsdorf) [2122319]
- regmap: cache: Fix syntax errors in comments (Mark Langsdorf) [2122319]
- PM: domains: Trust domain-idle-states from DT to be correct by genpd (Mark Langsdorf) [2122319]
- PM: domains: Measure power-on/off latencies in genpd based on a governor (Mark Langsdorf) [2122319]
- PM: domains: Allocate governor data dynamically based on a genpd governor (Mark Langsdorf) [2122319]
- PM: domains: Clean up some code in pm_genpd_init() and genpd_remove() (Mark Langsdorf) [2122319]
- PM: domains: Fix initialization of genpd's next_wakeup (Mark Langsdorf) [2122319]
- PM: domains: Fixup QoS latency measurements for IRQ safe devices in genpd (Mark Langsdorf) [2122319]
- PM: domains: Measure suspend/resume latencies in genpd based on governor (Mark Langsdorf) [2122319]
- PM: domains: Move the next_wakeup variable into the struct gpd_timing_data (Mark Langsdorf) [2122319]
- PM: domains: Allocate gpd_timing_data dynamically based on governor (Mark Langsdorf) [2122319]
- PM: domains: Skip another warning in irq_safe_dev_in_sleep_domain() (Mark Langsdorf) [2122319]
- PM: domains: Rename irq_safe_dev_in_no_sleep_domain() in genpd (Mark Langsdorf) [2122319]
- PM: domains: Don't check PM_QOS_FLAG_NO_POWER_OFF in genpd (Mark Langsdorf) [2122319]
- PM: domains: Drop redundant code for genpd always-on governor (Mark Langsdorf) [2122319]
- PM: domains: Add GENPD_FLAG_RPM_ALWAYS_ON for the always-on governor (Mark Langsdorf) [2122319]
- PM: wakeup: expose pm_wakeup_pending to modules (Mark Langsdorf) [2122319]
- driver core: fix deadlock in __device_attach (Mark Langsdorf) [2122319]
- driver: base: fix UAF when driver_attach failed (Mark Langsdorf) [2122319]
- driver core: location: Add "back" as a possible output for panel (Mark Langsdorf) [2122319]
- driver core: location: Free struct acpi_pld_info *pld (Mark Langsdorf) [2122319]
- regmap: Add missing map->bus check (Mark Langsdorf) [2122319]
- device property: Advertise fwnode and device property count API calls (Mark Langsdorf) [2122319]
- driver core: location: Check for allocations failure (Mark Langsdorf) [2122319]
- regmap: Add bulk read/write callbacks into regmap_config (Mark Langsdorf) [2122319]
- device property: Fix recent breakage of fwnode_get_next_parent_dev() (Mark Langsdorf) [2122319]
- drivers/base/memory: fix an unlikely reference counting issue in __add_memory_block() (Mark Langsdorf) [2122319]
- driver core: Add dma_cleanup callback in bus_type (Mark Langsdorf) [2122319]
- driver core: Add sysfs support for physical location of a device (Mark Langsdorf) [2122319]
- drivers/base/node.c: fix compaction sysfs file leak (Mark Langsdorf) [2122319]
- driver core: Prevent overriding async driver of a device before it probe (Mark Langsdorf) [2122319]
- Documentation: dd: Use ReST lists for return values of driver_deferred_probe_check_state() (Mark Langsdorf) [2122319]
- regmap: cache: set max_register with reg_stride (Mark Langsdorf) [2122319]
- firmware_loader: Check fw_state_is_done in loading_store (Mark Langsdorf) [2122319]
- driver: platform: Add helper for safer setting of driver_override (Mark Langsdorf) [2122319]
- PM: domains: Move genpd's time-accounting to ktime_get_mono_fast_ns() (Mark Langsdorf) [2122319]
- PM: runtime: Allow to call __pm_runtime_set_status() from atomic context (Mark Langsdorf) [2122319]
- device property: Drop 'test' prefix in parameters of fwnode_is_ancestor_of() (Mark Langsdorf) [2122319]
- device property: Introduce fwnode_for_each_parent_node() (Mark Langsdorf) [2122319]
- device property: Allow error pointer to be passed to fwnode APIs (Mark Langsdorf) [2122319]
- device property: Check fwnode->secondary in fwnode_graph_get_next_endpoint() (Mark Langsdorf) [2122319]
- PM: runtime: Avoid device usage count underflows (Mark Langsdorf) [2122319]
- PM: domains: Extend dev_pm_domain_detach() doc (Mark Langsdorf) [2122319]

* Wed Jan 25 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-453.el8]
- gitlab-ci: use CI templates from production branch (Michael Hofmann)
- cpufreq: ACPI: Remove unused variables 'acpi_cpufreq_online' and 'ret' (Mark Langsdorf) [2038200]
- cpufreq: ACPI: Only set boost MSRs on supported CPUs (Mark Langsdorf) [2038200]
- cpufreq: ACPI: Defer setting boost MSRs (Mark Langsdorf) [2038200]
- s390/kexec: fix ipl report address for kdump (Tobias Huschle) [2161328]
- iavf: schedule watchdog immediately when changing primary MAC (Michal Schmidt) [2152493]
- iavf: Move netdev_update_features() into watchdog task (Michal Schmidt) [2152493]
- iavf: fix temporary deadlock and failure to set MAC address (Michal Schmidt) [2152493]
- iavf: Fix error handling in iavf_init_module() (Michal Schmidt) [2152493]

* Mon Jan 23 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-452.el8]
- net: ethernet: move from strlcpy with unused retval to strscpy (Ken Cox) [2103955]
- ixgbe: stop resetting SYSTIME in ixgbe_ptp_start_cyclecounter (Ken Cox) [2103955]
- ixgbe: Manual AN-37 for troublesome link partners for X550 SFI (Ken Cox) [2103955]
- ixgbe: Don't call kmap() on page allocated with GFP_ATOMIC (Ken Cox) [2103955]
- ixgbe: convert .adjfreq to .adjfine (Ken Cox) [2103955]
- ixgbe: drop unexpected word 'for' in comments (Ken Cox) [2103955]
- ixgbe: remove unexpected word "the" (Ken Cox) [2103955]
- intel: remove unused macros (Ken Cox) [2103955]
- ixgbe: Fix typos in comments (Ken Cox) [2103955]
- drivers, ixgbe: export vf statistics (Ken Cox) [2103955]
- ixgbe: fix unexpected VLAN Rx in promisc mode on VF (Ken Cox) [2103955]
- ixgbe: fix bcast packets Rx on VF after promisc removal (Ken Cox) [2103955]
- ixgbe: propagate XFRM offload state direction instead of flags (Ken Cox) [2103955]
- ixgbe: Fix module_param allow_unsupported_sfp type (Ken Cox) [2103955]
- ixgbe: ensure IPsec VF<->PF compatibility (Ken Cox) [2103955]
- ixgbe, xsk: Get rid of redundant 'fallthrough' (Ken Cox) [2103955]
- ixgbe, xsk: Diversify return values from xsk_wakeup call paths (Ken Cox) [2103955]
- ixgbe, xsk: Terminate Rx side of NAPI when XSK Rx queue gets full (Ken Cox) [2103955]
- ixgbe, xsk: Decorate IXGBE_XDP_REDIR with likely() (Ken Cox) [2103955]
- ixgbe: add improvement for MDD response functionality (Ken Cox) [2103955]
- ixgbe: add the ability for the PF to disable VF link state (Ken Cox) [2103955]
- ixgbe: xsk: change !netif_carrier_ok() handling in ixgbe_xmit_zc() (Ken Cox) [2103955]
- ixgbe: Remove non-inclusive language (Ken Cox) [2103955]
- ixgbe: Use irq_update_affinity_hint() (Ken Cox) [2103955]
- net: convert users of bitmap_foo() to linkmode_foo() (Ken Cox) [2103955]
- ethernet: use eth_hw_addr_set() for dev->addr_len cases (Ken Cox) [2103955]
- net: Use skb_frag_off accessors (Ken Cox) [2103955]
- drm/i915: Fix watermark calculations for DG2 CCS+CC modifier (Jocelyn Falempe) [2041686]
- drm/i915: Fix watermark calculations for DG2 CCS modifiers (Jocelyn Falempe) [2041686]
- drm/i915: Fix watermark calculations for gen12+ CCS+CC modifier (Jocelyn Falempe) [2041686]
- drm/i915: Fix watermark calculations for gen12+ MC CCS modifier (Jocelyn Falempe) [2041686]
- drm/i915: Fix watermark calculations for gen12+ RC CCS modifier (Jocelyn Falempe) [2041686]
- drm/i915/uc: fix device/bus include on rhel8 (Jocelyn Falempe) [2041686]
- drm/i915/display: consider DG2_RC_CCS_CC when migrating buffers (Jocelyn Falempe) [2041686]
- drm/i915: allow control over the flags when migrating (Jocelyn Falempe) [2041686]
- drm/i915/display: handle migration for dpt (Jocelyn Falempe) [2041686]
- drm/i915/huc: better define HuC status getparam possible return values. (Jocelyn Falempe) [2041686]
- drm/i915/huc: stall media submission until HuC is loaded (Jocelyn Falempe) [2041686]
- drm/i915/huc: track delayed HuC load with a fence (Jocelyn Falempe) [2041686]
- drm/i915/dg2: setup HuC loading via GSC (Jocelyn Falempe) [2041686]
- drm/i915/pxp: add huc authentication and loading command (Jocelyn Falempe) [2041686]
- drm/i915/pxp: implement function for sending tee stream command (Jocelyn Falempe) [2041686]
- drm/i915/pxp: load the pxp module when we have a gsc-loaded huc (Jocelyn Falempe) [2041686]
- drm/i915/gt: Flush to global observation point before breadcrumb write (Jocelyn Falempe) [2041686]
- drm/i915/guc/slpc: Add SLPC selftest live_slpc_power (Jocelyn Falempe) [2041686]
- drm/i915/guc/slpc: Run SLPC selftests on all tiles (Jocelyn Falempe) [2041686]
- drm/i915: Remove unwanted pointer unpacking (Jocelyn Falempe) [2041686]
- drm/i915/guc: Enable compute scheduling on DG2 (Jocelyn Falempe) [2041686]
- drm/i915/dg2: introduce Wa_22015475538 (Jocelyn Falempe) [2041686]
- drm/i915/uc: Update to latest GuC and use new-format GuC/HuC names (Jocelyn Falempe) [2041686]
- Revert "drm/i915/dg2: extend Wa_1409120013 to DG2" (Jocelyn Falempe) [2041686]
- drm/i915/gsc: allocate extended operational memory in LMEM (Jocelyn Falempe) [2041686]
- drm/i915/gsc: add GSC XeHP SDV platform definition (Jocelyn Falempe) [2041686]
- drm/i915/gsc: add slow_firmware flag to the gsc device definition (Jocelyn Falempe) [2041686]
- drm/i915/gsc: skip irq initialization if using polling (Jocelyn Falempe) [2041686]
- drm/i915/uc: Add patch level version number support (Jocelyn Falempe) [2041686]
- drm/i915/uc: Support for version reduced and multiple firmware files (Jocelyn Falempe) [2041686]
- drm/i915/ttm: Abort suspend on i915_ttm_backup failure (Jocelyn Falempe) [2041686]
- drm/i915/dg2: Incorporate Wa_16014892111 into DRAW_WATERMARK tuning (Jocelyn Falempe) [2041686]
- drm/i915/guc: Record CTB info in error logs (Jocelyn Falempe) [2041686]
- drm/i915/guc: Add GuC <-> kernel time stamp translation information (Jocelyn Falempe) [2041686]
- drm/i915/guc: Don't use pr_err when not necessary (Jocelyn Falempe) [2041686]
- drm/i915/dg2: Add support for DC5 state (Jocelyn Falempe) [2041686]
- drm/i915/dmc: Update DG2 DMC firmware to v2.07 (Jocelyn Falempe) [2041686]
- drm/i915/dg2: Add additional tuning settings (Jocelyn Falempe) [2041686]
- drm/i915/gt: Add dedicated function for non-ctx register tuning settings (Jocelyn Falempe) [2041686]
- drm/i915/dg2: Add Wa_1509727124 (Jocelyn Falempe) [2041686]
- drm/i915/dg2: Update DG2 to GuC v70.4.1 (Jocelyn Falempe) [2041686]
- drm/i915/dg2: Add additional HDMI pixel clock frequencies (Jocelyn Falempe) [2041686]
- Revert "drm/i915/dg2: Add preemption changes for Wa_14015141709" (Jocelyn Falempe) [2041686]
- config: Enable TDX Guest (Wander Lairson Costa) [1836977]
- x86/tdx: mark TDX as a tech preview (Wander Lairson Costa) [1836977]
- x86/tdx: Panic on bad configs that #VE on "private" memory access (Wander Lairson Costa) [1836977]
- x86/tdx: Prepare for using "INFO" call for a second purpose (Wander Lairson Costa) [1836977]
- x86/tdx: Handle load_unaligned_zeropad() page-cross to a shared page (Wander Lairson Costa) [1836977]
- x86/tdx: Clarify RIP adjustments in #VE handler (Wander Lairson Costa) [1836977]
- vt: Initialize conswitchp to dummy_con if unset (Wander Lairson Costa) [1836977]
- x86/tdx: Fix early #VE handling (Wander Lairson Costa) [1836977]
- x86/tdx: Fix RETs in TDX asm (Wander Lairson Costa) [1836977]
- x86/apic: Do apic driver probe for "nosmp" use case (Wander Lairson Costa) [1836977]
- x86/mm: Fix spacing within memory encryption features message (Wander Lairson Costa) [1836977]
- x86/kaslr: Fix build warning in KASLR code in boot stub (Wander Lairson Costa) [1836977]
- Documentation/x86: Document TDX kernel architecture (Wander Lairson Costa) [1836977]
- ACPICA: Avoid cache flush inside virtual machines (Wander Lairson Costa) [1836977]
- x86/tdx/ioapic: Add shared bit for IOAPIC base address (Wander Lairson Costa) [1836977]
- x86/mm: Make DMA memory shared for TD guest (Wander Lairson Costa) [1836977]
- x86/mm/cpa: Add support for TDX shared memory (Wander Lairson Costa) [1836977]
- x86/tdx: Make pages shared in ioremap() (Wander Lairson Costa) [1836977]
- x86/topology: Disable CPU online/offline control for TDX guests (Wander Lairson Costa) [1836977]
- x86/boot: Avoid #VE during boot for TDX platforms (Wander Lairson Costa) [1836977]
- x86/boot/compressed/64: Use TEST reg,reg instead of CMP $0,reg (Wander Lairson Costa) [1836977]
- x86/boot/compressed/64: Do not corrupt EDX on EFER.LME=1 setting (Wander Lairson Costa) [1836977]
- x86/boot/compressed/64: Set EFER.LME=1 in 32-bit trampoline before returning to long mode (Wander Lairson Costa) [1836977]
- x86/boot: Set CR0.NE early and keep it set during the boot (Wander Lairson Costa) [1836977]
- x86/acpi/x86/boot: Add multiprocessor wake-up support (Wander Lairson Costa) [1836977]
- x86/boot: Add a trampoline for booting APs via firmware handoff (Wander Lairson Costa) [1836977]
- x86/asm/realmode: Use SYM_DATA_* instead of GLOBAL (Wander Lairson Costa) [1836977]
- x86/realmode: Remove trampoline_status (Wander Lairson Costa) [1836977]
- x86/tdx: Wire up KVM hypercalls (Wander Lairson Costa) [1836977]
- x86/tdx: Port I/O: Add early boot support (Wander Lairson Costa) [1836977]
- x86/tdx: Port I/O: Add runtime hypercalls (Wander Lairson Costa) [1836977]
- x86/boot: Port I/O: Add decompression-time support for TDX (Wander Lairson Costa) [1836977]
- x86/boot: Port I/O: Allow to hook up alternative helpers (Wander Lairson Costa) [1836977]
- x86: Consolidate port I/O helpers (Wander Lairson Costa) [1836977]
- x86: Adjust types used in port I/O helpers (Wander Lairson Costa) [1836977]
- x86/tdx: Detect TDX at early kernel decompression time (Wander Lairson Costa) [1836977]
- x86/tdx: Handle in-kernel MMIO (Wander Lairson Costa) [1836977]
- x86/tdx: Handle CPUID via #VE (Wander Lairson Costa) [1836977]
- x86/tdx: Add MSR support for TDX guests (Wander Lairson Costa) [1836977]
- x86/tdx: Add HLT support for TDX guests (Wander Lairson Costa) [1836977]
- x86/traps: Add #VE support for TDX guest (Wander Lairson Costa) [1836977]
- x86/traps: Refactor exc_general_protection() (Wander Lairson Costa) [1836977]
- x86/traps: Cleanup do_general_protection() (Wander Lairson Costa) [1836977]
- x86/dumpstack: Introduce die_addr() for die() with #GP fault address (Wander Lairson Costa) [1836977]
- x86/traps: Print address on #GP (Wander Lairson Costa) [1836977]
- x86/kprobes: Inline kprobe_exceptions_notify() into do_general_protection() (Wander Lairson Costa) [1836977]
- x86/tdx: Exclude shared bit from __PHYSICAL_MASK (Wander Lairson Costa) [1836977]
- x86/tdx: Extend the confidential computing API to support TDX guests (Wander Lairson Costa) [1836977]
- x86/tdx: Add __tdx_module_call() and __tdx_hypercall() helper functions (Wander Lairson Costa) [1836977]
- x86/tdx: Provide common base for SEAMCALL and TDCALL C wrappers (Wander Lairson Costa) [1836977]
- x86/tdx: Detect running as a TDX guest in early boot (Wander Lairson Costa) [1836977]
- x86/mm/cpa: Generalize __set_memory_enc_pgtable() (Wander Lairson Costa) [1836977]
- x86/mm/pat: Don't flush cache if hardware enforces cache coherency across encryption domnains (Wander Lairson Costa) [1836977]
- x86/coco: Add API to handle encryption mask (Wander Lairson Costa) [1836977]
- x86/cc: Move arch/x86/{kernel/cc_platform.c => coco/core.c} (Wander Lairson Costa) [1836977]
- x86/sev-es: Use insn_decode_mmio() for MMIO implementation (Wander Lairson Costa) [1836977]
- x86/insn-eval: Introduce insn_decode_mmio() (Wander Lairson Costa) [1836977]
- x86/insn-eval: Introduce insn_get_modrm_reg_ptr() (Wander Lairson Costa) [1836977]
- x86/insn-eval: Handle insn_get_opcode() failure (Wander Lairson Costa) [1836977]
- x86/sev: Move common memory encryption code to mem_encrypt.c (Wander Lairson Costa) [1836977]
- x86/sev: Rename mem_encrypt.c to mem_encrypt_amd.c (Wander Lairson Costa) [1836977]
- x86/virtio: Have SEV guests enforce restricted virtio memory access (Wander Lairson Costa) [1836977]
- devlink: protect devlink dump by the instance lock (Petr Oros) [2131116]
- devlink: hold region lock when flushing snapshots (Petr Oros) [2131116]
- net: devlink: enable parallel ops on netlink interface (Petr Oros) [2131116]
- net: devlink: remove devlink_mutex (Petr Oros) [2131116]
- net: devlink: convert reload command to take implicit devlink->lock (Petr Oros) [2131116]
- net: devlink: introduce "unregistering" mark and use it during devlinks iteration (Petr Oros) [2131116]
- devlink: Fix use-after-free after a failed reload (Petr Oros) [2131116]
- net: devlink: Fix missing mutex_unlock() call (Petr Oros) [2131116]
- Documentation: devlink: add add devlink-selftests to the table of contents (Petr Oros) [2131116]
- devlink: Hold the instance lock in health callbacks (Petr Oros) [2131116]
- net/mlx4: Lock mlx4 devlink reload callback (Petr Oros) [2131116]
- net/mlx4: Use devl_ API for devlink port register / unregister (Petr Oros) [2131116]
- net/mlx4: Use devl_ API for devlink region create / destroy (Petr Oros) [2131116]
- net: devlink: remove region snapshots list dependency on devlink->lock (Petr Oros) [2131116]
- net: devlink: remove region snapshot ID tracking dependency on devlink->lock (Petr Oros) [2131116]
- devlink: introduce framework for selftests (Petr Oros) [2131116]
- net: devlink: remove redundant net_eq() check from sb_pool_get_dumpit() (Petr Oros) [2131116]
- net: devlink: move net check into devlinks_xa_for_each_registered_get() (Petr Oros) [2131116]
- net: devlink: make sure that devlink_try_get() works with valid pointer during xarray iteration (Petr Oros) [2131116]
- netdevsim: convert driver to use unlocked devlink API during init/fini (Petr Oros) [2131116]
- net: devlink: add unlocked variants of devlink_region_create/destroy() functions (Petr Oros) [2131116]
- net: devlink: add unlocked variants of devlink_dpipe*() functions (Petr Oros) [2131116]
- net: devlink: add unlocked variants of devlink_sb*() functions (Petr Oros) [2131116]
- net: devlink: add unlocked variants of devlink_resource*() functions (Petr Oros) [2131116]
- net: devlink: add unlocked variants of devling_trap*() functions (Petr Oros) [2131116]
- net: devlink: avoid false DEADLOCK warning reported by lockdep (Petr Oros) [2131116]
- net: devlink: fix return statement in devlink_port_new_notify() (Petr Oros) [2131116]
- net: devlink: fix a typo in function name devlink_port_new_notifiy() (Petr Oros) [2131116]
- net: devlink: make devlink_dpipe_headers_register() return void (Petr Oros) [2131116]
- net: devlink: move unlocked function prototypes alongside the locked ones (Petr Oros) [2131116]
- net: devlink: use helpers to work with devlink->lock mutex (Petr Oros) [2131116]
- net: devlink: fix unlocked vs locked functions descriptions (Petr Oros) [2131116]
- devlink: Hold the instance lock in port_new / port_del callbacks (Petr Oros) [2131116]
- powercap: intel_rapl: Add support for RAPTORLAKE_S (Prarit Bhargava) [2120363]
- selftests/bpf: Fix test_varlen verification failure with latest llvm (Yauheni Kaliuta) [2149222]
- iwlwifi: remove firmware version limit for AC9560 (Íñigo Huguet) [2129361]
- wifi: iwlwifi: fw: skip PPAG for JF (Íñigo Huguet) [2129361]
- sched: Improve wake_up_all_idle_cpus() take #2 (Julia Denham) [2134931]
- selftests/livepatch: better synchronize test_klp_callbacks_busy (Julia Denham) [2121204]
- sched,livepatch: Use wake_up_if_idle() (Joe Lawrence) [2134931]
- sched: Simplify wake_up_*idle*() (Joe Lawrence) [2134931]
- sched,livepatch: Use task_call_func() (Joe Lawrence) [2134931]
- sched,rcu: Rework try_invoke_on_locked_down_task() (Joe Lawrence) [2134931]
- sched: Improve try_invoke_on_locked_down_task() (Joe Lawrence) [2134931]
- arm64/bpf: Remove 128MB limit for BPF JIT programs (Yauheni Kaliuta) [2140163]
- bpf: Define bpf_jit_alloc_exec_limit for arm64 JIT (Yauheni Kaliuta) [2140163]
- arm64: extable: add `type` and `data` fields (Yauheni Kaliuta) [2140163]
- arm64: extable: use `ex` for `exception_table_entry` (Yauheni Kaliuta) [2140163]
- arm64: extable: make fixup_exception() return bool (Yauheni Kaliuta) [2140163]
- arm64: extable: consolidate definitions (Yauheni Kaliuta) [2140163]
- arm64: kvm: use kvm_exception_table_entry (Yauheni Kaliuta) [2140163]
- s390/cio: check the subchannel validity for dev_busid (Tobias Huschle) [2160494]
- s390/cio: add dev_busid sysfs entry for each subchannel (Tobias Huschle) [2160494]

* Thu Jan 19 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-451.el8]
- intel_idle: Add AlderLake-N support (Prarit Bhargava) [2144692]
- selftests/timens: add a test for vfork+exit (Oleg Nesterov) [2116444]
- fs/exec: switch timens when a task gets a new mm (Oleg Nesterov) [2116444]
- namespace: make timens_on_fork() return nothing (Oleg Nesterov) [2116444]
- timens: make vdso_join_timens() always succeed (Oleg Nesterov) [2116444]
- xfrm: Fix oops in __xfrm_state_delete() (Sabrina Dubroca) [2156048]
- tcp: Fix data races around icsk->icsk_af_ops. (Guillaume Nault) [2143904] {CVE-2022-3566}
- ice: synchronize the misc IRQ when tearing down Tx tracker (Petr Oros) [2148858]
- ice: fix handling of burst Tx timestamps (Petr Oros) [2148858]
- vhost/vsock: Fix error handling in vhost_vsock_init() (Stefano Garzarella) [2159969]
- net: vmw_vsock: vmci: Check memcpy_from_msg() (Stefano Garzarella) [2159969]
- vhost/vsock: Use kvmalloc/kvfree for larger packets. (Stefano Garzarella) [2159969]
- vsock: Set socket state back to SS_UNCONNECTED in vsock_connect_timeout() (Stefano Garzarella) [2159969]
- vsock: Fix memory leak in vsock_connect() (Stefano Garzarella) [2159969]
- tools/power turbostat: Add support for RPL-S (Prarit Bhargava) [2122848]

* Tue Jan 17 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-450.el8]
- nvme: re-order nvme_alloc_ns to match "nvme: use blk_mq_alloc_disk" (Chris Leech) [2152742]
- perf vendor events amd: Add Zen 4 mapping (Michael Petlan) [2148294]
- perf vendor events amd: Add Zen 4 metrics (Michael Petlan) [2148294]
- perf vendor events amd: Add Zen 4 uncore events (Michael Petlan) [2148294]
- perf vendor events amd: Add Zen 4 core events (Michael Petlan) [2148294]
- cpuhotplug: Fix KABI breakage (Prarit Bhargava) [2156529]
- scsi: target: core: Fix hard lockup when executing a compare-and-write command (Maurizio Lombardi) [2119897]
- x86/topology: Fix duplicated core ID within a package (Prarit Bhargava) [2159553]
- x86/topology: Fix multiple packages shown on a single-package system (Prarit Bhargava) [2159553]
- hwmon/coretemp: Handle large core ID value (Prarit Bhargava) [2159553]
- x86: Remove vendor checks from prefer_mwait_c1_over_halt (Prarit Bhargava) [2150067]
- x86: Handle idle=nomwait cmdline properly for x86_idle (Prarit Bhargava) [2150067]
- cpufreq: intel_pstate: Support Sapphire Rapids OOB mode (Prarit Bhargava) [2117767]
- KVM: nVMX: Inject #GP, not #UD, if "generic" VMXON CR0/CR4 check fails (Emanuele Giuseppe Esposito) [2159433]
- vmxnet3: correctly report csum_level for encapsulated packet (Izabela Bakollari) [2158809]
- mei: pxp: support matching with a gfx discrete card (Jocelyn Falempe) [2147557]
- mei: pxp: add command streamer API to the PXP driver (Jocelyn Falempe) [2147557]
- mei: bus: extend bus API to support command streamer API (Jocelyn Falempe) [2147557]
- mei: adjust extended header kdocs (Jocelyn Falempe) [2147557]
- mei: bus: enable sending gsc commands (Jocelyn Falempe) [2147557]
- mei: add support to GSC extended header (Jocelyn Falempe) [2147557]
- mei: debugfs: add pxp mode to devstate in debugfs (Jocelyn Falempe) [2147557]
- mei: drop ready bits check after start (Jocelyn Falempe) [2147557]
- mei: gsc: add transition to PXP mode in resume flow (Jocelyn Falempe) [2147557]
- mei: gsc: setup gsc extended operational memory (Jocelyn Falempe) [2147557]
- mei: mkhi: add memory ready command (Jocelyn Falempe) [2147557]
- mei: bus: export common mkhi definitions into a separate header (Jocelyn Falempe) [2147557]
- mei: extend timeouts on slow devices (Jocelyn Falempe) [2147557]
- mei: gsc: wait for reset thread on stop (Jocelyn Falempe) [2147557]
- mei: gsc: use polling instead of interrupts (Jocelyn Falempe) [2147557]
- mei: add slow_firmware flag to the mei auxiliary device (Jocelyn Falempe) [2147557]
- mei: add kdoc for struct mei_aux_device (Jocelyn Falempe) [2147557]
- mei: me: fix clang -Wformat warning (Jocelyn Falempe) [2147557]
- mei: me: add raptor lake point S DID (Jocelyn Falempe) [2147557]
- mei: hbm: drop capability response on early shutdown (Jocelyn Falempe) [2147557]
- mei: me: set internal pg flag to off on hardware reset (Jocelyn Falempe) [2147557]
- misc/mei: Add NULL check to component match callback functions (Jocelyn Falempe) [2147557]
- drm/display: Move HDCP helpers into display-helper module (Jocelyn Falempe) [2147557]
- mei: gsc: retrieve the firmware version (Jocelyn Falempe) [2147557]
- mei: gsc: add runtime pm handlers (Jocelyn Falempe) [2147557]
- mei: gsc: setup char driver alive in spite of firmware handshake failure (Jocelyn Falempe) [2147557]
- mei: add support for graphics system controller (gsc) devices (Jocelyn Falempe) [2147557]
- mei: avoid iterator usage outside of list_for_each_entry (Jocelyn Falempe) [2147557]
- mei: do not overwrite state on hw start (Jocelyn Falempe) [2147557]
- mei: me: fix reset policy on read error in interrupt (Jocelyn Falempe) [2147557]
- mei: me: avoid link reset on shutdown (Jocelyn Falempe) [2147557]
- mei: me: disable driver on the ign firmware (Jocelyn Falempe) [2147557]
- mei: me: Use dma_set_mask_and_coherent() and simplify code (Jocelyn Falempe) [2147557]
- mei: hbm: fix client dma reply status (Jocelyn Falempe) [2147557]
- mei: cleanup status before client dma setup call (Jocelyn Falempe) [2147557]
- mei: add POWERING_DOWN into device state print (Jocelyn Falempe) [2147557]
- mei: Remove some dead code (Jocelyn Falempe) [2147557]
- mei: bus: add client dma interface (Jocelyn Falempe) [2147557]
- mei: hbm: drop hbm responses on early shutdown (Jocelyn Falempe) [2147557]
- mei: me: add Ice Lake-N device id. (Jocelyn Falempe) [2147557]
- mei: pxp: export pavp client to me client bus (Jocelyn Falempe) [2147557]
- mei: Remove usage of the deprecated "pci-dma-compat.h" API (Jocelyn Falempe) [2147557]
- mei: constify passed buffers and structures (Jocelyn Falempe) [2147557]
- mei: revamp mei extension header structure layout. (Jocelyn Falempe) [2147557]
- mei: fix kdoc in the driver (Jocelyn Falempe) [2147557]
- mei: hdcp: SPDX tag should be the first line (Jocelyn Falempe) [2147557]
- mei: request autosuspend after sending rx flow control (Jocelyn Falempe) [2147557]
- mei: Drop unnecessary NULL check after container_of (Jocelyn Falempe) [2147557]
- mei: me: add Alder Lake P device id. (Jocelyn Falempe) [2147557]
- mei: allow map and unmap of client dma buffer only for disconnected client (Jocelyn Falempe) [2147557]
- mei: use sysfs_emit() in tx_queue_limit_show sysfs (Jocelyn Falempe) [2147557]
- mei: bus: block send with vtag on non-conformat FW (Jocelyn Falempe) [2147557]
- mei: bus: change remove callback to return void (Jocelyn Falempe) [2147557]
- mei: bus: simplify mei_cl_device_remove() (Jocelyn Falempe) [2147557]
- mei: implement client dma setup. (Jocelyn Falempe) [2147557]
- mei: hbm: add client dma hbm messages (Jocelyn Falempe) [2147557]
- mei: add support for client dma capability (Jocelyn Falempe) [2147557]
- mei: allow clients on bus to communicate in remove callback (Jocelyn Falempe) [2147557]
- mei: me: add adler lake point LP DID (Jocelyn Falempe) [2147557]
- mei: hbm: drop hbm responses on shutdown (Jocelyn Falempe) [2147557]
- mei: hbm: call mei_set_devstate() on hbm stop response (Jocelyn Falempe) [2147557]
- mei: document that mei_msg_hdr_init returns ERR_PTR (Jocelyn Falempe) [2147557]
- mei: fix transfer over dma with extended header (Jocelyn Falempe) [2147557]
- misc/mei/hdcp: Fix AUTH_STREAM_REQ cmd buffer len (Jocelyn Falempe) [2147557]
- mei: bus: enable pavp device. (Jocelyn Falempe) [2147557]
- mei: bus: add vtag support (Jocelyn Falempe) [2147557]
- Revert "mei: virtio: virtualization frontend driver" (Jocelyn Falempe) [2147557]
- mei: bus: fix a kernel-doc markup (Jocelyn Falempe) [2147557]
- mei: protect mei_cl_mtu from null dereference (Jocelyn Falempe) [2147557]
- mei: bus: deinitialize callback functions on init failure (Jocelyn Falempe) [2147557]
- mei: bus: do not start a read for disconnected clients (Jocelyn Falempe) [2147557]
- misc: mei: remove unneeded break (Jocelyn Falempe) [2147557]
- mei: hw: Replace zero-length array with flexible-array member (Jocelyn Falempe) [2147557]
- mei: virtio: virtualization frontend driver (Jocelyn Falempe) [2147557]
- mei: add connect with vtag ioctl (Jocelyn Falempe) [2147557]
- mei: bus: unconditionally enable clients with vtag support (Jocelyn Falempe) [2147557]
- mei: bus: use zero vtag for bus clients. (Jocelyn Falempe) [2147557]
- mei: handle tx queue flushing for vtag connections (Jocelyn Falempe) [2147557]
- mei: add a vtag map for each client (Jocelyn Falempe) [2147557]
- mei: add a spin lock to protect rd_completed queue (Jocelyn Falempe) [2147557]
- mei: bump hbm version to 2.2 (Jocelyn Falempe) [2147557]
- mei: add support for mei extended header. (Jocelyn Falempe) [2147557]
- mei: add vtag support bit in client properties (Jocelyn Falempe) [2147557]
- mei: restrict vtag support to hbm version 2.2 (Jocelyn Falempe) [2147557]
- mei: hbm: add capabilities message (Jocelyn Falempe) [2147557]
- Revert "scsi: iscsi: ql4xxx: Use per-session workqueue for unbinding" (Chris Leech) [2122624]
- Revert "scsi: iscsi: Use the session workqueue for recovery" (Chris Leech) [2122624]
- l2tp: Don't sleep and disable BH under writer-side sk_callback_lock (Guillaume Nault) [2145235] {CVE-2022-4129}
- l2tp: Serialize access to sk_user_data with sk_callback_lock (Guillaume Nault) [2145235] {CVE-2022-4129}
- net: fix a concurrency bug in l2tp_tunnel_register() (Guillaume Nault) [2145235] {CVE-2022-4129}
- net: tap: fix general protection fault when freeing an skb when the ring is full (Antoine Tenart) [2152802]
- platform/x86/intel/pmt: Sapphire Rapids PMT errata fix (Prarit Bhargava) [2144689]
- RDMA/core: Fix null-ptr-deref in ib_core_cleanup() (Kamal Heib) [2120677]
- RDMA/rxe: Fix mr leak in RESPST_ERR_RNR (Kamal Heib) [2120677]
- IB/hfi1: Correctly move list in sc_disable() (Kamal Heib) [2120677]
- RDMA/cma: Use output interface for net_dev check (Kamal Heib) [2120677]
- RDMA/usnic: fix set-but-not-unused variable 'flags' warning (Kamal Heib) [2120677]
- IB/rdmavt: Add __init/__exit annotations to module init/exit funcs (Kamal Heib) [2120677]
- RDMA/rxe: Fix resize_finish() in rxe_queue.c (Kamal Heib) [2120677]
- IB: Set IOVA/LENGTH on IB_MR in core/uverbs layers (Kamal Heib) [2120677]
- RDMA/cm: Use SLID in the work completion as the DLID in responder side (Kamal Heib) [2120677]
- RDMA/siw: Fix QP destroy to wait for all references dropped. (Kamal Heib) [2120677]
- RDMA/srp: Fix srp_abort() (Kamal Heib) [2120677]
- RDMA/irdma: Validate udata inlen and outlen (Kamal Heib) [2120677]
- RDMA/irdma: Align AE id codes to correct flush code and event (Kamal Heib) [2120677]
- RDMA/rxe: Fix the error caused by qp->sk (Kamal Heib) [2120677]
- RDMA/rxe: Fix "kernel NULL pointer dereference" error (Kamal Heib) [2120677]
- RDMA/rxe: Remove an unused member from struct rxe_mr (Kamal Heib) [2120677]
- x86/fpu: Fix copy_xstate_to_uabi() to copy init states correctly (Dean Nelson) [2122850]
- x86/fpu: Exclude dynamic states from init_fpstate (Dean Nelson) [2122850]
- x86/fpu: Fix the init_fpstate size check with the actual size (Dean Nelson) [2122850]
- x86/fpu: Configure init_fpstate attributes orderly (Dean Nelson) [2122850]
- x86/fpu/xstate: Fix the ARCH_REQ_XCOMP_PERM implementation (Dean Nelson) [2122850]
- ceph: rely on vfs for setgid stripping (Andrey Albershteyn) [2128904]
- fs: move S_ISGID stripping into the vfs_*() helpers (Andrey Albershteyn) [2128904]
- fs: Add missing umask strip in vfs_tmpfile (Andrey Albershteyn) [2128904]
- fs: add mode_strip_sgid() helper (Andrey Albershteyn) [2128904]

* Thu Jan 12 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-449.el8]
- x86/insn: Add AMX instructions to the x86 instruction decoder (Prarit Bhargava) [2117765]
- intel_idle: Add a new flag to initialize the AMX state (Prarit Bhargava) [2117765]
- x86/fpu: Add a helper to prepare AMX state for low-power CPU idle (Prarit Bhargava) [2117765]
- intel_idle: make SPR C1 and C1E be independent (Prarit Bhargava) [2117765]
- rpmspec: drop traceevent files instead of just excluding them from files list (Michael Petlan) [2155509]
- powerpc/bpf/64: Add instructions for atomic_[cmp]xchg (Mamatha Inamdar) [2113254]
- powerpc/bpf/64: add support for atomic fetch operations (Mamatha Inamdar) [2113254]
- powerpc/bpf/64: add support for BPF_ATOMIC bitwise operations (Mamatha Inamdar) [2113254]
- powerpc/bpf: Simplify bpf_to_ppc() and adopt it for powerpc64 (Mamatha Inamdar) [2113254]
- powerpc64/bpf: Store temp registers' bpf to ppc mapping (Mamatha Inamdar) [2113254]
- powerpc/bpf: Use _Rn macros for GPRs (Mamatha Inamdar) [2113254]
- powerpc/bpf: Move bpf_jit64.h into bpf_jit_comp64.c (Mamatha Inamdar) [2113254]
- powerpc/bpf: Cleanup bpf_jit.h (Mamatha Inamdar) [2113254]
- powerpc64/bpf: Get rid of PPC_BPF_[LL|STL|STLU] macros (Mamatha Inamdar) [2113254]
- powerpc64/bpf: Convert some of the uses of PPC_BPF_[LL|STL] to PPC_BPF_[LD|STD] (Mamatha Inamdar) [2113254]
- powerpc64/bpf: Optimize instruction sequence used for function calls (Mamatha Inamdar) [2113254]
- powerpc64/bpf elfv1: Do not load TOC before calling functions (Mamatha Inamdar) [2113254]
- powerpc64/bpf elfv2: Setup kernel TOC in r2 on entry (Mamatha Inamdar) [2113254]
- powerpc64: Set PPC64_ELF_ABI_v[1|2] macros to 1 (Mamatha Inamdar) [2113254]
- powerpc64/bpf: Use r12 for constant blinding (Mamatha Inamdar) [2113254]
- powerpc64/bpf: Do not save/restore LR on each call to bpf_stf_barrier() (Mamatha Inamdar) [2113254]
- powerpc/bpf: Handle large branch ranges with BPF_EXIT (Mamatha Inamdar) [2113254]
- powerpc/bpf: Emit a single branch instruction for known short branch ranges (Mamatha Inamdar) [2113254]
- powerpc/bpf: Skip branch range validation during first pass (Mamatha Inamdar) [2113254]
- powerpc64/bpf: Limit 'ldbrx' to processors compliant with ISA v2.06 (Mamatha Inamdar) [2113254]
- tools/bpf: Rename 'struct event' to avoid naming conflict (Mamatha Inamdar) [2113254]
- bpf: Guard against accessing NULL pt_regs in bpf_get_task_stack() (Mamatha Inamdar) [2113254]
- bpf ppc64: Access only if addr is kernel address (Mamatha Inamdar) [2113254]
- bpf ppc64: Add BPF_PROBE_MEM support for JIT (Mamatha Inamdar) [2113254]
- powerpc/ppc-opcode: introduce PPC_RAW_BRANCH() macro (Mamatha Inamdar) [2113254]
- bpf powerpc: refactor JIT compiler code (Mamatha Inamdar) [2113254]
- bpf powerpc: Remove extra_pass from bpf_jit_build_body() (Mamatha Inamdar) [2113254]
- bpf powerpc: Remove unused SEEN_STACK (Mamatha Inamdar) [2113254]
- powerpc/bpf: Emit stf barrier instruction sequences for BPF_NOSPEC (Mamatha Inamdar) [2113254]
- powerpc/security: Add a helper to query stf_barrier type (Mamatha Inamdar) [2113254]
- powerpc/bpf: Fix BPF_SUB when imm == 0x80000000 (Mamatha Inamdar) [2113254]
- powerpc/bpf: Fix BPF_MOD when imm == 1 (Mamatha Inamdar) [2113254]
- powerpc/bpf: Validate branch ranges (Mamatha Inamdar) [2113254]
- powerpc/lib: Add helper to check if offset is within conditional branch range (Mamatha Inamdar) [2113254]
- powerpc/lib/feature-fixups: Use PPC_RAW_xxx() macros (Mamatha Inamdar) [2113254]
- powerpc: Move PPC_HA() PPC_HI() and PPC_LO() to ppc-opcode.h (Mamatha Inamdar) [2113254]
- swapfile: fix soft lockup in scan_swap_map_slots (Waiman Long) [2155734]
- mm/swap: add helper swap_offset_available() (Waiman Long) [2155734]
- pNFS/filelayout: Fix coalescing test for single DS (Benjamin Coddington) [2158520]
- arm64: kdump: Support crashkernel=X fall back to reserve region above DMA zones (Pingfan Liu) [1940674]
- arm64: kdump: Provide default size when crashkernel=Y,low is not specified (Pingfan Liu) [1940674]
- media: dmxdev: fix UAF when dvb_register_device() fails (Dean Nelson) [2123301] {CVE-2022-41218}
- crypto: s390/aes - drop redundant xts key check (Vladis Dronov) [2158893]
- crypto: xts - implement xts_verify_key() with xts_check_key() (Vladis Dronov) [2158893]
- audit: cache ctx->major in audit_filter_syscall() (Richard Guy Briggs) [2123854]
- audit: free audit_proctitle only on task exit (Richard Guy Briggs) [2123854]
- audit: explicitly check audit_context->context enum value (Richard Guy Briggs) [2123854]
- audit: move audit_return_fixup before the filters (Richard Guy Briggs) [2123854]
- audit: fix potential double free on error path from fsnotify_add_inode_mark (Richard Guy Briggs) [2123854]
- i2c: ismt: Fix an out-of-bounds bug in ismt_access() (Prarit Bhargava) [2119066] {CVE-2022-2873}
- net: dropreason: add SKB_DROP_REASON_FRAG_TOO_FAR (Antoine Tenart) [2155186]
- net: dropreason: add SKB_DROP_REASON_FRAG_REASM_TIMEOUT (Antoine Tenart) [2155186]
- net: dropreason: add SKB_DROP_REASON_DUP_FRAG (Antoine Tenart) [2155186]
- net: dropreason: propagate drop_reason to skb_release_data() (Antoine Tenart) [2155186]
- net: dropreason: add SKB_CONSUMED reason (Antoine Tenart) [2155186]
- ipv4: remove redundant null pointer check before kfree_skb (Antoine Tenart) [2155186]

* Mon Jan 09 2023 Lucas Zampieri <lzampier@redhat.com> [4.18.0-448.el8]
- turbostat: Bring code up-to-date with upstream (Prarit Bhargava) [2117769]
- tools/power turbostat: Enable accumulate RAPL display (Prarit Bhargava) [2117769]
- tools/power turbostat: version 2022.07.28 (Prarit Bhargava) [2117769]
- tools/power turbostat: do not decode ACC for ICX and SPR (Prarit Bhargava) [2117769]
- tools/power turbostat: fix SPR PC6 limits (Prarit Bhargava) [2117769]
- tools/power turbostat: cleanup 'automatic_cstate_conversion_probe()' (Prarit Bhargava) [2117769]
- tools/power turbostat: separate SPR from ICX (Prarit Bhargava) [2117769]
- tools/power turbosstat: fix comment (Prarit Bhargava) [2117769]
- tools/power turbostat: Support RAPTORLAKE P (Prarit Bhargava) [2117769]
- tools/power turbostat: add support for ALDERLAKE_N (Prarit Bhargava) [2117769]
- tools/power turbostat: dump secondary Turbo-Ratio-Limit (Prarit Bhargava) [2117769]
- tools/power turbostat: simplify dump_turbo_ratio_limits() (Prarit Bhargava) [2117769]
- tools/power turbostat: dump CPUID.7.EDX.Hybrid (Prarit Bhargava) [2117769]
- tools/power turbostat: update turbostat.8 (Prarit Bhargava) [2117769]
- tools/power turbostat: Show uncore frequency (Prarit Bhargava) [2117769]
- tools/power turbostat: Fix file pointer leak (Prarit Bhargava) [2117769]
- tools/power turbostat: replace strncmp with single character compare (Prarit Bhargava) [2117769]
- tools/power turbostat: print the kernel boot commandline (Prarit Bhargava) [2117769]
- tools/power turbostat: Introduce support for RaptorLake (Prarit Bhargava) [2117769]
- tools/power turbostat: version 2022.04.16 (Prarit Bhargava) [2117769]
- tools/power turbostat: No build warnings with -Wextra (Prarit Bhargava) [2117769]
- tools/power turbostat: be more useful as non-root (Prarit Bhargava) [2117769]
- tools/power turbostat: fix ICX DRAM power numbers (Prarit Bhargava) [2117769]
- tools/power turbostat: Support thermal throttle count print (Prarit Bhargava) [2117769]
- tools/power turbostat: Allow printing header every N iterations (Prarit Bhargava) [2117769]
- tools/power turbostat: Allow -e for all names. (Prarit Bhargava) [2117769]
- tools/power turbostat: print power values upto three decimal (Prarit Bhargava) [2117769]
- tools/power turbostat: Add Power Limit4 support (Prarit Bhargava) [2117769]
- tools/power turbostat: fix dump for AMD cpus (Prarit Bhargava) [2117769]
- tools/power turbostat: tweak --show and --hide capability (Prarit Bhargava) [2117769]
- NFSv4: Retry LOCK on OLD_STATEID during delegation return (Benjamin Coddington) [2137826]
- KVM: s390: pv: don't allow userspace to set the clock under PV (Tobias Huschle) [2154284]
- net: mana: Fix race on per-CQ variable napi work_done (Emanuele Giuseppe Esposito) [2151722]
- powercap: intel_rapl: support new layout of Psys PowerLimit Register on SPR (Prarit Bhargava) [2106143]
- ceph: choose auth MDS for getxattr with the Xs caps (Milind Changire) [2126703]
- ceph: try to choose the auth MDS if possible for getattr (Milind Changire) [2126703]
- ceph: convert to generic_file_llseek (Milind Changire) [2126707]
- ceph: don't leak snap_rwsem in handle_cap_grant (Milind Changire) [2126706]
- ceph: prevent a client from exceeding the MDS maximum xattr size (Milind Changire) [2126704]
- ceph: add session already open notify support (Milind Changire) [2126701]
- ceph: use correct index when encoding client supported features (Milind Changire) [2143875]
- ceph: switch TASK_INTERRUPTIBLE to TASK_KILLABLE (Milind Changire) [2126700]
- ceph: allow ceph.dir.rctime xattr to be updatable (Milind Changire) [2126699]
- ipv6: Use ipv6_only_sock() helper in condition. (Izabela Bakollari) [2144855]
- ipv6: Remove __ipv6_only_sock(). (Izabela Bakollari) [2144855]
- redhat/configs: Switch CONFIG_X86_AMD_PSTATE to built-in (Prarit Bhargava) [2150424]
- Documentation: add amd-pstate kernel command line options (Prarit Bhargava) [2150424]
- cpufreq: amd-pstate: add amd-pstate driver parameter for mode selection (Prarit Bhargava) [2150424]
- cpufreq: amd-pstate: change amd-pstate driver to be built-in type (Prarit Bhargava) [2150424]
- cpufreq: amd-pstate: cpufreq: amd-pstate: reset MSR_AMD_PERF_CTL register at init (Prarit Bhargava) [2150424]
- scsi: target: iscsi: Fix a race condition between login_work and the login thread (Maurizio Lombardi) [2153832]
- virtio_console: Introduce an ID allocator for virtual console numbers (Cédric Le Goater) [2072437]
- blk-throttle: fix that io throttle can only work for single bio (Ming Lei) [2088193]
- scsi: zfcp: Fix double free of FSF request when qdio send fails (Tobias Huschle) [2155157]
- scsi: qla2xxx: Fix crash when I/O abort times out (Nilesh Javali) [2115820]
- perf trace: Fix SIGSEGV when processing syscall args (Michael Petlan) [2145089]
- config: mhi: set CONFIG_MHI_BUS_EP to disabled (Íñigo Huguet) [2136123]
- config: rtw89: set CONFIG_RTW89_8852C to disabled (Íñigo Huguet) [2136123]
- wifi: ath11k: avoid deadlock during regulatory update in ath11k_regd_update() (Íñigo Huguet) [2136123 2139481]
- wifi: mac80211: mlme: Fix double unlock on assoc success handling (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: Fix missing unlock on beacon RX (Íñigo Huguet) [2136123]
- wifi: mac80211: fix memory corruption in minstrel_ht_update_rates() (Íñigo Huguet) [2136123]
- wifi: mac80211: fix regression with non-QoS drivers (Íñigo Huguet) [2136123]
- wifi: mac80211: ensure vif queues are operational after start (Íñigo Huguet) [2136123]
- wifi: mac80211: don't start TX with fq->lock to fix deadlock (Íñigo Huguet) [2136123]
- wifi: cfg80211: fix MCS divisor value (Íñigo Huguet) [2136123]
- wifi: mt76: fix 5 GHz connection regression on mt76x0/mt76x2 (Íñigo Huguet) [2136123]
- wifi: mt76: fix reading current per-tid starting sequence number for aggregation (Íñigo Huguet) [2136123]
- wifi: iwlwifi: Mark IWLMEI as broken (Íñigo Huguet) [2136123]
- wifi: iwlwifi: don't spam logs with NSS>2 messages (Íñigo Huguet) [2136123]
- wifi: use struct_group to copy addresses (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: check length for virtio packets (Íñigo Huguet) [2136123]
- wifi: mac80211: fix locking in auth/assoc timeout (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: release deflink channel in error case (Íñigo Huguet) [2136123]
- wifi: mac80211: fix link warning in RX agg timer expiry (Íñigo Huguet) [2136123]
- bus: mhi: host: Fix up null pointer access in mhi_irq_handler (Íñigo Huguet) [2136123]
- net: Use u64_stats_fetch_begin_irq() for stats fetch. (Íñigo Huguet) [2136123]
- wifi: mt76: mt7921e: fix crash in chip reset fail (Íñigo Huguet) [2136123]
- wifi: mac80211: potential NULL dereference in ieee80211_tx_control_port() (Íñigo Huguet) [2136123]
- wifi: cfg80211: debugfs: fix return type in ht40allow_map_read() (Íñigo Huguet) [2136123]
- wifi: mac80211: Don't finalize CSA in IBSS mode if state is disconnected (Íñigo Huguet) [2136123]
- wifi: mac80211: fix possible leak in ieee80211_tx_control_port() (Íñigo Huguet) [2136123]
- wifi: mac80211: always free sta in __sta_info_alloc in case of error (Íñigo Huguet) [2136123]
- wifi: mac80211: Fix UAF in ieee80211_scan_rx() (Íñigo Huguet) [2136123]
- net: qrtr: start MHI channel after endpoit creation (Íñigo Huguet) [2136123]
- wifi: cfg80211: Fix validating BSS pointers in __cfg80211_connect_result (Íñigo Huguet) [2136123]
- wifi: rtw88: check the return value of alloc_workqueue() (Íñigo Huguet) [2136123]
- wifi: rtw89: 8852a: adjust IMR for SER L1 (Íñigo Huguet) [2136123]
- wifi: rtw89: 8852a: update RF radio A/B R56 (Íñigo Huguet) [2136123]
- wifi: brcmfmac: prevent double-free on hardware-reset (Íñigo Huguet) [2136123]
- wifi: brcmfmac: support brcm,ccode-map-trivial DT property (Íñigo Huguet) [2136123]
- wifi: brcmfmac: Replace default (not configured) MAC with a random MAC (Íñigo Huguet) [2136123]
- wifi: brcmfmac: Add brcmf_c_set_cur_etheraddr() helper (Íñigo Huguet) [2136123]
- wifi: brcmfmac: Remove #ifdef guards for PM related functions (Íñigo Huguet) [2136123]
- wifi: brcmfmac: use strreplace() in brcmf_of_probe() (Íñigo Huguet) [2136123]
- wifi: rtl8xxxu: Fix the error handling of the probe function (Íñigo Huguet) [2136123]
- wifi: mwifiex: clean up one inconsistent indenting (Íñigo Huguet) [2136123]
- wifi: rtlwifi: Remove duplicate word and Fix typo (Íñigo Huguet) [2136123]
- wifi: mwifiex: Fix comment typo (Íñigo Huguet) [2136123]
- wifi: iwlwifi: mvm: fix clang -Wformat warnings (Íñigo Huguet) [2136123]
- Revert "ath11k: add support for hardware rfkill for QCA6390" (Íñigo Huguet) [2136123]
- wifi: ath11k: Fix register write failure on QCN9074 (Íñigo Huguet) [2136123]
- wifi: mac80211: fix link data leak (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: fix disassoc with MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: add macros to loop over active links (Íñigo Huguet) [2136123]
- wifi: mac80211: remove erroneous sband/link validation (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: transmit assoc frame with address translation (Íñigo Huguet) [2136123]
- wifi: mac80211: verify link addresses are different (Íñigo Huguet) [2136123]
- wifi: mac80211: rx: track link in RX data (Íñigo Huguet) [2136123]
- wifi: mac80211: optionally implement MLO multicast TX (Íñigo Huguet) [2136123]
- wifi: mac80211: expand ieee80211_mgmt_tx() for MLO (Íñigo Huguet) [2136123]
- wifi: nl80211: add MLO link ID to the NL80211_CMD_FRAME TX API (Íñigo Huguet) [2136123]
- wifi: mac80211: report link ID to cfg80211 on mgmt RX (Íñigo Huguet) [2136123]
- wifi: cfg80211: report link ID in NL80211_CMD_FRAME (Íñigo Huguet) [2136123]
- wifi: mac80211: add hardware timestamps for RX and TX (Íñigo Huguet) [2136123]
- wifi: cfg80211: add hardware timestamps to frame RX info (Íñigo Huguet) [2136123]
- wifi: cfg80211/nl80211: move rx management data into a struct (Íñigo Huguet) [2136123]
- wifi: cfg80211: add a function for reporting TX status with hardware timestamps (Íñigo Huguet) [2136123]
- wifi: nl80211: add RX and TX timestamp attributes (Íñigo Huguet) [2136123]
- nl80211: document uapi for CMD_FRAME_WAIT_CANCEL (Íñigo Huguet) [2136123]
- wifi: ieee80211: add helper functions for detecting TM/FTM frames (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: handle links for wmediumd/virtio (Íñigo Huguet) [2136123]
- wifi: mac80211: sta_info: fix link_sta insertion (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: fix link_sta setup (Íñigo Huguet) [2136123]
- wifi: nl80211/mac80211: clarify link ID in control port TX (Íñigo Huguet) [2136123]
- wifi: mac80211: return error from control port TX for drops (Íñigo Huguet) [2136123]
- wifi: nl80211: require MLD address on link STA add/modify (Íñigo Huguet) [2136123]
- wifi: mac80211: more station handling sanity checks (Íñigo Huguet) [2136123]
- wifi: mac80211: fix link sta hash table handling (Íñigo Huguet) [2136123]
- wifi: mac80211: validate link address doesn't change (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: set sta.mlo to mlo state (Íñigo Huguet) [2136123]
- wifi: mac80211: fast-xmit: handle non-MLO clients (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: fix address translation for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: fix RX MLD address translation (Íñigo Huguet) [2136123]
- wifi: mac80211: fix NULL pointer deref with non-MLD STA (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: fix override calculation (Íñigo Huguet) [2136123]
- wifi: mac80211: tx: use AP address in some places for MLO (Íñigo Huguet) [2136123]
- net: add missing includes and forward declarations under net/ (Íñigo Huguet) [2136123]
- wifi: rtl8192se: fix repeated words in comments (Íñigo Huguet) [2136123]
- wifi: rtlwifi: fix repeated words in comments (Íñigo Huguet) [2136123]
- wifi: rt2x00: fix repeated words in comments (Íñigo Huguet) [2136123]
- wifi: brcmsmac: fix repeated words in comments (Íñigo Huguet) [2136123]
- wifi: brcmfmac: fix repeated words in comments (Íñigo Huguet) [2136123]
- wifi: mac80211: do not abuse fq.lock in ieee80211_do_stop() (Íñigo Huguet) [2136123]
- wifi: mt7601u: fix clang -Wformat warning (Íñigo Huguet) [2136123]
- wifi: mt7601u: eeprom: fix clang -Wformat warning (Íñigo Huguet) [2136123]
- wifi: ath: fix repeated words in comments (Íñigo Huguet) [2136123]
- wifi: ath11k: mac: fix long line (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: set sta.mlo correctly (Íñigo Huguet) [2136123]
- wifi: mac80211: remove stray printk (Íñigo Huguet) [2136123]
- wifi: mac80211: support MLO authentication/association with one link (Íñigo Huguet) [2136123]
- wifi: mac80211: add API to parse multi-link element (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: fix TX link selection (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: use MLO link ID for TX (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: do rc update per link (Íñigo Huguet) [2136123]
- wifi: mac80211: do link->MLD address translation on RX (Íñigo Huguet) [2136123]
- wifi: mac80211: select link when transmitting to non-MLO stations (Íñigo Huguet) [2136123]
- wifi: mac80211: fix up link station creation/insertion (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: implement sta_state for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: limit A-MSDU subframes for client too (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: refactor ieee80211_set_associated() (Íñigo Huguet) [2136123]
- wifi: cfg80211: add cfg80211_get_iftype_ext_capa() (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: look up beacon elems only if needed (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: refactor assoc link setup (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: remove address arg to ieee80211_mark_sta_auth() (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: refactor assoc success handling (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: refactor ieee80211_prep_channel() a bit (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: refactor assoc req element building (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: switch some things back to deflink (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: change flags in ieee80211_determine_chantype() (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: shift some code around (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: refactor link station setup (Íñigo Huguet) [2136123]
- wifi: mac80211: move IEEE80211_SDATA_OPERATING_GMODE to link (Íñigo Huguet) [2136123]
- wifi: mac80211: make ieee80211_check_rate_mask() link-aware (Íñigo Huguet) [2136123]
- wifi: mac80211: add multi-link element to AUTH frames (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: clean up supported channels element code (Íñigo Huguet) [2136123]
- wifi: mac80211: release channel context on link stop (Íñigo Huguet) [2136123]
- wifi: mac80211: prohibit DEAUTH_NEED_MGD_TX_PREP in MLO (Íñigo Huguet) [2136123]
- wifi: nl80211: fix some attribute policy entries (Íñigo Huguet) [2136123]
- wifi: nl80211: reject fragmented and non-inheritance elements (Íñigo Huguet) [2136123]
- wifi: nl80211: reject link specific elements on assoc link (Íñigo Huguet) [2136123]
- wifi: cfg80211: set country_elem to NULL (Íñigo Huguet) [2136123]
- wifi: mac80211: remove link_id parameter from link_info_changed() (Íñigo Huguet) [2136123]
- wifi: mac80211: replace link_id with link_conf in switch/(un)assign_vif_chanctx() (Íñigo Huguet) [2136123]
- wifi: nl80211: advertise MLO support (Íñigo Huguet) [2136123]
- wifi: mac80211: Support multi link in ieee80211_recalc_min_chandef() (Íñigo Huguet) [2136123]
- wifi: mac80211: don't check carrier in chanctx code (Íñigo Huguet) [2136123]
- wifi: nl80211: allow link ID in set_wiphy with frequency (Íñigo Huguet) [2136123]
- wifi: mac80211: Allow EAPOL tx from specific link (Íñigo Huguet) [2136123]
- wifi: mac80211: Allow EAPOL frames from link addresses (Íñigo Huguet) [2136123]
- wifi: cfg80211/mac80211: Support control port TX from specific link (Íñigo Huguet) [2136123]
- wifi: nl80211: Support MLD parameters in nl80211_set_station() (Íñigo Huguet) [2136123]
- wifi: nl80211: check MLO support in authenticate (Íñigo Huguet) [2136123]
- wifi: mac80211: add a helper to fragment an element (Íñigo Huguet) [2136123]
- wifi: mac80211: skip rate statistics for MLD STAs (Íñigo Huguet) [2136123]
- wifi: nl80211: set BSS to NULL if IS_ERR() (Íñigo Huguet) [2136123]
- wifi: nl80211: add EML/MLD capabilities to per-iftype capabilities (Íñigo Huguet) [2136123]
- wifi: nl80211: better validate link ID for stations (Íñigo Huguet) [2136123]
- wifi: mac80211: fix link manipulation (Íñigo Huguet) [2136123]
- wifi: mac80211: tighten locking check (Íñigo Huguet) [2136123]
- wifi: cfg80211: clean up links appropriately (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: simplify adding ht/vht/he/eht elements (Íñigo Huguet) [2136123]
- wifi: mac80211: refactor adding custom elements (Íñigo Huguet) [2136123]
- wifi: mac80211: refactor adding rates to assoc request (Íñigo Huguet) [2136123]
- wifi: mac80211: use only channel width in ieee80211_parse_bitrates() (Íñigo Huguet) [2136123]
- wifi: cfg80211: add ieee80211_chanwidth_rate_flags() (Íñigo Huguet) [2136123]
- wifi: mac80211: remove redundant condition (Íñigo Huguet) [2136123]
- wifi: mac80211: don't set link address for station (Íñigo Huguet) [2136123]
- wifi: mac80211: fix multi-BSSID element parsing (Íñigo Huguet) [2136123]
- wifi: mac80211: move tdls_chan_switch_prohibited to link data (Íñigo Huguet) [2136123]
- wifi: mac80211: don't re-parse elems in ieee80211_assoc_success() (Íñigo Huguet) [2136123]
- wifi: mac80211: replace link_id with link_conf in start/stop_ap() (Íñigo Huguet) [2136123]
- wifi: mac80211: refactor elements parsing with parameter struct (Íñigo Huguet) [2136123]
- wifi: cfg80211: extend cfg80211_rx_assoc_resp() for MLO (Íñigo Huguet) [2136123]
- wifi: cfg80211: put cfg80211_rx_assoc_resp() arguments into a struct (Íñigo Huguet) [2136123]
- wifi: cfg80211: adjust assoc comeback for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: unify assoc data event sending (Íñigo Huguet) [2136123]
- wifi: cfg80211: prepare association failure APIs for MLO (Íñigo Huguet) [2136123]
- wifi: cfg80211: remove BSS pointer from cfg80211_disassoc_request (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: use correct link_sta (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: remove sta argument from ieee80211_config_bw (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: use ieee80211_get_link_sband() (Íñigo Huguet) [2136123]
- wifi: mac80211: split IEEE80211_STA_DISABLE_WMM to link data (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: first adjustments for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: do IEEE80211_STA_RESET_SIGNAL_AVE per link (Íñigo Huguet) [2136123]
- wifi: mac80211: mlme: track AP (MLD) address separately (Íñigo Huguet) [2136123]
- wifi: mac80211: remove unused bssid variable (Íñigo Huguet) [2136123]
- wifi: mac80211: change QoS settings API to take link into account (Íñigo Huguet) [2136123]
- wifi: mac80211: expect powersave handling in driver for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: move ps setting to vif config (Íñigo Huguet) [2136123]
- wifi: mac80211: provide link ID in link_conf (Íñigo Huguet) [2136123]
- wifi: mac80211: set up/tear down client vif links properly (Íñigo Huguet) [2136123]
- wifi: mac80211: move ieee80211_request_smps_mgd_work (Íñigo Huguet) [2136123]
- wifi: nl80211: acquire wdev mutex for dump_survey (Íñigo Huguet) [2136123]
- wifi: mac80211: fix key lookup (Íñigo Huguet) [2136123]
- wifi: mac80211: separate out connection downgrade flags (Íñigo Huguet) [2136123]
- wifi: mac80211: Align with Draft P802.11be_D2.0 (Íñigo Huguet) [2136123]
- wifi: mac80211: Align with Draft P802.11be_D1.5 (Íñigo Huguet) [2136123]
- wifi: mac80211: skip powersave recalc if driver SUPPORTS_DYNAMIC_PS (Íñigo Huguet) [2136123]
- wifi: mac80211: debug: omit link if non-MLO connection (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: Ack link addressed frames (Íñigo Huguet) [2136123]
- wifi: cfg80211: drop BSS elements from assoc trace for now (Íñigo Huguet) [2136123]
- wifi: cfg80211: make cfg80211_auth_request::key_idx signed (Íñigo Huguet) [2136123]
- wifi: nl80211: enable setting the link address at new station (Íñigo Huguet) [2136123]
- wifi: mac80211: RCU-ify link/link_conf pointers (Íñigo Huguet) [2136123]
- wifi: nl80211: hold wdev mutex for station APIs (Íñigo Huguet) [2136123]
- wifi: nl80211: hold wdev mutex for channel switch APIs (Íñigo Huguet) [2136123]
- wifi: nl80211: hold wdev mutex in add/mod/del link station (Íñigo Huguet) [2136123]
- wifi: mac80211: implement callbacks for <add/mod/del>_link_station (Íñigo Huguet) [2136123]
- wifi: cfg80211/mac80211: separate link params from station params (Íñigo Huguet) [2136123]
- wifi: cfg80211: add API to add/modify/remove a link station (Íñigo Huguet) [2136123]
- wifi: mac80211: add an ieee80211_get_link_sband (Íñigo Huguet) [2136123]
- wifi: mac80211: Remove AP SMPS leftovers (Íñigo Huguet) [2136123]
- wifi: cfg80211: Allow MLO TX with link source address (Íñigo Huguet) [2136123]
- wifi: mac80211: Consider MLO links in offchannel logic (Íñigo Huguet) [2136123]
- wifi: mac80211: rx: accept link-addressed frames (Íñigo Huguet) [2136123]
- wifi: mac80211: consistently use sdata_dereference() (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: Support link channel matching on rx (Íñigo Huguet) [2136123]
- wifi: mac80211: fix mesh airtime link metric estimating (Íñigo Huguet) [2136123]
- wifi: mac80211: make 4addr null frames using min_rate for WDS (Íñigo Huguet) [2136123]
- wifi: cfg80211: use strscpy to replace strlcpy (Íñigo Huguet) [2136123]
- wifi: mac80211: exclude multicast packets from AQL pending airtime (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: use 32-bit skb cookie (Íñigo Huguet) [2136123]
- mt76: mt7921: Let PCI core handle power state and use pm_sleep_ptr() (Íñigo Huguet) [2136123]
- mediatek: mt76: mac80211: Fix missing of_node_put() in mt76_led_init() (Íñigo Huguet) [2136123]
- mt76: get rid of mt76_wcid_hw routine (Íñigo Huguet) [2136123]
- mt76: convert MT_TX_HW_QUEUE_EXT_PHY to MT_TX_HW_QUEUE_PHY (Íñigo Huguet) [2136123]
- mt76: add phy_idx to mt76_wcid (Íñigo Huguet) [2136123]
- mt76: introduce phys array in mt76_dev structure (Íñigo Huguet) [2136123]
- mt76: add phy_idx in mt76_rx_status (Íñigo Huguet) [2136123]
- mt76: introduce MT_RXQ_BAND2 and MT_RXQ_BAND2_WA in mt76_rxq_id (Íñigo Huguet) [2136123]
- mt76: add len parameter to __mt76_mcu_msg_alloc signature (Íñigo Huguet) [2136123]
- mt76: mt7915 add ht mpdu density (Íñigo Huguet) [2136123]
- mt76: mt7921: reduce the mutex lock scope during reset (Íñigo Huguet) [2136123]
- mt76: mt7921: reduce log severity levels for informative messages (Íñigo Huguet) [2136123]
- mt76: connac: move tx initialization/cleanup in mt76_connac module (Íñigo Huguet) [2136123]
- mt76: mt7921: make mt7921_pci_driver static (Íñigo Huguet) [2136123]
- mt76: mt7921: enable HW beacon filter in the initialization stage (Íñigo Huguet) [2136123]
- mt76: mt7921: enable HW beacon filter not depending on PM flag (Íñigo Huguet) [2136123]
- mt76: remove q->qid (Íñigo Huguet) [2136123]
- mt76: do not use skb_set_queue_mapping for internal purposes (Íñigo Huguet) [2136123]
- mt76: pass original queue id from __mt76_tx_queue_skb to the driver (Íñigo Huguet) [2136123]
- mt76: allow receiving frames with invalid CCMP PN via monitor interfaces (Íñigo Huguet) [2136123]
- mt76: mt76x02: improve reliability of the beacon hang check (Íñigo Huguet) [2136123]
- mt76: mt7615: add sta_rec with EXTRA_INFO_NEW for the first time only (Íñigo Huguet) [2136123]
- mt76: mt7915: update the maximum size of beacon offload (Íñigo Huguet) [2136123]
- mt76: do not check the ccmp pn for ONLY_MONITOR frame (Íñigo Huguet) [2136123]
- mt76: mt7915: add sta_rec with EXTRA_INFO_NEW for the first time only (Íñigo Huguet) [2136123]
- mt76: mt7915: update mpdu density in 6g capability (Íñigo Huguet) [2136123]
- mt76: mt7915: do not copy ieee80211_ops pointer in mt7915_mmio_probe (Íñigo Huguet) [2136123]
- mt76: mt7915: disable UL MU-MIMO for mt7915 (Íñigo Huguet) [2136123]
- mt76: move mt76_connac2_mcu_fill_message in mt76_connac module (Íñigo Huguet) [2136123]
- mt76: move mcu_txd/mcu_rxd structures in shared code (Íñigo Huguet) [2136123]
- mt76: mt7915: rely on mt76_connac_tx_free (Íñigo Huguet) [2136123]
- mt76: connac: move mt7615_txp_skb_unmap in common code (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac_write_hw_txp in shared code (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac_tx_complete_skb in shared code (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac_tx_free in shared code (Íñigo Huguet) [2136123]
- mt76: move mt7615_txp_ptr in mt76_connac module (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac_fw_txp in common module (Íñigo Huguet) [2136123]
- mt76: mt7915: get rid of unnecessary new line in mt7915_mac_write_txwi (Íñigo Huguet) [2136123]
- mt76: mt7921s: remove unnecessary goto in mt7921s_mcu_drv_pmctrl (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac2_mac_fill_rx_rate in connac module (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac2_reverse_frag0_hdr_trans in mt76-connac module (Íñigo Huguet) [2136123]
- mt76: connac: move HE radiotap parsing in connac module (Íñigo Huguet) [2136123]
- mt76: mt7921: fix command timeout in AP stop period (Íñigo Huguet) [2136123]
- mt76: mt7921: not support beacon offload disable command (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac2_mac_add_txs_skb in connac module (Íñigo Huguet) [2136123]
- mt76: connac: move connac2_mac_write_txwi in mt76_connac module (Íñigo Huguet) [2136123]
- mt76: connac: move mac connac2 defs in mt76_connac2_mac.h (Íñigo Huguet) [2136123]
- mt76: mt7915: rely on mt76_dev in mt7915_mac_write_txwi signature (Íñigo Huguet) [2136123]
- mt76: mt7921: rely on mt76_dev in mt7921_mac_write_txwi signature (Íñigo Huguet) [2136123]
- mt76: enable the VHT extended NSS BW feature (Íñigo Huguet) [2136123]
- mt76: mt7663: rely on mt76_connac2_fw_trailer (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac2_load_patch in connac module (Íñigo Huguet) [2136123]
- mt76: connac: move mt76_connac2_load_ram in connac module (Íñigo Huguet) [2136123]
- mt76: mt7921: move fw toggle in mt7921_load_firmware (Íñigo Huguet) [2136123]
- mt76: connac: move shared fw structures in connac module (Íñigo Huguet) [2136123]
- mt76: mt7921: get rid of mt7921_mcu_exit (Íñigo Huguet) [2136123]
- mt76: mt7921: add missing bh-disable around rx napi schedule (Íñigo Huguet) [2136123]
- mt76: mt7615: add missing bh-disable around rx napi schedule (Íñigo Huguet) [2136123]
- mt76: mt7915: add missing bh-disable around tx napi enable/schedule (Íñigo Huguet) [2136123]
- mt76: mt7921: add PATCH_FINISH_REQ cmd response handling (Íñigo Huguet) [2136123]
- mt76: add DBDC rxq handlings into mac_reset_work (Íñigo Huguet) [2136123]
- mt76: mt7915: add more ethtool stats (Íñigo Huguet) [2136123]
- mt76: mt7921: introduce ACPI SAR config in tx power (Íñigo Huguet) [2136123]
- mt76: mt7921: introduce ACPI SAR support (Íñigo Huguet) [2136123]
- mt76: add 6 GHz band support in mt76_sar_freq_ranges (Íñigo Huguet) [2136123]
- mt76: mt7915: fix endian bug in mt7915_rf_regval_set() (Íñigo Huguet) [2136123]
- mt76: mt76x02u: fix possible memory leak in __mt76x02u_mcu_send_msg (Íñigo Huguet) [2136123]
- mt76: mt7915: fix endianness in mt7915_rf_regval_get (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: add back erroneously removed cast (Íñigo Huguet) [2136123]
- wifi: mac80211: fix queue selection for mesh/OCB interfaces (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: fix race condition in pending packet (Íñigo Huguet) [2136123]
- wifi: mac80211: Use the bitmap API to allocate bitmaps (Íñigo Huguet) [2136123]
- wifi: mac80211: fix center freq calculation in ieee80211_chandef_downgrade (Íñigo Huguet) [2136123]
- wifi: nl80211: fix sending link ID info of associated BSS (Íñigo Huguet) [2136123]
- wifi: cfg80211: fix a comment in cfg80211_mlme_mgmt_tx() (Íñigo Huguet) [2136123]
- wifi: nl80211: Fix reading NL80211_ATTR_MLO_LINK_ID in nl80211_pre_doit (Íñigo Huguet) [2136123]
- bus: mhi: ep: Check dev_set_name() return value (Íñigo Huguet) [2136123]
- ath9k: remove unexpected words "the" in comments (Íñigo Huguet) [2136123]
- ath11k: Fix typo in comments (Íñigo Huguet) [2136123]
- wifi: nl80211: retrieve EHT related elements in AP mode (Íñigo Huguet) [2136123]
- wifi: cfg80211: Increase akm_suites array size in cfg80211_crypto_settings (Íñigo Huguet) [2136123]
- wifi: cfg80211: remove chandef check in cfg80211_cac_event() (Íñigo Huguet) [2136123]
- wifi: nl80211: relax wdev mutex check in wdev_chandef() (Íñigo Huguet) [2136123]
- wifi: nl80211: acquire wdev mutex earlier in start_ap (Íñigo Huguet) [2136123]
- wifi: nl80211: hold wdev mutex for tid config (Íñigo Huguet) [2136123]
- wifi: cfg80211: handle IBSS in channel switch (Íñigo Huguet) [2136123]
- wifi: mac80211: properly skip link info driver update (Íñigo Huguet) [2136123]
- wifi: mac80211: only accumulate airtime deficit for active clients (Íñigo Huguet) [2136123]
- wifi: mac80211: add debugfs file to display per-phy AQL pending airtime (Íñigo Huguet) [2136123]
- wifi: mac80211: add a per-PHY AQL limit to improve fairness (Íñigo Huguet) [2136123]
- wifi: mac80211: keep recently active tx queues in scheduling list (Íñigo Huguet) [2136123]
- wifi: mac80211: consider aql_tx_pending when checking airtime deficit (Íñigo Huguet) [2136123]
- wifi: mac80211: make sta airtime deficit field s32 instead of s64 (Íñigo Huguet) [2136123]
- wifi: mac80211: fix a kernel-doc complaint (Íñigo Huguet) [2136123]
- wifi: cfg80211: remove redundant documentation (Íñigo Huguet) [2136123]
- wifi: mac80211: sta_info: fix a missing kernel-doc struct element (Íñigo Huguet) [2136123]
- wifi: mac80211: add a missing comma at kernel-doc markup (Íñigo Huguet) [2136123]
- wifi: cfg80211: fix kernel-doc warnings all over the file (Íñigo Huguet) [2136123]
- wifi: ieee80211: s1g action frames are not robust (Íñigo Huguet) [2136123]
- bus: mhi: host: pci_generic: Add another Foxconn T99W175 (Íñigo Huguet) [2136123]
- wifi: cfg80211: Allow P2P client interface to indicate port authorization (Íñigo Huguet) [2136123]
- wifi: mac80211: do not wake queues on a vif that is being stopped (Íñigo Huguet) [2136123]
- wifi: mac80211: check skb_shared in ieee80211_8023_xmit() (Íñigo Huguet) [2136123]
- wifi: mac80211: add gfp_t parameter to ieeee80211_obss_color_collision_notify (Íñigo Huguet) [2136123]
- bus: mhi: host: Move IRQ allocation to controller registration phase (Íñigo Huguet) [2136123]
- bus: mhi: host: pci_generic: Add Cinterion MV31-W with new baseline (Íñigo Huguet) [2136123]
- bus: mhi: host: pci_generic: Add support for Quectel EM120 FCCL modem (Íñigo Huguet) [2136123]
- wifi: rtw89: disable invalid phy reports for all ICs (Íñigo Huguet) [2136123]
- wifi: rtw89: pci: fix PCI doesn't reclaim TX BD properly (Íñigo Huguet) [2136123]
- wifi: rtw89: fix long RX latency in low power mode (Íñigo Huguet) [2136123]
- wifi: rtw89: drop invalid TX rate report of legacy rate (Íñigo Huguet) [2136123]
- wifi: rtw89: add UNEXP debug mask to keep monitor messages unexpected to happen frequently (Íñigo Huguet) [2136123]
- wifi: rtw89: enable VO TX AMPDU (Íñigo Huguet) [2136123]
- wifi: rtw89: fix potential TX stuck (Íñigo Huguet) [2136123]
- wifi: rtw89: support TDLS (Íñigo Huguet) [2136123]
- wifi: rtw89: allocate BSSID CAM per TDLS peer (Íñigo Huguet) [2136123]
- wifi: rtw89: separate BSSID CAM operations (Íñigo Huguet) [2136123]
- wifi: rtw89: allocate address CAM and MAC ID to TDLS peer (Íñigo Huguet) [2136123]
- cfg80211: Indicate MLO connection info in connect and roam callbacks (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: print the link id (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: support creating MLO-capable radios (Íñigo Huguet) [2136123]
- wifi: nl80211: expose link ID for associated BSSes (Íñigo Huguet) [2136123]
- wifi: nl80211: expose link information for interfaces (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: send a beacon per link (Íñigo Huguet) [2136123]
- wifi: mac80211: set STA deflink addresses (Íñigo Huguet) [2136123]
- wifi: mac80211: maintain link-sta hash table (Íñigo Huguet) [2136123]
- wifi: mac80211: RCU-ify link STA pointers (Íñigo Huguet) [2136123]
- wifi: mac80211: ethtool: use deflink for now (Íñigo Huguet) [2136123]
- wifi: mac80211: move ieee80211_bssid_match() function (Íñigo Huguet) [2136123]
- wifi: mac80211: return a beacon for a specific link (Íñigo Huguet) [2136123]
- wifi: mac80211: pass the link id in start/stop ap (Íñigo Huguet) [2136123]
- wifi: mac80211: use link in start/stop ap (Íñigo Huguet) [2136123]
- wifi: mac80211: implement add/del interface link callbacks (Íñigo Huguet) [2136123]
- wifi: cfg80211: add optional link add/remove callbacks (Íñigo Huguet) [2136123]
- wifi: cfg80211: sort trace.h (Íñigo Huguet) [2136123]
- wifi: mac80211: add sta link addition/removal (Íñigo Huguet) [2136123]
- wifi: mac80211: add MLO link ID to TX frame metadata (Íñigo Huguet) [2136123]
- wifi: mac80211: remove band from TX info in MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: add vif link addition/removal (Íñigo Huguet) [2136123]
- wifi: nl80211: support MLO in auth/assoc (Íñigo Huguet) [2136123]
- wifi: mac80211: ignore IEEE80211_CONF_CHANGE_SMPS in chanctx mode (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: split bss_info_changed to vif/link info_changed (Íñigo Huguet) [2136123]
- wifi: cfg80211: simplify cfg80211_mlme_auth() prototype (Íñigo Huguet) [2136123]
- wifi: ieee80211: add definitions for multi-link element (Íñigo Huguet) [2136123]
- wifi: nl80211: refactor BSS lookup in nl80211_associate() (Íñigo Huguet) [2136123]
- wifi: cfg80211: mlme: get BSS entry outside cfg80211_mlme_assoc() (Íñigo Huguet) [2136123]
- wifi: mac80211: tx: simplify chanctx_conf handling (Íñigo Huguet) [2136123]
- wifi: mac80211: status: look up band only where needed (Íñigo Huguet) [2136123]
- wifi: mac80211: sort trace.h file (Íñigo Huguet) [2136123]
- wifi: mac80211: correct link config data in tracing (Íñigo Huguet) [2136123]
- wifi: mac80211: make ieee80211_he_cap_ie_to_sta_he_cap() MLO-aware (Íñigo Huguet) [2136123]
- wifi: mac80211: make some SMPS code MLD-aware (Íñigo Huguet) [2136123]
- wifi: mac80211: HT: make ieee80211_ht_cap_ie_to_sta_ht_cap() MLO-aware (Íñigo Huguet) [2136123]
- wifi: mac80211: add link_id to eht.c code for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: add link_id to vht.c code for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: refactor some link setup code (Íñigo Huguet) [2136123]
- wifi: mac80211: validate some driver features for MLO (Íñigo Huguet) [2136123]
- wifi: mac80211: use IEEE80211_MLD_MAX_NUM_LINKS (Íñigo Huguet) [2136123]
- wifi: mac80211: refactor some sta_info link handling (Íñigo Huguet) [2136123]
- wifi: mac80211: remove sta_info_tx_streams() (Íñigo Huguet) [2136123]
- wifi: mac80211: make channel context code MLO-aware (Íñigo Huguet) [2136123]
- wifi: mac80211: pass link ID where already present (Íñigo Huguet) [2136123]
- wifi: mac80211: add per-link configuration pointer (Íñigo Huguet) [2136123]
- wifi: mac80211: split bss_info_changed method (Íñigo Huguet) [2136123]
- mac80211: fix maybe-unused warning (Íñigo Huguet) [2136123]
- wifi: mac80211: reorg some iface data structs for MLD (Íñigo Huguet) [2136123]
- wifi: mac80211: move interface config to new struct (Íñigo Huguet) [2136123]
- wifi: mac80211: move some future per-link data to bss_conf (Íñigo Huguet) [2136123]
- wifi: cfg80211: do some rework towards MLO link APIs (Íñigo Huguet) [2136123]
- wifi: mac80211: reject WEP or pairwise keys with key ID > 3 (Íñigo Huguet) [2136123]
- wifi: mac80211_hwsim: Directly use ida_alloc()/free() (Íñigo Huguet) [2136123]
- wifi: mac80211: refactor some key code (Íñigo Huguet) [2136123]
- wifi: mac80211: remove cipher scheme support (Íñigo Huguet) [2136123]
- wifi: nl80211: fix typo in comment (Íñigo Huguet) [2136123]
- treewide: Replace GPLv2 boilerplate/reference with SPDX - gpl-2.0_391.RULE (Íñigo Huguet) [2136123]
- rtw88: 8821c: fix access const table of channel parameters (Íñigo Huguet) [2136123]
- rtw89: add new state to CFO state machine for UL-OFDMA (Íñigo Huguet) [2136123]
- rtw89: 8852c: add trigger frame counter (Íñigo Huguet) [2136123]
- ieee80211: add trigger frame definition (Íñigo Huguet) [2136123]
- ath10k: fix recently introduced checkpatch warning (Íñigo Huguet) [2136123]
- wifi: rtw89: support MULTI_BSSID and correct BSSID mask of H2C (Íñigo Huguet) [2136123]
- wifi: ray_cs: Drop useless status variable in parse_addr() (Íñigo Huguet) [2136123]
- wifi: ray_cs: Utilize strnlen() in parse_addr() (Íñigo Huguet) [2136123]
- wifi: rtw88: use *ph to print small buffer (Íñigo Huguet) [2136123]
- ath11k: Fix warnings reported by checkpatch (Íñigo Huguet) [2136123]
- ath11k: Fix LDPC config in set_bitrate_mask hook (Íñigo Huguet) [2136123]
- wifi: mac80211: fix use-after-free in chanctx code (Íñigo Huguet) [2136123]
- ath10k: fix regdomain info of iw reg set/get (Íñigo Huguet) [2136123]
- ath11k: support avg signal in station dump (Íñigo Huguet) [2136123]
- wifi: rtlwifi: fix error codes in rtl_debugfs_set_write_h2c() (Íñigo Huguet) [2136123]
- wifi: rtw88: Fix Sparse warning for rtw8821c_hw_spec (Íñigo Huguet) [2136123]
- wifi: rtw88: Fix Sparse warning for rtw8723d_hw_spec (Íñigo Huguet) [2136123]
- wifi: rtw88: Fix Sparse warning for rtw8822c_hw_spec (Íñigo Huguet) [2136123]
- wifi: rtw88: Fix sparse warning for rtw8822b_hw_spec (Íñigo Huguet) [2136123]
- rtw88: fix null vif pointer when hw_scan fails (Íñigo Huguet) [2136123]
- rtw89: sar: adjust and support SAR on 6GHz band (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: re-calibrate RX DCK once thermal changes a lot (Íñigo Huguet) [2136123]
- rtw89: pci: handle hardware watchdog timeout interrupt status (Íñigo Huguet) [2136123]
- rtw89: fix null vif pointer when hw_scan fails (Íñigo Huguet) [2136123]
- rtw89: fix channel inconsistency during hw_scan (Íñigo Huguet) [2136123]
- wifi: rtw88: add a work to correct atomic scheduling warning of ::set_tim (Íñigo Huguet) [2136123]
- wifi: iwlwifi: pcie: rename CAUSE macro (Íñigo Huguet) [2136123]
- wifi: brcmfmac: work around a GCC 12 -Warray-bounds warning (Íñigo Huguet) [2136123]
- wifi: iwlwifi: use unsigned to silence a GCC 12 warning (Íñigo Huguet) [2136123]
- wifi: rtlwifi: remove always-true condition pointed out by GCC 12 (Íñigo Huguet) [2136123]
- wifi: ath9k: silence array-bounds warning on GCC 12 (Íñigo Huguet) [2136123]
- ath9k: replace ternary operator with max() (Íñigo Huguet) [2136123]
- ath11k: Init hw_params before setting up AHB resources (Íñigo Huguet) [2136123]
- ath11k: Fix warning on variable 'sar' dereference before check (Íñigo Huguet) [2136123]
- ath10k: fix misreported tx bandwidth for 160Mhz (Íñigo Huguet) [2136123]
- ath10k: add encapsulation offloading support (Íñigo Huguet) [2136123]
- ath10k: turn rawmode into frame_mode (Íñigo Huguet) [2136123]
- ath10k: improve tx status reporting (Íñigo Huguet) [2136123]
- ath10k: do not enforce interrupt trigger type (Íñigo Huguet) [2136123]
- iwlwifi: mei: fix potential NULL-ptr deref (Íñigo Huguet) [2136123]
- iwlwifi: mei: clear the sap data header before sending (Íñigo Huguet) [2136123]
- iwlwifi: mvm: remove vif_count (Íñigo Huguet) [2136123]
- iwlwifi: mvm: always tell the firmware to accept MCAST frames in BSS (Íñigo Huguet) [2136123]
- iwlwifi: mvm: add OTP info in case of init failure (Íñigo Huguet) [2136123]
- iwlwifi: mvm: fix assert 1F04 upon reconfig (Íñigo Huguet) [2136123]
- iwlwifi: mvm: clean up authorized condition (Íñigo Huguet) [2136123]
- iwlwifi: mvm: use NULL instead of ERR_PTR when parsing wowlan status (Íñigo Huguet) [2136123]
- iwlwifi: pcie: simplify MSI-X cause mapping (Íñigo Huguet) [2136123]
- ath11k: update missing MU-MIMO and OFDMA stats (Íñigo Huguet) [2136123]
- rtw89: pci: only mask out INT indicator register for disable interrupt v1 (Íñigo Huguet) [2136123]
- rtw89: convert rtw89_band to nl80211_band precisely (Íñigo Huguet) [2136123]
- rtw89: 8852c: update txpwr tables to HALRF_027_00_052 (Íñigo Huguet) [2136123]
- rtw89: cfo: check mac_id to avoid out-of-bounds (Íñigo Huguet) [2136123]
- rtw89: 8852c: set TX antenna path (Íñigo Huguet) [2136123]
- rtw89: add ieee80211::sta_rc_update ops (Íñigo Huguet) [2136123]
- wireless: Fix Makefile to be in alphabetical order (Íñigo Huguet) [2136123]
- mac80211: refactor freeing the next_beacon (Íñigo Huguet) [2136123]
- cfg80211: fix kernel-doc for cfg80211_beacon_data (Íñigo Huguet) [2136123]
- mac80211: minstrel_ht: support ieee80211_rate_status (Íñigo Huguet) [2136123]
- mac80211: extend current rate control tx status API (Íñigo Huguet) [2136123]
- mac80211: minstrel_ht: fill all requested rates (Íñigo Huguet) [2136123]
- mac80211: disable BSS color collision detection in case of no free colors (Íñigo Huguet) [2136123]
- nl80211: Parse NL80211_ATTR_HE_BSS_COLOR as a part of nl80211_parse_beacon (Íñigo Huguet) [2136123]
- mac80211: mlme: track assoc_bss/associated separately (Íñigo Huguet) [2136123]
- mac80211: remove useless bssid copy (Íñigo Huguet) [2136123]
- mac80211: remove unused argument to ieee80211_sta_connection_lost() (Íñigo Huguet) [2136123]
- mac80211: mlme: use local SSID copy (Íñigo Huguet) [2136123]
- mac80211: use ifmgd->bssid instead of ifmgd->associated->bssid (Íñigo Huguet) [2136123]
- mac80211: mlme: move in RSSI reporting code (Íñigo Huguet) [2136123]
- mac80211: remove stray multi_sta_back_32bit docs (Íñigo Huguet) [2136123]
- mac80211: fix typo in documentation (Íñigo Huguet) [2136123]
- mac80211: unify CCMP/GCMP AAD construction (Íñigo Huguet) [2136123]
- mt76: mt7921: add ipv6 NS offload support (Íñigo Huguet) [2136123]
- mt76: add gfp to mt76_mcu_msg_alloc signature (Íñigo Huguet) [2136123]
- mt76: mt7915: add more statistics from fw_util debugfs knobs (Íñigo Huguet) [2136123]
- mt76: mt7915: improve error handling for fw_debug knobs (Íñigo Huguet) [2136123]
- mt76: mt7615/mt7915: do reset_work with mt76's work queue (Íñigo Huguet) [2136123]
- mt76: mt7915: add support for 6G in-band discovery (Íñigo Huguet) [2136123]
- mt76: mt7915: add Wireless Ethernet Dispatch support (Íñigo Huguet) [2136123]
- net: ethernet: mtk_eth_soc: add support for Wireless Ethernet Dispatch (WED) (Íñigo Huguet) [2136123]
- mt76: make number of tokens configurable dynamically (Íñigo Huguet) [2136123]
- mt76: add support for overriding the device used for DMA mapping (Íñigo Huguet) [2136123]
- mt76: dma: add wrapper macro for accessing queue registers (Íñigo Huguet) [2136123]
- mt76: mt7915: move MT_INT_MASK_CSR to init.c (Íñigo Huguet) [2136123]
- mt76: mt7915: introduce mt7915_mac_severe_check() (Íñigo Huguet) [2136123]
- mt76: mt7915: rework SER debugfs knob (Íñigo Huguet) [2136123]
- mt76: mt7915: limit minimum twt duration (Íñigo Huguet) [2136123]
- mt76: mt7915: reject duplicated twt flows (Íñigo Huguet) [2136123]
- mt76: mt7915: update mt7986 patch in mt7986_wmac_adie_patch_7976() (Íñigo Huguet) [2136123]
- mt76: connac: use skb_put_data instead of open coding (Íñigo Huguet) [2136123]
- mt76: mt7915: configure soc clocks in mt7986_wmac_init (Íñigo Huguet) [2136123]
- mt76: fix encap offload ethernet type check (Íñigo Huguet) [2136123]
- mt76: mt7915: disable RX_HDR_TRANS_SHORT (Íñigo Huguet) [2136123]
- mt76: mt7603: move spin_lock_bh() to spin_lock() (Íñigo Huguet) [2136123]
- mt76: mt7915: add debugfs knob for RF registers read/write (Íñigo Huguet) [2136123]
- mt76: mt7921: make read-only array ppet16_ppet8_ru3_ru0 static const (Íñigo Huguet) [2136123]
- mt76: mt7915: make read-only array ppet16_ppet8_ru3_ru0 static const (Íñigo Huguet) [2136123]
- mt76: mt7915: remove SCS feature (Íñigo Huguet) [2136123]
- mt76: fix rx reordering with non explicit / psmp ack policy (Íñigo Huguet) [2136123]
- mt76: mt7921: Add AP mode support (Íñigo Huguet) [2136123]
- mt76: mt7915: use 0xff to initialize bitrate_mask in mt7915_init_bitrate_mask (Íñigo Huguet) [2136123]
- mt76: mt7915: always call mt7915_wfsys_reset() during init (Íñigo Huguet) [2136123]
- mt76: mt7921: rely on mt76_dev rxfilter in mt7921_configure_filter (Íñigo Huguet) [2136123]
- mt76: mt7921u: add suspend/resume support (Íñigo Huguet) [2136123]
- mt76: fix MBSS index condition in DBDC mode (Íñigo Huguet) [2136123]
- mt76: fix use-after-free by removing a non-RCU wcid pointer (Íñigo Huguet) [2136123]
- mt76: mt7921: accept rx frames with non-standard VHT MCS10-11 (Íñigo Huguet) [2136123]
- mt76: mt7915: accept rx frames with non-standard VHT MCS10-11 (Íñigo Huguet) [2136123]
- mt76: dma: use kzalloc instead of devm_kzalloc for txwi (Íñigo Huguet) [2136123]
- mt76: reduce tx queue lock hold time (Íñigo Huguet) [2136123]
- mt76: mt7915: rework hardware/phy initialization (Íñigo Huguet) [2136123]
- rtlwifi: Use pr_warn instead of WARN_ONCE (Íñigo Huguet) [2136123]
- rtw89: add debug entry to dump BSSID CAM (Íñigo Huguet) [2136123]
- rtw89: add debug select to dump MAC pages 0x30 to 0x33 (Íñigo Huguet) [2136123]
- rtw89: correct CCA control (Íñigo Huguet) [2136123]
- rtw89: correct setting of RX MPDU length (Íñigo Huguet) [2136123]
- rtw89: 8852c: add settings to decrease the effect of DC (Íñigo Huguet) [2136123]
- brcmfmac: allow setting wlan MAC address using device tree (Íñigo Huguet) [2136123]
- ath11k: remove redundant assignment to variables vht_mcs and he_mcs (Íñigo Huguet) [2136123]
- ath11k: Reuse the available memory after firmware reload (Íñigo Huguet) [2136123]
- ath11k: Designating channel frequency when sending management frames (Íñigo Huguet) [2136123]
- ath11k: Implement remain-on-channel support (Íñigo Huguet) [2136123]
- ath11k: Handle keepalive during WoWLAN suspend and resume (Íñigo Huguet) [2136123]
- bus: mhi: host: Add support for Foxconn T99W373 and T99W368 (Íñigo Huguet) [2136123]
- bus: mhi: host: pci_generic: add Telit FN990 (Íñigo Huguet) [2136123]
- bus: mhi: host: pci_generic: add Telit FN980 v1 hardware revision (Íñigo Huguet) [2136123]
- bus: mhi: replace snprintf with sysfs_emit (Íñigo Huguet) [2136123]
- rtw88: adjust adaptivity option to 1 (Íñigo Huguet) [2136123]
- ath11k: Fix RX de-fragmentation issue on WCN6750 (Íñigo Huguet) [2136123]
- ath10k: support bus and device specific API 1 BDF selection (Íñigo Huguet) [2136123]
- ath10k: mac: fix too long lines (Íñigo Huguet) [2136123]
- ath11k: mac: fix too long line (Íñigo Huguet) [2136123]
- mac80211: support disabling EHT mode (Íñigo Huguet) [2136123]
- cfg80211: support disabling EHT mode (Íñigo Huguet) [2136123]
- mac80211: upgrade passive scan to active scan on DFS channels after beacon rx (Íñigo Huguet) [2136123]
- mac80211: tx: delete a redundant if statement in ieee80211_check_fast_xmit() (Íñigo Huguet) [2136123]
- mac80211: consider Order bit to fill CCMP AAD (Íñigo Huguet) [2136123]
- cfg80211: declare MODULE_FIRMWARE for regulatory.db (Íñigo Huguet) [2136123]
- nl80211: rework internal_flags usage (Íñigo Huguet) [2136123]
- nl80211: don't hold RTNL in color change request (Íñigo Huguet) [2136123]
- cfg80211: remove cfg80211_get_chan_state() (Íñigo Huguet) [2136123]
- ath11k: Add support for targets without trustzone (Íñigo Huguet) [2136123]
- rtw89: 8852c: add 8852ce to Makefile and Kconfig (Íñigo Huguet) [2136123]
- rtw89: 8852c: fix warning of FIELD_PREP() mask type (Íñigo Huguet) [2136123]
- rtw89: 8852c: correct register definitions used by 8852c (Íñigo Huguet) [2136123]
- rtw89: correct AID settings of beamformee (Íñigo Huguet) [2136123]
- rtw89: ps: fine tune polling interval while changing low power mode (Íñigo Huguet) [2136123]
- rtw89: 8852c: add basic and remaining chip_info (Íñigo Huguet) [2136123]
- rtw89: 8852c: add chip_ops::bb_ctrl_btc_preagc (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: get calibrated channels to notify firmware (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add DPK (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add IQK (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add RX DCK (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add RCK (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add TSSI (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add LCK (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add DACK (Íñigo Huguet) [2136123]
- rtw89: 8852c: rfk: add RFK tables (Íñigo Huguet) [2136123]
- rtw88: remove a copy of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2136123]
- ath10k: remove a copy of the NAPI_POLL_WEIGHT define (Íñigo Huguet) [2136123]
- ath11k: Add support for WCN6750 device (Íñigo Huguet) [2136123]
- ath11k: Datapath changes to support WCN6750 (Íñigo Huguet) [2136123]
- ath11k: HAL changes to support WCN6750 (Íñigo Huguet) [2136123]
- ath11k: Add QMI changes for WCN6750 (Íñigo Huguet) [2136123]
- ath11k: Fetch device information via QMI for WCN6750 (Íñigo Huguet) [2136123]
- ath11k: Add register access logic for WCN6750 (Íñigo Huguet) [2136123]
- ath11k: Add HW params for WCN6750 (Íñigo Huguet) [2136123]
- ath11k: Move parameters in bus_params to hw_params (Íñigo Huguet) [2136123]
- ath11k: change management tx queue to avoid connection timed out (Íñigo Huguet) [2136123]
- ath11k: fix warning of not found station for bssid in message (Íñigo Huguet) [2136123]
- rtw88: fix hw scan may cause disconnect issue (Íñigo Huguet) [2136123]
- rtw88: fix not disabling beacon filter after disconnection (Íñigo Huguet) [2136123]
- rtw88: add HT MPDU density value for each chip (Íñigo Huguet) [2136123]
- ath11k: Don't use GFP_KERNEL in atomic context (Íñigo Huguet) [2136123]
- ath10k: skip ath10k_halt during suspend for driver state RESTARTING (Íñigo Huguet) [2136123]
- rtw89: remove unneeded semicolon (Íñigo Huguet) [2136123]
- ath10k: simplify if-if to if-else (Íñigo Huguet) [2136123]
- ath11k: read country code from SMBIOS for WCN6855/QCA6390 (Íñigo Huguet) [2136123]
- ath11k: disable spectral scan during spectral deinit (Íñigo Huguet) [2136123]
- ath11k: Update WBM idle ring HP after FW mode on (Íñigo Huguet) [2136123]
- ath11k: WMI changes to support WCN6750 (Íñigo Huguet) [2136123]
- ath11k: Do not put HW in DBS mode for WCN6750 (Íñigo Huguet) [2136123]
- rtlwifi: btcoex: fix if == else warning (Íñigo Huguet) [2136123]
- rtw88: use the correct bit in the REG_HCI_OPT_CTRL register (Íñigo Huguet) [2136123]
- mwifiex: Add SD8997 SDIO-UART firmware (Íñigo Huguet) [2136123]
- mwifiex: Select firmware based on strapping (Íñigo Huguet) [2136123]
- rtw89: 8852c: add chip_ops related to BTC (Íñigo Huguet) [2136123]
- rtw89: 8852c: fill freq and band of RX status by PPDU report (Íñigo Huguet) [2136123]
- rtw89: 8852c: implement chip_ops::get_thermal (Íñigo Huguet) [2136123]
- rtw89: 8852c: implement chip_ops related to TX power (Íñigo Huguet) [2136123]
- rtw89: 8852c: configure default BB TX/RX path (Íñigo Huguet) [2136123]
- rtw89: add RF H2C to notify firmware (Íñigo Huguet) [2136123]
- rtw89: don't flush hci queues and send h2c if power is off (Íñigo Huguet) [2136123]
- rtw89: pci: allow to process RPP prior to TX BD (Íñigo Huguet) [2136123]
- rtw89: ps: access TX/RX rings via another registers in low power mode (Íñigo Huguet) [2136123]
- rtw89: ser: re-enable interrupt in threadfn if under_recovery (Íñigo Huguet) [2136123]
- rtw89: pci: add a separate interrupt handler for low power mode (Íñigo Huguet) [2136123]
- rtw89: pci: reclaim TX BD only if it really need (Íñigo Huguet) [2136123]
- rtw89: pci: add variant RPWM/CPWM to enter low power mode (Íñigo Huguet) [2136123]
- rtw89: pci: add variant IMR/ISR and configure functions (Íñigo Huguet) [2136123]
- bus: mhi: host: Add support for Cinterion MV32-WA/MV32-WB (Íñigo Huguet) [2136123]
- bus: mhi: host: Optimize and update MMIO register write method (Íñigo Huguet) [2136123]
- bus: mhi: host: Bail on writing register fields if read fails (Íñigo Huguet) [2136123]
- bus: mhi: host: Wait for ready state after reset (Íñigo Huguet) [2136123]
- bus: mhi: host: Add soc_reset sysfs (Íñigo Huguet) [2136123]
- bus: mhi: host: pci_generic: Sort mhi_pci_id_table based on the PID (Íñigo Huguet) [2136123]
- bus: mhi: host: Use cached values for calculating the shared write pointer (Íñigo Huguet) [2136123]
- rtw88: pci: 8821c: Disable 21ce completion timeout (Íñigo Huguet) [2136123]
- rtw88: fix uninitialized 'tim_offset' warning (Íñigo Huguet) [2136123]
- rtw89: 8852c: add help function of set channel (Íñigo Huguet) [2136123]
- rtw89: 8852c: add set channel of BB part (Íñigo Huguet) [2136123]
- rtw89: 8852c: set channel of MAC part (Íñigo Huguet) [2136123]
- rtw89: 8852c: add set channel function of RF part (Íñigo Huguet) [2136123]
- rtw89: 8852c: add HFC parameters (Íñigo Huguet) [2136123]
- rtw89: 8852c: add efuse gain offset parser (Íñigo Huguet) [2136123]
- rtw89: 8852c: support bb gain info (Íñigo Huguet) [2136123]
- rtw89: 8852c: add BB initial and reset functions (Íñigo Huguet) [2136123]
- rtw89: 8852c: phy: configure TSSI bandedge (Íñigo Huguet) [2136123]
- rtw89: 8852c: add TX power track tables (Íñigo Huguet) [2136123]
- rtw89: 8852c: add TX power by rate and limit tables (Íñigo Huguet) [2136123]
- rtw89: 8852c: add BB and RF parameters tables (Íñigo Huguet) [2136123]
- ath9k: fix QCA9561 PA bias level (Íñigo Huguet) [2136123]
- ath9k_htc: fix potential out of bounds access with invalid rxstatus->rs_keyix (Íñigo Huguet) [2136123]
- ath11k: Fix build warning without CONFIG_IPV6 (Íñigo Huguet) [2136123]
- ath11k: fix missing unlock on error in ath11k_wow_op_resume() (Íñigo Huguet) [2136123]
- ath11k: Add support for SAR (Íñigo Huguet) [2136123]
- ath11k: add support for extended wmi service bit (Íñigo Huguet) [2136123]
- rtw89: pci: correct return value handling of rtw89_write16_mdio_mask() (Íñigo Huguet) [2136123]
- rtw89: configure security CAM for V1 chip (Íñigo Huguet) [2136123]
- rtw89: add new H2C to configure security CAM via DCTL for V1 chip (Íñigo Huguet) [2136123]
- rtw89: extend H2C of CMAC control info (Íñigo Huguet) [2136123]
- rtlwifi: rtl8192cu: Fix spelling mistake "writting" -> "writing" (Íñigo Huguet) [2136123]
- rtlwifi: Fix spelling mistake "cacluated" -> "calculated" (Íñigo Huguet) [2136123]
- rtw88: 8821ce: Disable PCIe ASPM L1 for 8821CE using chip ID (Íñigo Huguet) [2136123]
- rtw88: 8821ce: add support for device ID 0xb821 (Íñigo Huguet) [2136123]
- rtw88: 8821c: fix debugfs rssi value (Íñigo Huguet) [2136123]
- rtw88: do PHY calibration while starting AP (Íñigo Huguet) [2136123]
- rtw88: 8821c: Enable TX report for management frames (Íñigo Huguet) [2136123]
- rtw88: Add update beacon flow for AP mode (Íñigo Huguet) [2136123]
- rtw88: fix incorrect frequency reported (Íñigo Huguet) [2136123]
- rtw88: add ieee80211:sta_rc_update ops (Íñigo Huguet) [2136123]
- rtw89: rtw89_ser: add const to struct state_ent and event_ent (Íñigo Huguet) [2136123]
- rtw89: 8852c: add 8852c specific BT-coexistence initial function (Íñigo Huguet) [2136123]
- rtw89: Skip useless dig gain and igi related settings for 8852C (Íñigo Huguet) [2136123]
- rtw89: 8852c: disable firmware watchdog if CPU disabled (Íñigo Huguet) [2136123]
- rtw89: reset BA CAM (Íñigo Huguet) [2136123]
- rtw89: change station scheduler setting for hardware TX mode (Íñigo Huguet) [2136123]
- rtw89: ser: configure top ERR IMR for firmware to recover (Íñigo Huguet) [2136123]
- rtw89: ser: configure C-MAC interrupt mask (Íñigo Huguet) [2136123]
- rtw89: ser: configure D-MAC interrupt mask (Íñigo Huguet) [2136123]
- rtw89: ser: fix unannotated fall-through (Íñigo Huguet) [2136123]
- ath9k: Remove unnecessary print function dev_err() (Íñigo Huguet) [2136123]
- ath11k: Fix spelling mistake "reseting" -> "resetting" (Íñigo Huguet) [2136123]
- ath9k: fix ath_get_rate_txpower() to respect the rate list end tag (Íñigo Huguet) [2136123]
- mac80211: prepare sta handling for MLO support (Íñigo Huguet) [2136123]
- mac80211: minstrel_ht: fix where rate stats are stored (fixes debugfs output) (Íñigo Huguet) [2136123]
- nl80211: show SSID for P2P_GO interfaces (Íñigo Huguet) [2136123]
- mac80211: introduce BSS color collision detection (Íñigo Huguet) [2136123]
- mac80211: Improve confusing comment around tx_info clearing (Íñigo Huguet) [2136123]
- mac80211: protect ieee80211_assign_beacon with next_beacon check (Íñigo Huguet) [2136123]
- rtl8xxxu: fill up txrate info for gen1 chips (Íñigo Huguet) [2136123]
- rtl8xxxu: feed antenna information for cfg80211 (Íñigo Huguet) [2136123]
- rtlwifi: replace usage of found with dedicated list iterator variable (Íñigo Huguet) [2136123]
- brcmfmac: Avoid keeping power to SDIO card unless WOWL is used (Íñigo Huguet) [2136123]
- mwifiex: add mutex lock for call in mwifiex_dfs_chan_sw_work_queue (Íñigo Huguet) [2136123]
- rtw89: fix misconfiguration on hw_scan channel time (Íñigo Huguet) [2136123]
- rtw89: coex: Add case for scan offload (Íñigo Huguet) [2136123]
- rtw89: packet offload handler to avoid warning (Íñigo Huguet) [2136123]
- rtw89: change idle mode condition during hw_scan (Íñigo Huguet) [2136123]
- rtw89: update ptcl_init (Íñigo Huguet) [2136123]
- rtw89: update TMAC parameters (Íñigo Huguet) [2136123]
- rtw89: initialize NAV control (Íñigo Huguet) [2136123]
- rtw89: update scheduler setting (Íñigo Huguet) [2136123]
- rtw89: 8852c: update security engine setting (Íñigo Huguet) [2136123]
- rtw89: Turn on CR protection of CMAC (Íñigo Huguet) [2136123]
- rtw89: add chip_ops::{enable,disable}_bb_rf to support v1 chip (Íñigo Huguet) [2136123]
- rtw89: update STA scheduler parameters for v1 chip (Íñigo Huguet) [2136123]
- rtw89: extend dmac_pre_init to support 8852C (Íñigo Huguet) [2136123]
- rtw89: pci: add L1 settings (Íñigo Huguet) [2136123]
- rtw89: pci: add deglitch setting (Íñigo Huguet) [2136123]
- rtw89: pci: set address info registers depends on chips (Íñigo Huguet) [2136123]
- rtw89: pci: add LTR setting for v1 chip (Íñigo Huguet) [2136123]
- rtw89: pci: refine pci pre_init function (Íñigo Huguet) [2136123]
- rtw89: pci: add pci attributes to configure operating mode (Íñigo Huguet) [2136123]
- rtw89: pci: add register definition to rtw89_pci_info to generalize pci code (Íñigo Huguet) [2136123]
- ath11k: mhi: remove unnecessary goto from ath11k_mhi_start() (Íñigo Huguet) [2136123]
- ath11k: mhi: add error handling for suspend and resume (Íñigo Huguet) [2136123]
- ath11k: mhi: remove state machine (Íñigo Huguet) [2136123]
- rtw89: handle potential uninitialized variable (Íñigo Huguet) [2136123]
- rtw89: read RX bandwidth from v1 type RX descriptor (Íñigo Huguet) [2136123]
- rtw89: support hardware generate security header (Íñigo Huguet) [2136123]
- rtw89: support variant of fill_txdesc (Íñigo Huguet) [2136123]
- rtw89: pci: support variant of fill_txaddr_info (Íñigo Huguet) [2136123]
- rtw89: add chip_info::h2c_desc_size/fill_txdesc_fwcmd to support new chips (Íñigo Huguet) [2136123]
- rtw89: disabled IGI configuration for unsupported hardware (Íñigo Huguet) [2136123]
- rtw89: packed IGI configuration flow into function for DIG feature (Íñigo Huguet) [2136123]
- rtw89: regd: update mapping table to R59-R32 (Íñigo Huguet) [2136123]
- rtw89: regd: consider 6G band (Íñigo Huguet) [2136123]
- rtw89: 8852a: update txpwr tables to HALRF_027_00_038 (Íñigo Huguet) [2136123]
- rtw89: add UK to regulation type (Íñigo Huguet) [2136123]
- rtw89: reduce export symbol number of mac size and quota (Íñigo Huguet) [2136123]
- rtw89: support FW crash simulation (Íñigo Huguet) [2136123]
- rtw89: reconstruct fw feature (Íñigo Huguet) [2136123]
- rtw89: ser: dump fw backtrace while L2 reset (Íñigo Huguet) [2136123]
- rtw89: ser: dump memory for fw payload engine while L2 reset (Íñigo Huguet) [2136123]
- rtw89: ser: control hci interrupts on/off by state (Íñigo Huguet) [2136123]
- rtw89: mac: correct decision on error status by scenario (Íñigo Huguet) [2136123]
- rtw89: mac: move table of mem base addr to common (Íñigo Huguet) [2136123]
- rtw89: ser: fix CAM leaks occurring in L2 reset (Íñigo Huguet) [2136123]
- rtw88: change idle mode condition during hw_scan (Íñigo Huguet) [2136123]
- iwlwifi: mei: Replace zero-length array with flexible-array member (Íñigo Huguet) [2136123]
- iwlwifi: fw: Replace zero-length arrays with flexible-array members (Íñigo Huguet) [2136123]
- ath11k: fix driver initialization failure with WoW unsupported hw (Íñigo Huguet) [2136123]
- ath11k: Remove unnecessary delay in ath11k_core_suspend (Íñigo Huguet) [2136123]
- ath11k: Change max no of active probe SSID and BSSID to fw capability (Íñigo Huguet) [2136123]
- ath11k: Remove core PCI references from PCI common code (Íñigo Huguet) [2136123]
- ath11k: Refactor MSI logic to support WCN6750 (Íñigo Huguet) [2136123]
- ath11k: Choose MSI config based on HW revision (Íñigo Huguet) [2136123]
- ath11k: Refactor PCI code to support WCN6750 (Íñigo Huguet) [2136123]
- ath11k: PCI changes to support WCN6750 (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add uevent support for module autoloading (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for suspending and resuming channels (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for queueing SKBs to the host (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for processing channel rings (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for reading from the host (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for processing command rings (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for handling SYS_ERR condition (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for handling MHI_RESET (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for powering down the MHI endpoint stack (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for powering up the MHI endpoint stack (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for processing MHI endpoint interrupts (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for managing MHI state machine (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for sending events to the host (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for ring management (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for managing MMIO registers (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for creating and destroying MHI EP devices (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for registering MHI endpoint client drivers (Íñigo Huguet) [2136123]
- bus: mhi: ep: Add support for registering MHI endpoint controllers (Íñigo Huguet) [2136123]
- ath9k: make is2ghz consistent in ar9003_eeprom (Íñigo Huguet) [2136123]
- ath10k: add support for MSDU IDs for USB devices (Íñigo Huguet) [2136123]
- ath11k: add support to search regdb data in board-2.bin for WCN6855 (Íñigo Huguet) [2136123]
- ath11k: store and send country code to firmware after recovery (Íñigo Huguet) [2136123]
- ath9k: add functions to get paprd rate mask (Íñigo Huguet) [2136123]
- ath9k: refactor ar9003_hw_spur_mitigate_ofdm (Íñigo Huguet) [2136123]
- ath9k: fix ar9003_get_eepmisc (Íñigo Huguet) [2136123]
- ath9k: use AR9300_MAX_CHAINS when appropriate (Íñigo Huguet) [2136123]
- ath9k: split set11nRateFlags and set11nChainSel (Íñigo Huguet) [2136123]
- ath9k: make ATH_SREV macros more consistent (Íñigo Huguet) [2136123]
- ath11k: Add peer rhash table support (Íñigo Huguet) [2136123]
- ath11k: add read variant from SMBIOS for download board data (Íñigo Huguet) [2136123]
- ath11k: add fallback board name without variant while searching board-2.bin (Íñigo Huguet) [2136123]
- ath11k: enable PLATFORM_CAP_PCIE_GLOBAL_RESET QMI host capability (Íñigo Huguet) [2136123]
- ath11k: Add hw-restart option to simulate_fw_crash (Íñigo Huguet) [2136123]
- ath11k: add synchronization operation between reconfigure of mac80211 and ath11k_base (Íñigo Huguet) [2136123]
- ath11k: add support for device recovery for QCA6390/WCN6855 (Íñigo Huguet) [2136123]
- ath11k: disable regdb support for QCA6390 (Íñigo Huguet) [2136123]
- ath11k: remove unused ATH11K_BD_IE_BOARD_EXT (Íñigo Huguet) [2136123]
- ath11k: change fw build id format in driver init log (Íñigo Huguet) [2136123]
- ath11k: Refactor the peer delete (Íñigo Huguet) [2136123]
- ath10k: Use of_device_get_match_data() helper (Íñigo Huguet) [2136123]
- ath10k: Trigger sta disconnect on hardware restart (Íñigo Huguet) [2136123]
- ath9k: Use platform_get_irq() to get the interrupt (Íñigo Huguet) [2136123]
- ath11k: support GTK rekey offload (Íñigo Huguet) [2136123]
- ath11k: support ARP and NS offload (Íñigo Huguet) [2136123]
- ath11k: purge rx pktlog when entering WoW (Íñigo Huguet) [2136123]
- ath11k: implement hardware data filter (Íñigo Huguet) [2136123]
- ath11k: Add WoW net-detect functionality (Íñigo Huguet) [2136123]
- ath11k: Add basic WoW functionalities (Íñigo Huguet) [2136123]
- x86/cpu: Add several Intel server CPU model numbers (Prarit Bhargava) [2158037]
- ice: Implement devlink port split operations (Petr Oros) [2009705]
- ice: Add additional flags to ice_nvm_write_activate (Petr Oros) [2009705]
- ice: Add port option admin queue commands (Petr Oros) [2009705]
- hwmon: (coretemp) Check for null before removing sysfs attrs (Phil Auld) [2152429]
- KVM: x86/mmu: fix NULL pointer dereference on guest INVPCID (Jon Maloy) [2099301] {CVE-2022-1789}
- redhat/configs: enable HP_WATCHDOG for aarch64 (Mark Salter) [2113079]
- watchdog/hpwdt: Enable HP_WATCHDOG for ARM64 systems. (Mark Salter) [2113079]
- watchdog: Improve Kconfig entry ordering and dependencies (Mark Salter) [2113079]
- watchdog/hpwdt: Include nmi.h only if CONFIG_HPWDT_NMI_DECODING (Mark Salter) [2113079]
- uprobes/x86: Allow to probe a NOP instruction with 0x66 prefix (Oleg Nesterov) [2133797]
- platform/mellanox: Remove redundant 'NULL' check (Mark Langsdorf) [2122314]
- platform/mellanox: Remove unnecessary code (Mark Langsdorf) [2122314]
- platform/mellanox: mlxreg-lc: Fix locking issue (Mark Langsdorf) [2122314]
- platform/mellanox: mlxreg-lc: Fix coverity warning (Mark Langsdorf) [2122314]
- platform/mellanox: mlxreg-lc: Fix error flow and extend verbosity (Mark Langsdorf) [2122314]
- platform/mellanox: mlxreg-io: Add locking for io operations (Mark Langsdorf) [2122314]
- platform/mellanox: nvsw-sn2201: fix error code in nvsw_sn2201_create_static_devices() (Mark Langsdorf) [2122314]
- platform/mellanox: Add static in struct declaration. (Mark Langsdorf) [2122314]
- platform/mellanox: Spelling s/platfom/platform/ (Mark Langsdorf) [2122314]
- redhat/configs: Enable Mellanox SN2201 management device (Mark Langsdorf) [2122314]
- platform/mellanox: Add support for new SN2201 system (Mark Langsdorf) [2122314]
- platform_data/mlxreg: Add field for notification callback (Mark Langsdorf) [2122314]
- Bluetooth: btintel: Fix WBS setting for Intel legacy ROM products (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Fix broken LED quirk for legacy ROM  devices (Gopal Tiwari) [2129295]
- Bluetooth: Add support hdev to allocate private data (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Fix the legacy bootloader returns tlv based version (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Clean the exported function to static (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Move hci quirks to setup routine (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Refactoring setup routine for bootloader devices (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Add combined set_diag functions (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Fix the LED is not turning off immediately (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Fix the first HCI command not work with ROM device (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Add btintel data struct (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Refactoring setup routine for legacy ROM sku (Gopal Tiwari) [2129295]
- Bluetooth: btintel: Add combined setup and shutdown functions (Gopal Tiwari) [2129295]
- EDAC/mc_sysfs: Increase legacy channel support to 12 (Aristeu Rozanski) [2139861]
- NFS: Trigger the "ls -l" readdir heuristic sooner (Benjamin Coddington) [2025991]
- NFS: Cache all entries in the readdirplus reply (Benjamin Coddington) [2025991]
- NFS: Optimise away the previous cookie field (Benjamin Coddington) [2025991]
- NFS: Fix up forced readdirplus (Benjamin Coddington) [2025991]
- NFS: Convert readdir page cache to use a cookie based index (Benjamin Coddington) [2025991]
- NFS: Clean up page array initialisation/free (Benjamin Coddington) [2025991]
- NFS: Trace effects of the readdirplus heuristic (Benjamin Coddington) [2025991]
- NFS: Trace effects of readdirplus on the dcache (Benjamin Coddington) [2025991]
- NFS: Add basic readdir tracing (Benjamin Coddington) [2025991]
- NFS: Don't request readdirplus when revalidation was forced (Benjamin Coddington) [2025991]
- NFSv4: Ask for a full XDR buffer of readdir goodness (Benjamin Coddington) [2025991]
- NFS: Don't ask for readdirplus unless it can help nfs_getattr() (Benjamin Coddington) [2025991]
- NFS: Improve heuristic for readdirplus (Benjamin Coddington) [2025991]
- NFS: Reduce use of uncached readdir (Benjamin Coddington) [2025991]
- NFS: Simplify nfs_readdir_xdr_to_array() (Benjamin Coddington) [2025991]
- NFS: If the cookie verifier changes, we must invalidate the page cache (Benjamin Coddington) [2025991]
- NFS: Adjust the amount of readahead performed by NFS readdir (Benjamin Coddington) [2025991]
- NFS: Don't advance the page pointer unless the page is full (Benjamin Coddington) [2025991]
- NFS: Don't re-read the entire page cache to find the next cookie (Benjamin Coddington) [2025991]
- NFS: Store the change attribute in the directory page cache (Benjamin Coddington) [2025991]
- NFS: Calculate page offsets algorithmically (Benjamin Coddington) [2025991]
- NFS: Use kzalloc() to avoid initialising the nfs_open_dir_context (Benjamin Coddington) [2025991]
- NFS: Initialise the readdir verifier as best we can in nfs_opendir() (Benjamin Coddington) [2025991]
- NFS: Trace lookup revalidation failure (Benjamin Coddington) [2025991]
- NFS: constify nfs_server_capable() and nfs_have_writebacks() (Benjamin Coddington) [2025991]
- NFS: Return valid errors from nfs2/3_decode_dirent() (Benjamin Coddington) [2025991]
- NFS: Avoid duplicate uncached readdir calls on eof (Benjamin Coddington) [2025991]
- NFS: Don't skip directory entries when doing uncached readdir (Benjamin Coddington) [2025991]
- NFS: Don't overfill uncached readdir pages (Benjamin Coddington) [2025991]
- block: unhash blkdev part inode when the part is deleted (Ming Lei) [2148497]

* Thu Dec 22 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-447.el8]
- x86/fpu: Drop fpregs lock before inheriting FPU permissions (Eder Zulian) [2153549]
- cpufreq: amd-pstate: Add resume and suspend callbacks (Mark Langsdorf) [2122310]
- cpufreq: CPPC: Enable dvfs_possible_from_any_cpu (Mark Langsdorf) [2122310]
- cpufreq: check only freq_table in __resolve_freq() (Mark Langsdorf) [2122310]
- cpufreq: ondemand: Use cpumask_var_t for on-stack cpu mask (Mark Langsdorf) [2122310]
- cpufreq: Change order of online() CB and policy->cpus modification (Mark Langsdorf) [2122310]
- cpufreq: Warn users while freeing active policy (Mark Langsdorf) [2122310]
- cpufreq: Drop unnecessary cpus locking from store() (Mark Langsdorf) [2122310]
- cpufreq: Optimize cpufreq_show_cpus() (Mark Langsdorf) [2122310]
- cpufreq: make interface functions and lock holding state clear (Mark Langsdorf) [2122310]
- cpufreq: Abort show()/store() for half-initialized policies (Mark Langsdorf) [2122310]
- cpufreq: Rearrange locking in cpufreq_remove_dev() (Mark Langsdorf) [2122310]
- cpufreq: Split cpufreq_offline() (Mark Langsdorf) [2122310]
- cpufreq: Reorganize checks in cpufreq_offline() (Mark Langsdorf) [2122310]
- cpufreq: Clear real_cpus mask from remove_cpu_dev_symlink() (Mark Langsdorf) [2122310]
- cpufreq: Prepare cleanup of powerpc's asm/prom.h (Mark Langsdorf) [2122310]
- cpufreq: governor: Use kobject release() method to free dbs_data (Mark Langsdorf) [2122310]
- ipv6: fix panic when fib_lookup_arg->result is fib6_info (Jiri Benc) [2140599]
- tipc: re-fetch skb cb after tipc_msg_validate (Xin Long) [2142732]
- Documentation: bonding: correct xmit hash steps (Jonathan Toppins) [2150390]
- Documentation: bonding: update miimon default to 100 (Jonathan Toppins) [2150390]
- selftests: bonding: up/down delay w/ slave link flapping (Jonathan Toppins) [2150390]
- bonding (gcc13): synchronize bond_{a,t}lb_xmit() types (Jonathan Toppins) [2150390]
- selftests: net: Fix cross-tree inclusion of scripts (Jonathan Toppins) [2150390]
- treewide: use get_random_u32() when possible (Jonathan Toppins) [2150390]
- selftests/bonding: re-add lladdr target test (Jonathan Toppins) [2150390]
- selftests: bonding: cause oops in bond_rr_gen_slave_id (Jonathan Toppins) [2150390]
- selftests/bonding: add a test for bonding lladdr target (Jonathan Toppins) [2150390]
- net: Add tests for bonding and team address list management (Jonathan Toppins) [2150390]
- net: bonding: Unsync device addresses on ndo_stop (Jonathan Toppins) [2150390]
- net: bonding: Share lacpdu_mcast_addr definition (Jonathan Toppins) [2150390]
- Documentation: bonding: clarify supported modes for tlb_dynamic_lb (Jonathan Toppins) [2150390]
- selftests: include bonding tests into the kselftest infra (Jonathan Toppins) [2150390]
- bonding: fix reference count leak in balance-alb mode (Jonathan Toppins) [2150390]
- net:bonding:support balance-alb interface with vlan to bridge (Jonathan Toppins) [2150390]
- bonding: cleanup bond_create (Jonathan Toppins) [2150390]
- bonding: netlink error message support for options (Jonathan Toppins) [2150390]
- bonding: Update layer2 and layer2+3 hash formula documentation (Jonathan Toppins) [2150390]
- net: bonding: Add support for IPV6 ns/na to balance-alb/balance-tlb mode (Jonathan Toppins) [2150390]
- net: remove bond_slave_has_mac_rcu() (Jonathan Toppins) [2150390]
- net: bonding: debug: avoid printing debug logs when bond is not notifying peers (Jonathan Toppins) [2150390]
- net: bonding: constify and use dev_addr_set() (Jonathan Toppins) [2150390]
- net: use dev_addr_set() (Jonathan Toppins) [2150390]
- bonding: remove extraneous definitions from bonding.h (Jonathan Toppins) [2150390]
- net: bonding: bond_alb: Fix some typos in bond_alb.c (Jonathan Toppins) [2150390]
- net: bonding: use tabs instead of space for code indent (Jonathan Toppins) [2150390]
- net: bonding: remove unnecessary braces (Jonathan Toppins) [2150390]
- net: bonding: fix code indent for conditional statements (Jonathan Toppins) [2150390]
- net: bonding: add some required blank lines (Jonathan Toppins) [2150390]
- docs: networking: bonding.rst Fix a typo in bonding.rst (Jonathan Toppins) [2150390]
- docs: networking: bonding.rst resources section cleanup (Jonathan Toppins) [2150390]
- bonding: Replace zero-length array with flexible-array member (Jonathan Toppins) [2150390]
- include/net/bond_3ad: Simplify the code by using the ARRAY_SIZE (Jonathan Toppins) [2150390]
- vmxnet3: use correct intrConf reference when using extended queues (Izabela Bakollari) [2150917]
- vmxnet3: correctly report encapsulated LRO packet (Izabela Bakollari) [2150917]
- net: move from strlcpy with unused retval to strscpy (Izabela Bakollari) [2150917]
- vmxnet3: Implement ethtool's get_channels command (Izabela Bakollari) [2150917]
- vmxnet3: Record queue number to incoming packets (Izabela Bakollari) [2150917]
- [rt] Revert "mm/memcg: disable threshold event handlers on PREEMPT_RT" (Chris White) [2152035]
- s390/pci: allow zPCI zbus without a function zero (Tobias Huschle) [2043829]
- PCI: Extend isolated function probing to s390 (Tobias Huschle) [2043829]
- PCI: Move jailhouse's isolated function handling to pci_scan_slot() (Tobias Huschle) [2043829]
- PCI: Split out next_ari_fn() from next_fn() (Tobias Huschle) [2043829]
- PCI: Clean up pci_scan_slot() (Tobias Huschle) [2043829]
- KVM: selftests: Build the memslot tests for arm64 (Gavin Shan) [2134650]
- KVM: selftests: memslot_perf_test: Report optimal memory slots (Gavin Shan) [2134650]
- KVM: selftests: memslot_perf_test: Consolidate memory (Gavin Shan) [2134650]
- KVM: selftests: memslot_perf_test: Support variable guest page size (Gavin Shan) [2134650]
- KVM: selftests: memslot_perf_test: Probe memory slots for once (Gavin Shan) [2134650]
- KVM: selftests: memslot_perf_test: Consolidate loop conditions in prepare_vm() (Gavin Shan) [2134650]
- KVM: selftests: memslot_perf_test: Use data->nslots in prepare_vm() (Gavin Shan) [2134650]
- KVM: selftests: Make memslot_perf_test arch independent (Gavin Shan) [2134650]
- selftests: netfilter: Fix and review rpath.sh (Phil Sutter) [1961152]
- netfilter: Use l3mdev flow key when re-routing mangled packets (Phil Sutter) [1961152]
- netfilter: Update ip6_route_me_harder to consider L3 domain (Phil Sutter) [1961152]
- netfilter: Dissect flow after packet mangling (Phil Sutter) [1961152]
- netfilter: rpfilter/fib: Populate flowic_l3mdev field (Phil Sutter) [1961152]
- selftests: netfilter: Test reverse path filtering (Phil Sutter) [1961152]
- netfilter: nft_fib: Fix for rpath check with VRF devices (Phil Sutter) [1961152]
- net: seg6: fix seg6_lookup_any_nexthop() to handle VRFs using flowi_l3mdev (Phil Sutter) [1961152]
- net: Handle l3mdev in ip_tunnel_init_flow (Phil Sutter) [1961152]
- xfrm: Pass flowi_oif or l3mdev as oif to xfrm_dst_lookup (Phil Sutter) [1961152]
- net: Add l3mdev index to flow struct and avoid oif reset for port devices (Phil Sutter) [1961152]
- l3mdev: l3mdev_master_upper_ifindex_by_index_rcu should be using netdev_master_upper_dev_get_rcu (Phil Sutter) [1961152]
- l3mdev: add function to retreive upper master (Phil Sutter) [1961152]
- sfc: move deprecation message to sfc_siena (Íñigo Huguet) [2112205 2136107]
- sfc/siena: add entries for new CONFIG_SFC_SIENA* configs (Íñigo Huguet) [2112205 2136107]
- sfc: Fix an error handling path in efx_pci_probe() (Íñigo Huguet) [2112205]
- sfc: support PTP over Ethernet (Íñigo Huguet) [2112205 2065017]
- sfc: support PTP over IPv6/UDP (Íñigo Huguet) [2112205 2065017]
- sfc: allow more flexible way of adding filters for PTP (Íñigo Huguet) [2112205 2065017]
- sfc: correct filter_table_remove method for EF10 PFs (Íñigo Huguet) [2112205]
- sfc/siena: fix null pointer dereference in efx_hard_start_xmit (Íñigo Huguet) [2112205]
- sfc/siena: fix TX channel offset when using legacy interrupts (Íñigo Huguet) [2112205]
- sfc: implement ethtool get/set RX ring size for EF100 reps (Íñigo Huguet) [2112205]
- sfc: use a dynamic m-port for representor RX and set it promisc (Íñigo Huguet) [2112205]
- sfc: move table locking into filter_table_{probe,remove} methods (Íñigo Huguet) [2112205]
- sfc: insert default MAE rules to connect VFs to representors (Íñigo Huguet) [2112205]
- sfc: receive packets from EF100 VFs into representors (Íñigo Huguet) [2112205]
- sfc: check ef100 RX packets are from the wire (Íñigo Huguet) [2112205]
- sfc: determine wire m-port at EF100 PF probe time (Íñigo Huguet) [2112205]
- sfc: ef100 representor RX top half (Íñigo Huguet) [2112205]
- sfc: ef100 representor RX NAPI poll (Íñigo Huguet) [2112205]
- sfc: plumb ef100 representor stats (Íñigo Huguet) [2112205]
- sfc: disable softirqs for ptp TX (Íñigo Huguet) [2112205]
- sfc/siena: fix repeated words in comments (Íñigo Huguet) [2112205]
- sfc: attach/detach EF100 representors along with their owning PF (Íñigo Huguet) [2112205]
- sfc: hook up ef100 representor TX (Íñigo Huguet) [2112205]
- sfc: support passing a representor to the EF100 TX path (Íñigo Huguet) [2112205]
- sfc: determine representee m-port for EF100 representors (Íñigo Huguet) [2112205]
- sfc: phys port/switch identification for ef100 reps (Íñigo Huguet) [2112205]
- sfc: add basic ethtool ops to ef100 reps (Íñigo Huguet) [2112205]
- sfc: add skeleton ef100 VF representors (Íñigo Huguet) [2112205]
- sfc: detect ef100 MAE admin privilege/capability at probe time (Íñigo Huguet) [2112205]
- sfc: update EF100 register descriptions (Íñigo Huguet) [2112205]
- sfc: update MCDI protocol headers (Íñigo Huguet) [2112205]
- sfc/siena: Use the bitmap API to allocate bitmaps (Íñigo Huguet) [2112205]
- sfc: Separate netdev probe/remove from PCI probe/remove (Íñigo Huguet) [2112205]
- sfc: replace function name in string with __func__ (Íñigo Huguet) [2112205]
- sfc: Unsplit literal string. (Íñigo Huguet) [2112205]
- sfc: Move EF100 efx_nic_type structs to the end of the file (Íñigo Huguet) [2112205]
- sfc: Separate efx_nic memory from net_device memory (Íñigo Huguet) [2112205]
- sfc: Encapsulate access to netdev_priv() (Íñigo Huguet) [2112205]
- sfc: Change BUG_ON to WARN_ON and recovery code. (Íñigo Huguet) [2112205]
- sfc: Remove netdev init from efx_init_struct (Íñigo Huguet) [2112205]
- sfc: Add a PROBED state for EF100 VDPA use. (Íñigo Huguet) [2112205]
- sfc: Split STATE_READY in to STATE_NET_DOWN and STATE_NET_UP. (Íñigo Huguet) [2112205]
- sfc: fix repeated words in comments (Íñigo Huguet) [2112205]
- sfc: siena: fix repeated words in comments (Íñigo Huguet) [2112205]
- sfc/siena: Fix typo in comment (Íñigo Huguet) [2112205]
- sfc: Fix typo in comment (Íñigo Huguet) [2112205]
- sfc/siena: fix wrong tx channel offset with efx_separate_tx_channels (Íñigo Huguet) [2112205]
- sfc/siena: fix considering that all channels have TX queues (Íñigo Huguet) [2112205]
- sfc/siena: Remove duplicate check on segments (Íñigo Huguet) [2112205 2136107]
- sfc: siena: Have a unique wrapper ifndef for efx channels header (Íñigo Huguet) [2112205 2136107]
- eth: sfc: remove remnants of the out-of-tree napi_weight module param (Íñigo Huguet) [2112205]
- sfc: siena: Fix Kconfig dependencies (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Reinstate SRIOV init/fini function calls (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Make PTP and reset support specific for Siena (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Make MCDI logging support specific for Siena (Íñigo Huguet) [2112205 2136107]
- siena: Make HWMON support specific for Siena (Íñigo Huguet) [2112205 2136107]
- siena: Make SRIOV support specific for Siena (Íñigo Huguet) [2112205 2136107]
- siena: Make MTD support specific for Siena (Íñigo Huguet) [2112205 2136107]
- sfc: Add a basic Siena module (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Inline functions in sriov.h to avoid conflicts with sfc (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Rename functions in nic_common.h to avoid conflicts with sfc (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Rename functions in mcdi headers to avoid conflicts with sfc (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Rename peripheral functions to avoid conflicts with sfc (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Rename RX/TX functions to avoid conflicts with sfc (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Rename functions in efx headers to avoid conflicts with sfc (Íñigo Huguet) [2112205 2136107]
- sfc/siena: Remove build references to missing functionality (Íñigo Huguet) [2112205 2136107]
- sfc: Copy shared files needed for Siena (part 2) (Íñigo Huguet) [2112205 2136107]
- sfc: Copy shared files needed for Siena (part 1) (Íñigo Huguet) [2112205 2136107]
- sfc: Move Siena specific files (Íñigo Huguet) [2112205 2136107]
- sfc: Copy a subset of mcdi_pcol.h to siena (Íñigo Huguet) [2112205 2136107]
- sfc: Disable Siena support (Íñigo Huguet) [2112205 2136107]
- sfc: add EF100 VF support via a write to sriov_numvfs (Íñigo Huguet) [2112205]
- sfc: Remove global definition of efx_reset_type_names (Íñigo Huguet) [2112205]
- sfc: Remove duplicate definition of efx_xmit_done (Íñigo Huguet) [2112205]
- sfc: efx_default_channel_type APIs can be static (Íñigo Huguet) [2112205]
- sfc: Fix spelling mistake "writting" -> "writing" (Íñigo Huguet) [2112205]
- sfc: ef10: Fix assigning negative value to unsigned variable (Íñigo Huguet) [2112205]
- sfc: use hardware tx timestamps for more than PTP (Íñigo Huguet) [2112205 2065017]
- net: ethernet: sfc: Make subdir logic consistent with other vendors (Íñigo Huguet) [2112205 2136107]
- hugetlbfs: fix mount mode command line processing (Bill O'Donnell) [2148876]
- igc: Correct the launchtime offset (Corinna Vinschen) [2103954]
- net: Remove the obsolte u64_stats_fetch_*_irq() users (drivers). (Corinna Vinschen) [2103954]
- igc: Remove IGC_MDIC_INT_EN definition (Corinna Vinschen) [2103954]
- igc: Remove forced_speed_duplex value (Corinna Vinschen) [2103954]
- igc: Remove MSI-X PBA Clear register (Corinna Vinschen) [2103954]
- igc: Lift TAPRIO schedule restriction (Corinna Vinschen) [2103954]
- wifi: brcmfmac: Fix potential buffer overflow in brcmf_fweh_event_worker() (Wander Lairson Costa) [2150964] {CVE-2022-3628}
- net: ethernet: move from strlcpy with unused retval to strscpy (Corinna Vinschen) [2103949]
- tipc: call tipc_lxc_xmit without holding node_read_lock (Xin Long) [2141640]
- mptcp: fix sleep in atomic at close time (Davide Caratti) [2150361]
- mptcp: don't orphan ssk in mptcp_close() (Davide Caratti) [2150361]
- net: Avoid overwriting valid skb->napi_id (Antoine Tenart) [2142593]
- x86/microcode/AMD: Apply the patch early on every logical thread (Waiman Long) [2139856]
- x86/bugs: Enable STIBP for IBPB mitigated RETBleed (Waiman Long) [2139856]
- x86/bugs: Add "unknown" reporting for MMIO Stale Data (Waiman Long) [2139856]
- tracing: Use a copy of the va_list for __assign_vstr() (Íñigo Huguet) [2143356]
- tracing/events: Add __vstring() and __assign_vstr() helper macros (Íñigo Huguet) [2143356]
- rtnetlink: add IFLA_PARENT_[DEV|DEV_BUS]_NAME (Jose Ignacio Tornos Martinez) [2144853]
- rtnetlink: add alloc() method to rtnl_link_ops (Jose Ignacio Tornos Martinez) [2144853]
- ipv6: Fix data races around sk->sk_prot. (Guillaume Nault) [2144805] {CVE-2022-3567}
- ipv6: annotate some data-races around sk->sk_prot (Guillaume Nault) [2144805] {CVE-2022-3567}
- ipv6: use indirect call wrappers for {tcp, udpv6}_{recv, send}msg() (Guillaume Nault) [2144805] {CVE-2022-3567}
- mm/mremap: hold the rmap lock in write mode when moving page table entries. (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap: use pmd/pud_poplulate to update page table entries (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap: don't enable optimized PUD move if page table levels is 2 (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap: convert huge PUD move to separate helper (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap: fix BUILD_BUG_ON() error in get_extent (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap.c: fix extent calculation (Waiman Long) [2140945] {CVE-2022-41222}
- x86: mremap speedup - Enable HAVE_MOVE_PUD (Waiman Long) [2140945] {CVE-2022-41222}
- mm: speedup mremap on 1GB or larger regions (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap: start addresses are properly aligned (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap: calculate extent in one place (Waiman Long) [2140945] {CVE-2022-41222}
- mm/mremap: it is sure to have enough space when extent meets requirement (Waiman Long) [2140945] {CVE-2022-41222}

* Mon Dec 19 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-446.el8]
- irqchip/gic, gic-v3: Make SGIs use handle_percpu_devid_irq() (Charles Mirabile) [2133892]
- irqchip/gic-common: Don't enable SGIs by default (Charles Mirabile) [2133892]
- irqchip/gic: Configure SGIs as standard interrupts (Charles Mirabile) [2133892]
- irqchip/gic: Refactor SMP configuration (Charles Mirabile) [2133892]
- irqchip/gic-v3: Configure SGIs as standard interrupts (Charles Mirabile) [2133892]
- irqchip/gic-v3: Describe the SGI range (Charles Mirabile) [2133892]
- arm64: Allow IPIs to be handled as normal interrupts (Charles Mirabile) [2133892]
- irqchip/gic, gic-v3: Prevent GSI to SGI translations (Charles Mirabile) [2133892]
- Workaround to enable support for IPI (Charles Mirabile) [2133892]
- net: ethernet: move from strlcpy with unused retval to strscpy (Ken Cox) [2112182]
- tg3: Disable tg3 device on system reboot to avoid triggering AER (Ken Cox) [2112182]
- aquantia: Do not purge addresses when setting the number of rings (Izabela Bakollari) [2122571]
- openvswitch: add nf_ct_is_confirmed check before assigning the helper (Antoine Tenart) [2135414]
- net: openvswitch: allow conntrack in non-initial user namespace (Antoine Tenart) [2135414]
- net: openvswitch: allow metering in non-initial user namespace (Antoine Tenart) [2135414]
- openvswitch: Change the return type for vport_ops.send function hook to int (Antoine Tenart) [2135414]
- net: openvswitch: fix repeated words in comments (Antoine Tenart) [2135414]
- openvswitch: add OVS_DP_ATTR_PER_CPU_PIDS to get requests (Antoine Tenart) [2135414]
- openvswitch: allow specifying ifindex of new interfaces (Antoine Tenart) [2135414]
- openvswitch: move from strlcpy with unused retval to strscpy (Antoine Tenart) [2135414]
- openvswitch: Fix overreporting of drops in dropwatch (Antoine Tenart) [2135414]
- openvswitch: Fix double reporting of drops in dropwatch (Antoine Tenart) [2135414]
- openvswitch: fix memory leak at failed datapath creation (Antoine Tenart) [2135414]
- net: remove noblock parameter from skb_recv_datagram() (Íñigo Huguet) [2143359]
- i40e: Fix error handling in i40e_init_module() (Stefan Assmann) [2103661]
- i40e: Add appropriate error message logged for incorrect duplex setting (Stefan Assmann) [2103661]
- i40e: Add i40e_napi_poll tracepoint (Stefan Assmann) [2103661]
- i40e: Record number of RXes cleaned during NAPI (Stefan Assmann) [2103661]
- i40e: Record number TXes cleaned during NAPI (Stefan Assmann) [2103661]
- i40e: Store the irq number in i40e_q_vector (Stefan Assmann) [2103661]
- ptp: introduce helpers to adjust by scaled parts per million (Stefan Assmann) [2103661]
- net: Remove the obsolte u64_stats_fetch_*_irq() users (drivers). (Stefan Assmann) [2103661]
- i40e: Fix flow-type by setting GL_HASH_INSET registers (Stefan Assmann) [2103661]
- i40e: Fix ethtool rx-flow-hash setting for X722 (Stefan Assmann) [2103661]
- i40e: Fix ADQ rate limiting for PF (Stefan Assmann) [2103661]
- i40e: add description and modify interrupts configuration procedure (Stefan Assmann) [2103661]
- i40e: Add basic support for I710 devices (Stefan Assmann) [2103661]
- net: ethernet: move from strlcpy with unused retval to strscpy (Stefan Assmann) [2103661]
- i40e: Fix incorrect address type for IPv6 flow rules (Stefan Assmann) [2103661]
- i40e: Fix to stop tx_timeout recovery if GLOBR fails (Stefan Assmann) [2103661]
- i40e: convert .adjfreq to .adjfine (Stefan Assmann) [2103661]
- i40e: use mul_u64_u64_div_u64 for PTP frequency calculation (Stefan Assmann) [2103661]
- i40e: Fix interface init with MSI interrupts (no MSI-X) (Stefan Assmann) [2103661]
- i40e: Refactor tc mqprio checks (Stefan Assmann) [2103661]
- i40e: Fix erroneous adapter reinitialization during recovery process (Stefan Assmann) [2103661]
- i40e: Fix VF's MAC Address change on VM (Stefan Assmann) [2103661]
- i40e: Fix dropped jumbo frames statistics (Stefan Assmann) [2103661]
- intel/i40e:fix repeated words in comments (Stefan Assmann) [2103661]
- intel: remove unused macros (Stefan Assmann) [2103661]
- i40e: read the XDP program once per NAPI (Stefan Assmann) [2103661]
- intel/i40e: delete if NULL check before dev_kfree_skb (Stefan Assmann) [2103661]
- i40e: Remove unnecessary synchronize_irq() before free_irq() (Stefan Assmann) [2103661]
- i40e: Add support for ethtool -s <interface> speed <speed in Mb> (Stefan Assmann) [2103661]
- i40e: Add VF VLAN pruning (Stefan Assmann) [2103661]
- xsk: Wipe out dead zero_copy_allocator declarations (Stefan Assmann) [2103661]
- gpio: amdpt: add new device ID and 24-pin support (Prarit Bhargava) [2097868]
- platform/x86/intel: pmc/core: Add Raptor Lake support to pmc core driver (Prarit Bhargava) [2076732]
- HID: hyperv: fix possible memory leak in mousevsc_probe() (Mohammed Gamal) [2139468]
- HID: hyperv: Correctly access fields declared as __le16 (Mohammed Gamal) [2139468]
- Drivers: hv: vmbus: fix possible memory leak in vmbus_device_register() (Mohammed Gamal) [2139473]
- Drivers: hv: vmbus: fix double free in the error path of vmbus_add_channel_work() (Mohammed Gamal) [2139473]
- Drivers: hv: fix repeated words in comments (Mohammed Gamal) [2139473]
- Drivers: hv: vmbus: Split memcpy of flex-array (Mohammed Gamal) [2139473]
- Drivers: hv: vmbus: Don't wait for the ACPI device upon initialization (Mohammed Gamal) [2139473]
- Drivers: hv: vmbus: Use PCI_VENDOR_ID_MICROSOFT for better discoverability (Mohammed Gamal) [2139473]
- PCI: Move PCI_VENDOR_ID_MICROSOFT/PCI_DEVICE_ID_HYPERV_VIDEO definitions to pci_ids.h (Mohammed Gamal) [2139473]
- Drivers: hv: vmbus: Fix kernel-doc (Mohammed Gamal) [2139473]
- Drivers: hv: vmbus: Optimize vmbus_on_event (Mohammed Gamal) [2139473]
- Drivers: hv: Never allocate anything besides framebuffer from framebuffer memory region (Mohammed Gamal) [2139473]
- Drivers: hv: Always reserve framebuffer region for Gen1 VMs (Mohammed Gamal) [2139473]
- Drivers: hv: remove duplicate word in a comment (Mohammed Gamal) [2139473]
- Drivers: hv: Create debugfs file with hyper-v balloon usage information (Mohammed Gamal) [2139473]
- Drivers: hv: vm_bus: Handle vmbus rescind calls after vmbus is suspended (Mohammed Gamal) [2139473]
- scsi: storvsc: remove an extraneous "to" in a comment (Cathy Avery) [2143320]
- Drivers: hv: vmbus: Optimize vmbus_on_event (Cathy Avery) [2143320]
- scsi: storvsc: Drop DID_TARGET_FAILURE use (Cathy Avery) [2143320]
- scsi: storvsc: Remove WQ_MEM_RECLAIM from storvsc_error_wq (Cathy Avery) [2143320]
- scsi: storvsc: Correct reporting of Hyper-V I/O size limits (Cathy Avery) [2143320]
- scsi: storvsc: Removing Pre Win8 related logic (Cathy Avery) [2143320]
- scsi: storvsc: Fix typo in comment (Cathy Avery) [2143320]
- scsi: storvsc: Remove support for Hyper-V 2008 and 2008R2/Win7 (Cathy Avery) [2143320]
- vdpa/mlx5: re-create forwarding rules after mac modified (Laurent Vivier) [2145136]
- ipv6: Fix crash when IPv6 is administratively disabled (Guillaume Nault) [2140779]
- raw: fix a typo in raw_icmp_error() (Guillaume Nault) [2140779]
- raw: remove unused variables from raw6_icmp_error() (Guillaume Nault) [2140779]
- raw: complete rcu conversion (Guillaume Nault) [2140779]
- raw: Use helpers for the hlist_nulls variant. (Guillaume Nault) [2140779]
- raw: Fix mixed declarations error in raw_icmp_error(). (Guillaume Nault) [2140779]
- raw: convert raw sockets to RCU (Guillaume Nault) [2140779]
- raw: use more conventional iterators (Guillaume Nault) [2140779]
- raw: Add missing annotations to raw_seq_start() and raw_seq_stop() (Guillaume Nault) [2140779]
- net: ethernet: move from strlcpy with unused retval to strscpy (Ken Cox) [2103941]
- e1000e: convert .adjfreq to .adjfine (Ken Cox) [2103941]
- e1000e: remove unnecessary range check in e1000e_phc_adjfreq (Ken Cox) [2103941]
- Revert "e1000e: Fix possible HW unit hang after an s0ix exit" (Ken Cox) [2103941]
- e1000e: Enable GPT clock before sending message to CSME (Ken Cox) [2103941]
- intel/e1000e:fix repeated words in comments (Ken Cox) [2103941]
- intel: remove unused macros (Ken Cox) [2103941]
- net: move netif_set_gso_max helpers (Ivan Vecera) [2137564]
- net: make drivers set the TSO limit not the GSO limit (Ivan Vecera) [2137564]
- net: don't allow user space to lift the device limits (Ivan Vecera) [2137564]
- net: add netif_inherit_tso_max() (Ivan Vecera) [2137564]
- net: extract a few internals from netdevice.h (Ivan Vecera) [2137564]
- net: unexport a handful of dev_* functions (Ivan Vecera) [2137564]
- bpf: Fix extable address check. (Felix Maurer) [2138532]
- bpf, x64: Factor out emission of REX byte in more cases (Felix Maurer) [2138532]
- bpf: Support dual-stack sockets in bpf_tcp_check_syncookie (Felix Maurer) [2138532]
- bpf: Fix extable fixup offset. (Felix Maurer) [2138532]
- bpf: Fix the off-by-two error in range markings (Felix Maurer) [2138532]
- bpf: Fix potential race in tail call compatibility check (Felix Maurer) [2138532]
- bpf: Fix possible out of bound write in narrow load handling (Felix Maurer) [2138532]
- bpf: Fix potential memleak and UAF in the verifier. (Felix Maurer) [2138532]
- KVM: s390: vsie: Fix the initialization of the epoch extension (epdx) field (Thomas Huth) [2151854]
- PM: core: Remove static qualifier in DEFINE_SIMPLE_DEV_PM_OPS macro (Íñigo Huguet) [2143354]
- PM: core: Add new *_PM_OPS macros, deprecate old ones (Íñigo Huguet) [2143354]
- PM: Make *_DEV_PM_OPS macros use __maybe_unused (Íñigo Huguet) [2143354]
- PM: core: Redefine pm_ptr() macro (Íñigo Huguet) [2143354]
- linux/kconfig.h: replace IF_ENABLED() with PTR_IF() in <linux/kernel.h> (Íñigo Huguet) [2143354]
- net: Remove unused inline function sk_nulls_node_init() (Guillaume Nault) [2143239]
- ping: convert to RCU lookups, get rid of rwlock (Guillaume Nault) [2143239]
- mm/cgroup/reclaim: fix dirty pages throttling on cgroup v1 (Waiman Long) [2149544]
- mm: vmscan: remove deadlock due to throttling failing to make progress (Waiman Long) [2149544]
- mm: vmscan: reduce throttling due to a failure to make progress -fix (Waiman Long) [2149544]
- mm: vmscan: Reduce throttling due to a failure to make progress (Waiman Long) [2149544]
- mm/vmscan: delay waking of tasks throttled on NOPROGRESS (Waiman Long) [2149544]
- mm/vmscan: increase the timeout if page reclaim is not making progress (Waiman Long) [2149544]
- mm/vmscan: centralise timeout values for reclaim_throttle (Waiman Long) [2149544]
- mm/page_alloc: remove the throttling logic from the page allocator (Waiman Long) [2149544]
- mm/writeback: throttle based on page writeback instead of congestion (Waiman Long) [2149544]
- mm/vmscan: throttle reclaim when no progress is being made (Waiman Long) [2149544]
- mm/vmscan: throttle reclaim and compaction when too may pages are isolated (Waiman Long) [2149544]
- mm/vmscan: throttle reclaim until some writeback completes if congested (Waiman Long) [2149544]
- mm/vmscan.c: delete or fix duplicated words (Waiman Long) [2149544]
- powerpc/pseries/vas: Add VAS IRQ primary handler (Mamatha Inamdar) [2131675]
- powerpc: Ignore DSI error caused by the copy/paste instruction (Mamatha Inamdar) [2131675]
- powerpc/pseries: Move vas_migration_handler early during migration (Mamatha Inamdar) [2131675]
- vt: drop old FONT ioctls (Wander Lairson Costa) [2109164] {CVE-2021-33656}

* Wed Dec 14 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-445.el8]
- x86/mce: Reduce number of machine checks taken during recovery (Prarit Bhargava) [2104388]
- scsi: storvsc: Fix handling of srb_status and capacity change events (Mohammed Gamal) [2139728]
- clocksource: hyper-v: unexport __init-annotated hv_init_clocksource() (Mohammed Gamal) [2139463]
- hv_netvsc: Fix race between VF offering and VF association message from host (Mohammed Gamal) [2139475]
- sbitmap: fix lockup while swapping (Ming Lei) [2140214]
- sbitmap: fix batched wait_cnt accounting (Ming Lei) [2140214]
- sbitmap: Avoid leaving waitqueue in invalid state in __sbq_wake_up() (Ming Lei) [2140214]
- sbitmap: fix possible io hung due to lost wakeup (Ming Lei) [2140214]
- sbitmap: add helper to clear a batch of tags (Ming Lei) [2140214]
- x86/hyperv: Restore VP assist page after cpu offlining/onlining (Mohammed Gamal) [2139454]
- clocksource/drivers/hyperv: add data structure for reference TSC MSR (Mohammed Gamal) [2139454]
- x86/hyperv: fix root partition faults when writing to VP assist page MSR (Mohammed Gamal) [2139454]
- x86/hyperv: fix invalid writes to MSRs during root partition kexec (Mohammed Gamal) [2139454]
- x86/hyperv: Remove BUG_ON() for kmap_local_page() (Mohammed Gamal) [2139454]
- x86/hyperv: Disable hardlockup detector by default in Hyper-V guests (Mohammed Gamal) [2139454]
- x86/hyperv: Update 'struct hv_enlightened_vmcs' definition (Mohammed Gamal) [2139454]
- x86/hyperv: Fix 'struct hv_enlightened_vmcs' definition (Mohammed Gamal) [2139454]
- x86/hyperv: Replace kmap() with kmap_local_page() (Mohammed Gamal) [2139454]
- hyperv: simplify and rename generate_guest_id (Mohammed Gamal) [2139454]
- x86/Hyper-V: Add SEV negotiate protocol support in Isolation VM (Mohammed Gamal) [2139454]
- x86/sev: Define the Linux-specific guest termination reasons (Mohammed Gamal) [2139454]
- x86/sev: Shorten GHCB terminate macro names (Mohammed Gamal) [2139454]
- x86/sev: Save the negotiated GHCB version (Mohammed Gamal) [2139454]
- locking: Add __sched to semaphore functions (Waiman Long) [2141429]
- locking/rwsem: Disable preemption while trying for rwsem lock (Waiman Long) [2141429]
- locking/percpu-rwsem: Add percpu_is_write_locked() and percpu_is_read_locked() (Waiman Long) [2141429]
- locking/rwsem: Conditionally wake waiters in reader/writer slowpaths (Waiman Long) [2141429]
- locking: Mark racy reads of owner->on_cpu (Waiman Long) [2141429]
- locking: Make owner_on_cpu() into <linux/sched.h> (Waiman Long) [2141429]
- locking/rwsem: Optimize down_read_trylock() under highly contended case (Waiman Long) [2141429]
- locking/rwsem: Fix comments about reader optimistic lock stealing conditions (Waiman Long) [2141429]
- locking/rwsem: Disable preemption for spinning region (Waiman Long) [2141429]
- locking: Remove rcu_read_{,un}lock() for preempt_{dis,en}able() (Waiman Long) [2141429]
- NFSD: Mark exports of NFS as unsupported (Benjamin Coddington) [2150902]
- fuse: lock inode unconditionally in fuse_fallocate() (Miklos Szeredi) [2110883]
- fuse: add file_modified() to fallocate (Miklos Szeredi) [2110883]
- mei: me: add adler lake point S DID (Prarit Bhargava) [2141602]
- ocfs2/dlm: move BITS_TO_BYTES() to bitops.h for wider use (Izabela Bakollari) [2144858]
- libnvdimm/namespace: Fix visibility of namespace resource attribute (Jeff Moyer) [2016347]
- PCI: hv: Only reuse existing IRTE allocation for Multi-MSI (Mohammed Gamal) [2139458]
- PCI: hv: Fix the definition of vector in hv_compose_msi_msg() (Mohammed Gamal) [2139458]
- PCI: hv: Take a const cpumask in hv_compose_msi_req_get_cpu() (Mohammed Gamal) [2139458]
- PCI: hv: Fix synchronization between channel callback and hv_pci_bus_exit() (Mohammed Gamal) [2139458]
- PCI: hv: Add validation for untrusted Hyper-V values (Mohammed Gamal) [2139458]
- PCI: hv: Fix interrupt mapping for multi-MSI (Mohammed Gamal) [2139458]
- PCI: hv: Reuse existing IRTE allocation in compose_msi_msg() (Mohammed Gamal) [2139458]
- PCI: hv: Fix hv_arch_irq_unmask() for multi-MSI (Mohammed Gamal) [2139458]
- PCI: hv: Fix synchronization between channel callback and hv_compose_msi_msg() (Mohammed Gamal) [2139458]
- PCI: hv: Use vmbus_requestor to generate transaction IDs for VMbus hardening (Mohammed Gamal) [2139458]
- PCI: hv: Fix multi-MSI to allow more than one MSI vector (Mohammed Gamal) [2139458]
- net: mana: Add rmb after checking owner bits (Mohammed Gamal) [2139462]
- net: mana: Add support of XDP_REDIRECT action (Mohammed Gamal) [2139462]
- net: mana: Add the Linux MANA PF driver (Mohammed Gamal) [2139462]
- NFSD: Protect against send buffer overflow in NFSv3 READ (Scott Mayhew) [2141774] {CVE-2022-43945}
- NFSD: Protect against send buffer overflow in NFSv2 READ (Scott Mayhew) [2141774] {CVE-2022-43945}
- NFSD: Protect against send buffer overflow in NFSv3 READDIR (Scott Mayhew) [2141774] {CVE-2022-43945}
- NFSD: Protect against send buffer overflow in NFSv2 READDIR (Scott Mayhew) [2141774] {CVE-2022-43945}
- SUNRPC: Fix svcxdr_init_encode's buflen calculation (Scott Mayhew) [2141774] {CVE-2022-43945}
- SUNRPC: Fix svcxdr_init_decode's end-of-buffer calculation (Scott Mayhew) [2141774] {CVE-2022-43945}
- KVM: VMX: fully disable SGX if SECONDARY_EXEC_ENCLS_EXITING unavailable (Emanuele Giuseppe Esposito) [2127128]
- cgroup/cpuset: Reduce cpuset_rwsem writer latency (Waiman Long) [2149031]
- rcu/exp: Mark current CPU as exp-QS in IPI loop second pass (Waiman Long) [2149031]
- rcu: Always inline rcu_dynticks_task*_{enter,exit}() (Waiman Long) [2149031]
- rcu: Fix existing exp request check in sync_sched_exp_online_cleanup() (Waiman Long) [2149031]
- rcu: Fix macro name CONFIG_TASKS_RCU_TRACE (Waiman Long) [2149031]
- rcu: Fix stall-warning deadlock due to non-release of rcu_node ->lock (Waiman Long) [2149031]
- rcu: Fix to include first blocked task in stall warning (Waiman Long) [2149031]
- cgroup: Use cgroup_attach_{lock,unlock}() from cgroup_attach_task_all() (Waiman Long) [2149031]
- cgroup: Add missing cpus_read_lock() to cgroup_attach_task_all() (Waiman Long) [2149031]
- cgroup: Fix threadgroup_rwsem <-> cpus_read_lock() deadlock (Waiman Long) [2149031]
- cgroup: Elide write-locking threadgroup_rwsem when updating csses on an empty subtree (Waiman Long) [2149031]
- cgroup/cpuset: Fix a race between cpuset_attach() and cpu hotplug (Waiman Long) [2149031]
- cgroup: reduce dependency on cgroup_mutex (Waiman Long) [2149031]

* Mon Dec 12 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-444.el8]
- drm/i915: fix TLB invalidation for Gen12 video and compute engines (Wander Lairson Costa) [2148150] {CVE-2022-4139}
- redhat/configs: Set CONFIG_X86_AMD_PSTATE to 'm' (Prarit Bhargava) [2145246]
- bonding: uninitialized variable in bond_miimon_inspect() (Jonathan Toppins) [1973124]
- bonding: fix link recovery in mode 2 when updelay is nonzero (Jonathan Toppins) [1973124]
- RHEL: ALSA: update configuration (Jaroslav Kysela) [2125544]
- RHEL: ALSA: fix compilation issues (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: pci-mtl: fix firmware name (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Correct pin configs for ASUS G533Z (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: remove ALC289_FIXUP_DUAL_SPK for Dell 5530 (Jaroslav Kysela) [2125544]
- ALSA: ac97: Use snd_ctl_rename() to rename a control (Jaroslav Kysela) [2125544]
- ALSA: ca0106: Use snd_ctl_rename() to rename a control (Jaroslav Kysela) [2125544]
- ALSA: emu10k1: Use snd_ctl_rename() to rename a control (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Use snd_ctl_rename() to rename a control (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Use snd_ctl_rename() to rename a control (Jaroslav Kysela) [2125544]
- ALSA: control: add snd_ctl_rename() (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: Use only dynamic PCM device allocation (Jaroslav Kysela) [2125544]
- regmap: add reg_sequence helpers (Jaroslav Kysela) [2125544]
- regmap: fix the kerneldoc for regmap_test_bits() (Jaroslav Kysela) [2125544]
- regmap: provide helpers for simple bit operations (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Free the ida when IPC fails in sof_ipc4_widget_setup() (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic31xx: Handle BCLK set as PLL input configuration (Jaroslav Kysela) [2125544]
- ASoC: test-component: Migrate to new style legacy DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic31xx: Add support for pll_r coefficient (Jaroslav Kysela) [2125544]
- ASoC: ssm4567: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: rk3328: fix disabling mclk on pclk probe failure (Jaroslav Kysela) [2125544]
- ASoC: pcm3060: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: cs42l42: remove redundant test (Jaroslav Kysela) [2125544]
- ALSA: ppc: beep: fix clang -Wimplicit-fallthrough (Jaroslav Kysela) [2125544]
- ASoC: soc-component: Add comment for the endianness flag (Jaroslav Kysela) [2125544]
- ASoC: codecs: wsa881x: handle timeouts in resume path (Jaroslav Kysela) [2125544]
- ASoC: wsa881x: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: codecs: wsa881x: add runtime pm support (Jaroslav Kysela) [2125544]
- ASoC: wm_adsp: Fix event generation for wm_adsp_fw_put() (Jaroslav Kysela) [2125544]
- ASoC: wm_adsp: Minor clean and redundant code removal (Jaroslav Kysela) [2125544]
- ASoC: wm_adsp: Compressed stream DSP memory structs should be __packed (Jaroslav Kysela) [2125544]
- ASoC: wm8998: Fix event generation for input mux (Jaroslav Kysela) [2125544]
- ASoC: arizona: Fix a wrong free in wm8997_probe (Jaroslav Kysela) [2125544]
- ASoC: wm8962: Allow switching between analog and digital inputs (Jaroslav Kysela) [2125544]
- ASoC: wm8960: Fix clock configuration on slave mode (Jaroslav Kysela) [2125544]
- ASoC: wm8962: Fix suspend while playing music (Jaroslav Kysela) [2125544]
- ASoC: codecs: wm8962: using pm_runtime_resume_and_get instead of pm_runtime_get_sync (Jaroslav Kysela) [2125544]
- ASoC: wm8960: Add ACPI support (Jaroslav Kysela) [2125544]
- ASoC: wm8958: Fix change notifications for DSP controls (Jaroslav Kysela) [2125544]
- ASoC: wm8940: add devicetree support (Jaroslav Kysela) [2125544]
- ASoC: wm*: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: wm8903: Fix the error handling of wm8903_i2c_probe() (Jaroslav Kysela) [2125544]
- ASoC: wm8731: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: arizona: Make the wm5102, wm5110, wm8997 and wm8998 drivers use the new jack library (Jaroslav Kysela) [2125544]
- ASoC: wm5102: Fix event generation for output compensation (Jaroslav Kysela) [2125544]
- ASoC: wcd9335: Use int array instead of bitmask for TX mixers (Jaroslav Kysela) [2125544]
- ASoC: wcd9335: Use DT bindings instead of local DAI definitions (Jaroslav Kysela) [2125544]
- ASoC: wcd9335: Fix spurious event generation (Jaroslav Kysela) [2125544]
- ASoC: wcd9335: Remove RX channel from old list before adding it to a new one (Jaroslav Kysela) [2125544]
- ASoC: codecs: wcd9335: move gains from SX_TLV to S8_TLV (Jaroslav Kysela) [2125544]
- ASoC: wcd9335: remove redundant tests (Jaroslav Kysela) [2125544]
- ASoC: uda1380: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: uda1334: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: twl4030: Drop legacy, non DT boot support (Jaroslav Kysela) [2125544]
- ASoC: tscs*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: ts3a227e: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: tpa6130: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: tlv320dac3x: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic33: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: codec: tlv320aic32x4: fix mono playback via I2S (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic32x4: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic31xx: Fix typo in BCLK clock name (Jaroslav Kysela) [2125544]
- ASoC: tlv320*: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: Rename tlv320aic31xx-micbias.h as tlv320aic31xx.h (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic31xx: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic26: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tlv320aic23: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tlv320*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: tas6424: Return zero in remove callback (Jaroslav Kysela) [2125544]
- ASoC: tda7419: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: tas6424: Fix the error handling of tas6424_i2c_probe() (Jaroslav Kysela) [2125544]
- ASoC: tas6424: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tas5720: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tas571x: Fix the error handling of tas571x_i2c_probe() (Jaroslav Kysela) [2125544]
- ASoC: tas5086: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tas2552: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: tas2770: Reinit regcache on reset (Jaroslav Kysela) [2125544]
- ASoC: tas2562: Propagate the error in tas2562_dac_event() (Jaroslav Kysela) [2125544]
- ASoC: tas2562: Fix mute/unmute (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Fix mute/unmute (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Drop conflicting set_bias_level power setting (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Allow mono streams (Jaroslav Kysela) [2125544]
- ASoC: tas2770: Fix handling of mute/unmute (Jaroslav Kysela) [2125544]
- ASoC: tas2770: Drop conflicting set_bias_level power setting (Jaroslav Kysela) [2125544]
- ASoC: tas2770: Allow mono streams (Jaroslav Kysela) [2125544]
- ASoC: tas2770: Set correct FSYNC polarity (Jaroslav Kysela) [2125544]
- ASoC: tas2770: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tas*: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: tas2552: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: sti-sas: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: sta350: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: sta350: Remove redundant big endian formats (Jaroslav Kysela) [2125544]
- ASoC: sta*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: sta32x: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: sta32x: Remove redundant big endian formats (Jaroslav Kysela) [2125544]
- ASoC: ssm2602: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: ssm2518: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: sgtl5000: Fix noise on shutdown/remove (Jaroslav Kysela) [2125544]
- ASoC: rt9120: Fix 3byte read, valule offset typo (Jaroslav Kysela) [2125544]
- ASoC: rt9120: Use pm_runtime and regcache to optimize 'pwdnn' logic (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt715-sdca: remove useless assignment of ops (Jaroslav Kysela) [2125544]
- ASoC: rt5682s: Separate the regulator consumer controls (Jaroslav Kysela) [2125544]
- ASoC: rt5645: Fix the error handling of rt5645_i2c_probe() (Jaroslav Kysela) [2125544]
- ASoC: rt5640: Fix the issue of the abnormal JD2 status (Jaroslav Kysela) [2125544]
- ASoC: rt5640: Fix the JD voltage dropping issue (Jaroslav Kysela) [2125544]
- ASoC: rt5640: Fix the wrong state of JD1 and JD2 (Jaroslav Kysela) [2125544]
- ASoC: rt5640: Add the MICBIAS1 to the dapm routing (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt298: Fix jack detection (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt298: Fix NULL jack in interrupt (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt298: Set component to NULL on remove (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt286: Set component to NULL on remove (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt274: Set component to NULL on remove (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt274: Always init jack_detect_work (Jaroslav Kysela) [2125544]
- ASoC: rt1308-sdw: add the default value of register 0xc320 (Jaroslav Kysela) [2125544]
- ASoC: rk3328: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: pcm1789: Make pcm1789_common_exit() return void (Jaroslav Kysela) [2125544]
- ASoC: pcm186x: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: pcm186x: simplify the return expression of pcm186x_power_off() (Jaroslav Kysela) [2125544]
- ASoC: pcm*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: nau8825: Implement hw constraint for rates (Jaroslav Kysela) [2125544]
- ASoC: nau8825: Declare 2 channels for DAI of capture stream (Jaroslav Kysela) [2125544]
- ASoC: nau8824: Fix semaphore is released unexpectedly (Jaroslav Kysela) [2125544]
- ASoC: nau8824: Implement hw constraint for rates (Jaroslav Kysela) [2125544]
- ASoC: nau8824: Fix semaphore unbalance at error paths (Jaroslav Kysela) [2125544]
- ASoC: nau8822: Don't reconfigure PLL to the same values (Jaroslav Kysela) [2125544]
- ASoC: nau8822: Disable internal PLL if freq_out is zero (Jaroslav Kysela) [2125544]
- ASoC: nau8821: Implement hw constraint for rates (Jaroslav Kysela) [2125544]
- ASoC: nau8821: Don't unconditionally free interrupt (Jaroslav Kysela) [2125544]
- ASoC: nau8821: add new widget to control system clock (Jaroslav Kysela) [2125544]
- ASoC: nau8821: Add headset button detection (Jaroslav Kysela) [2125544]
- ASoC: codecs: mt6359-accdet: remove useless initialization (Jaroslav Kysela) [2125544]
- ASoC: mediatek: mt6366: support for mt6366 codec (Jaroslav Kysela) [2125544]
- ASoC: msm8916-wcd-digital: Check failure for devm_snd_soc_register_component (Jaroslav Kysela) [2125544]
- ASoC: nau8540: Implement hw constraint for rates (Jaroslav Kysela) [2125544]
- ASoC: nau8*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: mt6660: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: mt6359: Fix refcount leak bug (Jaroslav Kysela) [2125544]
- ASoC: mediatek: mt6358: add missing EXPORT_SYMBOLs (Jaroslav Kysela) [2125544]
- ASoC: msm8916-wcd-digital: Fix missing clk_disable_unprepare() in msm8916_wcd_digital_probe (Jaroslav Kysela) [2125544]
- ASoC: codecs: msm8916-wcd-digital: move gains from SX_TLV to S8_TLV (Jaroslav Kysela) [2125544]
- ASoC: ml26124: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: max9860: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: max98390: use linux/gpio/consumer.h to fix build (Jaroslav Kysela) [2125544]
- ASoC: max98390: Add reset gpio control (Jaroslav Kysela) [2125544]
- ASoC: codecs: soundwire: call pm_runtime_resume() in component probe (Jaroslav Kysela) [2125544]
- ASoC: max98373: Removing 0x203E from the volatile reg (Jaroslav Kysela) [2125544]
- ASoC: max98090: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: max98090: Fix event generation for custom controls (Jaroslav Kysela) [2125544]
- ASoC: codecs: max98088: Clean up some inconsistent indenting (Jaroslav Kysela) [2125544]
- ASoC: max980*: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: lm4857: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: da732x: Drop no-op remove function (Jaroslav Kysela) [2125544]
- ASoC: da7219: Drop no-op remove function (Jaroslav Kysela) [2125544]
- ASoC: max9*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: lm49xxx: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: hdmi-codec: Remove redundant big endian formats (Jaroslav Kysela) [2125544]
- ASoC: es83*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: codes: Add support for ES8316 producer mode (Jaroslav Kysela) [2125544]
- ASoC: dmic: Add support for DSD data format (Jaroslav Kysela) [2125544]
- ASoC: da[79]*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: da7219: cancel AAD related work earlier for jack removal (Jaroslav Kysela) [2125544]
- ASoC: da7219: Fix pole orientation detection on certain headsets (Jaroslav Kysela) [2125544]
- ASoC: da7218: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: cx2072x: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: cx2072x: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: cs4349: Remove redundant big endian formats (Jaroslav Kysela) [2125544]
- ASoC: cs42l56: Fix the error handling of cs42l56_i2c_probe() (Jaroslav Kysela) [2125544]
- ASoC: cs42l51: Remove redundant big endian formats (Jaroslav Kysela) [2125544]
- ASoC: cs42l42: Only report button state if there was a button interrupt (Jaroslav Kysela) [2125544]
- ASoC: cs4270: update kernel-doc (Jaroslav Kysela) [2125544]
- ASoC: cs4270: Remove redundant big endian formats (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Add support for CLSA3541 ACPI device ID (Jaroslav Kysela) [2125544]
- ALSA: cs35l41: Enable Internal Boost in shared lib (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Do not print error when waking from hibernation (Jaroslav Kysela) [2125544]
- ASoC: cs35l36: Fix the error handling of cs35l36_i2c_probe() (Jaroslav Kysela) [2125544]
- ASoC: cs*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: arizona: Update arizona_aif_cfg_changed to use RX_BCLK_RATE (Jaroslav Kysela) [2125544]
- ASoC: alc56*: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: ak4613: cares Simple-Audio-Card case for TDM (Jaroslav Kysela) [2125544]
- ASoC: ak4613: add TDM256 support (Jaroslav Kysela) [2125544]
- ASoC: ak4613: rename constraint to constraint_rates (Jaroslav Kysela) [2125544]
- ASoC: ak4613: priv has ctrl1 instead of iface (Jaroslav Kysela) [2125544]
- ASoC: ak4613: return error if it was setup as clock provider (Jaroslav Kysela) [2125544]
- ASoC: ak4613: tidyup ak4613_interface (Jaroslav Kysela) [2125544]
- ASoC: ak4613: add missing mutex_lock() (Jaroslav Kysela) [2125544]
- ASoC: ak4642: Drop no-op remove function (Jaroslav Kysela) [2125544]
- ASoC: ak*: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: ak4*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: adau1761: Add ADAU1761-as-ADAU1361 compatibility mode (Jaroslav Kysela) [2125544]
- ASoC: ada*, ssm*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: ab8500: Remove some leftover from the "Replace GPLv2 boilerplate/reference with SPDX" rules (Jaroslav Kysela) [2125544]
- ASoC: ad1*, ada*, ssm*: use i2c_match_id and simple i2c probe (Jaroslav Kysela) [2125544]
- ASoC: test-component: Rename set_fmt_new back to set_fmt (Jaroslav Kysela) [2125544]
- ASoC: simple-card-utils: rename asoc_simple_init_dai_link_params() to asoc_simple_init_for_codec2codec() (Jaroslav Kysela) [2125544]
- ASoC: simple-card-utils.c: care Codec2Codec vs DPCM:BE (Jaroslav Kysela) [2125544]
- ASoC: simple-card-utils.c: ignore Codec2Codec setting if it already have (Jaroslav Kysela) [2125544]
- ASoC: simple-card-utils: Make asoc_simple_clean_reference() return void (Jaroslav Kysela) [2125544]
- ASoC: audio-graph-card2: indicate "Experimental stage" warning only when successed (Jaroslav Kysela) [2125544]
- ASoC: audio-graph-card2: Add of_node_put() in fail path (Jaroslav Kysela) [2125544]
- ASoc: audio-graph-card2: Fix refcount leak bug in __graph_get_type() (Jaroslav Kysela) [2125544]
- ASoC: audio-graph-card2.c: remove pre-alloced Codec2Codec space (Jaroslav Kysela) [2125544]
- ASoC: audio-graph-card2.c: make Codec2Codec settings optional (Jaroslav Kysela) [2125544]
- ASoC: audio-graph-card2.c: use of_property_read_u32() for rate (Jaroslav Kysela) [2125544]
- ASoC: audio_graph_card2: Fix port numbers in example (Jaroslav Kysela) [2125544]
- ASoC: audio-graph-card2-custom-sample.dtsi: add verbose explanation (Jaroslav Kysela) [2125544]
- ASoC: audio-graph-card: Add of_node_put() in fail path (Jaroslav Kysela) [2125544]
- ASoC: test-component: Update to use set_fmt_new callback (Jaroslav Kysela) [2125544]
- ASoC: Intel: boards: use software node API in Atom boards (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_ssp_amp: remove 'set-but-not-used' warning (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_sdw: avoid oops in error handling (Jaroslav Kysela) [2125544]
- ASoC: Intel: use software node API in SoundWire machines (Jaroslav Kysela) [2125544]
- ASoC: Intel: boards: sof_sdw: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: Intel: catpt: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: Intel: catpt: Drop redundant enum constant (Jaroslav Kysela) [2125544]
- ASoC: Intel: catpt: remove duplicating driver data retrieval (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_ssp_amp: enable capture stream from cs35l41 (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_sdw: allow HDaudio/HDMI disable (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_sdw: add quirk for HP Omen 16-k0005TX (Jaroslav Kysela) [2125544]
- ASoC: intel: sof_sdw: add RT711 SDCA card for MTL platform (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_pcm512x: remove unnecessary init (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_nau8825: Move quirk check to the front in late probe (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_sdw: add support for Dell SKU 0AFF (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_sdw: add support for Dell SKU 0AF0 (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_rt5682: Perform quirk check first in card late probe (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_rt5682: Add support for mtl_mx98357_rt5682 (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_rt5682: fix out-of-bounds array access (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_rt5682: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: boards: rename RTL1019 compatible driver to rt1019p (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_nau8825: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: kbl_da7219_max98927: remap jack pins (Jaroslav Kysela) [2125544]
- ALSA: x86: intel_hdmi_audio: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ALSA: x86: intel_hdmi_audio: enable pm_runtime and set autosuspend delay (Jaroslav Kysela) [2125544]
- ASoC: xtensa: Update to use set_fmt_new callback (Jaroslav Kysela) [2125544]
- ASoC: xtensa: Migrate to new style legacy DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: uniphier: make arrays mul and div static const, makes object smaller (Jaroslav Kysela) [2125544]
- ASoC: uniphier: simplify the return expression of uniphier_aio_compr_set_params() (Jaroslav Kysela) [2125544]
- ASoC: spear: Migrate to new style legacy DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-topology: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-stream: test DMA buffer first in hw_params (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-stream: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-ipc: Do not process IPC reply before firmware boot (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dsp: report error on power-up/down (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: Drop misleading comment regarding dma_data (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: Intel: fix sof_es8336 probe (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_es8336: remove hard-coded SSP selection (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_es8336: reset the num_links during probe (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_es8336: add support for HDMI_In capture (Jaroslav Kysela) [2125544]
- ASoC: Intel: common: fix typo for tplg naming (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_rt5682: Add support for adl_rt1019_rt5682s (Jaroslav Kysela) [2125544]
- ASoC: Intel: soc-acpi: add table for HP Omen 16-k0005TX (Jaroslav Kysela) [2125544]
- ASoC: Intel: soc-acpi: Add entry for sof_es8336 in ADL match table (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_es8336: ignore GpioInt when looking for speaker/headset GPIO lines (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_es8336: Fix GPIO quirks set via module option (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_da7219_max98373: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_cs42l42: add adl_mx98360a_cs4242 board config (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_cs42l42: support BT offload audio (Jaroslav Kysela) [2125544]
- ASoC: Intel: sof_cs42l42: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: skl_nau88l25_ssm4567: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: skl_nau88l25_max98357a: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: kbl_rt5663_rt5514_max98927: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: kbl_rt5663_max98927: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: kbl_da7219_max98357a: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: boards: hda: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: Intel: glk_rt5682_max98357a: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: cml_rt1011_rt5682: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: boards: Use temporary variable for struct device (Jaroslav Kysela) [2125544]
- ASoC: Intel: boards: reset acpi_chan_package (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt298: Reorganize jack detect handling (Jaroslav Kysela) [2125544]
- ASoC: Intel: bxt_da7219_max98357a: remap jack pins (Jaroslav Kysela) [2125544]
- ASoC: Intel: hsw_rt5640: Mark BE DAI as nonatomic (Jaroslav Kysela) [2125544]
- ASoC: Intel: hsw_rt5640: Improve hw_params() debug-ability (Jaroslav Kysela) [2125544]
- ASoC: Intel: hsw_rt5640: Improve probe() function quality (Jaroslav Kysela) [2125544]
- ASoC: Intel: hsw_rt5640: Update file comments (Jaroslav Kysela) [2125544]
- ASoC: Intel: hsw_rt5640: Update code indentation (Jaroslav Kysela) [2125544]
- ASoC: Intel: hsw_rt5640: Reword driver name (Jaroslav Kysela) [2125544]
- ASoC: Intel: hsw_rt5640: Reword prefixes of all driver members (Jaroslav Kysela) [2125544]
- ASoC: Intel: Rename haswell source file to hsw_rt5640 (Jaroslav Kysela) [2125544]
- ASoC: Intel: atom: sst_ipc: remove redundant test (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Mark BE DAI as nonatomic (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Remove FE DAI ops (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Improve codec_init() quality (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Improve hw_params() debug-ability (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Improve probe() function quality (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Update file comments (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Update code indentation (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Reword driver name (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt286: Reword prefixes of all driver members (Jaroslav Kysela) [2125544]
- ASoC: Intel: Rename broadwell source file to bdw_rt286 (Jaroslav Kysela) [2125544]
- ASoC: codecs: rt286: Reorganize jack detect handling (Jaroslav Kysela) [2125544]
- ASoC: Intel: broadwell: Make broadwell_disable_jack() return void (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt5677: Mark BE DAI as nonatomic (Jaroslav Kysela) [2125544]
- ASoC: Intel: bdw_rt5650: Mark BE DAI as nonatomic (Jaroslav Kysela) [2125544]
- ASoC: Intel: atom: sst_ipc: remove useless initializations (Jaroslav Kysela) [2125544]
- ASoC: Intel: atom: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: Intel: atom: sst: remove useless initialization (Jaroslav Kysela) [2125544]
- ASoC: intel: atom: Remove superfluous flush_scheduled_work() (Jaroslav Kysela) [2125544]
- ASoC: Intel: Update to use set_fmt_new callback (Jaroslav Kysela) [2125544]
- ASoC: Intel: atom: controls: remove useless initializations (Jaroslav Kysela) [2125544]
- ASoC: Intel: Migrate to new style legacy DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: Intel: skylake: skl-pcm: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: Intel: Skylake: remove redundant re-assignments to pointer array (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: bdw: remove duplicating driver data retrieval (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: byt: remove duplicating driver data retrieval (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: cnl: Do not process IPC reply before firmware boot (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: Do snd_hdac_ext_stream_decouple() only once (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: Fix potential buffer overflow by snprintf() (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: add sanity check on SSP index reported by NHLT (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: only fixup topology name if not set already (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: don't set fw_filename (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: enable dmic handling with 2 or fewer SoundWire links (Jaroslav Kysela) [2125544]
- ASoC: soc-core: accept zero format at snd_soc_runtime_set_dai_fmt() (Jaroslav Kysela) [2125544]
- ASoC: SOF: compress: Prevent current kernel running with older FW (Jaroslav Kysela) [2125544]
- ASoC: SOF: Copy compress parameters into extended data (Jaroslav Kysela) [2125544]
- ASoC: SOF: compress: Dynamically allocate pcm params struct (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: atom: don't keep a temporary string in fixup_tplg_name (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: add trigger callback into sdw_callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: Correct the ROM/FW state reporting code (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: MTL: remove redundant snd_sof_dsp_read() call (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: mtl: Do not process IPC reply before firmware boot (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: mtl: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: Introduce skip_imr_boot flag (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: disable IMR boot when resuming from ACPI S4 and S5 states (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: IPC4: enable IMR boot (Jaroslav Kysela) [2125544]
- ASoC: SOC: Intel: introduce cl_init callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: Do not (wrongly) assume positive return value in IMR path (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: Revisit IMR boot sequence (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-dtrace: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-loader: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-loader: Print out the non matching ext_man magic number (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-topology: Fix clang -Wformat warning (Jaroslav Kysela) [2125544]
- ASoC: SOF: remove warning on ABI checks (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Fix error code in sof_ipc4_volume_put() (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-pcm: set pcm rate to dai setting (Jaroslav Kysela) [2125544]
- ASoC: SOF: reduce default verbosity of IPC logs (Jaroslav Kysela) [2125544]
- Revert "RedHat: ASoC: SOF: Intel: do not enable IMR boot when resuming by default" (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: fix alh_group_ida max value (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: fix wrong use of sizeof in sof_ipc4_widget_setup_comp_src() (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: set domain bit based on dp domain type (Jaroslav Kysela) [2125544]
- ASoC: SOF: add ipc4 SRC module support (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: move ida allocate/free to widget_setup/free (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: free memories allocated in sof_ipc4_get_audio_fmt (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: check dai->private in ipc_free() (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: add SoundWire/ALH aggregation support (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ASoC: SOF: Compile and runtime IPC version selection (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Align mt8186 clock names with dt-bindings (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Fix error code in probe (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Revise mt8195 boot flow (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: fix mt8195 StatvectorSel wrong setting (Jaroslav Kysela) [2125544]
- ASoC: SOF: pcm: use pm_resume_and_get() on component probe (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc-msg-injector: fix copy in sof_msg_inject_ipc4_dfs_write() (Jaroslav Kysela) [2125544]
- ASoC: sof: Migrate to new style legacy DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client-probes: Only load the driver if IPC3 is used (Jaroslav Kysela) [2125544]
- ASoC: SOF: probes: rename assign/free callbacks as startup/shutdown (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add cont_update_posn to platform parameters (Jaroslav Kysela) [2125544]
- ASoC: SOF: pm: add definitions for S4 and S5 states (Jaroslav Kysela) [2125544]
- ASoC: SOF: pm: add explicit behavior for ACPI S1 and S2 (Jaroslav Kysela) [2125544]
- ASoC: SOF: debug: Clarify the IPC timeout handling path (Jaroslav Kysela) [2125544]
- ASoC: SOF: topology: remove unused variable (Jaroslav Kysela) [2125544]
- ASoC: SOF: Switch to IPC generic firmware tracing (Jaroslav Kysela) [2125544]
- ALSA: sc6000: Fix the missing snd_card_free() call at probe error (Jaroslav Kysela) [2125544]
- ALSA: gus: Fix memory leaks at memory allocator error paths (Jaroslav Kysela) [2125544]
- ALSA: sound/isa/gus: check the return value of kstrdup() (Jaroslav Kysela) [2125544]
- ALSA: gus: Fix erroneous memory allocation (Jaroslav Kysela) [2125544]
- ALSA: galaxy: Fix the missing snd_card_free() call at probe error (Jaroslav Kysela) [2125544]
- ALSA: cs4236: fix an incorrect NULL check on list iterator (Jaroslav Kysela) [2125544]
- ALSA: aloop: Fix random zeros in capture data when using jiffies timer (Jaroslav Kysela) [2125544]
- ALSA: Add generic serial MIDI driver using serial bus API (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Fix potential buffer overflow by snprintf() (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Use lookup table to create modules (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Update AVS_FW_INIT_TIMEOUT_US declaration (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Lower UNLOAD_MULTIPLE_MODULES IPC timeout (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Replace hardcodes with SD_CTL_STREAM_RESET (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Recognize FW_CFG_RESERVED (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Use helper function to set up DMA (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Set max DMA segment size (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Block IPC channel on suspend (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Shield LARGE_CONFIG_GETs against zero payload_size (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Copy only as many RX bytes as necessary (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Relax DSP core transition timings (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Assign I2S gateway when parsing topology (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Fix i2s_test card name initialization (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: correct config reference for I2S test board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Fix parsing UUIDs in topology (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add da7219 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add max98373 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add max98357a machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add ssm4567 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add nau8825 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add rt5682 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add rt298 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add rt286 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add rt274 machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add I2S-test machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add DMIC machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Fix build error on arc, m68k and sparc (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: APL-based platforms support (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: SKL-based platforms support (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Power management (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Machine board registration (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Replace link_mask usage with i2s_link_mask (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Event tracing (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: D0ix power state support (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Prepare for firmware tracing (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Register HDAudio ext-bus operations (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add HDAudio machine board (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: PCI driver implementation (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Coredump and recovery flow (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Drop direct ACPI dependency (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Depend on SND_INTEL_DSP_CONFIG (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Enable AVS driver only on x86 platforms (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: HDA PCM BE operations (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: non-HDA PCM BE operations (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Generic PCM FE operations (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Generic soc component driver (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Account for libraries when booting basefw (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Configure modules according to their type (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Prepare modules before bindings them (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Arm paths after creating them (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Path state management (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Path creation and freeing (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Declare path and its components (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Support link_mask formatted string (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add topology loading operations (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Parse path and path templates tuples (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Parse pipeline and module tuples (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Parse pplcfg and binding tuples (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Parse module-extension tuples (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Add topology parsing infrastructure (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: add MeteorLake machines (Jaroslav Kysela) [2125544]
- ASoC: Intel: avs: Declare vendor tokens (Jaroslav Kysela) [2125544]
- ASoC: SOF: dai-intel: add SOF_DAI_INTEL_SSP_CLKCTRL_MCLK_AON bit (Jaroslav Kysela) [2125544]
- uapi: sof: abi: Bump SOF ABI for ext_data_length (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add two new structures for topology manifest data (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: introduce cont_update_posn in sof_ipc_stream_params struct (Jaroslav Kysela) [2125544]
- ASoC: SOF: bump SOF_ABI_MINOR (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add header for IPC4 manifest (Jaroslav Kysela) [2125544]
- ASoC: SOF: topology: add code to parse config params for ACPDMIC dai (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add topology tokens for IPC4 (Jaroslav Kysela) [2125544]
- ASoC: hdac_hda: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: max98504: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: adau1372: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: cx2072x: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: mt6351: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: mt6358: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: mt6359: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: mt6660: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: pcm3060: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: rt9120: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: wcd9335: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: rt700: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: rt715: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: rt715-sdca: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: rt1308-sdw: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: rt1316-sdw: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: wsa881x: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: sdw-mockup: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: lochnagar: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: lochnagar: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: tfa*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: tfa9879: Use modern ASoC DAI format terminology (Jaroslav Kysela) [2125544]
- ASoC: tlv320*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: cs*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: wm*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: wm9090: Remove redundant endianness flag (Jaroslav Kysela) [2125544]
- ASoC: wm8731: Factor out the I2C and SPI bus code into separate modules (Jaroslav Kysela) [2125544]
- ASoC: wm8731: Factor our MCLK and mutex initialisation (Jaroslav Kysela) [2125544]
- ASoC: wm8731: Move regulator request into wm8731_init() (Jaroslav Kysela) [2125544]
- ASoC: wm8731: Factor component init out of bus code (Jaroslav Kysela) [2125544]
- ASoC: wm8731: Update to modern DAI terminology (Jaroslav Kysela) [2125544]
- ASoC: wm2000: fix missing clk_disable_unprepare() on error in wm2000_anc_transition() (Jaroslav Kysela) [2125544]
- ASoC: wm2000: Remove redundant endianness flag (Jaroslav Kysela) [2125544]
- ASoC: wm*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Fix amp gain register offset & default (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Correct playback volume range (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Fix and extend FSYNC polarity handling (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Add post reset delays (Jaroslav Kysela) [2125544]
- ASoC: tas*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: tas*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: tas2764: constify static struct snd_soc_dai_ops (Jaroslav Kysela) [2125544]
- ASoC: tas*: sync parameter naming (rate/sample_bits) (Jaroslav Kysela) [2125544]
- ASoC: tas2764: Add the driver for the TAS2764 (Jaroslav Kysela) [2125544]
- ASoC: max98396: Fix TDM mode BSEL settings (Jaroslav Kysela) [2125544]
- ASoC: max*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: max98396: Implement DSP speaker monitor (Jaroslav Kysela) [2125544]
- ASoC: max98396: Fix register access for PCM format settings (Jaroslav Kysela) [2125544]
- ASoC: max98396: Improve some error prints (Jaroslav Kysela) [2125544]
- ASoC: max98396: add voltage regulators (Jaroslav Kysela) [2125544]
- ASoC: max98396: Fix build error for implicit function declaration (Jaroslav Kysela) [2125544]
- ASoC: max98396: add amplifier driver (Jaroslav Kysela) [2125544]
- ASoC: rt*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: rt1019: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: rt*: use simple i2c probe function (Jaroslav Kysela) [2125544]
- ASoC: fsl: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: pistachio: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: samsung: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: sunxi: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: tegra: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: test-component: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: uniphier: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ad*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ak*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: alc*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: da*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: es*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: msm*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: nau*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: pcm*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: spdif: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ssm*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: sta*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: twl*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: uda*: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: 88pm860x: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ab8500: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ac97: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ads117x: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: bd28623: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: bt-sco: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: cpcap: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: cq93vc: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: cx20442: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: dmic: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: gtm601: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: hdac_hdmi: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: hdmi-codec: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ics43432: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: inno_rk3036: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: isabelle: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: jz4740: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: lm49453: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: mc13783: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: ml26124: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: sgtl5000: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: si476x: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: stac9766: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: sti-sas: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: tscs42xx: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: wl1273: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: zl38060: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: fsl_micfil: Add legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: fsl_asrc_dma: Add legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: soc-component: Remove non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: simple-card-utils: Move snd_soc_component_is_codec to be local (Jaroslav Kysela) [2125544]
- ASoC: soc-component: Add legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: core: Add new SOC_DOUBLE_SX_TLV macro (Jaroslav Kysela) [2125544]
- ASoC: Remove unused hw_write_t type (Jaroslav Kysela) [2125544]
- ASoC: soc.h: Add SOC_SINGLE_S_EXT_TLV macro (Jaroslav Kysela) [2125544]
- ASoC: soc.h: Introduce SOC_DOUBLE_R_S_EXT_TLV() macro (Jaroslav Kysela) [2125544]
- ASoC: soc.h: Add SOC_SINGLE_S_TLV() macro (Jaroslav Kysela) [2125544]
- ASoC: hdmi-codec: Update to modern DAI terminology (Jaroslav Kysela) [2125544]
- ALSA: hda: Skip event processing for unregistered codecs (Jaroslav Kysela) [2125544]
- ASoC: codecs: Add HD-Audio codec driver (Jaroslav Kysela) [2125544]
- ASoC: cs42l42: Move CS42L42 register descriptions to general include (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Read System Name from ACPI _SUB to identify firmware (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Add common cs35l41 enter hibernate function (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Move cs35l41 exit hibernate function into shared code (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Move cs_dsp config struct into shared code (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Move cs35l41 fs errata into shared code (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Move cs35l41_set_cspl_mbox_cmd to shared code (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Add endianness flag in snd_soc_component_driver (Jaroslav Kysela) [2125544]
- ASoC: cs35l41: Support external boost (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: Add support for MeteorLake (MTL) (Jaroslav Kysela) [2125544]
- treewide: Replace zero-length arrays with flexible-array members (Jaroslav Kysela) [2125544]
- ASoC: SOF: add definitions for different IPC types (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: enhance debug messages (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-dtrace: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: SOF: IPC4: add sdw blob (Jaroslav Kysela) [2125544]
- AsoC: SOF: ipc4-topology: Add dai_get_clk op (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add support for SSP/DMIC DAI's (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add a new IPC op for parsing topology manifest (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: init NHLT for IPC4 (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add ops_free (Jaroslav Kysela) [2125544]
- ASoC: SOF: IPC4: set the BE DAI ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-pcm: Expose sof_ipc4_set_pipeline_state() (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add the dai_config op (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add route_setup/route_free ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add widget_setup/widget_free ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: IPC4: Add pcm ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add control IO ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add control_setup op (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add support for parsing mixer widgets (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add support for parsing and preparing pga widgets (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add prepare op for DAI type widgets (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add prepare op for AIF type widgets (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add support for parsing DAI_IN/DAI_OUT widgets (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4-topology: Add support for parsing AIF_IN/AIF_OUT widgets (Jaroslav Kysela) [2125544]
- ASoC: SOF: IPC4: Introduce topology ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-dtrace: Return from dtrace_read if there is no new data available (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-dtrace: Add helper function to update the sdev->host_offset (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-dtrace: Introduce SOF_DTRACE_INITIALIZING state (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4: implement pm ctx_save callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: Switch to use the generic pm_ops.set_core_state (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4: Add set_core_state pm_ops implementation (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add initial header file for ipc4 (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Add set_core_state pm_ops implementation (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof_ipc_pm_ops: Add support for DSP core power management (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: mt8195 suspend check dsp idle (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: mt8195 modify dram type as non-cache (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add shared_size for mediatek common chip information (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: revise mt8195 clock sequence (Jaroslav Kysela) [2125544]
- ASoC: SOF: amd: Add SOF pm ops callback for Renoir (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc-msg-injector: Fix reversed if statement (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc-msg-injector: Propagate write errors correctly (Jaroslav Kysela) [2125544]
- ASoC: SOF: Fix potential NULL pointer dereference (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client-ipc-flood-test: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: remove duplicate include in mt8195.c (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add mt8195 debug dump (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add mediatek common debug dump (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-dtrace: Move dtrace related variables local from sof_dev (Jaroslav Kysela) [2125544]
- ASoC: SOF: Introduce opaque storage of private data for firmware tracing (Jaroslav Kysela) [2125544]
- ASoC: SOF: Modify the host trace_init parameter list to include dmab (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-dtrace: Move host ops wrappers from generic header to private (Jaroslav Kysela) [2125544]
- ASoC: SOF: Clone the trace code to ipc3-dtrace as fw_tracing implementation (Jaroslav Kysela) [2125544]
- ASoC: SOF: Rename dtrace_is_supported flag to fw_trace_is_supported (Jaroslav Kysela) [2125544]
- ASoC: SOF: Introduce IPC independent ops for firmware tracing support (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc-msg-injector: Cap the rmaining to count in IPC4 mode (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add mt8186 ipc support (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add ipc support for mt8195 (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: HDA: Set up sof_ipc4_fw_data for IPC4 (Jaroslav Kysela) [2125544]
- ASoC: SOF: IPC4: Add FW loader ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add IPC4 private header (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: HDA: Set IPC4-specific DSP ops for CaVS platforms (Jaroslav Kysela) [2125544]
- ASoC: SOF: trace: The dtrace is only available with SOF_IPC (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client: IPC flood test can only work with SOF_IPC (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc-msg-injector: Add support for IPC4 messages (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc-msg-injector: Separate the message sending (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client: Add support IPC4 message sending (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client: Add API to get the ipc_type (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client-probes: Query the maximum IPC payload size (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc-msg-injector: Query the maximum IPC payload size (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client: Add API to get the maximum IPC payload size (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc4: Add support for mandatory message handling functionality (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add rx_data pointer to snd_sof_ipc_msg struct (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Remove the ipc3-ops.h header file (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-pci-dev: fix missing pci_release_regions() on error in sof_pci_probe() (Jaroslav Kysela) [2125544]
- ASoC: SOF: loader: Call optional query_fw_configuration on first boot (Jaroslav Kysela) [2125544]
- ASoC: SOF: loader: Remove snd_sof_parse_module_memcpy() as it is not used (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: mt8195: Do not set the load_module ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: bdw/byt/pci-tng: Do not set the load_module ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: imx: Do not set the load_module ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: amd: renoir: Do not set the load_module ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: loader: Switch to use the fw_loader ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Add check for fw_loader ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3-loader: Implement firmware parsing and loading (Jaroslav Kysela) [2125544]
- ASoC: SOF: Introduce IPC dependent ops for firmware handling, loading (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add a prepare op to IPC topology widget ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: clarify use of widget complete flag (Jaroslav Kysela) [2125544]
- ASoC: SOF: topology: Skip parsing DAI link tokens if not needed (Jaroslav Kysela) [2125544]
- ASoC: SOF: pcm: remove unnecessary function declaration (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add two new fields to struct snd_sof_widget (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add a route_free op in struct sof_ipc_tplg_ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: expose a couple of functions (Jaroslav Kysela) [2125544]
- ASoC: SOF: pcm: Move the call to snd_sof_pcm_platform_hw_params() (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-audio: Set up widgets from source to sink (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-audio: reset route status before freeing widget (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add a new op to set up volume table (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Fix allyesconfig build error (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: mt8195 change ipc timeout as 1 second (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-client-ipc-msg-injector: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: SOF: debug: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: SOF: control: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add DSP system PM callback for mt8186 (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add mt8186 dsp clock support (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add mt8186 sof fw loader and dsp ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: Add mt8186 hardware support (Jaroslav Kysela) [2125544]
- ASoC: SOF: loader: Remove the old fw_ready related code (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: Do not set fw_ready callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: imx: Do not set fw_ready callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: amd: Do not set fw_ready callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: Do not check for the fw_ready callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Add local implementation for handling fw_ready message (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: protect hw_params against successive calls (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: add helper for link DMA cleanups (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: reset dma_data and release stream (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: improve suspend case (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: move code to deal with hda dai/dailink suspend (Jaroslav Kysela) [2125544]
- ASOC: SOF: Intel: hda-dai: add hda_dai_hw_free_ipc() helper (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-audio: flag errors on pipeline teardown (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: regroup dai and link DMA operations (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: split link DMA and dai operations (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: use snd_soc_dai_get_widget() helper (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-dai: simplify hda_dai_widget_update() prototype (Jaroslav Kysela) [2125544]
- ASOC: SOF: Intel: hda-dai: consistent naming for HDA DAI and HDA link DMA (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: Add IPC-specific dai ops for IPC3 (Jaroslav Kysela) [2125544]
- ASoC: SOF: remove incorrect clearing of prepared flag (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: simplify NHLT handling (Jaroslav Kysela) [2125544]
- ASoC: SOF: topology: Check w->sname validity once in sof_connect_dai_widget() (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-audio: remove useless assignment (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: pci-tgl: add RPL-P support (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: pci-tgl: add ADL-PS support (Jaroslav Kysela) [2125544]
- ASOC: SOF: pci: add ipc_type override for Intel IPC4 tests (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-pci-dev: don't use the community key on APL Chromebooks (Jaroslav Kysela) [2125544]
- ASoC: SOF: amd: Use dedicated MBOX for ACP and PSP communication (Jaroslav Kysela) [2125544]
- ASoC: SOF: amd: Add psp_mbox_ready() and psp_send_cmd() callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: using pm_runtime_resume_and_get to simplify the code (Jaroslav Kysela) [2125544]
- ASoC: SOF: Kconfig: Make SND_SOC_SOF_HDA_PROBES tristate (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: add IP identifier (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: expose some codeloader functions (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: Define rom_status_reg in sof_intel_dsp_desc (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: define check_ipc_irq op (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: use BIT() macros for consistency (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: move HDA_CL_STREAM_FORMAT definition to header (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda: use common ops across platforms (Jaroslav Kysela) [2125544]
- ASoC: SOF: remove const qualifier for 'struct snd_sof_dsp_ops' (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-audio: preserve topology filename override in nocodec mode (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-pci-dev: add parameter to override topology filename (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-pci-dev: add parameter to override firmware filename (Jaroslav Kysela) [2125544]
- ASoC: SOF: add IPC-dependent file names (Jaroslav Kysela) [2125544]
- ASoC: SOF: add default IPC capability and file paths (Jaroslav Kysela) [2125544]
- ASoC: SOF: add path indirection to each IPC type (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: Check the bar size before remapping (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Move the ipc_set_get_comp_data() local to ipc3-control (Jaroslav Kysela) [2125544]
- ASoC: SOF: sof-audio: Use the widget_kcontrol_setup ops for kcontrol set up (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add widget_kcontrol_setup control ops for IPC3 (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Switch over to use the rx_msg ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Switch over to use the tx_msg and set_get_data ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Use the get_reply ops in snd_sof_ipc_get_reply() (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Add check for mandatory IPC message handling ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Separate the ops checks by functions/topics (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Implement rx_msg IPC ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Implement the get_reply IPC ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Implement the set_get_data IPC ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Use sof_ipc3_tx_msg() internally for message sending (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc3: Implement the tx_msg IPC ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add high level IPC IO callback definitions to ipc_ops (Jaroslav Kysela) [2125544]
- ASoC: SOF: Add helper function to prepare and send an IPC message (Jaroslav Kysela) [2125544]
- ASoC: SOF: mediatek: mt8195 add shutdown callback (Jaroslav Kysela) [2125544]
- ASoC: SOF: OF: Add shutdown callback for SOF OF device (Jaroslav Kysela) [2125544]
- ASoC: SOF: topology: Avoid open coded arithmetic in memory allocation (Jaroslav Kysela) [2125544]
- ASoC: SOF: topology: use new sound control LED layer (Jaroslav Kysela) [2125544]
- ASoC: SOF: Remove redundant return statements (Jaroslav Kysela) [2125544]
- ASoC: SOF: Remove header from struct snd_sof_ipc_msg (Jaroslav Kysela) [2125544]
- ASoC: SOF: Drop 'header' parameter from tx_message() API (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Use msg->reply_data directly in snd_sof_ipc_get_reply() (Jaroslav Kysela) [2125544]
- ASoC: SOF: disable dma trace in s0ix (Jaroslav Kysela) [2125544]
- ASoC: SOF: extend the interface to stop DMA trace (Jaroslav Kysela) [2125544]
- ASoC: SOF: Drop support for mapped control data (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Use ipc->max_payload_size for message/reply size checking (Jaroslav Kysela) [2125544]
- ASoC: SOF: ipc: Add max_payload_size field in struct snd_sof_ipc (Jaroslav Kysela) [2125544]
- ASoC: SOF: Remove dmab and dmab_bdl from snd_sof_dev struct (Jaroslav Kysela) [2125544]
- ASoC: SOF: Intel: hda-loader: Use local snd_dma_buffer (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: add missing platform_device_unregister() in acp_pci_probe() (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Fix initialization of ext_intr_stat1 in i2s_irq_handler() (Jaroslav Kysela) [2125544]
- ASoC: amd: vangogh: Use non-legacy DAI naming for cs35l41 (Jaroslav Kysela) [2125544]
- ASoC: amd: enable RPL Platform acp drivers build (Jaroslav Kysela) [2125544]
- ASoC: amd: add RPL Platform pci driver pm-ops (Jaroslav Kysela) [2125544]
- ASoC: amd: add RPL Platform init/de-init functions (Jaroslav Kysela) [2125544]
- ASoC: amd: add ACP PCI driver for RPL platform (Jaroslav Kysela) [2125544]
- ASoC: amd: add RPL Platform acp header file (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Add error handling cases (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Modify const resource struct variable to generic (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Drop superfluous mmap callback (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Modify local variables name to generic (Jaroslav Kysela) [2125544]
- ASoC: amd: yc: Decrease level of error message (Jaroslav Kysela) [2125544]
- ASoC: amd: yc: add new YC platform varaint support (Jaroslav Kysela) [2125544]
- ASoC: amd: fix Jadeite kconfig warning and build errors (Jaroslav Kysela) [2125544]
- ASoC: amd: Fix error pointer dereference (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Add legacy audio driver support for Rembrandt platform (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: ACP code generic to support newer platforms (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Remove rt1019_1 codec conf from machine driver (Jaroslav Kysela) [2125544]
- ASoC: amd: Remove duplicated include in acp-es8336.c (Jaroslav Kysela) [2125544]
- ASoC: amd: fix for variable set but not used warning (Jaroslav Kysela) [2125544]
- ASoC: amd: drop machine driver remove function (Jaroslav Kysela) [2125544]
- ASoC: amd: remove unused header file inclusion (Jaroslav Kysela) [2125544]
- ASoC: amd: acp-es8336: use static variables (Jaroslav Kysela) [2125544]
- ASoC: amd: fix ACPI dependency compile errors and warnings (Jaroslav Kysela) [2125544]
- ASoC: amd: enable machine driver build for Jadeite platform (Jaroslav Kysela) [2125544]
- ASoC: amd: add Machine driver for Jadeite platform (Jaroslav Kysela) [2125544]
- ASoC: amd: add I2S MICSP instance support (Jaroslav Kysela) [2125544]
- ASoC: amd: Migrate to new style legacy DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Fix error handling in .remove() (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: fix typo in comment (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Add support for rt5682s and rt1019 card with hs instance (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Add support for nau8825 and max98360 card (Jaroslav Kysela) [2125544]
- ASoC: amd: vangogh: Rename set_fmt_new back to set_fmt (Jaroslav Kysela) [2125544]
- ASoC: amd: vangogh: Update to use set_fmt_new callback (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Set Speaker enable/disable pin through rt1019 codec driver. (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Set Speaker enable/disable pin through rt1019 codec driver (Jaroslav Kysela) [2125544]
- ASoC: amd: vangogh: Remove duplicate include files (Jaroslav Kysela) [2125544]
- ASoC: amd: acp: Add pm ops callback in machine driver (Jaroslav Kysela) [2125544]
- ASoC: soc-utils: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: topology: Drop superfluous check of CONFIG_SND_CTL_VALIDATION (Jaroslav Kysela) [2125544]
- ASoC: topology: Rename soc_tplg_init_kcontrol() function (Jaroslav Kysela) [2125544]
- ASoC: topology: Correct error message (Jaroslav Kysela) [2125544]
- ASoC: topology: Rename SOC_TPLG_PASS_MIXER to _CONTROL (Jaroslav Kysela) [2125544]
- ASoC: topology: Return bool instead of int (Jaroslav Kysela) [2125544]
- ASoC: topology: Remove unnecessary looping (Jaroslav Kysela) [2125544]
- ASoC: topology: Use for loop instead of while (Jaroslav Kysela) [2125544]
- ASoC: topology: KUnit: Remove now redundant non_legacy_dai_naming flag (Jaroslav Kysela) [2125544]
- ASoC: topology: KUnit: Followup prototype change of snd_soc_unregister_card() (Jaroslav Kysela) [2125544]
- ASoC: DPCM: Don't pick up BE without substream (Jaroslav Kysela) [2125544]
- ASoC: soc-pcm: demote warnings on non-atomic BE connection (Jaroslav Kysela) [2125544]
- ASoC: soc-pcm: fix BE transition for TRIGGER_START (Jaroslav Kysela) [2125544]
- ASoC: soc-pcm: improve BE transition for TRIGGER_START (Jaroslav Kysela) [2125544]
- ASoC: soc-pcm: improve BE transition for PAUSE_RELEASE (Jaroslav Kysela) [2125544]
- ASoC: ops: Fix integer detection for when max possible values > 1 (Jaroslav Kysela) [2125544]
- ASoC: ops: Fix boolean/integer detection for simple controls (Jaroslav Kysela) [2125544]
- ASoC: ops: Don't modify the driver's plaform_max when reading state (Jaroslav Kysela) [2125544]
- ASoC: ops: Remove unneeded delay.h inclusion (Jaroslav Kysela) [2125544]
- ASoC: ops: Clarify snd_soc_info_volsw_sx() (Jaroslav Kysela) [2125544]
- ASoC: soc-generic-dmaengine-pcm: Use default config when none is given (Jaroslav Kysela) [2125544]
- ASoC: dapm: Move stereo autodisable check (Jaroslav Kysela) [2125544]
- ASoC: soc-dai: Remove set_fmt_new callback (Jaroslav Kysela) [2125544]
- ASoC: soc-core.c: share code for snd_soc_of_get_dai_link_cpus/codecs() (Jaroslav Kysela) [2125544]
- ASoC: soc-core.c: fixup snd_soc_of_get_dai_link_cpus() (Jaroslav Kysela) [2125544]
- ASoC: core: Switch core to new DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: core: Make snd_soc_unregister_card() return void (Jaroslav Kysela) [2125544]
- ASoC: core: Always send the CPU DAI a direct clock specifier (Jaroslav Kysela) [2125544]
- ASoC: core: Add set_fmt_new callback that directly specifies provider (Jaroslav Kysela) [2125544]
- ASoC: core: Pass legacy_dai_naming flag directly (Jaroslav Kysela) [2125544]
- ASoC: core: Correct spelling fliped -> flipped (Jaroslav Kysela) [2125544]
- ASoC: soc-core: remove always-false path (Jaroslav Kysela) [2125544]
- ASoC: Introduce snd_soc_of_get_dai_link_cpus (Jaroslav Kysela) [2125544]
- ASoC: soc-component: Update handling to component delays (Jaroslav Kysela) [2125544]
- ASoC: Introduce 'fixup_controls' card method (Jaroslav Kysela) [2125544]
- ASoC: soc-card: Create jack kcontrol without pins (Jaroslav Kysela) [2125544]
- ALSA: Replace acpi_bus_get_device() (Jaroslav Kysela) [2125544]
- Revert "ALSA: hda: cs35l41: Allow compilation test on non-ACPI configurations" (Jaroslav Kysela) [2125544]
- ALSA: hda: beep: Simplify keep-power-at-enable behavior (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: Don't skip notification handling during PM operation (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: Limit the maximal count of PCM devices to 8 (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: ELD procfs - print the codec NIDs (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: Simplify the pcm_idx condition in hdmi_pcm_setup_pin() (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: Fix the converter allocation for the silent stream (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: change type for the 'assigned' variable (Jaroslav Kysela) [2125544]
- ALSA: hda: intel-nhlt: Move structs out of #define block (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add a quirk for HP OMEN 16 (8902) mute LED (Jaroslav Kysela) [2125544]
- ALSA: hda/hdmi: Fix the converter reuse for the silent stream (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for ASUS GA503R laptop (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add pincfg for ASUS G533Z HP jack (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add pincfg for ASUS G513 HP jack (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Re-arrange quirk table entries (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Enable 4-speaker output Dell Precision 5530 laptop (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Enable 4-speaker output Dell Precision 5570 laptop (Jaroslav Kysela) [2125544]
- ALSA: hda: Fix Nvidia dp infoframe (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for Huawei WRT-WX9 (Jaroslav Kysela) [2125544]
- ALSA: hda/tegra: set depop delay for tegra (Jaroslav Kysela) [2125544]
- ALSA: hda: add Intel 5 Series / 3400 PCI DID (Jaroslav Kysela) [2125544]
- ALSA: hda: Fix hang at HD-audio codec unbinding due to refcount saturation (Jaroslav Kysela) [2125544]
- ALSA: emu10k1: Fix out of bounds access in snd_emu10k1_pcm_channel_alloc() (Jaroslav Kysela) [2125544]
- ALSA: hda/tegra: Align BDL entry to 4KB boundary (Jaroslav Kysela) [2125544]
- ALSA: hda/sigmatel: Fix unused variable warning for beep power change (Jaroslav Kysela) [2125544]
- ALSA: hda/sigmatel: Keep power up while beep is enabled (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add speaker AMP init for Samsung laptops with ALC298 (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for Clevo NS50PU, NS70PU (Jaroslav Kysela) [2125544]
- ALSA: hda/cs8409: Support new Dolphin Variants (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for Lenovo Yoga7 14IAL7 (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Clarify support for CSC3551 without _DSD Properties (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirks for ASUS Zenbooks using CS35L41 (Jaroslav Kysela) [2125544]
- ALSA: hda: Fix crash due to jack poll in suspend (Jaroslav Kysela) [2125544]
- ALSA: hda/cirrus - support for iMac 12,1 model (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add a quirk for HP OMEN 15 (8786) mute LED (Jaroslav Kysela) [2125544]
- ALSA: hda/conexant: Add quirk for LENOVO 20149 Notebook model (Jaroslav Kysela) [2125544]
- ALSA: ice1712: remove redundant assignment to new (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for another Asus K42JZ model (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for HP Spectre x360 15-eb0xxx (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for Clevo NV45PZ (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Add quirk for Lenovo Yoga9 14IAP7 (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Support CLSA0101 (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Use the CS35L41 HDA internal define (Jaroslav Kysela) [2125544]
- ALSA: hda/realtek: Enable speaker and mute LEDs for HP laptops (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Fix build error unused-function (Jaroslav Kysela) [2125544]
- ALSA: asihpi: fix repeated words in comments (Jaroslav Kysela) [2125544]
- ALSA: asihpi: Fix typo in comments (Jaroslav Kysela) [2125544]
- ALSA: emu10k1: Fix typo in comments (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Add module parameter to control firmware load (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Support Firmware switching and reloading (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Add defaulted values into dsp bypass config sequence (Jaroslav Kysela) [2125544]
- ALSA: hda: hda_cs_dsp_ctl: Add fw id strings (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Read Speaker Calibration data from UEFI variables (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Support Hibernation during Suspend (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Support Speaker ID for laptops (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Support multiple load paths for firmware (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Support reading subsystem id from ACPI (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Save Subsystem ID inside CS35L41 Driver (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Add initial DSP support and firmware loading (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Save codec object inside component struct (Jaroslav Kysela) [2125544]
- ALSA: hda: hda_cs_dsp_ctl: Add apis to write the controls directly (Jaroslav Kysela) [2125544]
- ALSA: hda: hda_cs_dsp_ctl: Add Library to support CS_DSP ALSA controls (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Consolidate selections under SND_HDA_SCODEC_CS35L41 (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Drop wrong use of ACPI_PTR() (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Allow compilation test on non-ACPI configurations (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Don't dereference fwnode handle (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Improve dev_err_probe() messaging (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Fix comments wrt serial-multi-instantiate reference (Jaroslav Kysela) [2125544]
- ALSA: hda: Fix put_device() inconsistency in error path (Jaroslav Kysela) [2125544]
- ALSA: hda: Make device usage_count consistent across subsequent probing (Jaroslav Kysela) [2125544]
- ALSA: hda: Fix null-ptr-deref when i915 fails and hdmi is denylisted (Jaroslav Kysela) [2125544]
- ALSA: hda/cs8409: change cs8409_fixups v.pins initializers to static (Jaroslav Kysela) [2125544]
- ASoC: doc: Update dead links (Jaroslav Kysela) [2125544]
- ALSA: hda/via: Delete does not require return (Jaroslav Kysela) [2125544]
- ALSA: ctxfi: fix typo in comment (Jaroslav Kysela) [2125544]
- ALSA: cs5535audio: fix typo in comment (Jaroslav Kysela) [2125544]
- ALSA: lola: Bounds check loop iterator against streams array size (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Add Amp Name based on channel and index (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Enable GPIO2 Interrupt for CLSA0100 laptops (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Add Support for Interrupts (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Remove Set Channel Map api from binding (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Set Speaker Position for CLSA0100 Laptop (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Fix error in spi cs35l41 hda driver name (Jaroslav Kysela) [2125544]
- ALSA: hda/cs8409: Add Speaker Playback Switch for Warlock (Jaroslav Kysela) [2125544]
- ALSA: hda/cs8409: Add Speaker Playback Switch for Cyborg (Jaroslav Kysela) [2125544]
- ALSA: hda/cs8409: Support new Odin Variants (Jaroslav Kysela) [2125544]
- ALSA: hda/cs8409: Support manual mode detection for CS42L42 (Jaroslav Kysela) [2125544]
- ALSA: hda/cs8409: Use general cs42l42 include in cs8409 hda driver (Jaroslav Kysela) [2125544]
- ALSA: hdsp: remove redundant assignment to pointer kctl (Jaroslav Kysela) [2125544]
- ALSA: hda/conexant: add a new hda codec SN6140 (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Move external boost handling to lib for ASoC use (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Handle all external boost setups the same way (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Reorganize log for playback actions (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Remove cs35l41_hda_reg_sequence struct (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Move boost config to initialization code (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Mute the device before shutdown (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Put the device into safe mode for external boost (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Add Boost type flag (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Always configure the DAI (Jaroslav Kysela) [2125544]
- ALSA: hda: cs35l41: Fix I2S params comments (Jaroslav Kysela) [2125544]
- ALSA: cs35l41: Move cs35l41_gpio_config to shared lib (Jaroslav Kysela) [2125544]
- ALSA: cs35l41: Check hw_config before using it (Jaroslav Kysela) [2125544]
- ALSA: cs35l41: Unify hardware configuration (Jaroslav Kysela) [2125544]
- ALSA: hda/tegra: Enable Jack poll for tegra (Jaroslav Kysela) [2125544]
- ALSA: hda: Jack detection poll in suspend state (Jaroslav Kysela) [2125544]
- ALSA: echoaudio: remove redundant assignment to variable i (Jaroslav Kysela) [2125544]
- ALSA: emu10k1: Stop using iommu_present() (Jaroslav Kysela) [2125544]
- ALSA: hda: intel-dsp-config: add missing RaptorLake PCI IDs (Jaroslav Kysela) [2125544]
- ALSA: hda: intel-nhlt: Correct the handling of fmt_config flexible array (Jaroslav Kysela) [2125544]
- ALSA: hda: Replace sprintf() with sysfs_emit() (Jaroslav Kysela) [2125544]
- ALSA: hda: Remove unused macro definition (Jaroslav Kysela) [2125544]
- ALSA: hda: Reset all SIE bits in INTCTL (Jaroslav Kysela) [2125544]
- tracing: ALSA: hda: Remove string manipulation out of the fast path (Jaroslav Kysela) [2125544]
- ALSA: hda: intel-nhlt: remove use of __func__ in dev_dbg (Jaroslav Kysela) [2125544]
- ALSA: hda: intel-dspcfg: use SOF for UpExtreme and UpExtreme11 boards (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Properly refcounting clock rate (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Clear fixed clock rate at closing EP (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Fix an out-of-bounds bug in __snd_usb_parse_audio_interface() (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Register card again for iface over delayed_register option (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Inform the delayed registration more properly (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Add quirk for LH Labs Geek Out HD Audio 1V5 (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: make read-only array marker static const (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: More comprehensive mixer map for ASUS ROG Zenith II (Jaroslav Kysela) [2125544]
- ALSA: scarlett2: Add Focusrite Clarett+ 8Pre support (Jaroslav Kysela) [2125544]
- ALSA: line6: Replace sprintf() with sysfs_emit() (Jaroslav Kysela) [2125544]
- ALSA: hiface: fix repeated words in comments (Jaroslav Kysela) [2125544]
- ALSA: usb/6fire: fix repeated words in comments (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Add quirk for Behringer UMC202HD (Jaroslav Kysela) [2125544]
- ALSA: bcd2000: Fix a UAF bug on the error path of probing (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Use atomic_try_cmpxchg in ep_state_update (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Add endianness annotations (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Turn off 'manual mode' on Dell dock (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Support jack detection on Dell dock (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: US16x08: Move overflow check before array access (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Cancel pending work at closing a MIDI substream (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Add mixer mapping for Gigabyte B450/550 Mobos (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Fix wrong kfree issue in snd_usb_endpoint_free_all (Jaroslav Kysela) [2125544]
- ALSA: usb-audio: Refcount multiple accesses on the single clock (Jaroslav Kysela) [2125544]
- mfd: arizona-spi: Add Android board ACPI table handling (Jaroslav Kysela) [2125544]
- mfd: arizona-spi: Split Windows ACPI init code into its own function (Jaroslav Kysela) [2125544]
- mfd: arizona: Add missing statics to the of_match_tables (Jaroslav Kysela) [2125544]
- firmware: cs_dsp: Add memory chunk helpers (Jaroslav Kysela) [2125544]
- firmware: cs_dsp: Add pre_stop callback (Jaroslav Kysela) [2125544]
- regmap: sdw: add required header files (Jaroslav Kysela) [2125544]
- regmap: soundwire: remove unused header mod_devicetable.h (Jaroslav Kysela) [2125544]
- regmap: Constify static regmap_bus structs (Jaroslav Kysela) [2125544]
- soundwire: peripheral: remove useless ops pointer (Jaroslav Kysela) [2125544]
- soundwire: intel: use pm_runtime_resume() on component probe (Jaroslav Kysela) [2125544]
- soundwire: qcom: fix device status array range (Jaroslav Kysela) [2125544]
- soundwire: qcom: remove duplicate reset control get (Jaroslav Kysela) [2125544]
- soundwire: Intel: add trigger callback (Jaroslav Kysela) [2125544]
- soundwire: qcom: Enable software clock gating requirement flag (Jaroslav Kysela) [2125544]
- soundwire: qcom: Check device status before reading devid (Jaroslav Kysela) [2125544]
- soundwire: qcom: Add flag for software clock gating check (Jaroslav Kysela) [2125544]
- soundwire: revisit driver bind/unbind and callbacks (Jaroslav Kysela) [2125544]
- soundwire: bus_type: fix remove and shutdown support (Jaroslav Kysela) [2125544]
- soundwire: intel: Migrate to new style legacy DAI naming flag (Jaroslav Kysela) [2125544]
- ASoC: qcom: soundwire: Add support for controlling audio CGCR from HLOS (Jaroslav Kysela) [2125544]
- soundwire: qcom: adjust autoenumeration timeout (Jaroslav Kysela) [2125544]
- soundwire: qcom: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- soundwire: intel: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- soundwire: cadence: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- soundwire: bus: use pm_runtime_resume_and_get() (Jaroslav Kysela) [2125544]
- soundwire: qcom: return error when pm_runtime_get_sync fails (Jaroslav Kysela) [2125544]
- soundwire: bus: pm_runtime_request_resume on peripheral attachment (Jaroslav Kysela) [2125544]
- soundwire: intel: disable WAKEEN in pm_runtime resume (Jaroslav Kysela) [2125544]
- soundwire: cadence: recheck device0 attachment after status change (Jaroslav Kysela) [2125544]
- soundwire: qcom: Add compatible name for v1.6.0 (Jaroslav Kysela) [2125544]
- soundwire: stream: Fix error return code in do_bank_switch() (Jaroslav Kysela) [2125544]
- soundwire: qcom: fix an error message in swrm_wait_for_frame_gen_enabled() (Jaroslav Kysela) [2125544]
- soundwire: qcom: use __maybe_unused for swrm_runtime_resume() (Jaroslav Kysela) [2125544]
- soundwire: qcom: constify static struct qcom_swrm_data global variables (Jaroslav Kysela) [2125544]
- soundwire: qcom: add in-band wake up interrupt support (Jaroslav Kysela) [2125544]
- soundwire: qcom: add runtime pm support (Jaroslav Kysela) [2125544]
- soundwire: Replace acpi_bus_get_device() (Jaroslav Kysela) [2125544]
- ALSA: Add snd_pcm_direction_name() helper (Jaroslav Kysela) [2125544]
- ALSA: core: Fix double-free at snd_card_new() (Jaroslav Kysela) [2125544]
- ALSA: hda: Once again fix regression of page allocations with IOMMU (Jaroslav Kysela) [2125544]
- ALSA: pcm: oss: Fix race at SNDCTL_DSP_SYNC (Jaroslav Kysela) [2125544]
- ALSA: control: Re-order bounds checking in get_ctl_id_hash() (Jaroslav Kysela) [2125544]
- ALSA: control: Fix an out-of-bounds bug in get_ctl_id_hash() (Jaroslav Kysela) [2125544]
- ALSA: seq: Fix data-race at module auto-loading (Jaroslav Kysela) [2125544]
- ALSA: seq: oss: Fix data-race for max_midi_devs access (Jaroslav Kysela) [2125544]
- ALSA: memalloc: Revive x86-specific WC page allocations again (Jaroslav Kysela) [2125544]
- ALSA: info: Fix llseek return value when using callback (Jaroslav Kysela) [2125544]
- ALSA: pcm: Replace sprintf() with sysfs_emit() (Jaroslav Kysela) [2125544]
- ALSA: core: Replace scnprintf() with sysfs_emit() (Jaroslav Kysela) [2125544]
- ALSA: control-led: Replace sprintf() with sysfs_emit() (Jaroslav Kysela) [2125544]
- ALSA: control: Use deferred fasync helper (Jaroslav Kysela) [2125544]
- ALSA: pcm: Use deferred fasync helper (Jaroslav Kysela) [2125544]
- ALSA: timer: Use deferred fasync helper (Jaroslav Kysela) [2125544]
- ALSA: core: Add async signal helpers (Jaroslav Kysela) [2125544]
- ALSA: core: Fix missing return value comments for kernel docs (Jaroslav Kysela) [2125544]
- ALSA: memalloc: Fix missing return value comments for kernel docs (Jaroslav Kysela) [2125544]
- ALSA: control: Fix missing return value comments for kernel docs (Jaroslav Kysela) [2125544]
- ALSA: compress: Fix kernel doc warnings (Jaroslav Kysela) [2125544]
- ALSA: dmaengine: Fix missing return value comments for kernel docs (Jaroslav Kysela) [2125544]
- ALSA: pcm: Fix missing return value comments for kernel docs (Jaroslav Kysela) [2125544]
- ALSA: compress: Enable kernel doc markers for some functions (Jaroslav Kysela) [2125544]
- ALSA: rawmidi: Take buffer refcount while draining output (Jaroslav Kysela) [2125544]
- ALSA: rawmidi: Check stream state at exported functions (Jaroslav Kysela) [2125544]
- ALSA: rawmidi: Take open_mutex around parameter changes (Jaroslav Kysela) [2125544]
- ALSA: rawmidi: Move lock to snd_rawmidi_substream (Jaroslav Kysela) [2125544]
- ALSA: rawmidi: Make internal functions local static (Jaroslav Kysela) [2125544]
- ALSA: control: Add input validation (Jaroslav Kysela) [2125544]
- ALSA: control: Drop superfluous ifdef CONFIG_SND_CTL_DEBUG (Jaroslav Kysela) [2125544]
- ALSA: control: Rename CONFIG_SND_CTL_VALIDATION to CONFIG_SND_CTL_DEBUG (Jaroslav Kysela) [2125544]
- ALSA: control: Use xarray for faster lookups (Jaroslav Kysela) [2125544]
- ALSA: seq: replace ternary operator with max() (Jaroslav Kysela) [2125544]
- ALSA: pcm: use DEVICE_ATTR_RO macro (Jaroslav Kysela) [2125544]
- pinctrl: amd: Don't save/restore interrupt status and wake status bits (Prarit Bhargava) [2130059]
- x86/paravirt: Add a dummy __x86_paravirt_patch_template() function (Waiman Long) [2144161]
- x86/paravirt: Fix kABI breakage in struct pv_mmu_ops (Waiman Long) [2144161]

* Mon Dec 05 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-442.el8.v2.g6f5f]
- can: af_can: fix NULL pointer dereference in can_rx_register() (Ivan Vecera) [2136823]
- net: disable preemption in dev_core_stats_XXX_inc() helpers (Ivan Vecera) [2136823]
- net: introduce CAN specific pointer in the struct net_device (Ivan Vecera) [2136823]
- can: af_can: can_pernet_exit(): no need to iterate over and cleanup registered CAN devices (Ivan Vecera) [2136823]
- net: add per-cpu storage and net->core_stats (Ivan Vecera) [2136823]
- tun: switch to net core provided statistics counters (Ivan Vecera) [2136823]
- tun: switch to u64_stats_t (Ivan Vecera) [2136823]
- ceph: avoid putting the realm twice when decoding snaps fails (Xiubo Li) [2139881]
- powerpc/64/kdump: Limit kdump base to 512MB (Mamatha Inamdar) [2132921]
- ice: virtchnl rss hena support (Petr Oros) [2136516]
- Documentation/admin-guide: Document nomodeset kernel parameter (Jocelyn Falempe) [2143952]
- drm: Move nomodeset kernel parameter to the DRM subsystem (Jocelyn Falempe) [2143952]
- usb: remove third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- sound: usb: remove third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- usb: remove third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- net: remove third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- media: remove third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- Input: remove third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- HID: usbhid: remove third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- usb: deprecate the third argument of usb_maxpacket() (Íñigo Huguet) [2143362]
- scsi: smartpqi: Change version to 2.1.20-035 (Don Brace) [2116976]
- scsi: smartpqi: Initialize feature section info (Don Brace) [2116976]
- scsi: smartpqi: Add controller cache flush during rmmod (Don Brace) [2116976]
- scsi: smartpqi: Correct device removal for multi-actuator devices (Don Brace) [2116976]
- scsi: smartpqi: Change sysfs raid_level attribute to N/A for controllers (Don Brace) [2116976]
- scsi: smartpqi: Correct max LUN number (Don Brace) [2116976]
- scsi: smartpqi: Add new controller PCI IDs (Don Brace) [2116976]
- scsi: smartpqi: Convert to host_tagset (Don Brace) [2116976]
- scsi: smartpqi: Stop using the SCSI pointer (Don Brace) [2116976]
- smartpqi: Change request pointer to scsi_cmd_to_rq (Don Brace) [2116976]
- scsi: smartpqi: Use scsi_cmd_to_rq() instead of scsi_cmnd.request (Don Brace) [2116976]
- EDAC/skx_common: Make output format similar (Aristeu Rozanski) [2124915]
- EDAC/skx_common: Use driver decoder first (Aristeu Rozanski) [2124915]
- ptp: introduce helpers to adjust by scaled parts per million (Izabela Bakollari) [2141639]
- ptp: add missing documentation for parameters (Izabela Bakollari) [2141639]
- mm: slub: fix flush_cpu_slab()/__free_slab() invocations in task context. (Nico Pache) [2144559]
- scsi: target: loop: Fix handling of aborted TMRs (Maurizio Lombardi) [2141713]
- ceph: fix NULL pointer dereference for req->r_session (Xiubo Li) [2137955]
- ceph: Use kcalloc for allocating multiple elements (Xiubo Li) [2137955]
- net/mlx5e: TC, Reject forwarding from internal port to internal port (Mohammad Kabat) [2131345]
- md/raid1: stop mdx_raid1 thread when raid1 array run failed (Nigel Croxon) [2143270]
- md: fix a crash in mempool_free (Nigel Croxon) [2143257]
- md/raid0, raid10: Don't set discard sectors for request queue (Nigel Croxon) [2143250]
- sgx: use ->f_mapping... (Vladis Dronov) [2130210]
- x86/sgx: Improve comments for sgx_encl_lookup/alloc_backing() (Vladis Dronov) [2130210]
- x86/sgx: Handle VA page allocation failure for EAUG on PF. (Vladis Dronov) [2130210]
- x86/sgx: Do not fail on incomplete sanitization on premature stop of ksgxd (Vladis Dronov) [2130210]
- selftests/sgx: Ignore OpenSSL 3.0 deprecated functions warning (Vladis Dronov) [2130210]
- x86/sgx: Set active memcg prior to shmem allocation (Vladis Dronov) [2130210]
- x86/sgx: Drop 'page_index' from sgx_backing (Vladis Dronov) [2130210]
- selftests/sgx: Page removal stress test (Vladis Dronov) [2130210]
- selftests/sgx: Test reclaiming of untouched page (Vladis Dronov) [2130210]
- selftests/sgx: Test invalid access to removed enclave page (Vladis Dronov) [2130210]
- selftests/sgx: Test faulty enclave behavior (Vladis Dronov) [2130210]
- selftests/sgx: Test complete changing of page type flow (Vladis Dronov) [2130210]
- selftests/sgx: Introduce TCS initialization enclave operation (Vladis Dronov) [2130210]
- selftests/sgx: Introduce dynamic entry point (Vladis Dronov) [2130210]
- selftests/sgx: Test two different SGX2 EAUG flows (Vladis Dronov) [2130210]
- selftests/sgx: Add test for TCS page permission changes (Vladis Dronov) [2130210]
- selftests/sgx: Add test for EPCM permission changes (Vladis Dronov) [2130210]
- Documentation/x86: Introduce enclave runtime management section (Vladis Dronov) [2130210]
- x86/sgx: Free up EPC pages directly to support large page ranges (Vladis Dronov) [2130210]
- x86/sgx: Support complete page removal (Vladis Dronov) [2130210]
- x86/sgx: Support modifying SGX page type (Vladis Dronov) [2130210]
- x86/sgx: Tighten accessible memory range after enclave initialization (Vladis Dronov) [2130210]
- x86/sgx: Support adding of pages to an initialized enclave (Vladis Dronov) [2130210]
- x86/sgx: Support restricting of enclave page permissions (Vladis Dronov) [2130210]
- x86/sgx: Support VA page allocation without reclaiming (Vladis Dronov) [2130210]
- x86/sgx: Export sgx_encl_page_alloc() (Vladis Dronov) [2130210]
- x86/sgx: Export sgx_encl_{grow,shrink}() (Vladis Dronov) [2130210]
- x86/sgx: Keep record of SGX page type (Vladis Dronov) [2130210]
- x86/sgx: Create utility to validate user provided offset and length (Vladis Dronov) [2130210]
- x86/sgx: Make sgx_ipi_cb() available internally (Vladis Dronov) [2130210]
- x86/sgx: Move PTE zap code to new sgx_zap_enclave_ptes() (Vladis Dronov) [2130210]
- x86/sgx: Rename sgx_encl_ewb_cpumask() as sgx_encl_cpumask() (Vladis Dronov) [2130210]
- x86/sgx: Export sgx_encl_ewb_cpumask() (Vladis Dronov) [2130210]
- x86/sgx: Support loading enclave page without VMA permissions check (Vladis Dronov) [2130210]
- x86/sgx: Add wrapper for SGX2 EAUG function (Vladis Dronov) [2130210]
- x86/sgx: Add wrapper for SGX2 EMODT function (Vladis Dronov) [2130210]
- x86/sgx: Add wrapper for SGX2 EMODPR function (Vladis Dronov) [2130210]
- x86/sgx: Add short descriptions to ENCLS wrappers (Vladis Dronov) [2130210]
- x86/sgx: Ensure no data in PCMD page after truncate (Vladis Dronov) [2130210]
- x86/sgx: Fix race between reclaimer and page fault handler (Vladis Dronov) [2130210]
- x86/sgx: Obtain backing storage page with enclave mutex held (Vladis Dronov) [2130210]
- x86/sgx: Mark PCMD page as dirty when modifying contents (Vladis Dronov) [2130210]
- x86/sgx: Disconnect backing page references from dirty status (Vladis Dronov) [2130210]
- HID: intel-ish-hid: ipc: Add Meteor Lake PCI device ID (Tony Camuso) [2132441]
- hid: intel-ish-hid: ishtp: Fix ishtp client sending disordered message (Tony Camuso) [2132441]
- HID: ishtp-hid-clientHID: ishtp-hid-client: Fix comment typo (Tony Camuso) [2132441]
- ID: intel-ish-hid: hid-client: drop unexpected word "the" in the comments (Tony Camuso) [2132441]
- HID: intel-ish-hid: ipc: use time_before to replace "jiffies < a" (Tony Camuso) [2132441]
- HID: intel-ish-hid: ipc: add ADL and RPL device id (Tony Camuso) [2132441]
- HID: intel-ish-hid: Use dma_alloc_coherent for firmware update (Tony Camuso) [2132441]
- HID: intel-ish-hid: ishtp-fw-loader: Fix a kernel-doc formatting issue (Tony Camuso) [2132441]
- HID: intel-ish-hid: ipc: Specify no cache snooping on TGL and ADL (Tony Camuso) [2132441]
- HID: intel-ish-hid: ipc: only enable IRQ wakeup when requested (Tony Camuso) [2132441]
- HID: intel-ish-hid: fix module device-id handling (Tony Camuso) [2132441]
- HID: intel-ish-hid: hid-client: only load for matching devices (Tony Camuso) [2132441]
- HID: intel-ish-hid: fw-loader: only load for matching devices (Tony Camuso) [2132441]
- HID: intel-ish-hid: use constants for modaliases (Tony Camuso) [2132441]
- s390/pci: add missing EX_TABLE entries to __pcistg_mio_inuser()/__pcilg_mio_inuser() (Tobias Huschle) [2141963]
- s390/futex: add missing EX_TABLE entry to __futex_atomic_op() (Tobias Huschle) [2141963]
- s390/uaccess: add missing EX_TABLE entries to __clear_user() (Tobias Huschle) [2141963]
- net: usb: ax88179_178a: Fix packet receiving (Jose Ignacio Tornos Martinez) [2142725] {CVE-2022-2964}
- net: usb: ax88179_178a: Fix out-of-bounds accesses in RX fixup (Jose Ignacio Tornos Martinez) [2142725] {CVE-2022-2964}
- drm/i915/rpl-p: Add PCI IDs (Jocelyn Falempe) [2115880]
- Revert "dma-buf: remove useless FMODE_LSEEK flag" (Jocelyn Falempe) [2115880]
- drm/amd/display: Increase stack frame size limit for a few files. (Jocelyn Falempe) [2115880]
- drm_crtc.h is missing include/linux/slab.h (Jocelyn Falempe) [2115880]
- drm/amd/display: remove a duplicated declaration (Jocelyn Falempe) [2115880]
- Revert "mm: shrinkers: provide shrinkers with names" (Jocelyn Falempe) [2115880]
- Revert "drm/amdkfd: add SPM support for SVM" (Jocelyn Falempe) [2115880]
- Merge DRM changes from upstream v5.19..v6.0 (Jocelyn Falempe) [2115880]
- drm/i915/gvt: IMPORT_MODULE_NS workaround (Jocelyn Falempe) [2115880]
- Replace EXPORT_SYMBOL_NS_GPL with EXPORT_SYMBOL_GPL (Jocelyn Falempe) [2115880]
- Revert "vfio/gvt: Fix open/close when multiple device FDs are open" (Michel Dänzer) [2115880]
- Revert "vfio/mdev: Pass in a struct vfio_device * to vfio_dma_rw()" (Jocelyn Falempe) [2115880]
- Revert "drm/i915/gvt: convert to use vfio_register_emulated_iommu_dev" (Jocelyn Falempe) [2115880]
- Revert "drm/i915/gvt: merge gvt.c into kvmgvt.c" (Jocelyn Falempe) [2115880]
- Revert "vfio/mdev: Remove mdev_parent_ops" (Jocelyn Falempe) [2115880]
- Revert "vfio: Make vfio_(un)register_notifier accept a vfio_device" (Jocelyn Falempe) [2115880]
- Revert "drm/i915/gvt: Change from vfio_group_(un)pin_pages to vfio_(un)pin_pages" (Jocelyn Falempe) [2115880]
- Revert "vfio: remove VFIO_GROUP_NOTIFY_SET_KVM" (Jocelyn Falempe) [2115880]
- Revert "i915: Call aops write_begin() and write_end() directly" (Jocelyn Falempe) [2115880]
- Merge DRM changes from upstream v5.18..v5.19 (Jocelyn Falempe) [2115880]
- crypto: testmgr - disallow plain cbcmac(aes) and ghash in FIPS mode (Vladis Dronov) [2107595]
- crypto: set the required FIPS_INTERNAL flag for gcm and ccm (Vladis Dronov) [2107595]
- crypto: seqiv - flag instantiations as FIPS compliant (Vladis Dronov) [2107595]
- crypto: xts - restrict key lengths to approved values in FIPS mode (Vladis Dronov) [2107595]
- crypto: api - allow algs only in specific constructions in FIPS mode (Vladis Dronov) [2107595]
- crypto: api - check for ERR pointers in crypto_destroy_tfm() (Vladis Dronov) [2107595]
- crypto: api - Fix use-after-free and race in crypto_spawn_alg (Vladis Dronov) [2107595]
- crypto: algapi - Avoid spurious modprobe on LOADED (Vladis Dronov) [2107595]
- crypto: api - Retain alg refcount in crypto_grab_spawn (Vladis Dronov) [2107595]
- crypto: api - Do not zap spawn->alg (Vladis Dronov) [2107595]
- crypto: api - Fix race condition in crypto_spawn_alg (Vladis Dronov) [2107595]
- crypto: api - Check spawn->alg under lock in crypto_drop_spawn (Vladis Dronov) [2107595]
- crypto: algapi - reject NULL crypto_spawn::inst (Vladis Dronov) [2107595]
- iavf: remove INITIAL_MAC_SET to allow gARP to work properly (Stefan Assmann) [1938635]
- mm, slab: remove duplicate kernel-doc comment for ksize() (Michal Schmidt) [2143367]
- slab: Introduce kmalloc_size_roundup() (Michal Schmidt) [2143367]
- thermal: int340x: Mode setting with new OS handshake (Prarit Bhargava) [2072652]
- thermal: int340x: Update OS policy capability handshake (Prarit Bhargava) [2072652]
- hugetlb: remove unnecessary set_page_count in prep_compound_gigantic_page (Chris von Recklinghausen) [2143631]
- mm/hugetlb: clear compound_nr before freeing gigantic pages (Chris von Recklinghausen) [2143631]
- uprobes: __replace_page() avoid BUG in munlock_vma_page() (Chris von Recklinghausen) [2143631]
- s390/boot: add secure boot trailer (Tobias Huschle) [2141967]
- ice: Fix configuring VIRTCHNL_OP_CONFIG_VSI_QUEUES with unbalanced queues (Michal Schmidt) [2137378]
- nvme: wait until quiesce is done (Ming Lei) [2144258]
- scsi: make sure that request queue queiesce and unquiesce balanced (Ming Lei) [2144258]
- scsi: avoid to quiesce sdev->request_queue two times (Ming Lei) [2144258]
- dm: don't stop request queue after the dm device is suspended (Ming Lei) [2144258]

* Tue Nov 29 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-441.el8]
- ata: libata-core: Print timeout value when internal command times (Ewan D. Milne) [1823688]
- ata: libata-core: fix sloppy parameter type in ata_exec_internal[_sg]() (Ewan D. Milne) [1823688]
- ata: libata-core: make ata_exec_internal_sg() *static* (Ewan D. Milne) [1823688]
- perf/x86/intel: Fix unchecked MSR access error for Alder Lake N (Michael Petlan) [2104807]
- perf/x86/intel: Fix PEBS data source encoding for ADL (Michael Petlan) [2104807]
- perf/x86/intel: Fix PEBS memory access info encoding for ADL (Michael Petlan) [2104807]
- i40e: Fix DMA mappings leak (Ivan Vecera) [2077847]
- fbcon: Fix delayed takeover locking (Jocelyn Falempe) [2134795]
- fbcon: use min() to make code cleaner (Jocelyn Falempe) [2134795]
- fbcon: Use array3_size() helper in scr_memcpyw() (Jocelyn Falempe) [2134795]
- fbcon: Maintain a private array of fb_info (Jocelyn Falempe) [2134795]
- fbcon: untangle fbcon_exit (Jocelyn Falempe) [2134795]
- fbcon: Move more code into fbcon_release (Jocelyn Falempe) [2134795]
- fbcon: Move console_lock for register/unlink/unregister (Jocelyn Falempe) [2134795]
- fbcon: Consistently protect deferred_takeover with console_lock() (Jocelyn Falempe) [2134795]
- fbcon: use lock_fb_info in fbcon_open/release (Jocelyn Falempe) [2134795]
- fbcon: move more common code into fb_open() (Jocelyn Falempe) [2134795]
- fbcon: Ditch error handling for con2fb_release_oldinfo (Jocelyn Falempe) [2134795]
- fbcon: Extract fbcon_open/release helpers (Jocelyn Falempe) [2134795]
- fb: Delete fb_info->queue (Jocelyn Falempe) [2134795]
- fbcon: Replace FBCON_FLAGS_INIT with a boolean (Jocelyn Falempe) [2134795]
- fbcon: Use delayed work for cursor (Jocelyn Falempe) [2134795]
- fbdev/sysfs: Fix locking (Jocelyn Falempe) [2134795]
- fbcon: delete delayed loading code (Jocelyn Falempe) [2134795]
- fbcon: Introduce wrapper for console->fb_info lookup (Jocelyn Falempe) [2134795]
- fbcon: Move fbcon_bmove(_rec) functions (Jocelyn Falempe) [2134795]
- fbcon: delete a few unneeded forward decl (Jocelyn Falempe) [2134795]
- fbcon: Avoid 'cap' set but not used warning (Jocelyn Falempe) [2134795]
- video: fbcon: Fix warnings by using pr_debug() in fbcon (Jocelyn Falempe) [2134795]
- fbcon: Fix user font detection test at fbcon_resize(). (Jocelyn Falempe) [2134795]
- fbcon: remove now unusued 'softback_lines' cursor() argument (Jocelyn Falempe) [2134795]
- fbcon: remove soft scrollback code (Jocelyn Falempe) [2134795]
- fbcon: prevent user font height or width change from causing potential out-of-bounds access (Jocelyn Falempe) [2134795]
- fbmem: pull fbcon_update_vcs() out of fb_set_var() (Jocelyn Falempe) [2134795]
- fbcon: fix null-ptr-deref in fbcon_switch (Jocelyn Falempe) [2134795]
- fbcon: Adjust indentation in set_con2fb_map (Jocelyn Falempe) [2134795]
- fbdev: Unexport unlink_framebuffer() (Jocelyn Falempe) [2134795]
- backlight: drop EARLY_EVENT_BLANK support (Jocelyn Falempe) [2134795]
- fbcon: Export fbcon_update_vcs (Jocelyn Falempe) [2134795]
- backlight: simplify lcd notifier (Jocelyn Falempe) [2134795]
- fbcon: Document what I learned about fbcon locking (Jocelyn Falempe) [2134795]
- fbcon: Call con2fb_map functions directly (Jocelyn Falempe) [2134795]
- fbcon: replace FB_EVENT_MODE_CHANGE/_ALL with direct calls (Jocelyn Falempe) [2134795]
- fb: Flatten control flow in fb_set_var (Jocelyn Falempe) [2134795]
- fbdev: remove FBINFO_MISC_USEREVENT around fb_blank (Jocelyn Falempe) [2134795]
- fbmem: pull fbcon_fb_blanked out of fb_blank (Jocelyn Falempe) [2134795]
- Revert "backlight/fbcon: Add FB_EVENT_CONBLANK" (Jocelyn Falempe) [2134795]
- fbdev: Call fbcon_get_requirement directly (Jocelyn Falempe) [2134795]
- fbcon: Call fbcon_mode_deleted/new_modelist directly (Jocelyn Falempe) [2134795]
- fbdev: directly call fbcon_suspended/resumed (Jocelyn Falempe) [2134795]
- fbdev: unify unlink_framebuffer paths (Jocelyn Falempe) [2134795]
- fbdev: make unregister/unlink functions not fail (Jocelyn Falempe) [2134795]
- fbcon: call fbcon_fb_bind directly (Jocelyn Falempe) [2134795]
- fbcon: call fbcon_fb_(un)registered directly (Jocelyn Falempe) [2134795]
- fbdev: fbmem: fix memory access if logo is bigger than the screen (Jocelyn Falempe) [2134795]
- fbdev: add kerneldoc do remove_conflicting_framebuffers() (Jocelyn Falempe) [2134795]
- fbdev: allow apertures == NULL in remove_conflicting_framebuffers() (Jocelyn Falempe) [2134795]
- fbdev: show fbdev number for debugging (Jocelyn Falempe) [2134795]
- fbcon: use kvmalloc() for scrollback buffer (Jocelyn Falempe) [2134795]
- fbdev: fbcon: Fix unregister crash when more than one framebuffer (Jocelyn Falempe) [2134795]
- fb: fix lost console when the user unplugs a USB adapter (Jocelyn Falempe) [2134795]
- fbcon: introduce for_each_registered_fb() helper (Jocelyn Falempe) [2134795]
- timers/nohz: Last resort update jiffies on nohz_full IRQ entry (Waiman Long) [2108387]
- irq: Call tick_irq_enter() inside HARDIRQ_OFFSET (Waiman Long) [2108387]
- irqtime: Move irqtime entry accounting after irq offset incrementation (Waiman Long) [2108387]
- sched/vtime: Consolidate IRQ time accounting (Waiman Long) [2108387]
- s390/vtime: Use the generic IRQ entry accounting (Waiman Long) [2108387]
- sched/cputime: Remove symbol exports from IRQ time accounting (Waiman Long) [2108387]
- genirq/irqdomain: Don't try to free an interrupt that has no mapping (Waiman Long) [2108387]
- genirq: Provide __irq_enter/exit_raw() (Waiman Long) [2108387]
- powerpc/time: Only set CONFIG_ARCH_HAS_SCALED_CPUTIME on PPC64 (Waiman Long) [2108387]
- powerpc/time: isolate scaled cputime accounting in dedicated functions. (Waiman Long) [2108387]
- perf: Fix list corruption in perf_cgroup_switch() (Aaron Tomlin) [2136548]
- gen_compile_commands: fix issues in RHEL-8 (Íñigo Huguet) [2136840]
- .gitignore: Add compilation database file (Íñigo Huguet) [2136840]
- gen_compile_commands: fix missing 'sys' package (Íñigo Huguet) [2136840]
- gen_compile_commands: extract compiler command from a series of commands (Íñigo Huguet) [2136840]
- gen_compile_commands: prune some directories (Íñigo Huguet) [2136840]
- scripts/clang-tools: switch explicitly to Python 3 (Íñigo Huguet) [2136840]
- Makefile: Add clang-tidy and static analyzer support to makefile (Íñigo Huguet) [2136840]
- kbuild: wire up the build rule of compile_commands.json to Makefile (Íñigo Huguet) [2136840]
- gen_compile_commands: remove the warning about too few .cmd files (Íñigo Huguet) [2136840]
- gen_compile_commands: support *.o, *.a, modules.order in positional argument (Íñigo Huguet) [2136840]
- gen_compile_commands: move directory walk to a generator function (Íñigo Huguet) [2136840]
- gen_compile_commands: make -o option independent of -d option (Íñigo Huguet) [2136840]
- gen_compile_commands: reword the help message of -d option (Íñigo Huguet) [2136840]
- gen_compile_commands: do not support .cmd files under tools/ directory (Íñigo Huguet) [2136840]
- gen_compile_commands: use choices for --log_levels option (Íñigo Huguet) [2136840]
- gen_compile_commands: parse only the first line of .*.cmd files (Íñigo Huguet) [2136840]
- gen_compile_commands: lower the entry count threshold (Íñigo Huguet) [2136840]
- scripts: add a tool to produce a compile_commands.json file (Íñigo Huguet) [2136840]
- iavf: Do not restart Tx queues after reset task failure (Petr Oros) [2134005]
- iavf: Fix a crash during reset task (Petr Oros) [2134005]
- spec: add bpf_testmod.ko to kselftests/bpf (Yauheni Kaliuta) [2140082]
- fuse: fix readdir cache race (Miklos Szeredi) [2131391]
- ice: config netdev tc before setting queues number (Petr Oros) [2103946]
- ice: Fix ice_xdp_xmit() when XDP TX queue number is not sufficient (Petr Oros) [2103946]
- ice: Don't double unplug aux on peer initiated reset (Petr Oros) [2103946]
- ice: use bitmap_free instead of devm_kfree (Petr Oros) [2103946]
- ice: Fix DMA mappings leak (Petr Oros) [2103946]
- ice: Fix call trace with null VSI during VF reset (Petr Oros) [2103946]
- ice: Fix VSI rebuild WARN_ON check for VF (Petr Oros) [2103946]
- net/ice: fix initializing the bitmap in the switch code (Petr Oros) [2103946]
- net: ice: fix error NETIF_F_HW_VLAN_CTAG_FILTER check in ice_vsi_sync_fltr() (Petr Oros) [2103946]
- ice: allow toggling loopback mode via ndo_set_features callback (Petr Oros) [2103946]
- ice: compress branches in ice_set_features() (Petr Oros) [2103946]
- ice: Add support for PPPoE hardware offload (Petr Oros) [2103946]
- ice: add i2c write command (Petr Oros) [2103946]
- ice: Remove pci_aer_clear_nonfatal_status() call (Petr Oros) [2103946]
- ice: Remove unnecessary NULL check before dev_put (Petr Oros) [2103946]
- ice: use eth_broadcast_addr() to set broadcast address (Petr Oros) [2103946]
- ice: switch: dynamically add VLAN headers to dummy packets (Petr Oros) [2103946]
- ice: Add support for VLAN TPID filters in switchdev (Petr Oros) [2103946]
- ice: Add support for double VLAN in switchdev (Petr Oros) [2103946]
- intel/ice:fix repeated words in comments (Petr Oros) [2103946]
- drivers/net/ethernet/intel: fix typos in comments (Petr Oros) [2103946]
- ice: Use correct order for the parameters of devm_kcalloc() (Petr Oros) [2103946]
- ice: remove u16 arithmetic in ice_gnss (Petr Oros) [2103946]
- ice: remove VLAN representor specific ops (Petr Oros) [2103946]
- ice: don't set VF VLAN caps in switchdev (Petr Oros) [2103946]
- kernel-doc: fix undefined args variable (Jan Stancek) [2134954]

* Tue Nov 22 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-440.el8]
- sunrpc: Set sk_allocation to GFP_NOFS to avoid using current->task_frag. (Guillaume Nault) [2089660]
- selftests/vm: enable running select groups of tests (Joel Savitz) [2089502]
- selftests: make use of GUP_TEST_FILE macro (Nico Pache) [2089502]
- selftests: clarify common error when running gup_test (Nico Pache) [2089502]
- tools/testing/selftests/vm/gup_test.c: clarify error statement (Nico Pache) [2089502]
- mm: remove the extra ZONE_DEVICE struct page refcount (Chris von Recklinghausen) [2082247]
- mm: simplify freeing of devmap managed pages (Chris von Recklinghausen) [2082247]
- mm: move free_devmap_managed_page to memremap.c (Chris von Recklinghausen) [2082247]
- mm/memremap: add ZONE_DEVICE support for compound pages (Chris von Recklinghausen) [2082247]
- mm/page_alloc: refactor memmap_init_zone_device() page init (Chris von Recklinghausen) [2082247]
- mm/page_alloc: split prep_compound_page into head and tail subparts (Chris von Recklinghausen) [2082247]
- mm/debug: sync up MR_CONTIG_RANGE and MR_LONGTERM_PIN (Chris von Recklinghausen) [2082247]
- mm: gup: use helper PAGE_ALIGNED in populate_vma_page_range() (Chris von Recklinghausen) [2082247]
- mm: gup: remove useless BUG_ON in __get_user_pages() (Chris von Recklinghausen) [2082247]
- mm: gup: remove unneed local variable orig_refs (Chris von Recklinghausen) [2082247]
- mm: gup: remove set but unused local variable major (Chris von Recklinghausen) [2082247]
- writeback: make the laptop_mode prototypes available unconditionally (Chris von Recklinghausen) [2082247]
- mm: hide laptop_mode_wb_timer entirely behind the BDI API (Chris von Recklinghausen) [2082247]
- mm: remove special swap entry functions (Chris von Recklinghausen) [2082247]
- hugetlb: address ref count racing in prep_compound_gigantic_page (Chris von Recklinghausen) [2082247]
- hugetlb: remove prep_compound_huge_page cleanup (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): get vma_address_end() earlier (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): use goto instead of while (1) (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): add a level of indentation (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): crossing page table boundary (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): prettify PVMW_MIGRATION block (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): use pmde for *pvmw->pmd (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): settle PageHuge on entry (Chris von Recklinghausen) [2082247]
- mm: page_vma_mapped_walk(): use page for pvmw->page (Chris von Recklinghausen) [2082247]
- mm/gup: longterm pin migration cleanup (Chris von Recklinghausen) [2082247]
- mm/gup: change index type to long as it counts pages (Chris von Recklinghausen) [2082247]
- mm/gup: migrate pinned pages out of movable zone (Chris von Recklinghausen) [2082247]
- mm: honor PF_MEMALLOC_PIN for all movable pages (Chris von Recklinghausen) [2082247]
- mm cma: rename PF_MEMALLOC_NOCMA to PF_MEMALLOC_PIN (Chris von Recklinghausen) [2082247]
- mm/huge_memory.c: use helper function migration_entry_to_page() (Chris von Recklinghausen) [2082247]
- block: add queue_to_disk() to get gendisk from request_queue (Chris von Recklinghausen) [2082247]
- mm/hugetlb: remove redundant check in preparing and destroying gigantic page (Chris von Recklinghausen) [2082247]
- mm/hugetlb: use helper huge_page_order and pages_per_huge_page (Chris von Recklinghausen) [2082247]
- mm: handle zone device pages in release_pages() (Chris von Recklinghausen) [2082247]
- mm/gup: remove the vma allocation from gup_longterm_locked() (Chris von Recklinghausen) [2082247]
- mm/mremap_pages: fix static key devmap_managed_key updates (Chris von Recklinghausen) [2082247]
- mm/memremap.c: convert devmap static branch to {inc,dec} (Chris von Recklinghausen) [2082247]
- mm/page_alloc: handle a missing case for memalloc_nocma_{save/restore} APIs (Chris von Recklinghausen) [2082247]
- mm: store compound_nr as well as compound_order (Chris von Recklinghausen) [2082247]
- mm: clean up the last pieces of page fault accountings (Chris von Recklinghausen) [2082247]
- mm/x86: use general page fault accounting (Chris von Recklinghausen) [2082247]
- mm/s390: use general page fault accounting (Chris von Recklinghausen) [2082247]
- mm/powerpc: use general page fault accounting (Chris von Recklinghausen) [2082247]
- mm/arm64: use general page fault accounting (Chris von Recklinghausen) [2082247]
- mm: do page fault accounting in handle_mm_fault (Chris von Recklinghausen) [2082247]
- include/linux/sched/mm.h: optimize current_gfp_context() (Chris von Recklinghausen) [2082247]
- mm/page_alloc: fix memalloc_nocma_{save/restore} APIs (Chris von Recklinghausen) [2082247]
- mm: remove redundant check non_swap_entry() (Chris von Recklinghausen) [2082247]
- mm: rename gfpflags_to_migratetype to gfp_migratetype for same convention (Chris von Recklinghausen) [2082247]
- mm,page_alloc,cma: conditionally prefer cma pageblocks for movable allocations (Chris von Recklinghausen) [2082247]
- mm/vma: introduce VM_ACCESS_FLAGS (Chris von Recklinghausen) [2082247]
- mm/vma: make vma_is_accessible() available for general use (Chris von Recklinghausen) [2082247]
- kernel/events/uprobes.c: only do FOLL_SPLIT_PMD for uprobe register (Chris von Recklinghausen) [2082247]
- uprobe: collapse THP pmd after removing all uprobes (Chris von Recklinghausen) [2082247]
- uprobe: use FOLL_SPLIT_PMD instead of FOLL_SPLIT (Chris von Recklinghausen) [2082247]
- mm, thp: introduce FOLL_SPLIT_PMD (Chris von Recklinghausen) [2082247]
- mm: clean up is_device_*_page() definitions (Chris von Recklinghausen) [2082247]
- driver core: Add helper device_find_child_by_name() (Chris von Recklinghausen) [2082247]
- mm/page_alloc.c: remove unnecessary parameter in rmqueue_pcplist (Chris von Recklinghausen) [2082247]
- sctp: handle the error returned from sctp_auth_asoc_init_active_key (Xin Long) [2134892]
- sctp: leave the err path free in sctp_stream_init to sctp_stream_free (Xin Long) [2134892]
- sctp: fix sleep in atomic context bug in timer handlers (Xin Long) [2134892]
- stcp: Use memset_after() to zero sctp_stream_out_ext (Xin Long) [2134892]
- sctp: read sk->sk_bound_dev_if once in sctp_rcv() (Xin Long) [2134892]
- ethtool: add header/data split indication (Ivan Vecera) [2135624]
- xfrm: store and rely on direction to construct offload flags (Sabrina Dubroca) [2137562]
- platform/x86/intel: pmc: Support Intel Raptorlake P (Prarit Bhargava) [2076736]

* Fri Nov 18 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-439.el8]
- KVM: selftests: Build the memslot tests for arm64 (Gavin Shan) [2132161]
- KVM: selftests: Fix number of pages for memory slot in memslot_modification_stress_test (Gavin Shan) [2132161]
- tools/include: Add _RET_IP_ and math definitions to kernel.h (Gavin Shan) [2132161]
- tcp: fix early ETIMEDOUT after spurious non-SACK RTO (Davide Caratti) [2136409]
- tcp: add a missing nf_reset_ct() in 3WHS handling (Davide Caratti) [2136409]
- sock: redo the psock vs ULP protection check (Davide Caratti) [2136409]
- tcp: tcp_rtx_synack() can be called from process context (Davide Caratti) [2136409]
- tcp: fix tcp_mtup_probe_success vs wrong snd_cwnd (Davide Caratti) [2136409]
- tcp: fix F-RTO may not work correctly when receiving DSACK (Davide Caratti) [2136409]
- selftests: xsk: do not send zero-length packets (Ivan Vecera) [2135634]
- selftests/xsk: Introduce XDP prog load based on existing AF_XDP socket (Ivan Vecera) [2135634]
- selftests, xsk: Fix rx_full stats test (Ivan Vecera) [2135634]
- selftests/bpf: Fix xdpxceiver failures for no hugepages (Ivan Vecera) [2135634]
- selftests/xsk: Add missing close() on netns fd (Ivan Vecera) [2135634]
- selftests, xsk: Fix bpf_res cleanup test (Ivan Vecera) [2135634]
- selftests: xsk: Add frame_headroom test (Ivan Vecera) [2135634]
- selftests: xsk: Change interleaving of packets in unaligned mode (Ivan Vecera) [2135634]
- selftests: xsk: Add single packet test (Ivan Vecera) [2135634]
- selftests: xsk: Introduce pacing of traffic (Ivan Vecera) [2135634]
- selftests: xsk: Fix socket creation retry (Ivan Vecera) [2135634]
- selftests: xsk: Put the same buffer only once in the fill ring (Ivan Vecera) [2135634]
- selftests: xsk: Fix missing initialization (Ivan Vecera) [2135634]
- selftests: xsk: Add tests for 2K frame size (Ivan Vecera) [2135634]
- selftests: xsk: Add tests for invalid xsk descriptors (Ivan Vecera) [2135634]
- selftests: xsk: Eliminate test specific if-statement in test runner (Ivan Vecera) [2135634]
- selftests: xsk: Add test for unaligned mode (Ivan Vecera) [2135634]
- selftests: xsk: Introduce replacing the default packet stream (Ivan Vecera) [2135634]
- selftests: xsk: Allow for invalid packets (Ivan Vecera) [2135634]
- selftests: xsk: Eliminate MAX_SOCKS define (Ivan Vecera) [2135634]
- selftests: xsx: Make pthreads local scope (Ivan Vecera) [2135634]
- selftests: xsk: Make xdp_flags and bind_flags local (Ivan Vecera) [2135634]
- selftests: xsk: Specify number of sockets to create (Ivan Vecera) [2135634]
- selftests: xsk: Replace second_step global variable (Ivan Vecera) [2135634]
- selftests: xsk: Introduce rx_on and tx_on in ifobject (Ivan Vecera) [2135634]
- selftests: xsk: Add use_poll to ifobject (Ivan Vecera) [2135634]
- selftests: xsx: Introduce test name in test spec (Ivan Vecera) [2135634]
- selftests: xsk: Make frame_size configurable (Ivan Vecera) [2135634]
- selftests: xsk: Move rxqsize into xsk_socket_info (Ivan Vecera) [2135634]
- selftests: xsk: Move num_frames and frame_headroom to xsk_umem_info (Ivan Vecera) [2135634]
- selftests: xsk: Introduce test specifications (Ivan Vecera) [2135634]
- selftests: xsk: Introduce type for thread function (Ivan Vecera) [2135634]
- selftests: xsk: Simplify xsk and umem arrays (Ivan Vecera) [2135634]
- selftests: xsk: Preface options with opt (Ivan Vecera) [2135634]
- selftests: xsk: Make enums lower case (Ivan Vecera) [2135634]
- selftests: xsk: Generate packets from specification (Ivan Vecera) [2135634]
- selftests: xsk: Generate packet directly in umem (Ivan Vecera) [2135634]
- selftests: xsk: Simplify cleanup of ifobjects (Ivan Vecera) [2135634]
- selftests: xsk: Decrease sending speed (Ivan Vecera) [2135634]
- selftests: xsk: Validate tx stats on tx thread (Ivan Vecera) [2135634]
- selftests: xsk: Simplify packet validation in xsk tests (Ivan Vecera) [2135634]
- selftests: xsk: Rename worker_* functions that are not thread entry points (Ivan Vecera) [2135634]
- selftests: xsk: Disassociate umem size with packets sent (Ivan Vecera) [2135634]
- selftests: xsk: Remove end-of-test packet (Ivan Vecera) [2135634]
- selftests: xsk: Simplify the retry code (Ivan Vecera) [2135634]
- selftests: xsk: Return correct error codes (Ivan Vecera) [2135634]
- selftests: xsk: Remove unused variables (Ivan Vecera) [2135634]
- selftests: xsk: Remove the num_tx_packets option (Ivan Vecera) [2135634]
- selftests: xsk: Remove color mode (Ivan Vecera) [2135634]
- xsk: Fix possible crash when multiple sockets are created (Ivan Vecera) [2135634]
- i40e: xsk: Move tmp desc array from driver to pool (Ivan Vecera) [2135634]
- xsk: Initialise xskb free_list_node (Ivan Vecera) [2135634]
- xsk: Fix corrupted packets for XDP_SHARED_UMEM (Ivan Vecera) [2135634]
- xsk: Fix clang build error in __xp_alloc (Ivan Vecera) [2135634]
- xsk: Do not write NULL in SW ring at allocation failure (Ivan Vecera) [2135634]
- xsk: Fix crash on double free in buffer pool (Ivan Vecera) [2135634]
- xsk: Optimize for aligned case (Ivan Vecera) [2135634]
- xsk: Batched buffer allocation for the pool (Ivan Vecera) [2135634]
- xsk: Get rid of unused entry in struct xdp_buff_xsk (Ivan Vecera) [2135634]
- redhat/configs: Move config files under common/generic/x86 to generic/x86_64 (Waiman Long) [2139172]
- fbmem: Check virtual screen sizes in fb_set_var() (Wander Lairson Costa) [2109116] {CVE-2021-33655}
- fbcon: Prevent that screen size is smaller than font size (Wander Lairson Costa) [2109116] {CVE-2021-33655}
- fbcon: Disallow setting font bigger than screen size (Wander Lairson Costa) [2109116] {CVE-2021-33655}
- video: of_display_timing.h: include errno.h (Wander Lairson Costa) [2109116] {CVE-2021-33655}
- MAINTAINERS: pick up all vfio_ap docs for VFIO AP maintainers (Cédric Le Goater) [1660908]
- s390/docs: fix warnings for vfio_ap driver doc (Cédric Le Goater) [1660908]
- s390/docs: fix warnings for vfio_ap driver lock usage doc (Cédric Le Goater) [1660908]
- s390/Docs: new doc describing lock usage by the vfio_ap device driver (Cédric Le Goater) [1660908]
- s390/vfio-ap: bypass unnecessary processing of AP resources (Cédric Le Goater) [1660908]
- s390/vfio-ap: update docs to include dynamic config support (Cédric Le Goater) [1660908]
- s390/vfio-ap: handle config changed and scan complete notification (Cédric Le Goater) [1660908]
- s390/vfio-ap: sysfs attribute to display the guest's matrix (Cédric Le Goater) [1660908]
- s390/vfio-ap: implement in-use callback for vfio_ap driver (Cédric Le Goater) [1660908]
- s390/vfio-ap: reset queues after adapter/domain unassignment (Cédric Le Goater) [1660908]
- s390/vfio-ap: hot plug/unplug of AP devices when probed/removed (Cédric Le Goater) [1660908]
- s390/vfio-ap: allow hot plug/unplug of AP devices when assigned/unassigned (Cédric Le Goater) [1660908]
- s390/vfio-ap: prepare for dynamic update of guest's APCB on queue probe/remove (Cédric Le Goater) [1660908]
- s390/vfio-ap: prepare for dynamic update of guest's APCB on assign/unassign (Cédric Le Goater) [1660908]
- s390/vfio-ap: use proper locking order when setting/clearing KVM pointer (Cédric Le Goater) [1660908]
- s390/vfio-ap: introduce new mutex to control access to the KVM pointer (Cédric Le Goater) [1660908]
- s390/vfio-ap: rename matrix_dev->lock mutex to matrix_dev->mdevs_lock (Cédric Le Goater) [1660908]
- s390/vfio-ap: allow assignment of unavailable AP queues to mdev device (Cédric Le Goater) [1660908]
- s390/vfio-ap: refresh guest's APCB by filtering AP resources assigned to mdev (Cédric Le Goater) [1660908]
- s390/vfio-ap: introduce shadow APCB (Cédric Le Goater) [1660908]
- s390/vfio-ap: manage link between queue struct and matrix mdev (Cédric Le Goater) [1660908]
- s390/vfio-ap: move probe and remove callbacks to vfio_ap_ops.c (Cédric Le Goater) [1660908]
- s390/vfio-ap: use new AP bus interface to search for queue devices (Cédric Le Goater) [1660908]
- s390/ap: fix error handling in __verify_queue_reservations() (Cédric Le Goater) [1660908]
- s390/zcrypt: code cleanup (Cédric Le Goater) [1660908]
- s390/zcrypt: fix wrong offset index for APKA master key valid state (Cédric Le Goater) [1660908]
- s390/ap: uevent on apmask/aqpmask change (Cédric Le Goater) [1660908]
- s390/vfio-ap: fix kernel doc and signature of group notifier functions (Cédric Le Goater) [1660908]
- s390/ap: enable sysfs attribute scans to force AP bus rescan (Cédric Le Goater) [1660908]
- s390/ap: fix crash on older machines based on QCI info missing (Cédric Le Goater) [1660908]
- s390/ap: notify drivers on config changed and scan complete callbacks (Cédric Le Goater) [1660908]
- s390/ap: driver callback to indicate resource in use (Cédric Le Goater) [1660908]
- MAINTAINERS: update file path for S390 VFIO AP DRIVER (Cédric Le Goater) [1660908]
- s390/vfio-ap: add status attribute to AP queue device's sysfs dir (Cédric Le Goater) [1660908]
- s390/ap: function rework based on compiler warning (Cédric Le Goater) [1660908]
- s390/vfio-ap: s390/crypto: fix all kernel-doc warnings (Cédric Le Goater) [1660908]
- s390/ap: new module option ap.useirq (Cédric Le Goater) [1660908]
- s390/ap: fix state machine hang after failure to enable irq (Cédric Le Goater) [1660908]
- s390/crypto: fix all kernel-doc warnings in vfio_ap_ops.c (Cédric Le Goater) [1660908]
- s390/ap: use the common device_driver pointer (Cédric Le Goater) [1660908]
- s390/vfio-ap: replace open coded locks for VFIO_GROUP_NOTIFY_SET_KVM notification (Cédric Le Goater) [1660908]
- s390/vfio-ap: r/w lock for PQAP interception handler function pointer (Cédric Le Goater) [1660908]
- s390/vfio-ap: clean up mdev resources when remove callback invoked (Cédric Le Goater) [1660908]
- s390/vfio-ap: clean up vfio_ap_drv's definition (Cédric Le Goater) [1660908]
- s390/vfio-ap: fix circular lockdep when setting/clearing crypto masks (Cédric Le Goater) [1660908]
- s390/vfio-ap: clean up vfio_ap resources when KVM pointer invalidated (Cédric Le Goater) [1660908]
- s390/vfio-ap: No need to disable IRQ after queue reset (Cédric Le Goater) [1660908]
- Documentation: s390/vfio-ap: eliminate duplicated word (Cédric Le Goater) [1660908]
- docs: s390: Fix wrong label Guest2 instead of Guest3 (Cédric Le Goater) [1660908]
- s390: vfio-ap: make local functions and data static (Cédric Le Goater) [1660908]
- i40e: Fix set max_tx_rate when it is lower than 1 Mbps (Petr Oros) [2106964]
- i40e: Fix VF set max MTU size (Petr Oros) [2106964]
- iavf: Fix set max MTU size with port VLAN and jumbo frames (Petr Oros) [2106964]
- iavf: Fix bad page state (Petr Oros) [2106964]
- i40e: Fix VF hang when reset is triggered on another VF (Ivan Vecera) [2103801]
- mpi3mr: a minor change (Tomas Henzl) [2115748]
- scsi: mpi3mr: Select CONFIG_SCSI_SAS_ATTRS (Tomas Henzl) [2115748]
- scsi: mpi3mr: Remove unnecessary cast (Tomas Henzl) [2115748]
- scsi: mpi3mr: Update driver version to 8.2.0.3.0 (Tomas Henzl) [2115748]
- scsi: mpi3mr: Fix scheduling while atomic type bug (Tomas Henzl) [2115748]
- scsi: mpi3mr: Scan the devices during resume time (Tomas Henzl) [2115748]
- scsi: mpi3mr: Free enclosure objects during driver unload (Tomas Henzl) [2115748]
- scsi: mpi3mr: Handle 0xF003 Fault Code (Tomas Henzl) [2115748]
- scsi: mpi3mr: Graceful handling of surprise removal of PCIe HBA (Tomas Henzl) [2115748]
- scsi: mpi3mr: Support new power management framework (Tomas Henzl) [2115748]
- scsi: mpi3mr: Update mpi3 header files (Tomas Henzl) [2115748]
- scsi: mpi3mr: Fix error code in mpi3mr_transport_smp_handler() (Tomas Henzl) [2115748]
- scsi: mpi3mr: Fix error codes in mpi3mr_report_manufacture() (Tomas Henzl) [2115748]
- scsi: mpi3mr: Block I/Os while refreshing target dev objects (Tomas Henzl) [2115748]
- scsi: mpi3mr: Refresh SAS ports during soft reset (Tomas Henzl) [2115748]
- scsi: mpi3mr: Support SAS transport class callbacks (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add framework to issue MPT transport cmds (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add SAS SATA end devices to STL (Tomas Henzl) [2115748]
- scsi: mpi3mr: Get target object based on rphy (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add expander devices to STL (Tomas Henzl) [2115748]
- scsi: mpi3mr: Enable STL on HBAs where multipath is disabled (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add helper functions to manage device's port (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add helper functions to retrieve device objects (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add framework to add phys to STL (Tomas Henzl) [2115748]
- scsi: mpi3mr: Enable Enclosure device add event (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add helper functions to retrieve config pages (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add framework to issue config requests (Tomas Henzl) [2115748]
- scsi: mpi3mr: Add config and transport related debug flags (Tomas Henzl) [2115748]
- scsi: mpi3mr: Delete a stray tab (Tomas Henzl) [2115748]
- scsi: mpi3mr: Unlock on error path (Tomas Henzl) [2115748]
- scsi: mpi3mr: Reduce VD queue depth on detecting throttling (Tomas Henzl) [2115748]
- scsi: mpi3mr: Resource Based Metering (Tomas Henzl) [2115748]
- scsi: mpi3mr: Increase cmd_per_lun to 128 (Tomas Henzl) [2115748]
- scsi: mpi3mr: Enable shared host tagset (Tomas Henzl) [2115748]
- lpfc version to 14.0.0.18. (Dick Kennedy) [2114050]
- scsi: lpfc: Create a sysfs entry called lpfc_xcvr_data for transceiver info (Dick Kennedy) [2114050]
- scsi: lpfc: Log when congestion management limits are in effect (Dick Kennedy) [2114050]
- scsi: lpfc: Fix hard lockup when reading the rx_monitor from debugfs (Dick Kennedy) [2114050]
- scsi: lpfc: Set sli4_param's cmf option to zero when CMF is turned off (Dick Kennedy) [2114050]
- scsi: lpfc: Fix various issues reported by tools (Dick Kennedy) [2114050]
- scsi: lpfc: Add reporting capability for Link Degrade Signaling (Dick Kennedy) [2114050]
- scsi: lpfc: Rework FDMI attribute registration for unintential padding (Dick Kennedy) [2114050]
- scsi: lpfc: Rework lpfc_fdmi_cmd() routine for cleanup and consistency (Dick Kennedy) [2114050]
- scsi: lpfc: Update congestion mode logging for Emulex SAN Manager application (Dick Kennedy) [2114050]
- scsi: lpfc: Fix multiple NVMe remoteport registration calls for the same NPort ID (Dick Kennedy) [2114050]
- scsi: lpfc: Add missing free iocb and nlp kref put for early return VMID cases (Dick Kennedy) [2114050]
- scsi: lpfc: Fix mbuf pool resource detected as busy at driver unload (Dick Kennedy) [2114050]
- scsi: lpfc: Fix FLOGI ACC with wrong SID in PT2PT topology (Dick Kennedy) [2114050]
- scsi: lpfc: Fix prli_fc4_req checks in PRLI handling (Dick Kennedy) [2114050]
- scsi: lpfc: Remove unneeded result variable (Dick Kennedy) [2114050]
- scsi: lpfc: Remove the unneeded result variable (Dick Kennedy) [2114050]
- scsi: lpfc: Copyright updates for 14.2.0.6 patches (Dick Kennedy) [2114050]
- scsi: lpfc: Add warning notification period to CMF_SYNC_WQE (Dick Kennedy) [2114050]
- scsi: lpfc: Rework MIB Rx Monitor debug info logic (Dick Kennedy) [2114050]
- scsi: lpfc: Fix null ndlp ptr dereference in abnormal exit path for GFT_ID (Dick Kennedy) [2114050]
- scsi: lpfc: Fix unsolicited FLOGI receive handling during PT2PT discovery (Dick Kennedy) [2114050]
- scsi: lpfc: Check the return value of alloc_workqueue() (Dick Kennedy) [2114050]
- scsi: lpfc: Rework FDMI initialization after link up (Dick Kennedy) [2114050]
- scsi: mpt3sas: Revert "scsi: mpt3sas: Fix ioc->base_readl() use" (Tomas Henzl) [2115763]
- scsi: mpt3sas: Revert "scsi: mpt3sas: Fix writel() use" (Tomas Henzl) [2115763]
- scsi: mpt3sas: Fix return value check of dma_get_required_mask() (Tomas Henzl) [2115763]
- scsi: mpt3sas: Fix use-after-free warning (Tomas Henzl) [2115763]
- scsi: mpt3sas: Update driver version to 43.100.00.00 (Tomas Henzl) [2115763]
- scsi: mpt3sas: Increase cmd_per_lun to 128 (Tomas Henzl) [2115763]
- scsi: mpt3sas: Fix trace buffer registration failed (Tomas Henzl) [2115763]
- scsi: mpt3sas: Don't change DMA mask while reallocating pools (Tomas Henzl) [2115763]
- scsi: mpt3sas: Prevent error handler escalation when device removed (Tomas Henzl) [2115763]
- scsi: mpt3sas: Disable MPI2_FUNCTION_FW_DOWNLOAD for ATTO devices (Tomas Henzl) [2115763]
- scsi: mpt3sas: Add support for ATTO ExpressSAS H12xx GT devices (Tomas Henzl) [2115763]
- scsi: mpt3sas: Remove flush_scheduled_work() call (Tomas Henzl) [2115763]
- scsi: mpt3sas: Fix whitespace and spelling mistake (Tomas Henzl) [2115763]
- scsi: mpt3sas: Fix typo in comment (Tomas Henzl) [2115763]
- scsi: mpt3sas: Fix out-of-bounds compiler warning (Tomas Henzl) [2115763]
- media: em28xx: initialize refcount before kref_get (Dean Nelson) [2128003] {CVE-2022-3239}
- gfs2: Register fs after creating workqueues (Bob Peterson) [2121201]
- sysctl: returns -EINVAL when a negative value is passed to proc_doulongvec_minmax (Vratislav Bendel) [2139096]
- mm/rmap: Fix anon_vma->degree ambiguity leading to double-reuse (Waiman Long) [2137585] {CVE-2022-42703}
- mm: rmap: explicitly reset vma->anon_vma in unlink_anon_vmas() (Waiman Long) [2137585] {CVE-2022-42703}
- mm/rmap: Fix typos in comments (Waiman Long) [2137585] {CVE-2022-42703}
- iavf: Fix set max MTU size with port VLAN and jumbo frames (Stefan Assmann) [2103944]
- iavf: Fix bad page state (Stefan Assmann) [2103944]
- iavf: Fix cached head and tail value for iavf_get_tx_pending (Stefan Assmann) [2103944]
- iavf: Fix change VF's mac address (Stefan Assmann) [2103944]
- iavf: Fix race between iavf_close and iavf_reset_task (Stefan Assmann) [2103944]
- net: ethernet: move from strlcpy with unused retval to strscpy (Stefan Assmann) [2103944]
- iavf: Fix 'tc qdisc show' listing too many queues (Stefan Assmann) [2103944]
- iavf: Fix max_rate limiting (Stefan Assmann) [2103944]
- iavf: Check for duplicate TC flower filter before parsing (Stefan Assmann) [2103944]
- iavf: Fix handling of dummy receive descriptors (Stefan Assmann) [2103944]
- iavf: Disallow changing rx/tx-frames and rx/tx-frames-irq (Stefan Assmann) [2103944]
- intel/iavf:fix repeated words in comments (Stefan Assmann) [2103944]
- intel: remove unused macros (Stefan Assmann) [2103944]
- iavf: Add waiting for response from PF in set mac (Stefan Assmann) [2103944]
- iavf: Use irq_update_affinity_hint() (Stefan Assmann) [2103944]
- net: Fix return value of qdisc ingress handling on success (Ivan Vecera) [2131361]

* Mon Nov 14 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-438.el8]
- PCI: hv: Do not set PCI_COMMAND_MEMORY to reduce VM boot time (Emanuele Giuseppe Esposito) [2082836]
- megaraid_sas: add #ifdef CONFIG_RHEL_DIFFERENCES (Tomas Henzl) [2119096]
- mpt3sas: add #ifdef CONFIG_RHEL_DIFFERENCES (Tomas Henzl) [2119096]
- mptcp: fix unreleased socket in accept queue (Paolo Abeni) [2135884]
- mptcp: factor out __mptcp_close() without socket lock (Paolo Abeni) [2135884]
- mptcp: do not queue data on closed subflows (Paolo Abeni) [2135884]
- mptcp: move subflow cleanup in mptcp_destroy_common() (Paolo Abeni) [2135884]
- mptcp: fix msk traversal in mptcp_nl_cmd_set_flags() (Paolo Abeni) [2135884]
- xfs: fix perag reference leak on iteration race with growfs (Brian Foster) [2081105]
- xfs: terminate perag iteration reliably on agcount (Brian Foster) [2081105]
- xfs: rename the next_agno perag iteration variable (Brian Foster) [2081105]
- xfs: fold perag loop iteration logic into helper function (Brian Foster) [2081105]
- xfs: prevent spoofing of rtbitmap blocks when recovering buffers (Brian Foster) [2081105]
- xfs: Enforce attr3 buffer recovery order (Brian Foster) [2081105]
- xfs: avoid unnecessary waits in xfs_log_force_lsn() (Brian Foster) [2081105]
- xfs: factor out forced iclog flushes (Brian Foster) [2081105]
- xfs: detect misaligned rtinherit directory extent size hints (Brian Foster) [2081105]
- xfs: fix an integer overflow error in xfs_growfs_rt (Brian Foster) [2081105]
- xfs: improve FSGROWFSRT precondition checking (Brian Foster) [2081105]
- xfs: reset child dir '..' entry when unlinking child (Brian Foster) [2081105]
- xfs: check for sparse inode clusters that cross new EOAG when shrinking (Brian Foster) [2081105]
- xfs: Fix multiple fall-through warnings for Clang (Brian Foster) [2081105]
- xfs: remove callback dequeue loop from xlog_state_do_iclog_callbacks (Brian Foster) [2081105]
- xfs: don't nest icloglock inside ic_callback_lock (Brian Foster) [2081105]
- xfs: Initialize error in xfs_attr_remove_iter (Brian Foster) [2081105]
- xfs: remove dead stale buf unpin handling code (Brian Foster) [2081105]
- xfs: hold buffer across unpin and potential shutdown processing (Brian Foster) [2081105]
- xfs: force the log offline when log intent item recovery fails (Brian Foster) [2081105]
- xfs: shorten the shutdown messages to a single line (Brian Foster) [2081105]
- xfs: print name of function causing fs shutdown instead of hex pointer (Brian Foster) [2081105]
- xfs: fix type mismatches in the inode reclaim functions (Brian Foster) [2081105]
- xfs: separate primary inode selection criteria in xfs_iget_cache_hit (Brian Foster) [2081105]
- xfs: refactor the inode recycling code (Brian Foster) [2081105]
- xfs: add iclog state trace events (Brian Foster) [2081105]
- xfs: xfs_log_force_lsn isn't passed a LSN (Brian Foster) [2081105]
- xfs: remove need_start_rec parameter from xlog_write() (Brian Foster) [2081105]
- xfs: remove xfs_blkdev_issue_flush (Brian Foster) [2081105]
- xfs: Fix 64-bit division on 32-bit in xlog_state_switch_iclogs() (Brian Foster) [2081105]
- xfs: log stripe roundoff is a property of the log (Brian Foster) [2081105]
- xfs: remove redundant initialization of variable error (Brian Foster) [2081105]
- xfs: perag may be null in xfs_imap() (Brian Foster) [2081105]
- xfs: Make attr name schemes consistent (Brian Foster) [2081105]
- xfs: Fix default ASSERT in xfs_attr_set_iter (Brian Foster) [2081105]
- xfs: rename struct xfs_eofblocks to xfs_icwalk (Brian Foster) [2081105]
- xfs: change the prefix of XFS_EOF_FLAGS_* to XFS_ICWALK_FLAG_ (Brian Foster) [2081105]
- xfs: selectively keep sick inodes in memory (Brian Foster) [2081105]
- xfs: drop IDONTCACHE on inodes when we mark them sick (Brian Foster) [2081105]
- xfs: drop the AGI being passed to xfs_check_agi_freecount (Brian Foster) [2081105]
- xfs: cleanup error handling in xfs_buf_get_map (Brian Foster) [2081105]
- xfs: remove ->b_offset handling for page backed buffers (Brian Foster) [2081105]
- xfs: refactor per-AG inode tagging functions (Brian Foster) [2081105]
- xfs: merge xfs_reclaim_inodes_ag into xfs_inode_walk_ag (Brian Foster) [2081105]
- xfs: pass struct xfs_eofblocks to the inode scan callback (Brian Foster) [2081105]
- xfs: make the icwalk processing functions clean up the grab state (Brian Foster) [2081105]
- xfs: clean up inode state flag tests in xfs_blockgc_igrab (Brian Foster) [2081105]
- xfs: remove indirect calls from xfs_inode_walk{,_ag} (Brian Foster) [2081105]
- xfs: remove iter_flags parameter from xfs_inode_walk_* (Brian Foster) [2081105]
- xfs: move xfs_inew_wait call into xfs_dqrele_inode (Brian Foster) [2081105]
- xfs: separate the dqrele_all inode grab logic from xfs_inode_walk_ag_grab (Brian Foster) [2081105]
- xfs: pass the goal of the incore inode walk to xfs_inode_walk() (Brian Foster) [2081105]
- xfs: rename xfs_inode_walk functions to xfs_icwalk (Brian Foster) [2081105]
- xfs: move the inode walk functions further down (Brian Foster) [2081105]
- xfs: detach inode dquots at the end of inactivation (Brian Foster) [2081105]
- xfs: move the quotaoff dqrele inode walk into xfs_icache.c (Brian Foster) [2081105]
- xfs: don't take a spinlock unconditionally in the DIO fastpath (Brian Foster) [2081105]
- xfs: mark xfs_bmap_set_attrforkoff static (Brian Foster) [2081105]
- xfs: Remove redundant assignment to busy (Brian Foster) [2081105]
- xfs: sort variable alphabetically to avoid repeated declaration (Brian Foster) [2081105]
- xfs: remove xfs_perag_t (Brian Foster) [2081105]
- xfs: use perag through unlink processing (Brian Foster) [2081105]
- xfs: clean up and simplify xfs_dialloc() (Brian Foster) [2081105]
- xfs: inode allocation can use a single perag instance (Brian Foster) [2081105]
- xfs: get rid of xfs_dir_ialloc() (Brian Foster) [2081105]
- xfs: collapse AG selection for inode allocation (Brian Foster) [2081105]
- xfs: simplify xfs_dialloc_select_ag() return values (Brian Foster) [2081105]
- xfs: remove agno from btree cursor (Brian Foster) [2081105]
- xfs: use perag for ialloc btree cursors (Brian Foster) [2081105]
- xfs: convert allocbt cursors to use perags (Brian Foster) [2081105]
- xfs: convert refcount btree cursor to use perags (Brian Foster) [2081105]
- xfs: convert rmap btree cursor to using a perag (Brian Foster) [2081105]
- xfs: add a perag to the btree cursor (Brian Foster) [2081105]
- xfs: pass perags around in fsmap data dev functions (Brian Foster) [2081105]
- xfs: push perags through the ag reservation callouts (Brian Foster) [2081105]
- xfs: pass perags through to the busy extent code (Brian Foster) [2081105]
- xfs: convert secondary superblock walk to use perags (Brian Foster) [2081105]
- xfs: convert xfs_iwalk to use perag references (Brian Foster) [2081105]
- xfs: convert raw ag walks to use for_each_perag (Brian Foster) [2081105]
- xfs: make for_each_perag... a first class citizen (Brian Foster) [2081105]
- xfs: move perag structure and setup to libxfs/xfs_ag.[ch] (Brian Foster) [2081105]
- xfs: prepare for moving perag definitions and support to libxfs (Brian Foster) [2081105]
- xfs: move xfs_perag_get/put to xfs_ag.[ch] (Brian Foster) [2081105]
- xfs: remove unnecessary shifts (Brian Foster) [2081105]
- xfs: clean up open-coded fs block unit conversions (Brian Foster) [2081105]
- xfs: Clean up xfs_attr_node_addname_clear_incomplete (Brian Foster) [2081105]
- xfs: Remove xfs_attr_rmtval_set (Brian Foster) [2081105]
- xfs: Add delay ready attr set routines (Brian Foster) [2081105]
- xfs: Add delay ready attr remove routines (Brian Foster) [2081105]
- xfs: Hoist node transaction handling (Brian Foster) [2081105]
- xfs: Hoist xfs_attr_leaf_addname (Brian Foster) [2081105]
- xfs: Hoist xfs_attr_node_addname (Brian Foster) [2081105]
- xfs: Add helper xfs_attr_node_addname_find_attr (Brian Foster) [2081105]
- xfs: Separate xfs_attr_node_addname and xfs_attr_node_addname_clear_incomplete (Brian Foster) [2081105]
- xfs: Refactor xfs_attr_set_shortform (Brian Foster) [2081105]
- xfs: Add xfs_attr_node_remove_name (Brian Foster) [2081105]
- xfs: Reverse apply 72b97ea40d (Brian Foster) [2081105]
- xfs: use xfs_buf_alloc_pages for uncached buffers (Brian Foster) [2081105]
- xfs: split up xfs_buf_allocate_memory (Brian Foster) [2081105]
- xfs: Fix fall-through warnings for Clang (Brian Foster) [2081105]
- scsi: qla2xxx: Use transport-defined speed mask for supported_speeds (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix serialization of DCBX TLV data request (Nilesh Javali) [2109830]
- scsi: qla2xxx: Remove unused declarations for qla2xxx (Nilesh Javali) [2109830]
- scsi: qla2xxx: Drop DID_TARGET_FAILURE use (Nilesh Javali) [2109830]
- scsi: qla2xxx: Update version to 10.02.07.900-k (Nilesh Javali) [2109830]
- scsi: qla2xxx: Add NVMe parameters support in Auxiliary Image Status (Nilesh Javali) [2109830]
- scsi: qla2xxx: Add debugfs create/delete helpers (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix response queue handler reading stale packets (Nilesh Javali) [2109830]
- scsi: qla2xxx: Revert "scsi: qla2xxx: Fix response queue handler reading stale packets" (Nilesh Javali) [2109830]
- scsi: qla2xxx: Log message "skipping scsi_scan_host()" as informational (Nilesh Javali) [2109830]
- scsi: qla2xxx: Avoid flush_scheduled_work() usage (Nilesh Javali) [2109830]
- scsi: qla2xxx: Always wait for qlt_sess_work_fn() from qlt_stop_phase1() (Nilesh Javali) [2109830]
- scsi: qla2xxx: Remove unused del_sess_list field (Nilesh Javali) [2109830]
- scsi: qla2xxx: Remove unused qlt_tmr_work() (Nilesh Javali) [2109830]
- scsi: qla2xxx: Update version to 10.02.07.800-k (Nilesh Javali) [2109830]
- scsi: qla2xxx: Update manufacturer details (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix discovery issues in FC-AL topology (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix dropped IKE message (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix response queue handler reading stale packets (Nilesh Javali) [2109830]
- scsi: qla2xxx: Zero undefined mailbox IN registers (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix incorrect display of max frame size (Nilesh Javali) [2109830]
- scsi: qla2xxx: Check correct variable in qla24xx_async_gffid() (Nilesh Javali) [2109830]
- scsi: qla2xxx: Update version to 10.02.07.700-k (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix losing FCP-2 targets on long port disable with I/Os (Nilesh Javali) [2109830]
- scsi: qla2xxx: Add debug prints in the device remove path (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix losing target when it reappears during delete (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix losing FCP-2 targets during port perturbation tests (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix crash due to stale SRB access around I/O timeouts (Nilesh Javali) [2109830]
- scsi: qla2xxx: Turn off multi-queue for 8G adapters (Nilesh Javali) [2109830]
- scsi: qla2xxx: Wind down adapter after PCIe error (Nilesh Javali) [2109830]
- scsi: qla2xxx: Update version to 10.02.07.600-k (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix slow session teardown (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Reduce N2N thrashing at app_start time (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix no logout on delete for N2N (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix session thrash (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Tear down session if keys have been removed (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix no login after app start (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Reduce disruption due to multiple app start (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Send LOGO for unexpected IKE message (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix I/O timeout due to over-subscription (Nilesh Javali) [2109830]
- scsi: qla2xxx: Update version to 10.02.07.500-k (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix n2n login retry for secure device (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix n2n discovery issue with secure target (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Remove old doorbell interface (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Add retry for ELS passthrough (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Synchronize NPIV deletion with authentication application (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Fix potential stuck session in sa update (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Add bsg interface to read doorbell events (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Wait for app to ack on sess down (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: bsg refactor (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Reduce Initiator-Initiator thrashing (Nilesh Javali) [2109830]
- scsi: qla2xxx: Remove unused 'ql_dm_tgt_ex_pct' parameter (Nilesh Javali) [2109830]
- scsi: qla2xxx: Remove setting of 'req' and 'rsp' parameters (Nilesh Javali) [2109830]
- scsi: qla2xxx: Fix missed DMA unmap for aborted commands (Nilesh Javali) [2109830]
- scsi: qla2xxx: edif: Remove unneeded variable (Nilesh Javali) [2109830]
- scsi: qla2xxx: Remove unneeded flush_workqueue() (Nilesh Javali) [2109830]
- scsi: qla2xxx: Remove free_sg command flag (Nilesh Javali) [2109830]
- scsi: megaraid_sas: Clean up some inconsistent indenting (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Move megasas_dbg_lvl init to megasas_init() (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Remove unnecessary memset() (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Simplify megasas_update_device_list (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Correct an error message (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Correct value passed to scsi_device_lookup() (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Use struct_size() in code related to struct MR_PD_CFG_SEQ_NUM_SYNC (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Use struct_size() in code related to struct MR_FW_RAID_MAP (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Replace one-element array with flexible-array member in MR_PD_CFG_SEQ_NUM_SYNC (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Replace one-element array with flexible-array member in MR_DRV_RAID_MAP (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Replace one-element array with flexible-array member in MR_FW_RAID_MAP_DYNAMIC (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Replace one-element array with flexible-array member in MR_FW_RAID_MAP (Tomas Henzl) [2120070]
- scsi: megaraid: Remove redundant assignment to variable mfiStatus (Tomas Henzl) [2120070]
- scsi: megaraid_sas: Remove redundant variable cmd_type (Tomas Henzl) [2120070]
- platform/x86/intel/vsec: Fix wrong type for local status variables (Prarit Bhargava) [2076744]
- platform/x86/intel/vsec: Add PCI error recovery support to Intel PMT (Prarit Bhargava) [2076744]
- platform/x86/intel/vsec: Add support for Raptor Lake (Prarit Bhargava) [2076744]
- platform/x86/intel/pmt: telemetry: Fix fixed region handling (Prarit Bhargava) [2076744]
- platform/x86/intel/vsec: Rework early hardware code (Prarit Bhargava) [2076744]
- platform/x86/intel: Fix pmt_crashlog array reference (Prarit Bhargava) [2076744]
- powerpc/kexec_file: Use current CPU info while setting up FDT (Mamatha Inamdar) [2126520]
- mm/kmemleak: prevent soft lockup in kmemleak_scan()'s object iteration loops (Waiman Long) [2095075]
- mm/kmemleak: prevent soft lockup in first object iteration loop of kmemleak_scan() (Waiman Long) [2095075]
- mm/kmemleak: skip unlikely objects in kmemleak_scan() without taking lock (Waiman Long) [2095075]
- mm/kmemleak: use _irq lock/unlock variants in kmemleak_scan/_clear() (Waiman Long) [2095075]
- mm/kmemleak: avoid scanning potential huge holes (Waiman Long) [2095075]
- KVM: s390: pci: fix GAIT physical vs virtual pointers usage (Thomas Huth) [1664379]
- KVM: s390: pci: fix plain integer as NULL pointer warnings (Thomas Huth) [1664379]
- KVM: s390/pci: fix include duplicates (Thomas Huth) [1664379]
- redhat: Use group notifier to get the KVM pointer in the vfio_pci_zdev code (Thomas Huth) [1664379]
- KVM: s390: pci: register pci hooks without interpretation (Thomas Huth) [1664379]
- KVM: s390: pci: Hook to access KVM lowlevel from VFIO (Thomas Huth) [1664379]
- Documentation: kvm: extend KVM_S390_ZPCI_OP subheading underline (Thomas Huth) [1664379]
- KVM: s390: add KVM_S390_ZPCI_OP to manage guest zPCI devices (Thomas Huth) [1664379]
- vfio-pci/zdev: different maxstbl for interpreted devices (Thomas Huth) [1664379]
- vfio-pci/zdev: add function handle to clp base capability (Thomas Huth) [1664379]
- vfio-pci/zdev: add open/close device hooks (Thomas Huth) [1664379]
- KVM: s390: pci: add routines to start/stop interpretive execution (Thomas Huth) [1664379]
- KVM: s390: pci: provide routines for enabling/disabling interrupt forwarding (Thomas Huth) [1664379]
- KVM: s390: mechanism to enable guest zPCI Interpretation (Thomas Huth) [1664379]
- KVM: s390: pci: enable host forwarding of Adapter Event Notifications (Thomas Huth) [1664379]
- KVM: s390: pci: do initial setup for AEN interpretation (Thomas Huth) [1664379]
- KVM: s390: pci: add basic kvm_zdev structure (Thomas Huth) [1664379]
- redhat: Enable the new CONFIG_VFIO_PCI_ZDEV_KVM switch (Thomas Huth) [1664379]
- vfio/pci: introduce CONFIG_VFIO_PCI_ZDEV_KVM (Thomas Huth) [1664379]
- vfio/pci: remove CONFIG_VFIO_PCI_ZDEV from Kconfig (Thomas Huth) [1664379]
- vfio-pci/zdev: fix possible segmentation fault issue (Thomas Huth) [1664379]
- s390/pci: stash dtsm and maxstbl (Thomas Huth) [1664379]
- s390/pci: stash associated GISA designation (Thomas Huth) [1664379]
- s390/pci: externalize the SIC operation controls and routine (Thomas Huth) [1664379]
- s390/airq: allow for airq structure that uses an input vector (Thomas Huth) [1664379]
- s390/airq: pass more TPI info to airq handlers (Thomas Huth) [1664379]
- s390/cio: add tpi.h header file (Thomas Huth) [1664379]
- s390/ap: fix kernel doc comments (Thomas Huth) [1664379]
- s390/sclp: detect the AISI facility (Thomas Huth) [1664379]
- s390/sclp: detect the AENI facility (Thomas Huth) [1664379]
- s390/sclp: detect the AISII facility (Thomas Huth) [1664379]
- s390/sclp: detect the zPCI load/store interpretation facility (Thomas Huth) [1664379]
- s390/sclp: add detection of IPL-complete-control facility (Thomas Huth) [1664379]
- s390/pci: add error record for CC 2 retries (Thomas Huth) [2134399]
- s390/pci: add PCI access type and length to error records (Thomas Huth) [2134399]
- s390/pci: don't log availability events as errors (Thomas Huth) [2134399]
- s390/pci: make better use of zpci_dbg() levels (Thomas Huth) [2134399]
- s390/pci: rename get_zdev_by_bus() to zdev_from_bus() (Thomas Huth) [2134399]
- redhat: Restore clp_rescan_pci_devices_simple() function (Thomas Huth) [2134399]
- s390/pci: improve zpci_dev reference counting (Thomas Huth) [2134399]
- s390/pci: make zpci_set_irq()/zpci_clear_irq() static (Thomas Huth) [2134399]
- s390/pci: simplify __pciwb_mio() inline asm (Thomas Huth) [2134399]
- s390/pci: use physical addresses in DMA tables (Thomas Huth) [2134399]
- s390/pci: use phys_to_virt() for AIBVs/DIBVs (Thomas Huth) [2134399]
- s390/pci: implement minimal PCI error recovery (Thomas Huth) [2134399]
- PCI: Export pci_dev_lock() (Thomas Huth) [2134399]
- PCI: Export pci_dev_trylock() and pci_dev_unlock() (Thomas Huth) [2134399]
- s390/pci: implement reset_slot for hotplug slot (Thomas Huth) [2134399]
- s390/pci: refresh function handle in iomap (Thomas Huth) [2134399]
- s390/pci: add simpler s390dbf traces for events (Thomas Huth) [2134399]
- s390/pci: tolerate inconsistent handle in recover (Thomas Huth) [2134399]
- s390/pci_mmio: fully validate the VMA before calling follow_pte() (Thomas Huth) [2134399]
- s390/pci: read clp_list_pci_req only once (Thomas Huth) [2134399]
- s390/pci: fix clp_get_state() handling of -ENODEV (Thomas Huth) [2134399]
- s390/pci: improve DMA translation init and exit (Thomas Huth) [2134399]
- s390/pci: simplify CLP List PCI handling (Thomas Huth) [2134399]
- s390/pci: handle FH state mismatch only on disable (Thomas Huth) [2134399]
- s390/pci: fix misleading rc in clp_set_pci_fn() (Thomas Huth) [2134399]
- s390/pci: reset zdev->zbus on registration failure (Thomas Huth) [2134399]
- s390/pci: cleanup resources only if necessary (Thomas Huth) [2134399]
- s390/pci: add zpci_set_irq()/zpci_clear_irq() (Thomas Huth) [2134399]
- s390/pci: use register pair instead of register asm (Thomas Huth) [2134399]
- s390: introduce register pair union (Thomas Huth) [2134399]
- s390/pci: handle stale deconfiguration events (Thomas Huth) [2134399]
- s390/pci: rename zpci_configure_device() (Thomas Huth) [2134399]
- s390/pci: narrow scope of zpci_configure_device() (Thomas Huth) [2134399]
- s390/pci: separate zbus registration from scanning (Thomas Huth) [2134399]
- s390/pci: use mutex not spinlock for zbus list (Thomas Huth) [2134399]
- s390/pci: separate zbus creation from scanning (Thomas Huth) [2134399]
- s390/pci: do more bus setup in zpci_bus_scan() (Thomas Huth) [2134399]
- s390/pci: introduce zpci_bus_scan_device() (Thomas Huth) [2134399]
- s390/pci: fix DMA cleanup on hard deconfigure (Thomas Huth) [2134399]
- s390/pci: move zpci_remove_device() to bus code (Thomas Huth) [2134399]
- s390/pci: unify de-/configure for slots and events (Thomas Huth) [2134399]
- s390/pci: add zpci_event_hard_deconfigured() (Thomas Huth) [2134399]
- s390/pci: deconfigure device on release (Thomas Huth) [2134399]
- s390/pci: refactor zpci function states (Thomas Huth) [2134399]
- s390/pci: inform when missing required facilities (Thomas Huth) [2134399]
- s390/pci: remove races against pte updates (Thomas Huth) [2134399]
- s390: remove orphaned function declarations (Thomas Huth) [2134399]
- s390/pci: add missing pci_iov.h include (Thomas Huth) [2134399]
- s390/pci: remove clp_rescan_pci_devices_simple() (Thomas Huth) [2134399]
- s390/pci: remove clp_rescan_pci_devices() (Thomas Huth) [2134399]
- s390/pci: consolidate SR-IOV specific code (Thomas Huth) [2134399]
- s390/pci: Implement ioremap_wc/prot() with MIO (Thomas Huth) [2134399]
- s390/mm: properly clear _PAGE_NOEXEC bit when it is not supported (Thomas Huth) [2134399]
- s390/pci: clarify comment in s390_mmio_read/write (Thomas Huth) [2134399]
- s390/pci: remove unused functions (Thomas Huth) [2134399]
- s390/pci: Log new handle in clp_disable_fh() (Thomas Huth) [2134399]
- s390/pci: ioremap() align with generic code (Thomas Huth) [2134399]
- s390: enforce CONFIG_SMP (Thomas Huth) [2134399]
- s390/pci: mark function(s) __always_inline (Thomas Huth) [2134399]
- s390/pci: avoid using strncmp with hardcoded length (Thomas Huth) [2134399]
- s390/pci: PCI_IOV_RESOURCES loop refactoring in zpci_map_resources (Thomas Huth) [2134399]
- s390: pci: no need to check return value of debugfs_create functions (Thomas Huth) [2134399]
- s390/pci: fix sleeping in atomic during hotplug (Thomas Huth) [2134399]
- s390/pci: remove fmb address from debug output (Thomas Huth) [2134399]
- s390/pci: add fmt3 fmb (Thomas Huth) [2134399]
- tools headers kvm s390: Sync headers with the kernel sources (Thomas Huth) [2111063]
- KVM: s390: resetting the Topology-Change-Report (Thomas Huth) [2111063]
- KVM: s390: guest support for topology function (Thomas Huth) [2111063]
- KVM: s390: Cleanup ipte lock access and SIIF facility checks (Thomas Huth) [2111063]
- KVM: s390: drop unexpected word 'and' in the comments (Thomas Huth) [2111063]
- Documentation: KVM: update s390-diag.rst reference (Thomas Huth) [2043872]
- Documentation: KVM: update msr.rst reference (Thomas Huth) [2043872]
- Documentation: KVM: update amd-memory-encryption.rst references (Thomas Huth) [2043872]
- Documentation: KVM: update s390-pv.rst reference (Thomas Huth) [2043872]
- Documentation/virt/kvm/api.rst: Explain rc/rrc delivery (Thomas Huth) [2043872]
- Documentation/virt/kvm/api.rst: Add protvirt dump/info api descriptions (Thomas Huth) [2043872]
- Documentation: KVM: add API issues section (Thomas Huth) [2043872]
- Documentation: virt: Protected virtual machine dumps (Thomas Huth) [2043872]
- Documentation: KVM: add separate directories for architecture-specific documentation (Thomas Huth) [2043872]
- KVM: s390: Add KVM_CAP_S390_PROTECTED_DUMP (Thomas Huth) [2043872]
- KVM: s390: Add CPU dump functionality (Thomas Huth) [2043872]
- KVM: s390: Add configuration dump functionality (Thomas Huth) [2043872]
- KVM: s390: pv: Add query dump information (Thomas Huth) [2043872]
- KVM: s390: pv: Add dump support definitions (Thomas Huth) [2043872]
- KVM: s390: pv: Add query interface (Thomas Huth) [2043872]
- s390/uv: Add dump fields to query (Thomas Huth) [2043872]
- s390/uv: Add SE hdr query information (Thomas Huth) [2043872]
- kvm: Move KVM_GET_XSAVE2 IOCTL definition at the end of kvm.h (Thomas Huth) [2043872]
- docs: kvm: fix WARNINGs from api.rst (Thomas Huth) [2043872]
- s390/mm: use non-quiescing sske for KVM switch to keyed guest (Thomas Huth) [2043872]
- s390/gmap: voluntarily schedule during key setting (Thomas Huth) [2043872]
- KVM: s390: Don't indicate suppression on dirtying, failing memop (Thomas Huth) [2043872]
- s390: uv: Add offset comments to UV query struct and fix naming (Thomas Huth) [2043872]
- KVM: s390: Use Makefile.kvm for common files (Thomas Huth) [2043872]
- KVM: s390: Skip gfn/size sanity checks on memslot DELETE or FLAGS_ONLY (Thomas Huth) [2043872]
- fs: dlm: fix invalid derefence of sb_lvbptr (Alexander Aring) [2121790]
- fs: dlm: handle -EBUSY first in unlock validation (Alexander Aring) [2121790]
- fs: dlm: handle -EBUSY first in lock arg validation (Alexander Aring) [2121790]
- fs: dlm: fix race between test_bit() and queue_work() (Alexander Aring) [2121790]
- scsi: core: Fix a use-after-free (Ming Lei) [1961010]
- net/mlx5e: Fix wrong use of skb_tcp_all_headers() with encapsulation (Petr Oros) [2135685]
- net: add skb_[inner_]tcp_all_headers helpers (Petr Oros) [2135685]
- net: marvell: clean up trigraph warning on ??! string (Petr Oros) [2135685]
- powerpc/pseries: Use lparcfg to reconfig VAS windows for DLPAR CPU (Steve Best) [2133103]
- flow_dissector: Do not count vlan tags inside tunnel payload (Ivan Vecera) [2136875]
- flow_offload: Introduce flow_match_pppoe (Ivan Vecera) [2136875]
- net/sched: flower: Add PPPoE filter (Ivan Vecera) [2136875]
- flow_dissector: Add PPPoE dissectors (Ivan Vecera) [2136875]
- net/sched: flower: Consider the number of tags for vlan filters (Ivan Vecera) [2136875]
- net/sched: flower: Add number of vlan tags filter (Ivan Vecera) [2136875]
- flow_dissector: Add number of vlan tags dissector (Ivan Vecera) [2136875]
- net/sched: flower: Reduce identation after is_key_vlan refactoring (Ivan Vecera) [2136875]
- net/sched: flower: Helper function for vlan ethtype checks (Ivan Vecera) [2136875]
- dissector: do not set invalid PPP protocol (Ivan Vecera) [2136875]
- dm bufio: use the acquire memory barrier when testing for B_READING (Benjamin Marzinski) [2139161]
- provide arch_test_bit_acquire for architectures that define test_bit (Benjamin Marzinski) [2139161]
- wait_on_bit: add an acquire memory barrier (Benjamin Marzinski) [2139161]
- add barriers to buffer_uptodate and set_buffer_uptodate (Benjamin Marzinski) [2139161]
- dm verity: Add documentation for try_verify_in_tasklet option (Benjamin Marzinski) [2139161]
- dm cache: delete the redundant word 'each' in comment (Benjamin Marzinski) [2139161]
- dm raid: fix typo in analyse_superblocks code comment (Benjamin Marzinski) [2139161]
- dm verity: enable WQ_HIGHPRI on verify_wq (Benjamin Marzinski) [2139161]
- dm raid: delete the redundant word 'that' in comment (Benjamin Marzinski) [2139161]
- dm: change from DMWARN to DMERR or DMCRIT for fatal errors (Benjamin Marzinski) [2139161]
- dm bufio: fix some cases where the code sleeps with spinlock held (Benjamin Marzinski) [2139161]
- dm writecache: fix smatch warning about invalid return from writecache_map (Benjamin Marzinski) [2139161]
- dm verity: fix verity_parse_opt_args parsing (Benjamin Marzinski) [2139161]
- dm verity: fix DM_VERITY_OPTS_MAX value yet again (Benjamin Marzinski) [2139161]
- dm bufio: simplify DM_BUFIO_CLIENT_NO_SLEEP locking (Benjamin Marzinski) [2139161]
- dm verity: have verify_wq use WQ_HIGHPRI if "try_verify_in_tasklet" (Benjamin Marzinski) [2139161]
- dm verity: remove WQ_CPU_INTENSIVE flag since using WQ_UNBOUND (Benjamin Marzinski) [2139161]
- dm verity: only copy bvec_iter in verity_verify_io if in_tasklet (Benjamin Marzinski) [2139161]
- dm verity: optimize verity_verify_io if FEC not configured (Benjamin Marzinski) [2139161]
- dm verity: conditionally enable branching for "try_verify_in_tasklet" (Benjamin Marzinski) [2139161]
- dm bufio: conditionally enable branching for DM_BUFIO_CLIENT_NO_SLEEP (Benjamin Marzinski) [2139161]
- dm verity: allow optional args to alter primary args handling (Benjamin Marzinski) [2139161]
- dm verity: Add optional "try_verify_in_tasklet" feature (Benjamin Marzinski) [2139161]
- dm bufio: Add DM_BUFIO_CLIENT_NO_SLEEP flag (Benjamin Marzinski) [2139161]
- dm bufio: Add flags argument to dm_bufio_client_create (Benjamin Marzinski) [2139161]
- dm: Start pr_preempt from the same starting path (Benjamin Marzinski) [2139161]
- dm: Fix PR release handling for non All Registrants (Benjamin Marzinski) [2139161]
- dm: Start pr_reserve from the same starting path (Benjamin Marzinski) [2139161]
- dm: Allow dm_call_pr to be used for path searches (Benjamin Marzinski) [2139161]
- Documentation: dm writecache: Render status list as list (Benjamin Marzinski) [2139161]
- Documentation: dm writecache: add blank line before optional parameters (Benjamin Marzinski) [2139161]
- dm snapshot: fix typo in snapshot_map() comment (Benjamin Marzinski) [2139161]
- dm raid: remove redundant "the" in parse_raid_params() comment (Benjamin Marzinski) [2139161]
- dm cache: fix typo in 2 comment blocks (Benjamin Marzinski) [2139161]
- dm verity: fix checkpatch close brace error (Benjamin Marzinski) [2139161]
- dm table: rename dm_target variable in dm_table_add_target() (Benjamin Marzinski) [2139161]
- dm table: audit all dm_table_get_target() callers (Benjamin Marzinski) [2139161]
- dm table: remove dm_table_get_num_targets() wrapper (Benjamin Marzinski) [2139161]
- writeback: Avoid skipping inode writeback (Waiman Long) [2138886]
- writeback: fix obtain a reference to a freeing memcg css (Waiman Long) [2138886]
- mm/memcg: disable threshold event handlers on PREEMPT_RT (Waiman Long) [2138886]
- memcg: increase MEMCG_CHARGE_BATCH to 64 (Waiman Long) [2138886]
- mm: page_counter: rearrange struct page_counter fields (Waiman Long) [2138886]
- mm: page_counter: remove unneeded atomic ops for low/min (Waiman Long) [2138886]
- memcg: reduce size of memcg vmstats structures (Waiman Long) [2138886]
- memcg: rearrange code (Waiman Long) [2138886]
- memcg: extract memcg_vmstats from struct mem_cgroup (Waiman Long) [2138886]
- mm: memcontrol: fix potential oom_lock recursion deadlock (Waiman Long) [2138886]
- mm: memcontrol: add {pgscan,pgsteal}_{kswapd,direct} items in memory.stat of cgroup v2 (Waiman Long) [2138886]
- mm/memcg: protect per-CPU counter by disabling preemption on PREEMPT_RT where needed. (Waiman Long) [2138886]
- writeback: memcg: simplify cgroup_writeback_by_id (Waiman Long) [2138886]
- writeback, cgroup: do not reparent dax inodes (Waiman Long) [2138886]
- writeback, cgroup: remove wb from offline list before releasing refcnt (Waiman Long) [2138886]
- writeback, cgroup: release dying cgwbs by switching attached inodes (Waiman Long) [2138886]
- writeback, cgroup: support switching multiple inodes at once (Waiman Long) [2138886]
- writeback, cgroup: split out the functional part of inode_switch_wbs_work_fn() (Waiman Long) [2138886]
- writeback, cgroup: keep list of inodes attached to bdi_writeback (Waiman Long) [2138886]
- writeback, cgroup: switch to rcu_work API in inode_switch_wbs() (Waiman Long) [2138886]
- writeback, cgroup: increment isw_nr_in_flight before grabbing an inode (Waiman Long) [2138886]
- writeback, cgroup: add smp_mb() to cgroup_writeback_umount() (Waiman Long) [2138886]
- writeback, cgroup: do not switch inodes with I_WILL_FREE flag (Waiman Long) [2138886]
- docs/admin-guide: cgroup-v2: typos and spaces (Waiman Long) [2138886]
- fs: improve comments for writeback_single_inode() (Waiman Long) [2138886]
- writeback: remove struct bdi_writeback_congested (Waiman Long) [2138886]
- writeback: remove {set,clear}_wb_congested (Waiman Long) [2138886]
- fs/writeback.c: use rcu_barrier() to wait for inflight wb switches going into workqueue when umount (Waiman Long) [2138886]
- blkcg: remove unused __blkg_release_rcu() (Waiman Long) [2138886]
- writeback: Add a bdi_writeback_rh extension to struct bdi_writeback (Waiman Long) [2138886]
- RDMA/irdma: Report the correct link speed (Kamal Heib) [2125102]
- blk-mq: avoid double ->queue_rq() because of early timeout (Ming Lei) [2132438]
- blk-mq: add one API for waiting until quiesce is done (Ming Lei) [2132438]
- blk-mq: support concurrent queue quiesce/unquiesce (Ming Lei) [2132438]
- bridge: Do not send empty IFLA_AF_SPEC attribute (Ivan Vecera) [2139133]
- net: bridge: Clear offload_fwd_mark when passing frame up bridge interface. (Ivan Vecera) [2139133]
- net: bridge: vlan: fix memory leak in __allowed_ingress (Ivan Vecera) [2139133]

* Fri Nov 11 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-437.el8]
- ice: Add additional CSR registers to ETHTOOL_GREGS (Petr Oros) [2131024]
- udp: Update reuse->has_conns under reuseport_lock. (Xin Long) [2135937]
- udp: Remove redundant __udp_sysctl_init() call from udp_init(). (Xin Long) [2135937]
- udp: Fix a data-race around sysctl_udp_l3mdev_accept. (Xin Long) [2135937]
- Documentation: fix udp_wmem_min in ip-sysctl.rst (Xin Long) [2135937]
- be2net: Fix buffer overflow in be_get_module_eeprom (Josef Oskera) [2126917]
- iommu/vt-d: Clean up si_domain in the init_dmars() error path (Jerry Snitselaar) [2133331]

* Wed Nov 09 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-436.el8]
- md: Fix spelling mistake in comments of r5l_log (Nigel Croxon) [2112935]
- md/raid5: Wait for MD_SB_CHANGE_PENDING in raid5d (Nigel Croxon) [2112935]
- md/raid10: convert resync_lock to use seqlock (Nigel Croxon) [2112935]
- md/raid10: fix improper BUG_ON() in raise_barrier() (Nigel Croxon) [2112935]
- md/raid10: prevent unnecessary calls to wake_up() in fast path (Nigel Croxon) [2112935]
- md/raid10: don't modify 'nr_waitng' in wait_barrier() for the case nowait (Nigel Croxon) [2112935]
- md/raid10: factor out code from wait_barrier() to stop_waiting_barrier() (Nigel Croxon) [2112935]
- md: Remove extra mddev_get() in md_seq_start() (Nigel Croxon) [2112935]
- md/raid5: Remove unnecessary bio_put() in raid5_read_one_chunk() (Nigel Croxon) [2112935 2111563]
- md/raid5: Ensure stripe_fill happens on non-read IO with journal (Nigel Croxon) [2112935]
- md/raid5: Don't read ->active_stripes if it's not needed (Nigel Croxon) [2112935]
- md/raid5: Cleanup prototype of raid5_get_active_stripe() (Nigel Croxon) [2112935]
- md/raid5: Drop extern on function declarations in raid5.h (Nigel Croxon) [2112935]
- md/raid5: Refactor raid5_get_active_stripe() (Nigel Croxon) [2112935]
- md: Replace snprintf with scnprintf (Nigel Croxon) [2112935]
- md/raid10: fix compile warning (Nigel Croxon) [2112935]
- md/raid5: Fix spelling mistakes in comments (Nigel Croxon) [2112935]
- md: call __md_stop_writes in md_stop (Nigel Croxon) [2112935]
- md: Flush workqueue md_rdev_misc_wq in md_alloc() (Nigel Croxon) [2112935]
- drivers:md:fix a potential use-after-free bug (Nigel Croxon) [2112935]
- md/raid5: Ensure batch_last is released before sleeping for quiesce (Nigel Croxon) [2112935]
- md/raid5: Move stripe_request_ctx up (Nigel Croxon) [2112935]
- md/raid5: Drop unnecessary call to r5c_check_stripe_cache_usage() (Nigel Croxon) [2112935]
- md/raid5: Make is_inactive_blocked() helper (Nigel Croxon) [2112935]
- md/raid5: Refactor raid5_get_active_stripe() (Nigel Croxon) [2112935]
- md-raid10: fix KASAN warning (Nigel Croxon) [2112935]
- md: fix build failure for !MODULE (Nigel Croxon) [2112935]
- raid5: fix duplicate checks for rdev->saved_raid_disk (Nigel Croxon) [2112935]
- md/raid5: Convert prepare_to_wait() to wait_woken() api (Nigel Croxon) [2112935]
- md/raid5: Fix sectors_to_do bitmap overflow in raid5_make_request() (Nigel Croxon) [2112935]
- md: Fix spelling mistake in comments (Nigel Croxon) [2112935]
- md/raid5: Increase restriction on max segments per request (Nigel Croxon) [2112935]
- md/raid5: Improve debug prints (Nigel Croxon) [2112935]
- md/raid5: Pivot raid5_make_request() (Nigel Croxon) [2112935]
- md/raid5: Check all disks in a stripe_head for reshape progress (Nigel Croxon) [2112935]
- md/raid5: Refactor add_stripe_bio() (Nigel Croxon) [2112935]
- md/raid5: Keep a reference to last stripe_head for batch (Nigel Croxon) [2112935]
- md/raid5: Refactor for loop in raid5_make_request() into while loop (Nigel Croxon) [2112935]
- md/raid5: Move read_seqcount_begin() into make_stripe_request() (Nigel Croxon) [2112935]
- md/raid5: Drop the do_prepare flag in raid5_make_request() (Nigel Croxon) [2112935]
- md/raid5: Factor out helper from raid5_make_request() loop (Nigel Croxon) [2112935]
- md/raid5: Move common stripe get code into new find_get_stripe() helper (Nigel Croxon) [2112935]
- md/raid5: Move stripe_add_to_batch_list() call out of add_stripe_bio() (Nigel Croxon) [2112935]
- md/raid5: Refactor raid5_make_request loop (Nigel Croxon) [2112935]
- md/raid5: Factor out ahead_of_reshape() function (Nigel Croxon) [2112935]
- md/raid5: Make logic blocking check consistent with logic that blocks (Nigel Croxon) [2112935]
- md: unlock mddev before reap sync_thread in action_store (Nigel Croxon) [2112935]
- md: Explicitly create command-line configured devices (Nigel Croxon) [2112935]
- md: Notify sysfs sync_completed in md_reap_sync_thread() (Nigel Croxon) [2112935]
- md: Ensure resync is reported after it starts (Nigel Croxon) [2112935]
- md: Use enum for overloaded magic numbers used by mddev->curr_resync (Nigel Croxon) [2112935]
- md/raid5-cache: Annotate pslot with __rcu notation (Nigel Croxon) [2112935]
- md/raid5-cache: Clear conf->log after finishing work (Nigel Croxon) [2112935]
- md/raid5-cache: Drop RCU usage of conf->log (Nigel Croxon) [2112935]
- md/raid5-cache: Take mddev_lock in r5c_journal_mode_show() (Nigel Croxon) [2112935]
- md/raid5: suspend the array for calls to log_exit() (Nigel Croxon) [2112935]
- md/raid5-ppl: Drop unused argument from ppl_handle_flush_request() (Nigel Croxon) [2112935]
- md/raid5-log: Drop extern decorators for function prototypes (Nigel Croxon) [2112935]
- md/raid5: missing error code in setup_conf() (Nigel Croxon) [2112935]
- Revert "md: don't unregister sync_thread with reconfig_mutex held" (Nigel Croxon) [2112935]
- qed: fix typos in comments (Manish Chopra) [2111885]
- net: qede: Remove unnecessary synchronize_irq() before free_irq() (Manish Chopra) [2111885]
- RDMA/qedr: Fix potential memory leak in __qedr_alloc_mr() (Manish Chopra) [2111885]
- qlogic: qed: fix clang -Wformat warnings (Manish Chopra) [2111885]
- qed: Use bitmap_empty() (Manish Chopra) [2111885]
- qed: Use the bitmap API to allocate bitmaps (Manish Chopra) [2111885]
- qlogic/qed: fix repeated words in comments (Manish Chopra) [2111885]
- net: qed: fix typos in comments (Manish Chopra) [2111885]
- RDMA/qedr: Remove unnecessary synchronize_irq() before free_irq() (Manish Chopra) [2111885]
- qed: Remove unnecessary synchronize_irq() before free_irq() (Manish Chopra) [2111885]
- qed: replace bitmap_weight with bitmap_empty in qed_roce_stop() (Manish Chopra) [2111885]
- qed: rework qed_rdma_bmap_free() (Manish Chopra) [2111885]
- qed: Remove IP services API. (Manish Chopra) [2111885]
- qed: remove an unneed NULL check on list iterator (Manish Chopra) [2111885]
- RDMA/irdma: Report RNR NAK generation in device caps (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Use s/g array in post send only when its valid (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Return correct WC error for bind operation failure (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Return error on MR deregister CQP failure (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Report the correct max cqes from query device (Kamal Heib) [2120676 2103957]
- RDMA/siw: Pass a pointer to virt_to_page() (Kamal Heib) [2120676]
- RDMA/cma: Fix arguments order in net device validation (Kamal Heib) [2120676]
- RDMA/irdma: Fix drain SQ hang with no completion (Kamal Heib) [2120676 2103957 2033244 2053376]
- IB/iser: Fix login with authentication (Kamal Heib) [2120676]
- RDMA/ib_srpt: Unify checking rdma_cm_id condition in srpt_cm_req_recv() (Kamal Heib) [2120676]
- RDMA/rxe: Fix error unwind in rxe_create_qp() (Kamal Heib) [2120676]
- RDMA/rxe: Split qp state for requester and completer (Kamal Heib) [2120676]
- RDMA/rxe: Generate error completion for error requester QP state (Kamal Heib) [2120676]
- RDMA/rxe: Update wqe_index for each wqe error completion (Kamal Heib) [2120676]
- RDMA/srpt: Fix a use-after-free (Kamal Heib) [2120676]
- RDMA/srpt: Introduce a reference count in struct srpt_device (Kamal Heib) [2120676]
- RDMA/srpt: Duplicate port name members (Kamal Heib) [2120676]
- Revert "RDMA/rxe: Create duplicate mapping tables for FMRs" (Kamal Heib) [2120676]
- RDMA/rxe: Replace __rxe_do_task by rxe_run_task (Kamal Heib) [2120676]
- RDMA/rxe: Limit the number of calls to each tasklet (Kamal Heib) [2120676]
- RDMA/rxe: Make the tasklet exits the same (Kamal Heib) [2120676]
- RDMA/rxe: Fix rnr retry behavior (Kamal Heib) [2120676]
- RDMA/rxe: Add rxe_is_fenced() subroutine (Kamal Heib) [2120676]
- RDMA/rxe: For invalidate compare according to set keys in mr (Kamal Heib) [2120676]
- RDMA: Fix comment typo (Kamal Heib) [2120676]
- IB: Fix repeated words 'the the' comments (Kamal Heib) [2120676]
- RDMA/rxe: Fix mw bind to allow any consumer key portion (Kamal Heib) [2120676]
- RDMA/rxe: Fix spelling mistake in error print (Kamal Heib) [2120676]
- RDMA/rxe: Remove unused qp parameter (Kamal Heib) [2120676]
- RDMA/hfi1: fix potential memory leak in setup_base_ctxt() (Kamal Heib) [2120676]
- RDMA/rxe: Remove unused mask parameter (Kamal Heib) [2120676]
- RDMA/rxe: Rename rxe_atomic_reply to atomic_reply (Kamal Heib) [2120676]
- RDMA/rxe: Add common rxe_prepare_res() (Kamal Heib) [2120676]
- RDMA/rxe: Fix BUG: KASAN: null-ptr-deref in rxe_qp_do_cleanup (Kamal Heib) [2120676]
- RDMA/siw: Fix duplicated reported IW_CM_EVENT_CONNECT_REPLY event (Kamal Heib) [2120676]
- RDMA/hfi1: Depend on !UML (Kamal Heib) [2120676]
- RDMA/irdma: Use the bitmap API to allocate bitmaps (Kamal Heib) [2120676 2103957]
- RDMA: remove useless condition in siw_create_cq() (Kamal Heib) [2120676]
- RDMA/irdma: Fix setting of QP context err_rq_idx_valid field (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Fix VLAN connection with wildcard address (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Fix a window for use-after-free (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Make resource distribution algorithm more QP oriented (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Make CQP invalid state error non-critical (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Add AE source to error log (Kamal Heib) [2120676 2103957]
- RDMA/irdma: Add 2 level PBLE support for FMR (Kamal Heib) [2120676 2103957]
- IB: Fix spelling of 'writable' (Kamal Heib) [2120676]
- RDMA/rxe: Remove unnecessary include statement (Kamal Heib) [2120676]
- RDMA/rxe: Replace include statement (Kamal Heib) [2120676]
- RDMA/rxe: Convert pr_warn/err to pr_debug in pyverbs (Kamal Heib) [2120676]
- RDMA/rxe: Fix deadlock in rxe_do_local_ops() (Kamal Heib) [2120676]
- RDMA/rxe: Merge normal and retry atomic flows (Kamal Heib) [2120676]
- RDMA/rxe: Move atomic original value to res (Kamal Heib) [2120676]
- RDMA/rxe: Move atomic responder res to atomic_reply (Kamal Heib) [2120676]
- RDMA/rxe: Add a responder state for atomic reply (Kamal Heib) [2120676]
- RDMA/rxe: Move code to rxe_prepare_atomic_res() (Kamal Heib) [2120676]
- RDMA/rxe: Convert read side locking to rcu (Kamal Heib) [2120676]
- RDMA/rxe: Stop lookup of partially built objects (Kamal Heib) [2120676]
- RDMA/rxe: Remove useless pkt parameters (Kamal Heib) [2120676]
- RDMA: Correct duplicated words in comments (Kamal Heib) [2120676]
- IB/iser: Drain the entire QP during destruction flow (Kamal Heib) [2120676]
- RDMA/rxe: fix xa_alloc_cycle() error return value check again (Kamal Heib) [2120676]
- RDMA/core: Add a netevent notifier to cma (Kamal Heib) [2120676 2117912]
- RDMA/core: Add an rb_tree that stores cm_ids sorted by ifindex and remote IP (Kamal Heib) [2120676 2117912]
- RDMA/hfi1: Fix typo in comment (Kamal Heib) [2120676]
- RDMA: Split kernel-only global device caps from uverbs device caps (Kamal Heib) [2120675]
- RDMA/hfi1: Remove all traces of diagpkt support (Kamal Heib) [2120675]
- RDMA/hfi1: Consolidate software versions (Kamal Heib) [2120675]
- RDMA/hfi1: Remove pointless driver version (Kamal Heib) [2120675]
- RDMA/hfi1: Prevent panic when SDMA is disabled (Kamal Heib) [2120675]
- RDMA/core: Fix typo in comment (Kamal Heib) [2120675]
- IB/hf1: Fix typo in comment (Kamal Heib) [2120675]
- IB/iser: Fix typo in comment (Kamal Heib) [2120675]
- IB/isert: Avoid flush_scheduled_work() usage (Kamal Heib) [2120675]
- RDMA/siw: Enable siw on tunnel devices (Kamal Heib) [2120675]
- RDMA/rxe: Enforce IBA C11-17 (Kamal Heib) [2120675]
- RDMA/rxe: Move mw cleanup code to rxe_mw_cleanup() (Kamal Heib) [2120675]
- RDMA/rxe: Move mr cleanup code to rxe_mr_cleanup() (Kamal Heib) [2120675]
- RDMA/rxe: Move qp cleanup code to rxe_qp_do_cleanup() (Kamal Heib) [2120675]
- RDMA/rxe: Check rxe_get() return value (Kamal Heib) [2120675]
- RDMA/rxe: Add rxe_srq_cleanup() (Kamal Heib) [2120675]
- RDMA/rxe: Remove IB_SRQ_INIT_MASK (Kamal Heib) [2120675]
- RDMA/rxe: Skip adjusting remote addr for write in retry operation (Kamal Heib) [2120675]
- RDMA/rxe: Optimize the mr pool struct (Kamal Heib) [2120675]
- RDMA/rxe: Replace paylen by payload (Kamal Heib) [2120675]
- RDMA/core: Avoid flush_workqueue(system_unbound_wq) usage (Kamal Heib) [2120675]
- RDMA/rxe: Remove useless parameters for update_state() (Kamal Heib) [2120675]
- RDMA/rxe: Remove reliable datagram support (Kamal Heib) [2120675]
- RDMA/rxe: Remove support for SMI QPs from rdma_rxe (Kamal Heib) [2120675]
- RDMA/rxe: Remove mc_grp_pool from struct rxe_dev (Kamal Heib) [2120675]
- RDMA/rxe: Remove type 2A memory window capability (Kamal Heib) [2120675]
- RDMA/usnic: Refactor usnic_uiom_alloc_pd() (Kamal Heib) [2120675]
- RDMA/usnic: Stop using iommu_present() (Kamal Heib) [2120675]
- IB/SA: Replace usage of found with dedicated list iterator variable (Kamal Heib) [2120675]
- IB/rdmavt: add missing locks in rvt_ruc_loopback (Kamal Heib) [2120675]
- IB/uverbs: Move part of enum ib_device_cap_flags to uapi (Kamal Heib) [2120675]
- IB/uverbs: Move enum ib_raw_packet_caps to uapi (Kamal Heib) [2120675]
- RDMA/pvrdma: Remove useless DMA-32 fallback configuration (Kamal Heib) [2120675]
- RDMA: switch from 'pci_' to 'dma_' API (Kamal Heib) [2120675]
- scsi: RDMA/srp: Use scsi_cmd_to_rq() instead of scsi_cmnd.request (Kamal Heib) [2120675]
- scsi: RDMA/iser: Use scsi_cmd_to_rq() instead of scsi_cmnd.request (Kamal Heib) [2120675]
- x86/fpu: Prevent FPU state corruption (Oleksandr Natalenko) [2130890]
- net: team: Unsync device addresses on ndo_stop (Hangbin Liu) [2135240]
- mmu_gather: fix the CONFIG_MMU_GATHER_NO_RANGE case (Waiman Long) [2130166] {CVE-2022-39188}
- mmu_gather: Force tlb-flush VM_PFNMAP vmas (Waiman Long) [2130166] {CVE-2022-39188}
- mmu_gather: Let there be one tlb_{start,end}_vma() implementation (Waiman Long) [2130166] {CVE-2022-39188}
- mmu_gather: Remove per arch tlb_{start,end}_vma() (Waiman Long) [2130166] {CVE-2022-39188}
- x86/ldt: Use tlb_gather_mmu_fullmm() when freeing LDT page-tables (Waiman Long) [2130166] {CVE-2022-39188}
- tlb: arch: Remove empty __tlb_remove_tlb_entry() stubs (Waiman Long) [2130166] {CVE-2022-39188}
- tlb: mmu_gather: Remove start/end arguments from tlb_gather_mmu() (Waiman Long) [2130166] {CVE-2022-39188}
- tlb: mmu_gather: Introduce tlb_gather_mmu_fullmm() (Waiman Long) [2130166] {CVE-2022-39188}
- tlb: mmu_gather: Remove unused start/end arguments from tlb_finish_mmu() (Waiman Long) [2130166] {CVE-2022-39188}
- mm: proc: Invalidate TLB after clearing soft-dirty page state (Waiman Long) [2130166] {CVE-2022-39188}
- mm: fix clear_refs_write locking (Waiman Long) [2130166] {CVE-2022-39188}
- s390/Kconfig: sort config S390 select list once again (Waiman Long) [2130166] {CVE-2022-39188}
- asm-generic/tlb: provide MMU_GATHER_TABLE_FREE (Waiman Long) [2130166] {CVE-2022-39188}
- asm-generic/tlb: rename HAVE_MMU_GATHER_NO_GATHER (Waiman Long) [2130166] {CVE-2022-39188}
- asm-generic/tlb: rename HAVE_MMU_GATHER_PAGE_SIZE (Waiman Long) [2130166] {CVE-2022-39188}
- asm-generic/tlb: rename HAVE_RCU_TABLE_FREE (Waiman Long) [2130166] {CVE-2022-39188}
- asm-generic/tlb: avoid potential double flush (Waiman Long) [2130166] {CVE-2022-39188}
- powerpc/mm/book3s64/radix: Flush the full mm even when need_flush_all is set (Waiman Long) [2130166] {CVE-2022-39188}
- powerpc/mm/book3s64/radix: Use freed_tables instead of need_flush_all (Waiman Long) [2130166] {CVE-2022-39188}
- mm/tlb: Remove CONFIG_HAVE_RCU_TABLE_INVALIDATE (Waiman Long) [2130166] {CVE-2022-39188}
- Add skb drop reasons to IPv6 UDP receive path (Antoine Tenart) [2059158]
- net: skb: export skb drop reaons to user by TRACE_DEFINE_ENUM (Antoine Tenart) [2059158]
- net: skb: prevent the split of kfree_skb_reason() by gcc (Antoine Tenart) [2059158]
- tcp: md5: fix IPv4-mapped support (Antoine Tenart) [2059158]
- net: dropreason: reformat the comment fo skb drop reasons (Antoine Tenart) [2059158]
- net: skb: use auto-generation to convert skb drop reason to string (Antoine Tenart) [2059158]
- net: skb: move enum skb_drop_reason to standalone header file (Antoine Tenart) [2059158]
- tcp_ipv6: set the drop_reason in the right place (Antoine Tenart) [2059158]
- net: tcp: reset 'drop_reason' to NOT_SPCIFIED in tcp_v{4,6}_rcv() (Antoine Tenart) [2059158]
- net: skb: change the definition SKB_DR_SET() (Antoine Tenart) [2059158]
- net: skb: check the boundrary of drop reason in kfree_skb_reason() (Antoine Tenart) [2059158]
- net: dm: check the boundary of skb drop reasons (Antoine Tenart) [2059158]
- tcp: fix signed/unsigned comparison (Antoine Tenart) [2059158]
- tcp: add drop reason support to tcp_ofo_queue() (Antoine Tenart) [2059158]
- tcp: add drop reasons to tcp_rcv_synsent_state_process() (Antoine Tenart) [2059158]
- tcp: make tcp_rcv_synsent_state_process() drop monitor friend (Antoine Tenart) [2059158]
- tcp: add drop reason support to tcp_prune_ofo_queue() (Antoine Tenart) [2059158]
- tcp: add two drop reasons for tcp_ack() (Antoine Tenart) [2059158]
- tcp: add drop reasons to tcp_rcv_state_process() (Antoine Tenart) [2059158]
- tcp: make tcp_rcv_state_process() drop monitor friendly (Antoine Tenart) [2059158]
- tcp: add drop reason support to tcp_validate_incoming() (Antoine Tenart) [2059158]
- tcp: get rid of rst_seq_match (Antoine Tenart) [2059158]
- tcp: consume incoming skb leading to a reset (Antoine Tenart) [2059158]
- tcp: tcp_send_challenge_ack delete useless param `skb` (Antoine Tenart) [2059158]
- ipv6: fix NULL deref in ip6_rcv_core() (Antoine Tenart) [2059158]
- net: ipv6: add skb drop reasons to ip6_protocol_deliver_rcu() (Antoine Tenart) [2059158]
- net: ipv6: add skb drop reasons to ip6_rcv_core() (Antoine Tenart) [2059158]
- net: ipv6: add skb drop reasons to TLV parse (Antoine Tenart) [2059158]
- net: ipv6: remove redundant statistics in ipv6_hop_jumbo() (Antoine Tenart) [2059158]
- net: icmp: introduce function icmpv6_param_prob_reason() (Antoine Tenart) [2059158]
- net: ip: add skb drop reasons to ip forwarding (Antoine Tenart) [2059158]
- net: ipv6: add skb drop reasons to ip6_pkt_drop() (Antoine Tenart) [2059158]
- net: ipv4: add skb drop reasons to ip_error() (Antoine Tenart) [2059158]
- skb: add some helpers for skb drop reasons (Antoine Tenart) [2059158]
- net: icmp: add skb drop reasons to icmp protocol (Antoine Tenart) [2059158]
- ping: Check return value of function 'ping_queue_rcv_skb' (Antoine Tenart) [2059158]
- net: icmp: introduce __ping_queue_rcv_skb() to report drop reasons (Antoine Tenart) [2059158]
- net: skb: rename SKB_DROP_REASON_PTYPE_ABSENT (Antoine Tenart) [2059158]
- net: sock: introduce sock_queue_rcv_skb_reason() (Antoine Tenart) [2059158]
- net: tcp: fix shim definition of tcp_inbound_md5_hash (Antoine Tenart) [2059158]
- skb: make drop reason booleanable (Antoine Tenart) [2059158]
- net/tcp: Merge TCP-MD5 inbound callbacks (Antoine Tenart) [2059158]
- tcp: md5: add tcp_md5_needed jump label (Antoine Tenart) [2059158]
- net: tun: track dropped skb via kfree_skb_reason() (Antoine Tenart) [2059158]
- net: tun: split run_ebpf_filter() and pskb_trim() into different "if statement" (Antoine Tenart) [2059158]
- net: tap: track dropped skb via kfree_skb_reason() (Antoine Tenart) [2059158]
- net: dev: use kfree_skb_reason() for __netif_receive_skb_core() (Antoine Tenart) [2059158]
- net: dev: use kfree_skb_reason() for sch_handle_ingress() (Antoine Tenart) [2059158]
- net: dev: use kfree_skb_reason() for do_xdp_generic() (Antoine Tenart) [2059158]
- net: dev: use kfree_skb_reason() for enqueue_to_backlog() (Antoine Tenart) [2059158]
- net: dev: add skb drop reasons to __dev_xmit_skb() (Antoine Tenart) [2059158]
- net: skb: introduce the function kfree_skb_list_reason() (Antoine Tenart) [2059158]
- net: dev: use kfree_skb_reason() for sch_handle_egress() (Antoine Tenart) [2059158]
- net: neigh: add skb drop reasons to arp_error_report() (Antoine Tenart) [2059158]
- net: neigh: use kfree_skb_reason() for __neigh_event_send() (Antoine Tenart) [2059158]
- net: ip: add skb drop reasons for ip egress path (Antoine Tenart) [2059158]
- net: tcp: use tcp_drop_reason() for tcp_data_queue_ofo() (Antoine Tenart) [2059158]
- net: tcp: use tcp_drop_reason() for tcp_data_queue() (Antoine Tenart) [2059158]
- net: tcp: use tcp_drop_reason() for tcp_rcv_established() (Antoine Tenart) [2059158]
- net: tcp: use kfree_skb_reason() for tcp_v{4,6}_do_rcv() (Antoine Tenart) [2059158]
- net: tcp: add skb drop reasons to tcp_add_backlog() (Antoine Tenart) [2059158]
- net: tcp: add skb drop reasons to tcp_v{4,6}_inbound_md5_hash() (Antoine Tenart) [2059158]
- ipv4/tcp: Pass dif and sdif to tcp_v4_inbound_md5_hash (Antoine Tenart) [2059158]
- ipv6/tcp: Pass dif and sdif to tcp_v6_inbound_md5_hash (Antoine Tenart) [2059158]
- ipv4/tcp: Use local variable for tcp_md5_addr (Antoine Tenart) [2059158]
- net: tcp: use kfree_skb_reason() for tcp_v6_rcv() (Antoine Tenart) [2059158]
- net: tcp: add skb drop reasons to tcp_v4_rcv() (Antoine Tenart) [2059158]
- net: tcp: introduce tcp_drop_reason() (Antoine Tenart) [2059158]
- ipv6: Add reasons for skb drops to __udp6_lib_rcv (Antoine Tenart) [2059158]
- net: drop_monitor: support drop reason (Antoine Tenart) [2059158]
- net: udp: use kfree_skb_reason() in __udp_queue_rcv_skb() (Antoine Tenart) [2059158]
- net: udp: use kfree_skb_reason() in udp_queue_rcv_one_skb() (Antoine Tenart) [2059158]
- net: ipv4: use kfree_skb_reason() in ip_protocol_deliver_rcu() (Antoine Tenart) [2059158]
- net: ipv4: use kfree_skb_reason() in ip_rcv_finish_core() (Antoine Tenart) [2059158]
- net: ipv4: use kfree_skb_reason() in ip_rcv_core() (Antoine Tenart) [2059158]
- net: netfilter: use kfree_drop_reason() for NF_DROP (Antoine Tenart) [2059158]
- net: skb_drop_reason: add document for drop reasons (Antoine Tenart) [2059158]
- net: socket: rename SKB_DROP_REASON_SOCKET_FILTER (Antoine Tenart) [2059158]
- net: skb: use kfree_skb_reason() in __udp4_lib_rcv() (Antoine Tenart) [2059158]
- net: skb: use kfree_skb_reason() in tcp_v4_rcv() (Antoine Tenart) [2059158]
- net: skb: introduce kfree_skb_reason() (Antoine Tenart) [2059158]
- bnx2x: Fix comment typo (Manish Chopra) [2111882]
- bnx2x: Fix spelling mistake "regiser" -> "register" (Manish Chopra) [2111882]
- bnx2x: Fix undefined behavior due to shift overflowing the constant (Manish Chopra) [2111882]
- net: sched: act_ct: fix possible refcount leak in tcf_ct_init() (Davide Caratti) [2133741]
- net: sched: fix possible refcount leak in tc_new_tfilter() (Davide Caratti) [2133741]
- sch_sfb: Also store skb len before calling child enqueue (Davide Caratti) [2133741]
- sch_sfb: Don't assume the skb is still around after enqueueing to child (Davide Caratti) [2133741]
- net/sched: fix netdevice reference leaks in attach_default_qdiscs() (Davide Caratti) [2133741]
- net: sched: tbf: don't call qdisc_put() while holding tree lock (Davide Caratti) [2133741]
- net: Fix data-races around weight_p and dev_weight_[rt]x_bias. (Davide Caratti) [2133741]
- net/sched: act_api: Notify user space if any actions were flushed before error (Davide Caratti) [2133741]
- tipc: fix an information leak in tipc_topsrv_kern_subscr (Xin Long) [2134962]
- tipc: Fix recognition of trial period (Xin Long) [2134962]
- tipc: fix shift wrapping bug in map_get() (Xin Long) [2134962]
- PCI/ASPM: Make Intel DG2 L1 acceptable latency unlimited (Myron Stowe) [2072656]
- x86/pci/xen: Use msi_msg shadow structs (Jerry Snitselaar) [2133518]
- iommu/intel: Use msi_msg shadow structs (Jerry Snitselaar) [2133518]
- PCI: MSI: Fix Kconfig dependencies for PCI_MSI_ARCH_FALLBACKS (Jerry Snitselaar) [2133518]
- x86/apic/msi: Unbreak DMAR and HPET MSI (Jerry Snitselaar) [2133518]
- iommu/amd: Remove domain search for PCI/MSI (Jerry Snitselaar) [2133518]
- iommu/vt-d: Remove domain search for PCI/MSI[X] (Jerry Snitselaar) [2133518]
- x86/irq: Make most MSI ops XEN private (Jerry Snitselaar) [2133518]
- x86/irq: Cleanup the arch_*_msi_irqs() leftovers (Jerry Snitselaar) [2133518]
- PCI/MSI: Make arch_.*_msi_irq[s] fallbacks selectable (Jerry Snitselaar) [2133518]
- x86/xen: Wrap XEN MSI management into irqdomain (Jerry Snitselaar) [2133518]
- x86/xen: Consolidate XEN-MSI init (Jerry Snitselaar) [2133518]
- x86/xen: Rework MSI teardown (Jerry Snitselaar) [2133518]
- x86/xen: Make xen_msi_init() static and rename it to xen_hvm_msi_init() (Jerry Snitselaar) [2133518]
- x86/irq: Move apic_post_init() invocation to one place (Jerry Snitselaar) [2133518]
- x86/msi: Use generic MSI domain ops (Jerry Snitselaar) [2133518]
- x86/msi: Remove pointless vcpu_affinity callback (Jerry Snitselaar) [2133518]
- netfilter: nf_conntrack_irc: Tighten matching on DCC message (Wander Lairson Costa) [2124092] {CVE-2022-2663}
- netfilter: nf_conntrack_irc: Fix forged IP logic (Wander Lairson Costa) [2124092] {CVE-2022-2663}
- ice: Add support Flex RXD (Michal Schmidt) [2131310]
- asm-generic: sections: refactor memory_intersects (Jerry Snitselaar) [2112119]
- swiotlb: fix passing local variable to debugfs_create_ulong() (Jerry Snitselaar) [2112119]
- swiotlb: move struct io_tlb_slot to swiotlb.c (Jerry Snitselaar) [2112119]
- swiotlb: ensure a segment doesn't cross the area boundary (Jerry Snitselaar) [2112119]
- swiotlb: consolidate rounding up default_nslabs (Jerry Snitselaar) [2112119]
- swiotlb: remove unused fields in io_tlb_mem (Jerry Snitselaar) [2112119]
- swiotlb: fix use after free on error handling path (Jerry Snitselaar) [2112119]
- swiotlb: split up the global swiotlb lock (Jerry Snitselaar) [2112119]
- swiotlb: fail map correctly with failed io_tlb_default_mem (Jerry Snitselaar) [2112119]
- swiotlb: remove a useless return in swiotlb_init (Jerry Snitselaar) [2112119]
- swiotlb: remove the unused swiotlb_force declaration (Jerry Snitselaar) [2112119]
- iommu/dma: Fix race condition during iova_domain initialization (Jerry Snitselaar) [2112119]
- iommu/amd: Fix compile warning in init code (Jerry Snitselaar) [2106599]
- iommu/amd: Simplify and Consolidate Virtual APIC (AVIC) Enablement (Jerry Snitselaar) [2106599]
- iommu/vt-d: Check correct capability for sagaw determination (Jerry Snitselaar) [2112119]
- iommu/vt-d: Correctly calculate sagaw value of IOMMU (Jerry Snitselaar) [2112119]
- iommu/vt-d: Fix kdump kernels boot failure with scalable mode (Jerry Snitselaar) [2080413]
- iommu/amd: use full 64-bit value in build_completion_wait() (Jerry Snitselaar) [2112119]
- swiotlb: avoid potential left shift overflow (Jerry Snitselaar) [2112119]
- dma-debug: improve search for partial syncs (Jerry Snitselaar) [2112119]
- iommu/iova: Improve 32-bit free space estimate (Jerry Snitselaar) [2112119]
- iommu/amd: Handle return of iommu_device_sysfs_add (Jerry Snitselaar) [2112119]
- swiotlb: fix setting ->force_bounce (Jerry Snitselaar) [2112119]
- swiotlb: use the right nslabs-derived sizes in swiotlb_init_late (Jerry Snitselaar) [2112119]
- swiotlb: use the right nslabs value in swiotlb_init_remap (Jerry Snitselaar) [2112119]
- swiotlb: don't panic when the swiotlb buffer can't be allocated (Jerry Snitselaar) [2112119]
- x86: remove cruft from <asm/dma-mapping.h> (Jerry Snitselaar) [2112119]
- swiotlb: remove swiotlb_init_with_tbl and swiotlb_init_late_with_tbl (Jerry Snitselaar) [2112119]
- swiotlb: provide swiotlb_init variants that remap the buffer (Jerry Snitselaar) [2112119]
- swiotlb: pass a gfp_mask argument to swiotlb_init_late (Jerry Snitselaar) [2112119]
- swiotlb: add a SWIOTLB_ANY flag to lift the low memory restriction (Jerry Snitselaar) [2112119]
- swiotlb: make the swiotlb_init interface more useful (Jerry Snitselaar) [2112119]
- x86: centralize setting SWIOTLB_FORCE when guest memory encryption is enabled (Jerry Snitselaar) [2112119]
- x86: remove the IOMMU table infrastructure (Jerry Snitselaar) [2112119]
- swiotlb: rename swiotlb_late_init_with_default_size (Jerry Snitselaar) [2112119]
- swiotlb: simplify swiotlb_max_segment (Jerry Snitselaar) [2112119]
- iommu/vt-d: avoid invalid memory access via node_online(NUMA_NO_NODE) (Jerry Snitselaar) [2112119]
- iommu/arm-smmu-v3: check return value after calling platform_get_resource() (Jerry Snitselaar) [2112119]
- iommu/arm-smmu: fix possible null-ptr-deref in arm_smmu_device_probe() (Jerry Snitselaar) [2112119]
- iommu/amd: Increase timeout waiting for GA log enablement (Jerry Snitselaar) [2112119]
- iommu/amd: Do not call sleep while holding spinlock (Jerry Snitselaar) [2112119]
- iommu/amd: Remove redundant check (Jerry Snitselaar) [2112119]
- swiotlb: simplify array allocation (Jerry Snitselaar) [2112119]
- swiotlb: tidy up includes (Jerry Snitselaar) [2112119]
- treewide: Replace the use of mem_encrypt_active() with cc_platform_has() (Jerry Snitselaar) [2112119]
- swiotlb: simplify debugfs setup (Jerry Snitselaar) [2112119]
- iommu: Log iova range in map/unmap trace events (Jerry Snitselaar) [2112119]
- iommu/amd: Improve amd_iommu_v2_exit() (Jerry Snitselaar) [2112119]
- iommu/amd: Remove unused struct fault.devid (Jerry Snitselaar) [2112119]
- iommu/amd: Clean up function declarations (Jerry Snitselaar) [2112119]
- iommu/amd: Improve error handling for amd_iommu_init_pci (Jerry Snitselaar) [2112119]
- iommu/iova: Separate out rcache init (Jerry Snitselaar) [2112119]
- iommu/iova: Temporarily include dma-mapping.h from iova.h (Jerry Snitselaar) [2112119]
- iommu: Move flush queue data into iommu_dma_cookie (Jerry Snitselaar) [2112119]
- iommu/iova: Move flush queue code to iommu-dma (Jerry Snitselaar) [2112119]
- iommu/iova: Consolidate flush queue code (Jerry Snitselaar) [2112119]
- iommu/vt-d: Use put_pages_list (Jerry Snitselaar) [2112119]
- iommu/amd: Use put_pages_list (Jerry Snitselaar) [2112119]
- iommu/amd: Simplify pagetable freeing (Jerry Snitselaar) [2112119]
- iommu/iova: Squash flush_cb abstraction (Jerry Snitselaar) [2112119]
- iommu/iova: Squash entry_dtor abstraction (Jerry Snitselaar) [2112119]
- iommu/iova: Move fast alloc size roundup into alloc_iova_fast() (Jerry Snitselaar) [2112119]
- iommu/arm-smmu-v3: fix event handling soft lockup (Jerry Snitselaar) [2112119]
- iommu/arm-smmu-v3: Avoid open coded arithmetic in memory allocation (Jerry Snitselaar) [2112119]
- iommu/amd: Fix loop timeout issue in iommu_ga_log_enable() (Jerry Snitselaar) [2112119]
- iommu/intel: Use msi_msg shadow structs (Jerry Snitselaar) [2112119]
- dma-mapping: use 'bitmap_zalloc()' when applicable (Jerry Snitselaar) [2112119]
- iommu/dma: Use kvcalloc() instead of kvzalloc() (Jerry Snitselaar) [2112119]
- iommu/vt-d: Convert the return type of first_pte_in_page to bool (Jerry Snitselaar) [2112119]
- iommu/vt-d: Use second level for GPA->HPA translation (Jerry Snitselaar) [2112119]
- iommu/vt-d: Remove duplicate identity domain flag (Jerry Snitselaar) [2112119]
- iommu/vt-d: Do not falsely log intel_iommu is unsupported kernel option (Jerry Snitselaar) [2112119]
- iommu/dma: Unexport IOVA cookie management (Jerry Snitselaar) [2112119]
- iommu/amd: Use struct_group() for memcpy() region (Jerry Snitselaar) [2112119]
- dma-mapping: remove bogus test for pfn_valid from dma_map_resource (Jerry Snitselaar) [2112119]
- iommu/vt-d: Use pci_dev_id() helper (Jerry Snitselaar) [2112119]
- swiotlb-xen: this is PV-only on x86 (Jerry Snitselaar) [2112119]
- xen/pci-swiotlb: reduce visibility of symbols (Jerry Snitselaar) [2112119]
- iova: Export alloc_iova_fast() and free_iova_fast() (Jerry Snitselaar) [2112119]
- iommu: Clarify default domain Kconfig (Jerry Snitselaar) [2112119]
- iommu/io-pgtable: Abstract iommu_iotlb_gather access (Jerry Snitselaar) [2112119]
- iommu/vt-d: Refactor Kconfig a bit (Jerry Snitselaar) [2112119]
- iommu: Allow enabling non-strict mode dynamically (Jerry Snitselaar) [2112119]
- iommu: Merge strictness and domain type configs (Jerry Snitselaar) [2112119]
- iommu: Only log strictness for DMA domains (Jerry Snitselaar) [2112119]
- iommu: Expose DMA domain strictness via sysfs (Jerry Snitselaar) [2112119]
- iommu: Express DMA strictness via the domain type (Jerry Snitselaar) [2112119]
- iommu/vt-d: Prepare for multiple DMA domain types (Jerry Snitselaar) [2112119]
- iommu/arm-smmu: Prepare for multiple DMA domain types (Jerry Snitselaar) [2112119]
- iommu/amd: Prepare for multiple DMA domain types (Jerry Snitselaar) [2112119]
- iommu: Introduce explicit type for non-strict DMA domains (Jerry Snitselaar) [2112119]
- iommu/io-pgtable: Remove non-strict quirk (Jerry Snitselaar) [2112119]
- iommu: Indicate queued flushes via gather data (Jerry Snitselaar) [2112119]
- iommu/amd: Remove stale amd_iommu_unmap_flush usage (Jerry Snitselaar) [2112119]
- iommu: Remove mode argument from iommu_set_dma_strict() (Jerry Snitselaar) [2112119]
- iommu/amd: Add support for IOMMU default DMA mode build options (Jerry Snitselaar) [2112119]
- iommu/vt-d: Add support for IOMMU default DMA mode build options (Jerry Snitselaar) [2112119]
- iommu: Enhance IOMMU default DMA mode build options (Jerry Snitselaar) [2112119]
- iommu: Print strict or lazy mode at init time (Jerry Snitselaar) [2112119]
- iommu: Deprecate Intel and AMD cmdline methods to enable strict mode (Jerry Snitselaar) [2112119]
- dma-debug: use memory_intersects() directly (Jerry Snitselaar) [2112119]
- dma-debug: fix return value of __setup handlers (Jerry Snitselaar) [2112119]
- arm-smmu-qcom: Ensure the qcom_scm driver has finished probing (Jerry Snitselaar) [2112119]
- iommu/io-pgtable-arm: Clean up faulty sanity check (Jerry Snitselaar) [2112119]
- iommu/vt-d: Fix RCU list debugging warnings (Jerry Snitselaar) [2112119]
- iommu/dma: add a new dma_map_ops of get_merge_boundary() (Jerry Snitselaar) [2112119]
- swiotlb: do not zero buffer in set_memory_decrypted() (Jerry Snitselaar) [2112119]
- iommu: iommu_ops RH_KABI cleanup (Jerry Snitselaar) [2112119]
- device: Fix RH_KABI work around (Jerry Snitselaar) [2112357]
- iommu/vt-d: Drop stop marker messages (Jerry Snitselaar) [2112119]
- iommu/vt-d: Remove unused function intel_svm_capable() (Jerry Snitselaar) [2112119]
- iommu/arm-smmu-v3: Fix size calculation in arm_smmu_mm_invalidate_range() (Jerry Snitselaar) [2112119]
- iommu/vt-d: Delete dev_has_feat callback (Jerry Snitselaar) [2112119]
- iommu/amd: Remove useless irq affinity notifier (Jerry Snitselaar) [2112119]

* Mon Nov 07 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-435.el8]
- scsi: qedi: Fix ABBA deadlock in qedi_process_tmf_resp() and qedi_process_cmd_cleanup_resp() (Nilesh Javali) [2109890]
- scsi: qedi: Remove set but unused 'page' variable (Nilesh Javali) [2109890]
- x86/elf: Disable automatic READ_IMPLIES_EXEC on 64-bit (Wander Lairson Costa) [2070700] {CVE-2022-25265}
- x86/elf: Split READ_IMPLIES_EXEC from executable PT_GNU_STACK (Wander Lairson Costa) [2070700] {CVE-2022-25265}
- x86/elf: Add table to document READ_IMPLIES_EXEC (Wander Lairson Costa) [2070700] {CVE-2022-25265}
- RHEL-only: KVM: selftests: Enable rseq_test on aarch64 (Gavin Shan) [2128974]
- KVM: selftests: Use getcpu() instead of sched_getcpu() in rseq_test (Gavin Shan) [2128974]
- selftests: kvm: Fix a compile error in selftests/kvm/rseq_test.c (Gavin Shan) [2128974]
- KVM: selftests: Fix target thread to be migrated in rseq_test (Gavin Shan) [2128974]
- selftests: KVM: Handle compiler optimizations in ucall (Gavin Shan) [2128974]
- selftests: kvm: replace ternary operator with min() (Gavin Shan) [2128974]
- KVM: selftests: Fix typo in vgic_init test (Gavin Shan) [2128974]
- KVM: selftests: Fix buggy-but-benign check in test_v3_new_redist_regions() (Gavin Shan) [2128974]
- KVM: arm64: vgic: Fix exit condition in scan_its_table() (Gavin Shan) [2128974]
- KVM: arm64: selftests: Add support for GICv2 on v3 (Gavin Shan) [2128974]
- KVM: arm64: Fix comment typo in nvhe/switch.c (Gavin Shan) [2128974]
- KVM: arm64: vgic: Remove duplicate check in update_affinity_collection() (Gavin Shan) [2128974]
- KVM: arm64: Don't return from void function (Gavin Shan) [2128974]
- KVM: arm64: Drop stale comment (Gavin Shan) [2128974]
- KVM: arm64: Warn if accessing timer pending state outside of vcpu context (Gavin Shan) [2128974]
- KVM: arm64: Replace vgic_v3_uaccess_read_pending with vgic_uaccess_read_pending (Gavin Shan) [2128974]
- KVM: arm64: vgic: Undo work in failed ITS restores (Gavin Shan) [2128974]
- KVM: arm64: vgic: Do not ignore vgic_its_restore_cte failures (Gavin Shan) [2128974]
- KVM: arm64: vgic: Add more checks when restoring ITS tables (Gavin Shan) [2128974]
- KVM: arm64: vgic: Check that new ITEs could be saved in guest memory (Gavin Shan) [2128974]
- KVM: arm64: nvhe: Eliminate kernel-doc warnings (Gavin Shan) [2128974]
- KVM: arm64: Print emulated register table name when it is unsorted (Gavin Shan) [2128974]
- KVM: arm64: Don't BUG_ON() if emulated register table is unsorted (Gavin Shan) [2128974]
- KVM: arm64: Inject exception on out-of-IPA-range translation fault (Gavin Shan) [2128974]
- KVM: arm64: vgic: Remove unnecessary type castings (Gavin Shan) [2128974]
- KVM: arm64: Drop unused param from kvm_psci_version() (Gavin Shan) [2128974]
- KVM: arm64: vgic: Add memcg accounting to vgic allocations (Gavin Shan) [2128974]
- x86/split_lock: Enable the split lock feature on Raptor Lake (Prarit Bhargava) [2076738]
- mm: prevent page_frag_alloc() from corrupting the memory (Izabela Bakollari) [2132265]
- RDMA/mlx5: Set local port to one when accessing counters (Mohammad Kabat) [2077119]
- scsi: ch: Do not initialise statics to 0 (Ewan D. Milne) [2132458]
- scsi: core: Fix warning in scsi_alloc_sgtables() (Ewan D. Milne) [2132458]
- scsi: core: Move the definition of SCSI_QUEUE_DELAY (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Fix zone transition to full condition (Ewan D. Milne) [2132458]
- scsi: sd_zbc: Prevent zone information memory leak (Ewan D. Milne) [2132458]
- scsi: sd: Fix potential NULL pointer dereference (Ewan D. Milne) [2132458]
- scsi: sr: Add memory allocation failure handling for get_capabilities() (Ewan D. Milne) [2132458]
- scsi: sd: Use cached ATA Information VPD page (Ewan D. Milne) [2132458]
- scsi: core: Do not truncate INQUIRY data on modern devices (Ewan D. Milne) [2132458]
- scsi: core: Pick suitable allocation length in scsi_report_opcode() (Ewan D. Milne) [2132458]
- scsi: core: Query VPD size before getting full page (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Add gap zone support (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Rename zone type constants (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Fix a typo (Ewan D. Milne) [2132458]
- scsi: sd: sd_zbc: Hide gap zones (Ewan D. Milne) [2132458]
- scsi: sd: sd_zbc: Return early in sd_zbc_check_zoned_characteristics() (Ewan D. Milne) [2132458]
- scsi: sd: sd_zbc: Introduce struct zoned_disk_info (Ewan D. Milne) [2132458]
- scsi: sd: sd_zbc: Use logical blocks as unit when querying zones (Ewan D. Milne) [2132458]
- scsi: sd: sd_zbc: Verify that the zone size is a power of two (Ewan D. Milne) [2132458]
- scsi: sd: sd_zbc: Improve source code documentation (Ewan D. Milne) [2132458]
- scsi: sr: Do not leak information in ioctl (Ewan D. Milne) [2132458]
- scsi: core: Remove unreachable code warning (Ewan D. Milne) [2132458]
- scsi: libfc: Fix use after free in fc_exch_abts_resp() (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Silence unexpected unlock warnings (Ewan D. Milne) [2132458]
- scsi: Remove unused member cmd_pool for structure scsi_host_template (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Add environmental reporting log subpage (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Add no_rwlock parameter (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Divide power on reset UNIT ATTENTION (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Use TASK SET FULL more (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Strengthen defer_t accesses (Ewan D. Milne) [2132458]
- scsi: ch: Don't use GFP_DMA (Ewan D. Milne) [2132458]
- scsi: scsi_transport_sas: Add 22.5 Gbps link rate definitions (Ewan D. Milne) [2132458]
- scsi: sd: Free scsi_disk device via put_device() (Ewan D. Milne) [2132458]
- scsi: scsi_debug: Adjust num_parts to create equally sized partitions (Ewan D. Milne) [2132458]
- scsi: ch: remove ch_mutex() (Ewan D. Milne) [2132458]
- scsi: ch: synchronize ch_probe() and ch_open() (Ewan D. Milne) [2132458]
- scsi: ch: fixup refcounting imbalance for SCSI devices (Ewan D. Milne) [2132458]
- scsi: mpi3mr: Schedule IRQ kthreads only on non-RT kernels (Tomas Henzl) [2134535]
- netfilter: flowtable: fix stuck flows on cleanup due to pending work (Phil Sutter) [2131370]
- netfilter: flowtable: add function to invoke garbage collection immediately (Phil Sutter) [2131370]
- netfilter: flowtable: pass flowtable to nf_flow_table_iterate() (Phil Sutter) [2131370]
- netfilter: flowtable: separate replace, destroy and stats to different workqueues (Phil Sutter) [2131370]
- drm/mgag200: Fix PLL setup for G200_SE_A rev >=4 (Jocelyn Falempe) [2130159]
- af_key: Do not call xfrm_probe_algs in parallel (Sabrina Dubroca) [2122369] {CVE-2022-3028}
- xfrm: Update ipcomp_scratches with NULL when freed (Sabrina Dubroca) [2136193]
- esp: choose the correct inner protocol for GSO on inter address family tunnels (Sabrina Dubroca) [2136193]
- xfrm: fix refcount leak in __xfrm_policy_check() (Sabrina Dubroca) [2136193]
- xfrm: xfrm_policy: fix a possible double xfrm_pols_put() in xfrm_bundle_lookup() (Sabrina Dubroca) [2136193]
- net: Fix esp GSO on inter address family tunnels. (Sabrina Dubroca) [2136193]
- esp: Fix BEET mode inter address family tunneling on GSO (Sabrina Dubroca) [2136193]
- cifs: fix check of dfs interlinks (Ronnie Sahlberg) [2132414]
- powerpc/pseries: Fix numa FORM2 parsing fallback code (Nico Pache) [2089496]
- powerpc/pseries: rename numa_dist_table to form2_distances (Nico Pache) [2089496]
- x86/pkey: Fix undefined behaviour with PKRU_WD_BIT (Nico Pache) [2089496]
- hugetlb: add lockdep check for i_mmap_rwsem held in huge_pmd_share (Nico Pache) [2089496]
- mm: page_io: fix psi memory pressure error on cold swapins (Nico Pache) [2089496]
- mm/memcg: Remove 'page' parameter to mem_cgroup_charge_statistics() (Nico Pache) [2089496]
- mm: workingset: replace IRQ-off check with a lockdep assert. (Nico Pache) [2089496]
- mm/madvise: fix potential pte_unmap_unlock pte error (Nico Pache) [2089496]
- mm/mmu_notifier.c: fix race in mmu_interval_notifier_remove() (Nico Pache) [2089496]
- mm/sparse.c: remove NULL check in clear_hwpoisoned_pages() (Nico Pache) [2089496]
- node: fix device cleanups in error handling code (Nico Pache) [2089496]
- x86/setup: Fix static memory detection (Nico Pache) [2089496]
- x86/fault: Don't send SIGSEGV twice on SEGV_PKUERR (Nico Pache) [2089496]
- s390/startup: round down "mem" option to page boundary (Nico Pache) [2089496]
- powerpc/64s: Remove 'dummy_copy_buffer' (Nico Pache) [2089496]
- page_alloc: fix invalid watermark check on a negative value (Nico Pache) [2089496]
- lib/radix-tree: remove unused argument of insert_entries (Nico Pache) [2089496]
- drm/radeon: fix incorrrect SPDX-License-Identifiers (Nico Pache) [2089496]
- mm/swap: fix the obsolete comment for SWP_TYPE_SHIFT (Nico Pache) [2089496]
- irq_work: use kasan_record_aux_stack_noalloc() record callstack (Nico Pache) [2089496]
- kdb: Fix the putarea helper function (Nico Pache) [2089496]
- mm: slab: Delete unused SLAB_DEACTIVATED flag (Nico Pache) [2089496]
- mm, kasan: use compare-exchange operation to set KASAN page tag (Nico Pache) [2089496]
- rcu: Avoid alloc_pages() when recording stack (Nico Pache) [2089496]
- workqueue, kasan: avoid alloc_pages() when recording stack (Nico Pache) [2089496]
- kasan: generic: introduce kasan_record_aux_stack_noalloc() (Nico Pache) [2089496]
- kasan: common: provide can_alloc in kasan_save_stack() (Nico Pache) [2089496]
- lib/stackdepot: remove unused function argument (Nico Pache) [2089496]
- lib/stackdepot: include gfp.h (Nico Pache) [2089496]
- blk-cgroup: blk_cgroup_bio_start() should use irq-safe operations on blkg->iostat_cpu (Nico Pache) [2089496]
- libnvdimm/pmem: Fix crash triggered when I/O in-flight during unbind (Nico Pache) [2089496]
- include/trace/events/vmscan.h: remove mm_vmscan_inactive_list_is_low (Nico Pache) [2089496]
- khugepaged: selftests: remove debug_cow (Nico Pache) [2089496]
- mm/mmzone.h: simplify is_highmem_idx() (Nico Pache) [2089496]
- mm/page-writeback: use __this_cpu_inc() in account_page_dirtied() (Nico Pache) [2089496]
- mm/page-writeback: update the comment of Dirty position control (Nico Pache) [2089496]
- mm/page-writeback: Fix performance when BDI's share of ratio is 0. (Nico Pache) [2089496]
- fuse: ignore PG_workingset after stealing (Nico Pache) [2089496]
- mm/slub: actually fix freelist pointer vs redzoning (Nico Pache) [2089496]
- mm/slub: clarify verification reporting (Nico Pache) [2089496]
- irq_work: Make irq_work_queue() NMI-safe again (Nico Pache) [2089496]
- mm/huge_memory.c: remove unused macro TRANSPARENT_HUGEPAGE_DEBUG_COW_FLAG (Nico Pache) [2089496]
- irq_work: record irq_work_queue() call stack (Nico Pache) [2089496]
- arm64: kasan: fix page_alloc tagging with DEBUG_VIRTUAL (Nico Pache) [2089496]
- mm/arm64: Correct obsolete comment in do_page_fault() (Nico Pache) [2089496]
- kernel: kexec: remove the lock operation of system_transition_mutex (Nico Pache) [2089496]
- libnvdimm/pmem: Remove unused header (Nico Pache) [2089496]
- workqueue: kasan: record workqueue stack (Nico Pache) [2089496]
- lib/test_kasan.c: add workqueue test case (Nico Pache) [2089496]
- page_frag: Recover from memory pressure (Nico Pache) [2089496]
- mm: use helper function put_write_access() (Nico Pache) [2089496]
- mm/swapfile.c: remove unnecessary goto out in _swap_info_get() (Nico Pache) [2089496]
- mm/swap.c: fix incomplete comment in lru_cache_add_inactive_or_unevictable() (Nico Pache) [2089496]
- mm/page_io.c: remove useless out label in __swap_writepage() (Nico Pache) [2089496]
- mm/swap_slots.c: remove always zero and unused return value of enable_swap_slots_cache() (Nico Pache) [2089496]
- mm/swap.c: fix confusing comment in release_pages() (Nico Pache) [2089496]
- mm: annotate a data race in page_zonenum() (Nico Pache) [2089496]
- mm/swap.c: annotate data races for lru_rotate_pvecs (Nico Pache) [2089496]
- mm/rmap: annotate a data race at tlb_flush_batched (Nico Pache) [2089496]
- mm/mempool: fix a data race in mempool_free() (Nico Pache) [2089496]
- mm/list_lru: fix a data race in list_lru_count_one (Nico Pache) [2089496]
- mm/memcontrol: fix a data race in scan count (Nico Pache) [2089496]
- mm/swapfile: fix and annotate various data races (Nico Pache) [2089496]
- mm: thp: remove debug_cow switch (Nico Pache) [2089496]
- page_alloc: consider highatomic reserve in watermark fast (Nico Pache) [2089496]
- mm: remove unnecessary wrapper function do_mmap_pgoff() (Nico Pache) [2089496]
- doc: don't use deprecated "---help---" markers in target docs (Nico Pache) [2089496]
- doc: cgroup: update note about conditions when oom killer is invoked (Nico Pache) [2089496]
- mm: add kvfree_sensitive() for freeing sensitive data objects (Nico Pache) [2089496]
- f2fs: fix retry logic in f2fs_write_cache_pages() (Nico Pache) [2089496]
- mm/hugetlb: avoid unnecessary check on pud and pmd entry in huge_pte_offset (Nico Pache) [2089496]
- mm/page-writeback.c: remove unused variable (Nico Pache) [2089496]
- zswap: docs/vm: Fix typo accept_threshold_percent in zswap.rst (Nico Pache) [2089496]
- tracing: Add a vmalloc_sync_mappings() for safe measure (Nico Pache) [2089496]
- mm/hugetlb: fix a addressing exception caused by huge_pte_offset (Nico Pache) [2089496]
- mm/page-writeback.c: write_cache_pages(): deduplicate identical checks (Nico Pache) [2089496]
- revert "topology: add support for node_to_mem_node() to determine the fallback node" (Nico Pache) [2089496]
- net: memcg: fix lockdep splat in inet_csk_accept() (Nico Pache) [2089496]
- net: memcg: late association of sock to memcg (Nico Pache) [2089496]
- tmpfs: deny and force are not huge mount options (Nico Pache) [2089496]
- mm/zswap.c: add allocation hysteresis if pool limit is hit (Nico Pache) [2089496]
- mm/swapfile.c: swap_next should increase position index (Nico Pache) [2089496]
- fat: use prandom_u32() for i_generation (Nico Pache) [2089496]
- mm/mmap.c: rb_parent is not necessary in __vma_link_list() (Nico Pache) [2089496]
- mm/mmap.c: __vma_unlink_prev() is not necessary now (Nico Pache) [2089496]
- docs: kmemleak: DEBUG_KMEMLEAK_EARLY_LOG_SIZE changed names (Nico Pache) [2089496]
- mm/mmap.c: prev could be retrieved from vma->vm_prev (Nico Pache) [2089496]
- mm/zsmalloc.c: fix a -Wunused-function warning (Nico Pache) [2089496]
- mm/rmap.c: remove set but not used variable 'cstart' (Nico Pache) [2089496]
- tools headers UAPI: Update tools's copy of mman.h headers (Nico Pache) [2089496]
- mm/mmap: move common defines to mman-common.h (Nico Pache) [2089496]
- mm: fix the MAP_UNINITIALIZED flag (Nico Pache) [2089496]
- mm: vmalloc: show number of vmalloc pages in /proc/meminfo (Nico Pache) [2089496]
- slab: remove /proc/slab_allocators (Nico Pache) [2089496]
- mm/huge_memory.c: fix "orig_pud" set but not used (Nico Pache) [2089496]
- mm: hwpoison: use do_send_sig_info() instead of force_sig() (Nico Pache) [2089496]
- mm, page_alloc: drop should_suppress_show_mem (Nico Pache) [2089496]
- mm,page_alloc: PF_WQ_WORKER threads must sleep at should_reclaim_retry() (Nico Pache) [2089496]
- powerpc/8xx: Use patch_site for perf counters setup (Nico Pache) [2089496]
- powerpc/8xx: Use patch_site for memory setup patching (Nico Pache) [2089496]
- Revert "powerpc/8xx: Use L1 entry APG to handle _PAGE_ACCESSED for CONFIG_SWAP" (Nico Pache) [2089496]
- mm/swapfile.c: put_swap_page: share more between huge/normal code path (Nico Pache) [2089496]
- mm, swap, get_swap_pages: use entry_size instead of cluster in parameter (Nico Pache) [2089496]
- mm/swapfile.c: add __swap_entry_free_locked() (Nico Pache) [2089496]
- mm/swapfile.c: unify normal/huge code path in put_swap_page() (Nico Pache) [2089496]
- mm/swapfile.c: unify normal/huge code path in swap_page_trans_huge_swapped() (Nico Pache) [2089496]
- mm/swapfile.c: replace some #ifdef with IS_ENABLED() (Nico Pache) [2089496]
- mm: swap: add comments to lock_cluster_or_swap_info() (Nico Pache) [2089496]
- mm/swapfile.c: use swap_count() in swap_page_trans_huge_swapped() (Nico Pache) [2089496]
- mm, oom: remove sleep from under oom_lock (Nico Pache) [2089496]
- mm/hugetlb: remove gigantic page support for HIGHMEM (Nico Pache) [2089496]
- mm/page-writeback.c: update stale account_page_redirty() comment (Nico Pache) [2089496]
- shmem: use monotonic time for i_generation (Nico Pache) [2089496]
- mptcp: increase default max additional subflows to 2 (Paolo Abeni) [2127136]
- ipv6/addrconf: fix a null-ptr-deref bug for ip6_ptr (Davide Caratti) [2103990]
- ipv6: Refactor fib6_ignore_linkdown (Davide Caratti) [2103990]
- Revert "net: af_key: add check for pfkey_broadcast in function pfkey_process" (Davide Caratti) [2103990]
- net: af_key: add check for pfkey_broadcast in function pfkey_process (Davide Caratti) [2103990]
- certs: Add FIPS selftests (Vladis Dronov) [2134828]
- certs: Move load_certificate_list() to be with the asymmetric keys code (Vladis Dronov) [2134828]

* Wed Nov 02 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-434.el8]
- selftests/bpf: Limit unroll_count for pyperf600 test (Viktor Malik) [2139128]

* Mon Oct 31 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-433.el8]
- perf affinity: Fix out of bound access to "sched_cpus" mask (Michael Petlan) [2125952]
- net: skb: introduce and use a single page frag cache (Paolo Abeni) [2063335]
- powerpc/pseries/vas: Pass hw_cpu_id to node associativity HCALL (Steve Best) [2131651]
- agp/intel: Rename intel-gtt symbols (Jocelyn Falempe) [2115871]
- drm/i915/gt: Split intel-gtt functions by arch (Jocelyn Falempe) [2115871]
- drm: Implement DRM aperture helpers under video/ (Jocelyn Falempe) [2115871]
- efi: Fix build error due to enum collision between efi.h and ima.h (Jocelyn Falempe) [2115871]
- Revert "workqueue: remove unused cancel_work()" (Jocelyn Falempe) [2115871]
- dma-buf: fix use of DMA_BUF_SET_NAME_{A,B} in userspace (Jocelyn Falempe) [2115871]
- drm/i915/gsc: add gsc as a mei auxiliary device (Jocelyn Falempe) [2115871]
- drm/i915: Prepare for multiple GTs (Jocelyn Falempe) [2115871]
- drm/i915/gt: add gt_is_root() helper (Jocelyn Falempe) [2115871]
- drm/i915: Rename INTEL_REGION_LMEM with INTEL_REGION_LMEM_0 (Jocelyn Falempe) [2115871]
- drm/i915: fixup the initial fb base on DGFX (Jocelyn Falempe) [2115871]
- drm/i915: add i915_gem_object_create_region_at() (Jocelyn Falempe) [2115871]
- drm/i915: Report steering details in debugfs (Jocelyn Falempe) [2115871]
- x86/gpu: include drm/i915_pciids.h directly in early quirks (Jocelyn Falempe) [2115871]
- staging: fbtft: core: set smem_len before fb_deferred_io_init call (Jocelyn Falempe) [2115871]
- fbdev: Put mmap for deferred I/O into drivers (Jocelyn Falempe) [2115871]
- fbdev: Track deferred-I/O pages in pageref struct (Jocelyn Falempe) [2115871]
- fbdev: defio: fix the pagelist corruption (Jocelyn Falempe) [2115871]
- fbdev: Don't sort deferred-I/O pages by default (Jocelyn Falempe) [2115871]
- staging: fbtft: Add spaces around / - Style (Jocelyn Falempe) [2115871]
- fbdev/defio: Early-out if page is already enlisted (Jocelyn Falempe) [2115871]
- panic, kexec: make __crash_kexec() NMI safe (Valentin Schneider) [2134126]
- kexec: turn all kexec_mutex acquisitions into trylocks (Valentin Schneider) [2134126]
- kexec: move locking into do_kexec_load (Valentin Schneider) [2134126]
- ice: Fix interface being down after reset with link-down-on-close flag on (Petr Oros) [2024110]
- ice: Add low latency Tx timestamp read (Petr Oros) [2092425]
- ice: introduce ice_ptp_reset_cached_phctime function (Petr Oros) [2092425]
- ice: re-arrange some static functions in ice_ptp.c (Petr Oros) [2092425]
- ice: track and warn when PHC update is late (Petr Oros) [2092425]
- ice: track Tx timestamp stats similar to other Intel drivers (Petr Oros) [2092425]
- ice: implement adjfine with mul_u64_u64_div_u64 (Petr Oros) [2092425]
- ice: Add EXTTS feature to the feature bitmap (Petr Oros) [2092425]
- math: Export mul_u64_u64_div_u64 (Petr Oros) [2092425]
- neighbour: allow NUD_NOARP entries to be forced GCed (Xin Long) [2076534]
- neighbour: Prevent Race condition in neighbour subsytem (Xin Long) [2076534]
- neighbour: Prevent a dead entry from updating gc_list (Xin Long) [2076534]
- net: Exempt multicast addresses from five-second neighbor lifetime (Xin Long) [2076534]
- neighbor: Reset gc_entries counter if new entry is released before insert (Xin Long) [2076534]
- neighbor: Remove externally learned entries from gc_list (Xin Long) [2076534]
- neighbor: Move neigh_update_ext_learned to core file (Xin Long) [2076534]
- neighbor: Remove state and flags arguments to neigh_del (Xin Long) [2076534]
- neighbor: Fix state check in neigh_forced_gc (Xin Long) [2076534]
- neighbor: Fix locking order for gc_list changes (Xin Long) [2076534]
- neighbor: gc_list changes should be protected by table lock (Xin Long) [2076534]
- neighbor: Improve garbage collection (Xin Long) [2076534]
- neighbour: send netlink notification if NTF_ROUTER changes (Xin Long) [2076534]
- neighbour: allow admin to set NTF_ROUTER (Xin Long) [2076534]
- s390/dasd: add device ping attribute (Tobias Huschle) [2043877]
- s390/dasd: suppress generic error messages for PPRC secondary devices (Tobias Huschle) [2043877]
- s390/dasd: add ioctl to perform a swap of the drivers copy pair (Tobias Huschle) [2043877]
- s390/dasd: add copy pair swap capability (Tobias Huschle) [2043877]
- s390/dasd: add copy pair setup (Tobias Huschle) [2043877]
- s390/dasd: add query PPRC function (Tobias Huschle) [2043877]
- s390/dasd: put block allocation in separate function (Tobias Huschle) [2043877]
- s390/dasd: fix Oops in dasd_alias_get_start_dev due to missing pavgroup (Tobias Huschle) [2043877]
- s390/qeth: Split memcpy() of struct qeth_ipacmd_addr_change flexible array (Tobias Huschle) [2110426]
- s390/qeth: Fix typo 'the the' in comment (Tobias Huschle) [2110426]
- s390/qdio: Fix spelling mistake (Tobias Huschle) [2110426]
- qeth: remove a copy of the NAPI_POLL_WEIGHT define (Tobias Huschle) [2110426]
- scsi: bnx2fc: Avoid using get_cpu() in bnx2fc_cmd_alloc() (Nilesh Javali) [2109895]
- scsi: bnx2fc: Fix spelling mistake "mis-match" -> "mismatch" (Nilesh Javali) [2109895]
- scsi: bnx2fc: Make use of the helper macro kthread_run() (Nilesh Javali) [2109895]
- scsi: bnx2fc: Fix typo in comments (Nilesh Javali) [2109895]
- scsi: qedf: Populate sysfs attributes for vport (Nilesh Javali) [2120219]
- scsi: qedf: Fix typo in comment (Nilesh Javali) [2109893]
- scsi: qedf: Remove redundant variable op (Nilesh Javali) [2109893]
- scsi: qedf: Remove an unneeded NULL check on list iterator (Nilesh Javali) [2109893]
- scsi: qedf: Remove unnecessary code (Nilesh Javali) [2109893]
- s390/sclp: reserve memory occupied by sclp early buffer (Mete Durlu) [2060830]
- s390: make command line configurable (Mete Durlu) [2060830]
- s390: support command lines longer than 896 bytes (Mete Durlu) [2060830]
- s390/kexec_file: move kernel image size check (Mete Durlu) [2060830]
- s390/boot: move sclp early buffer from fixed address in asm to C (Mete Durlu) [2060830]
- drivers/base: Fix unsigned comparison to -1 in CPUMAP_FILE_MAX_BYTES (Phil Auld) [2115518]
- sched/core: Do not requeue task on CPU excluded from cpus_mask (Phil Auld) [2115518]
- workqueue: Avoid a false warning in unbind_workers() (Phil Auld) [2115518]
- sched/core: Always flush pending blk_plug (Phil Auld) [2115518]
- sched/fair: fix case with reduced capacity CPU (Phil Auld) [2115518]
- sched: Remove unused function group_first_cpu() (Phil Auld) [2115518]
- sched/fair: Remove redundant word " *" (Phil Auld) [2115518]
- sched: only perform capability check on privileged operation (Phil Auld) [2115518]
- sched: Allow newidle balancing to bail out of load_balance (Phil Auld) [2115518]
- sched: Remove the limitation of WF_ON_CPU on wakelist if wakee cpu is idle (Phil Auld) [2115518]
- sched: Fix the check of nr_running at queue wakelist (Phil Auld) [2115518]
- sched: Fix balance_push() vs __sched_setscheduler() (Phil Auld) [2115518]
- sched/fair: Optimize and simplify rq leaf_cfs_rq_list (Phil Auld) [2115518]
- topology: Remove unused cpu_cluster_mask() (Phil Auld) [2115518]
- sched: Update task_tick_numa to ignore tasks without an mm (Phil Auld) [2115518]
- sched/deadline: Remove superfluous rq clock update in push_dl_task() (Phil Auld) [2115518]
- time/sched_clock: Fix formatting of frequency reporting code (Phil Auld) [2115518]
- time/sched_clock: Use Hz as the unit for clock rate reporting below 4kHz (Phil Auld) [2115518]
- time/sched_clock: Round the frequency reported to nearest rather than down (Phil Auld) [2115518]
- sched/fair: Delete useless condition in tg_unthrottle_up() (Phil Auld) [2115518]
- sched/fair: Fix cfs_rq_clock_pelt() for throttled cfs_rq (Phil Auld) [2115518]
- workqueue: Restrict kworker in the offline CPU pool running on housekeeping CPUs (Phil Auld) [2115518]
- kernel/sched: Remove dl_boosted flag comment (Phil Auld) [2115518]
- workqueue: Remove schedule() in unbind_workers() (Phil Auld) [2115518]
- workqueue: Remove outdated comment about exceptional workers in unbind_workers() (Phil Auld) [2115518]
- workqueue: Remove the advanced kicking of the idle workers in rebind_workers() (Phil Auld) [2115518]
- workqueue: Fix unbind_workers() VS wq_worker_running() race (Phil Auld) [2115518]
- sched/membarrier: fix missing local execution of ipi_sync_rq_state() (Phil Auld) [2115518]
- kthread: Move prio/affinite change into the newly created thread (Phil Auld) [2115518]

* Mon Oct 24 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-432.el8]
- dmaengine: idxd: Correct IAX operation code names (Jerry Snitselaar) [2112121]
- dmaengine: dmatest: use strscpy to replace strlcpy (Jerry Snitselaar) [2112121]
- dmaengine: remove DMA_MEMCPY_SG once again (Jerry Snitselaar) [2112121]
- MAINTAINERS: idxd driver maintainer update (Jerry Snitselaar) [2112121]
- dmaengine: dmatest: Replace symbolic permissions by octal permissions (Jerry Snitselaar) [2112121]
- dmaengine: dmatest: Remove spaces before tabs (Jerry Snitselaar) [2112121]
- dma:dw: remove reference to AVR32 architecture in core.c (Jerry Snitselaar) [2112121]
- dmaengine: idxd: Only call idxd_enable_system_pasid() if succeeded in enabling SVA feature (Jerry Snitselaar) [2112121]
- dmaengine: idxd: force wq context cleanup on device disable path (Jerry Snitselaar) [2112121]
- dmaengine: Revert "dmaengine: add verification of DMA_INTERRUPT capability for dmatest" (Jerry Snitselaar) [2112121]
- dmaengine: idxd: Separate user and kernel pasid enabling (Jerry Snitselaar) [2112121]
- dmaengine: ptdma: statify pt_tx_status (Jerry Snitselaar) [2112121]
- dmaengine: hidma: In hidma_prep_dma_memset treat value as a single byte (Jerry Snitselaar) [2112121]
- dmaengine: Document dmaengine_prep_dma_memset (Jerry Snitselaar) [2112121]
- dmaengine: PTDMA: support polled mode (Jerry Snitselaar) [2112121]
- dmaengine: Remove a useless mutex (Jerry Snitselaar) [2112121]
- dmaengine: idxd: update IAA definitions for user header (Jerry Snitselaar) [2112121]
- dmaengine: Clarify cyclic transfer residue documentation (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: Remove useless DMA-32 fallback configuration (Jerry Snitselaar) [2112121]
- dmaengine: iot: Remove useless DMA-32 fallback configuration (Jerry Snitselaar) [2112121]
- dmaengine: ioatdma: use default_groups in kobj_type (Jerry Snitselaar) [2112121]
- Documentation: dmaengine: Correctly describe dmatest with channel unset (Jerry Snitselaar) [2112121]
- Documentation: dmaengine: Add a description of what dmatest does (Jerry Snitselaar) [2112121]
- dmaengine: Add core function and capability check for DMA_MEMCPY_SG (Jerry Snitselaar) [2112121]
- dmaengine: Add documentation for new memcpy scatter-gather function (Jerry Snitselaar) [2112121]
- dmaengine: remove slave_id config field (Jerry Snitselaar) [2112121]
- dmaengine: ioat: switch from 'pci_' to 'dma_' API (Jerry Snitselaar) [2112121]
- dmaengine: hsu: switch from 'pci_' to 'dma_' API (Jerry Snitselaar) [2112121]
- dmaengine: dw: switch from 'pci_' to 'dma_' API (Jerry Snitselaar) [2112121]
- dmaengine: remove debugfs #ifdef (Jerry Snitselaar) [2112121]
- dmaengine: dmaengine_desc_callback_valid(): Check for `callback_result` (Jerry Snitselaar) [2112121]
- dmaengine: Remove redundant initialization of variable err (Jerry Snitselaar) [2112121]
- dmaengine: Extend the dma_slave_width for 128 bytes (Jerry Snitselaar) [2112121]
- dmaengine: ioat: depends on !UML (Jerry Snitselaar) [2112121]
- dmaengine: dw: Simplify DT property parser (Jerry Snitselaar) [2112121]
- dmaengine: dw: Convert members to u32 in platform data (Jerry Snitselaar) [2112121]
- dmaengine: dw: Remove error message from DT parsing code (Jerry Snitselaar) [2112121]
- dmaengine: of-dma: router_xlate to return -EPROBE_DEFER if controller is not yet available (Jerry Snitselaar) [2112121]
- dmaengine: hsu: Account transferred bytes (Jerry Snitselaar) [2112121]
- dmaengine: Move kdoc description of struct dma_chan_percpu closer to it (Jerry Snitselaar) [2112121]
- dmaengine: QCOM_HIDMA_MGMT depends on HAS_IOMEM (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: comment platform_driver_register call (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: remove unused code (Jerry Snitselaar) [2112121]
- dmaengine: Fix a double free in dma_async_device_register (Jerry Snitselaar) [2112121]
- dmaengine: hsu: disable spurious interrupt (Jerry Snitselaar) [2112121]
- dmaengine: Extend the dmaengine_alignment for 128 and 256 bytes (Jerry Snitselaar) [2112121]
- dmaengine: dmatest: Use dmaengine_get_dma_device (Jerry Snitselaar) [2112121]
- dmaengine: doc: client: Update for dmaengine_get_dma_device() usage (Jerry Snitselaar) [2112121]
- dmaengine: Add support for per channel coherency handling (Jerry Snitselaar) [2112121]
- dmaengine: of-dma: Add support for optional router configuration callback (Jerry Snitselaar) [2112121]
- dmaengine: add peripheral configuration (Jerry Snitselaar) [2112121]
- dmaengine: idma64: Switch to use __maybe_unused instead of ifdeffery (Jerry Snitselaar) [2112121]
- dmaengine: ioatdma: remove unused function missed during dma_v2 removal (Jerry Snitselaar) [2112121]
- dmaengine: Save few bytes and increase readability of dma_request_chan() (Jerry Snitselaar) [2112121]
- dmaengine: of-dma: Fix of_dma_router_xlate's of_dma_xlate handling (Jerry Snitselaar) [2112121]
- dmaengine: dw: Don't include unneeded header to platform data header (Jerry Snitselaar) [2112121]
- dmaengine: linux/dmaengine.h: drop duplicated word in a comment (Jerry Snitselaar) [2112121]
- dmaengine: ioat: Fix some parameter misspelling and provide description for phys_complete (Jerry Snitselaar) [2112121]
- dmaengine: of-dma: Fix misspellings/formatting issues in some function headers (Jerry Snitselaar) [2112121]
- Documentation/driver-api: dmaengine/provider: drop doubled word (Jerry Snitselaar) [2112121]
- dmaengine: Add support for repeating transactions (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: use true,false for bool variable (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: Simplify error handling path in hidma_probe (Jerry Snitselaar) [2112121]
- dmaengine: Fix misspelling of "Analog Devices" (Jerry Snitselaar) [2112121]
- docs: dmaengine: provider.rst: get rid of some warnings (Jerry Snitselaar) [2112121]
- dmaengine: doc: fix warnings/issues of client.rst (Jerry Snitselaar) [2112121]
- dmaengine: doc: Properly indent metadata title (Jerry Snitselaar) [2112121]
- dmaengine: doc: Add sections for per descriptor metadata support (Jerry Snitselaar) [2112121]
- dmaengine: Fix Kconfig indentation (Jerry Snitselaar) [2112121]
- dmaengine: qcom: hidma_mgmt: Add of_node_put() before goto (Jerry Snitselaar) [2112121]
- dmaengine: Remove dev_err() usage after platform_get_irq() (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: Remove call to memset after dmam_alloc_coherent (Jerry Snitselaar) [2112121]
- Documentation: dmaengine: clean up description of dmatest usage (Jerry Snitselaar) [2112121]
- dmaengine: hsu: Revert "set HSU_CH_MTSR to memory width" (Jerry Snitselaar) [2112121]
- dmaengine: qcom: hidma: no need to check return value of debugfs_create functions (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: assign channel cookie correctly (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: initialize tx flags in hidma_prep_dma_* (Jerry Snitselaar) [2112121]
- dmaengine: qcom_hidma: convert to DEFINE_SHOW_ATTRIBUTE (Jerry Snitselaar) [2112121]
- dmaengine: Documentation: Add documentation for multi chan testing (Jerry Snitselaar) [2112121]
- dmaengine: hsu: remove dma_slave_config direction usage (Jerry Snitselaar) [2112121]
- dmaengine: hsu: Support dmaengine_terminate_sync() (Jerry Snitselaar) [2112121]
- scsi: core: Allow the ALUA transitioning state enough time (Tomas Henzl) [2084250]
- scsi: core: Return BLK_STS_TRANSPORT for ALUA transitioning (Tomas Henzl) [2084250]
- macvlan: enforce a consistent minimal mtu (Davide Caratti) [2134032]
- ipvlan: Fix out-of-bound bugs caused by unset skb->mac_header (Davide Caratti) [2134032]
- net: ipvtap - add __init/__exit annotations to module init/exit funcs (Davide Caratti) [2134032]
- tunnels: do not assume mac header is set in skb_tunnel_check_pmtu() (Guillaume Nault) [2134099]
- erspan: do not assume transport header is always set (Guillaume Nault) [2134099]
- net: ip_gre: do not report erspan_ver for gre or gretap (Guillaume Nault) [2134099]
- selftests: Fix the if conditions of in test_extra_filter() (Hangbin Liu) [2135232]
- selftests: forwarding: add shebang for sch_red.sh (Hangbin Liu) [2135232]
- selftests: forwarding: fix error message in learning_test (Hangbin Liu) [2135232]
- selftests/net: pass ipv6_args to udpgso_bench's IPv6 TCP test (Hangbin Liu) [2135232]
- ping: remove pr_err from ping_lookup (Guillaume Nault) [2135424]
- ping: fix the dif and sdif check in ping_lookup (Guillaume Nault) [2135424]
- ping: fix the sk_bound_dev_if match in ping_lookup (Guillaume Nault) [2135424]
- tcp/udp: Call inet6_destroy_sock() in IPv6 sk->sk_destruct(). (Hangbin Liu) [2135259]
- udp: Call inet6_destroy_sock() in setsockopt(IPV6_ADDRFORM). (Hangbin Liu) [2135259]
- tcp/udp: Fix memory leak in ipv6_renew_options(). (Hangbin Liu) [2135259]
- ipv6: sr: fix out-of-bounds read when setting HMAC data. (Hangbin Liu) [2135259]
- ipv6: do not use RT_TOS for IPv6 flowlabel (Hangbin Liu) [2135259]
- ipv6/sit: fix ipip6_tunnel_get_prl return value (Hangbin Liu) [2135259]
- sit: use min (Hangbin Liu) [2135259]
- net: ipv6: unexport __init-annotated seg6_hmac_init() (Hangbin Liu) [2135259]
- sit: do not call ipip6_dev_free() from sit_init_net() (Hangbin Liu) [2135259]
- block: avoid sign extend problem with default queue flags mask (Nico Pache) [2131929]
- mm/hwpoison: do not lock page again when me_huge_page() successfully recovers (Aristeu Rozanski) [2110292]
- crypto: ccp - Remove the unneeded result variable (Vladis Dronov) [2130195]
- crypto: ccp - Release dma channels before dmaengine unrgister (Vladis Dronov) [2130195]
- crypto: ccp - Fail the PSP initialization when writing psp data file failed (Vladis Dronov) [2130195]
- crypto: ccp - Initialize PSP when reading psp data file failed (Vladis Dronov) [2130195]
- crypto: ccp - Add a quirk to firmware update (Vladis Dronov) [2130195]
- crypto: ccp - Add support for new CCP/PSP device ID (Vladis Dronov) [2130195]
- crypto: ccp - During shutdown, check SEV data pointer before using (Vladis Dronov) [2130195]
- crypto: ccp - Fix device IRQ counting by using platform_irq_count() (Vladis Dronov) [2130195]
- crypto: ccp - fix typo in comment (Vladis Dronov) [2130195]
- crypto: ccp - Use kzalloc for sev ioctl interfaces to prevent kernel memory leak (Vladis Dronov) [2130195]
- crypto: ccp - Fix the INIT_EX data file open failure (Vladis Dronov) [2130195]
- crypto: ccp - Log when resetting PSP SEV state (Vladis Dronov) [2130195]
- crypto: ccp - When TSME and SME both detected notify user (Vladis Dronov) [2130195]
- crypto: ccp - Allow PSP driver to load without SEV/TEE support (Vladis Dronov) [2130195]
- crypto: ccp - Export PSP security bits to userspace (Vladis Dronov) [2130195]
- crypto: ccp - cache capability into psp device (Vladis Dronov) [2130195]
- PCI: Add support for dev_groups to struct pci_driver (Vladis Dronov) [2130195]
- ACPI: processor idle: Practically limit "Dummy wait" workaround to old Intel systems (Wei Huang) [2130653]
- blk-mq: fix io hung due to missing commit_rqs (Ming Lei) [2130028]
- block: schedule queue restart after BLK_STS_ZONE_RESOURCE (Ming Lei) [2130028]
- blk-mq: call commit_rqs while list empty but error happen (Ming Lei) [2130028]
- null_blk: fix ida error handling in null_add_dev() (Ming Lei) [2130028]
- blktrace: Trace remapped requests correctly (Ming Lei) [2130028]
- virtio_blk: fix the discard_granularity and discard_alignment queue limits (Ming Lei) [2130028]
- block: fix bio_clone_blkg_association() to associate with proper blkcg_gq (Ming Lei) [2130028]
- blk-mq: do not update io_ticks with passthrough requests (Ming Lei) [2130028]
- blk-mq: don't touch ->tagset in blk_mq_get_sq_hctx (Ming Lei) [2130028]
- ipmi:ipmb: Fix refcount leak in ipmi_ipmb_probe (Tony Camuso) [2130238]
- ipmi: remove unnecessary type castings (Tony Camuso) [2130238]
- ipmi: Make two logs unique (Tony Camuso) [2130238]
- ipmi:si: Convert pr_debug() to dev_dbg() (Tony Camuso) [2130238]
- ipmi: Convert pr_debug() to dev_dbg() (Tony Camuso) [2130238]
- ipmi: Fix pr_fmt to avoid compilation issues (Tony Camuso) [2130238]
- ipmi: Add an intializer for ipmi_recv_msg struct (Tony Camuso) [2130238]
- ipmi: Add an intializer for ipmi_smi_msg struct (Tony Camuso) [2130238]
- ipmi:ssif: Check for NULL msg when handling events and messages (Tony Camuso) [2130238]
- ipmi: use simple i2c probe function (Tony Camuso) [2130238]
- ipmi: Add a sysfs count of total outstanding messages for an interface (Tony Camuso) [2130238]
- ipmi: Add a sysfs interface to view the number of users (Tony Camuso) [2130238]
- ipmi: Limit the number of message a user may have outstanding (Tony Camuso) [2130238]
- ipmi: Add a limit on the number of users that may use IPMI (Tony Camuso) [2130238]
- ipmi:ipmi_ipmb: Fix null-ptr-deref in ipmi_unregister_smi() (Tony Camuso) [2130238]
- ipmi: When handling send message responses, don't process the message (Tony Camuso) [2130238]
- ipmi: fix IPMI_SMI_MSG_TYPE_IPMB_DIRECT response length checking (Tony Camuso) [2130238]
- ipmi: fix oob access due to uninit smi_msg type (Tony Camuso) [2130238]
- ipmi: Make kABI adjustments (Tony Camuso) [2130238]
- ipmi: Add support for IPMB direct messages (Tony Camuso) [2130238]
- ice: Fix crash by keep old cfg when update TCs more than queues (Petr Oros) [2129902]
- ice: Fix tunnel checksum offload with fragmented traffic (Petr Oros) [2129902]
- ice: handle E822 generic device ID in PLDM header (Petr Oros) [2129902]
- ice: ethtool: Prohibit improper channel config for DCB (Petr Oros) [2129902]
- ice: ethtool: advertise 1000M speeds properly (Petr Oros) [2129902]
- ice: Fix switchdev rules book keeping (Petr Oros) [2129902]
- ice: fix access-beyond-end in the switch code (Petr Oros) [2129902]
- eth: ice: silence the GCC 12 array-bounds warning (Petr Oros) [2129902]
- ice: Expose RSS indirection tables for queue groups via ethtool (Petr Oros) [2129902]
- Revert "ice: Hide bus-info in ethtool for PRs in switchdev mode" (Petr Oros) [2129902]
- ice: remove period on argument description in ice_for_each_vf (Petr Oros) [2129902]
- ice: add a function comment for ice_cfg_mac_antispoof (Petr Oros) [2129902]
- ice: fix wording in comment for ice_reset_vf (Petr Oros) [2129902]
- ice: remove return value comment for ice_reset_all_vfs (Petr Oros) [2129902]
- ice: always check VF VSI pointer values (Petr Oros) [2129902]
- ice: add newline to dev_dbg in ice_vf_fdir_dump_info (Petr Oros) [2129902]
- ice: get switch id on switchdev devices (Petr Oros) [2129902]
- ice: return ENOSPC when exceeding ICE_MAX_CHAIN_WORDS (Petr Oros) [2129902]
- ice: introduce common helper for retrieving VSI by vsi_num (Petr Oros) [2129902]
- ice: use min_t() to make code cleaner in ice_gnss (Petr Oros) [2129902]
- ice: Add mpls+tso support (Petr Oros) [2129902]
- ice: switch: convert packet template match code to rodata (Petr Oros) [2129902]
- ice: switch: use convenience macros to declare dummy pkt templates (Petr Oros) [2129902]
- ice: switch: use a struct to pass packet template params (Petr Oros) [2129902]
- ice: switch: unobscurify bitops loop in ice_fill_adv_dummy_packet() (Petr Oros) [2129902]
- ice: switch: add and use u16[] aliases to ice_adv_lkup_elem::{h, m}_u (Petr Oros) [2129902]
- ice: Support GTP-U and GTP-C offload in switchdev (Petr Oros) [2129902]
- ice: Remove useless DMA-32 fallback configuration (Petr Oros) [2129902]
- ice: switch to napi_build_skb() (Petr Oros) [2129902]
- nbd: fix race between nbd_alloc_config() and module removal (Ming Lei) [2127601]
- nbd: call genl_unregister_family() first in nbd_cleanup() (Ming Lei) [2127601]
- kselftests: memcg: speed up the memory.high test (Waiman Long) [1839057]
- tools/testing/selftests/cgroup/cgroup_util.c: cg_read_strcmp: fix null pointer dereference (Waiman Long) [1839057]
- kselftest/cgroup: fix incorrect test_core skip (Waiman Long) [1839057]
- kselftest/cgroup: fix unexpected testing failure on test_core (Waiman Long) [1839057]
- selftests: cgroup: fix cleanup path in test_memcg_subtree_control() (Waiman Long) [1839057]
- cgroup: fix an error handling path in alloc_pagecache_max_30M() (Waiman Long) [1839057]
- selftests: memcg: expect no low events in unprotected sibling (Waiman Long) [1839057]
- selftests: memcg: fix compilation (Waiman Long) [1839057]
- kseltest/cgroup: Make test_stress.sh work if run interactively (Waiman Long) [1839057]
- cgroup: fix racy check in alloc_pagecache_max_30M() helper function (Waiman Long) [1839057]
- cgroup: remove racy check in test_memcg_sock() (Waiman Long) [1839057]
- cgroup: account for memory_localevents in test_memcg_oom_group_leaf_events() (Waiman Long) [1839057]
- cgroup: account for memory_recursiveprot in test_memcg_low() (Waiman Long) [1839057]
- cgroups: refactor children cgroups in memcg tests (Waiman Long) [1839057]
- kselftest/cgroup: fix test_stress.sh to use OUTPUT dir (Waiman Long) [1839057]
- selftests: cgroup: add a selftest for memory.reclaim (Waiman Long) [1839057]
- selftests: cgroup: fix alloc_anon_noexit() instantly freeing memory (Waiman Long) [1839057]
- selftests: cgroup: return -errno from cg_read()/cg_write() on failure (Waiman Long) [1839057]
- memcg: introduce per-memcg reclaim interface (Waiman Long) [1839057]
- kselftests: memcg: update the oom group leaf events test (Waiman Long) [1839057]
- mm/memcontrol: return 1 from cgroup.memory __setup() handler (Waiman Long) [1839057]
- memcg: synchronously enforce memory.high for large overcharges (Waiman Long) [1839057]
- selftests: memcg: test high limit for single entry allocation (Waiman Long) [1839057]
- memcg: unify force charging conditions (Waiman Long) [1839057]
- memcg: refactor mem_cgroup_oom (Waiman Long) [1839057]
- memcg: prohibit unconditional exceeding the limit of dying tasks (Waiman Long) [1839057]
- mm, oom: do not trigger out_of_memory from the #PF (Waiman Long) [1839057]
- mm, oom: pagefault_out_of_memory: don't force global OOM for dying tasks (Waiman Long) [1839057]
- mm: memcontrol: fix root_mem_cgroup charging (Waiman Long) [1839057]
- tests/cgroup: move cg_wait_for(), cg_prepare_for_wait() (Waiman Long) [1839057]
- mm: memcontrol: don't count limit-setting reclaim as memory pressure (Waiman Long) [1839057]
- selftests: Uninitialized variable in test_cgcore_proc_migration() (Waiman Long) [1839057]
- kselftests: cgroup: Avoid the reuse of fd after it is deallocated (Waiman Long) [1839057]
- selftests: cgroup: Run test_core under interfering stress (Waiman Long) [1839057]
- selftests: cgroup: Add task migration tests (Waiman Long) [1839057]
- selftests: cgroup: Simplify task self migration (Waiman Long) [1839057]
- cgroup: kselftest: relax fs_spec checks (Waiman Long) [1839057]
- kselftests: cgroup: remove duplicated include from test_freezer.c (Waiman Long) [1839057]
- kselftest/cgroup: fix unexpected testing failure on test_memcontrol (Waiman Long) [1839057]
- kselftests: cgroup: add freezer controller self-tests (Waiman Long) [1839057]
- Add tests for memory.oom.group (Waiman Long) [1839057]
- Fix cg_read_strcmp() (Waiman Long) [1839057]
- cgroup: kselftests: add test_core to .gitignore (Waiman Long) [1839057]
- selftests: cgroup: add gitignore file (Waiman Long) [1839057]
- Add cgroup core selftests (Waiman Long) [1839057]
- devdax: Fix soft-reservation memory description (Mark Langsdorf) [2122316]
- arm64: cacheinfo: Fix incorrect assignment of signed error value to unsigned fw_level (Mark Langsdorf) [2122316]
- ACPI: property: Remove default association from integer maximum values (Mark Langsdorf) [2122316]
- ACPI: property: Ignore already existing data node tags (Mark Langsdorf) [2122316]
- ACPI: property: Fix type detection of unified integer reading functions (Mark Langsdorf) [2122316]
- ACPI: processor: Remove freq Qos request for all CPUs (Mark Langsdorf) [2122316]
- ACPI: property: Fix error handling in acpi_init_properties() (Mark Langsdorf) [2122316]
- ACPI/IORT: Fix build error implicit-function-declaration (Mark Langsdorf) [2122316]
- ACPI/PCI: Remove useless NULL pointer checks (Mark Langsdorf) [2122316]
- ACPI: property: Read buffer properties as integers (Mark Langsdorf) [2122316]
- ACPI: property: Add support for parsing buffer property UUID (Mark Langsdorf) [2122316]
- ACPI: property: Unify integer value reading functions (Mark Langsdorf) [2122316]
- ACPI: property: Switch node property referencing from ifs to a switch (Mark Langsdorf) [2122316]
- ACPI: property: Move property ref argument parsing into a new function (Mark Langsdorf) [2122316]
- ACPI: property: Use acpi_object_type consistently in property ref parsing (Mark Langsdorf) [2122316]
- ACPI: property: Tie data nodes to acpi handles (Mark Langsdorf) [2122316]
- ACPI: property: Return type of acpi_add_nondev_subnodes() should be bool (Mark Langsdorf) [2122316]
- ACPI: CPPC: Do not prevent CPPC from working in the future (Mark Langsdorf) [2122316]
- ACPI: PM: x86: Print messages regarding LPS0 idle support (Mark Langsdorf) [2122316]
- ACPI: PPTT: Leave the table mapped for the runtime usage (Mark Langsdorf) [2122316]
- ACPI: resource: skip IRQ override on AMD Zen platforms (Mark Langsdorf) [2122316]
- ACPI: irq: Allow acpi_gsi_to_irq() to have an arch-specific fallback (Mark Langsdorf) [2122316]
- APCI: irq: Add support for multiple GSI domains (Mark Langsdorf) [2122316]
- irqchip/gic: Drop support for secondary GIC in non-DT systems (Mark Langsdorf) [2122316]
- ACPI: video: Use native backlight on Dell Inspiron N4010 (Mark Langsdorf) [2122316]
- ACPI: PM: s2idle: Use LPS0 idle if ACPI_FADT_LOW_POWER_S0 is unset (Mark Langsdorf) [2122316]
- Revert "[acpi] ACPI / PM: LPIT: Register sysfs attributes based on FADT" (Mark Langsdorf) [2122316]
- ACPI: utils: Add api to read _SUB from ACPI (Mark Langsdorf) [2122316]
- ACPI: video: Shortening quirk list by identifying Clevo by board_name only (Mark Langsdorf) [2122316]
- ACPI: video: Force backlight native for some TongFang devices (Mark Langsdorf) [2122316]
- PCI/ACPI: Guard ARM64-specific mcfg_quirks (Mark Langsdorf) [2122316]
- ACPI/IORT: Add a helper to retrieve RMR info directly (Mark Langsdorf) [2122316]
- ACPI/IORT: Add support to retrieve IORT RMR reserved regions (Mark Langsdorf) [2122316]
- ACPI/IORT: Provide a generic helper to retrieve reserve regions (Mark Langsdorf) [2122316]
- ACPI/IORT: Make iort_iommu_msi_get_resv_regions() return void (Mark Langsdorf) [2122316]
- iommu: Introduce a callback to struct iommu_resv_region (Mark Langsdorf) [2122316]
- ACPI: PM: s2idle: Add support for upcoming AMD uPEP HID AMDI008 (Mark Langsdorf) [2122316]
- ACPI: PPTT: Use table offset as fw_token instead of virtual address (Mark Langsdorf) [2122316]
- ACPI: Move PRM config option under the main ACPI config (Mark Langsdorf) [2122316]
- ACPI: Enable Platform Runtime Mechanism(PRM) support on ARM64 (Mark Langsdorf) [2122316]
- efi: Simplify arch_efi_call_virt() macro (Mark Langsdorf) [2122316]
- efi/x86: Avoid redundant cast of EFI firmware service pointer (Mark Langsdorf) [2122316]
- efi/libstub: Annotate firmware routines as __efiapi (Mark Langsdorf) [2122316]
- ACPI: PRM: Change handler_addr type to void pointer (Mark Langsdorf) [2122316]
- ACPI: bus: Drop driver member of struct acpi_device (Mark Langsdorf) [2122316]
- ACPI: bus: Drop redundant check in acpi_device_remove() (Mark Langsdorf) [2122316]
- ACPI: APEI: Fix _EINJ vs EFI_MEMORY_SP (Mark Langsdorf) [2122316]
- ACPI: LPSS: Fix missing check in register_device_clock() (Mark Langsdorf) [2122316]
- ACPI: APEI: Better fix to avoid spamming the console with old error logs (Mark Langsdorf) [2122316]
- ACPI: PM: save NVS memory for Lenovo G40-45 (Mark Langsdorf) [2122316]
- ACPI: EC: Drop unused ident initializers from dmi_system_id tables (Mark Langsdorf) [2122316]
- ACPI: EC: Re-use boot_ec when possible even when EC_FLAGS_TRUST_DSDT_GPE is set (Mark Langsdorf) [2122316]
- ACPI: EC: Drop the EC_FLAGS_IGNORE_DSDT_GPE quirk (Mark Langsdorf) [2122316]
- ACPI: EC: Remove duplicate ThinkPad X1 Carbon 6th entry from DMI quirks (Mark Langsdorf) [2122316]
- ACPI: processor: Drop leftover acpi_processor_get_limit_info() declaration (Mark Langsdorf) [2122316]
- ACPI: processor: Split out thermal initialization from ACPI PSS (Mark Langsdorf) [2122316]
- redhat/configs: move CONFIG_ACPI_VIDEO to common/generic (Mark Langsdorf) [2122316]
- ACPI: video: Drop X86 dependency from Kconfig (Mark Langsdorf) [2122316]
- ACPI: video: Fix acpi_video_handles_brightness_key_presses() (Mark Langsdorf) [2122316]
- ACPI: video: Change how we determine if brightness key-presses are handled (Mark Langsdorf) [2122316]
- ACPI / MMC: PM: Unify fixing up device power (Mark Langsdorf) [2122316]
- mmc: sdhci-acpi: Use the new soc_intel_is_byt() helper (Mark Langsdorf) [2122316]
- mmc: sdhci-acpi: Remove special handling for GPD win/pocket devices (Mark Langsdorf) [2122316]
- ACPI: scan: Walk ACPI device's children using driver core (Mark Langsdorf) [2122316]
- ACPI: bus: Introduce acpi_dev_for_each_child_reverse() (Mark Langsdorf) [2122316]
- ACPI: video: Use acpi_dev_for_each_child() (Mark Langsdorf) [2122316]
- ACPI: property: Use acpi_dev_for_each_child() for child lookup (Mark Langsdorf) [2122316]
- ACPI: container: Use acpi_dev_for_each_child() (Mark Langsdorf) [2122316]
- ACPI: bus: Export acpi_dev_for_each_child() to modules (Mark Langsdorf) [2122316]
- ACPI: glue: Introduce acpi_find_child_by_adr() (Mark Langsdorf) [2122316]
- ACPI: glue: Introduce acpi_dev_has_children() (Mark Langsdorf) [2122316]
- ACPI: glue: Use acpi_dev_for_each_child() (Mark Langsdorf) [2122316]
- ACPI: APEI: Fix double word in a comment (Mark Langsdorf) [2122316]
- ACPI: processor/idle: Annotate more functions to live in cpuidle section (Mark Langsdorf) [2122316]
- ACPI: DPTF: Support Meteor Lake (Mark Langsdorf) [2122316]
- ACPI: CPPC: fix typo in comment (Mark Langsdorf) [2122316]
- ACPI: video: improve PM notifer callback (Mark Langsdorf) [2122316]
- ACPI: utils: include UUID in _DSM evaluation warning (Mark Langsdorf) [2122316]
- cpufreq: CPPC: Enable fast_switch (Mark Langsdorf) [2122316]
- acpi/nfit: rely on mce->misc to determine poison granularity (Mark Langsdorf) [2122316]
- ACPI: PM: Block ASUS B1400CEAE from suspend to idle by default (Mark Langsdorf) [2122316]
- ACPI: clean up white space in a few places for consistency (Mark Langsdorf) [2122316]
- ACPI: glue: Rearrange find_child_checks() (Mark Langsdorf) [2122316]
- ACPI: DPTF: Add support for high frequency impedance notification (Mark Langsdorf) [2122316]
- ACPI: processor: idle: Expose max_cstate/nocst/bm_check_disable read-only in sysfs (Mark Langsdorf) [2122316]
- ACPI: battery: Make "not-charging" the default on no charging or full info (Mark Langsdorf) [2122316]
- PCI/ACPI: negotiate CXL _OSC (Mark Langsdorf) [2122316]
- PCI/ACPI: Prefer CXL _OSC instead of PCIe _OSC for CXL host bridges (Mark Langsdorf) [2122316]
- PCI/ACPI: add a helper for retrieving _OSC Control DWORDs (Mark Langsdorf) [2122316]
- ACPI: bus: Avoid non-ACPI device objects in walks over children (Mark Langsdorf) [2122316]
- ACPI: DPTF: Correct description of INT3407 / INT3532 attributes (Mark Langsdorf) [2122316]
- ACPI: BGRT: use static for BGRT_SHOW kobj_attribute defines (Mark Langsdorf) [2122316]
- ACPI, APEI, EINJ: Refuse to inject into the zero page (Mark Langsdorf) [2122316]
- ACPI: PM: Always print final debug message in acpi_device_set_power() (Mark Langsdorf) [2122316]
- ACPI: SPCR: Add support for NVIDIA 16550-compatible port subtype (Mark Langsdorf) [2122316]
- ACPI: APEI: Fix missing ERST record id (Mark Langsdorf) [2122316]
- ACPICA: Update version to 20220331 (Mark Langsdorf) [2122316]
- ACPICA: IORT: Updates for revision E.d (Mark Langsdorf) [2122316]
- ACPICA: iASL/MADT: Add OEM-defined subtable (Mark Langsdorf) [2122316]
- ACPICA: Add support for ARM Performance Monitoring Unit Table. (Mark Langsdorf) [2122316]
- ACPICA: Headers: Replace zero-length array with flexible-array member (Mark Langsdorf) [2122316]
- ACPICA: Removed some tabs and // comments (Mark Langsdorf) [2122316]
- ACPICA: Update copyright notices to the year 2022 (Mark Langsdorf) [2122316]
- ACPICA: Clean up double word in comment (Mark Langsdorf) [2122316]
- ACPICA: Add new ACPI 6.4 semantics for LoadTable() operator (Mark Langsdorf) [2122316]
- ACPICA: Add new ACPI 6.4 semantics to the Load() operator (Mark Langsdorf) [2122316]
- ACPICA: iASL: NHLT: Rename linux specific strucures to device_info (Mark Langsdorf) [2122316]
- ACPICA: iASL: NHLT: Fix parsing undocumented bytes at the end of Endpoint Descriptor (Mark Langsdorf) [2122316]
- ACPICA: iASL: NHLT: Treat Terminator as specific_config (Mark Langsdorf) [2122316]
- ACPICA: Add the subtable CFMWS to the CEDT table (Mark Langsdorf) [2122316]
- ACPICA: Add support for the Windows 11 _OSI string (Mark Langsdorf) [2122316]
- ACPI: sysfs: Fix BERT error region memory mapping (Mark Langsdorf) [2122316]
- ACPI: property: Release subnode properties with data nodes (Mark Langsdorf) [2122316]
- PCI: ACPI: PM: Power up devices in D3cold before scanning them (Mark Langsdorf) [2122316]
- ACPI: PM: Introduce acpi_dev_power_up_children_with_adr() (Mark Langsdorf) [2122316]
- ACPI: bus: Introduce acpi_dev_for_each_child() (Mark Langsdorf) [2122316]
- ACPI: PM: Unify debug messages in acpi_device_set_power() (Mark Langsdorf) [2122316]
- ACPI: PM: Convert debug message in acpi_device_get_power() (Mark Langsdorf) [2122316]
- device property: Add irq_get to fwnode operation (Mark Langsdorf) [2122316]
- device property: Add iomap to fwnode operations (Mark Langsdorf) [2122316]
- ACPI: property: Move acpi_fwnode_device_get_match_data() up (Mark Langsdorf) [2122316]
- device property: Convert device_{dma_supported,get_dma_attr} to fwnode (Mark Langsdorf) [2122316]
- ACPI: Add perf low power callback (Mark Langsdorf) [2122316]
- s390: fix double free of GS and RI CBs on fork() failure (Brian Foster) [1944540]
- wifi: iwlwifi: mvm: fix double list_add at iwl_mvm_mac_wake_tx_queue (other cases) (Jose Ignacio Tornos Martinez) [2086480]
- wifi: iwlwifi: mvm: fix double list_add at iwl_mvm_mac_wake_tx_queue (Jose Ignacio Tornos Martinez) [2086480]

* Mon Oct 17 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-431.el8]
- crypto: ecdh - disallow plain "ecdh" usage in FIPS mode (Vladis Dronov) [2129392]
- crypto: dh - disallow plain "dh" usage in FIPS mode (Vladis Dronov) [2129392]
- x86/cpu: Add new Raptor Lake CPU model number (Prarit Bhargava) [2120361]
- mm, oom: fix missing tlb_finish_mmu() in __oom_reap_task_mm(). (Waiman Long) [2130954]
- net: atlantic: remove aq_nic_deinit() when resume (Íñigo Huguet) [2130839]
- net: atlantic: remove deep parameter on suspend/resume functions (Íñigo Huguet) [2130839]
- efi: Allow EFI_MEMORY_XP and EFI_MEMORY_RO both to be cleared (Lenny Szubowicz) [2128172]
- bonding: 3ad: make ad_ticks_per_sec a const (Jonathan Toppins) [2020773]
- bonding: 802.3ad: fix no transmission of LACPDUs (Jonathan Toppins) [2020773]
- redhat: workaround CKI cross compilation for scripts (Jan Stancek) [2123399]
- nohz/full, sched/rt: Fix missed tick-reenabling bug in dequeue_task_rt() (Phil Auld) [2107238]
- gfs2: Make sure FITRIM minlen is rounded up to fs block size (Andrew Price) [2118256]
- ceph: don't truncate file in atomic_open (Xiubo Li) [2120924]
- of: address: Work around missing device_type property in pcie nodes (Jerry Snitselaar) [2118732]
- dma-mapping: introduce DMA range map, supplanting dma_pfn_offset (Jerry Snitselaar) [2118732]
- of/address: check for invalid range.cpu_addr (Jerry Snitselaar) [2118732]
- of: address: Fix parser address/size cells initialization (Jerry Snitselaar) [2118732]
- of_address: Guard of_bus_pci_get_flags with CONFIG_PCI (Jerry Snitselaar) [2118732]
- of_address: Add bus type match for pci ranges parser (Jerry Snitselaar) [2118732]
- of/address: Support multiple 'dma-ranges' entries (Jerry Snitselaar) [2118732]
- of/address: use range parser for of_dma_get_range (Jerry Snitselaar) [2118732]
- of/address: Rework of_pci_range parsing for non-PCI buses (Jerry Snitselaar) [2118732]
- of: Drop struct of_pci_range.pci_space field (Jerry Snitselaar) [2118732]
- of/address: Move range parser code out of CONFIG_PCI (Jerry Snitselaar) [2118732]
- of: Make of_dma_get_range() work on bus nodes (Jerry Snitselaar) [2118732]
- Revert "arm64: dts: juno: add dma-ranges property" (Jerry Snitselaar) [2118732]
- of/address: Fix of_pci_range_parser_one translation of DMA addresses (Jerry Snitselaar) [2118732]
- of/address: Translate 'dma-ranges' for parent nodes missing 'dma-ranges' (Jerry Snitselaar) [2118732]
- of: address: Follow DMA parent for "dma-coherent" (Jerry Snitselaar) [2118732]
- of: Factor out #{addr,size}-cells parsing (Jerry Snitselaar) [2118732]
- of/address: Introduce of_get_next_dma_parent() helper (Jerry Snitselaar) [2118732]
- of: address: Report of_dma_get_range() errors meaningfully (Jerry Snitselaar) [2118732]
- of: address: Add support for the parent DMA bus (Jerry Snitselaar) [2118732]
- of: address: Retrieve a parent through a callback in __of_translate_address (Jerry Snitselaar) [2118732]
- of: reserved_mem: fix reserve memory leak (Jerry Snitselaar) [2118732]
- of: Use device_type helpers to access the node type (Jerry Snitselaar) [2118732]
- of: make PowerMac cache node search conditional on CONFIG_PPC_PMAC (Jerry Snitselaar) [2118732]

* Fri Oct 07 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-430.el8]
- crypto: qat - add limit to linked list parsing (Vladis Dronov) [2129897]
- crypto: qat - use reference to structure in dma_map_single() (Vladis Dronov) [2129897]
- Revert "crypto: qat - reduce size of mapped region" (Vladis Dronov) [2129897]
- crypto: qat - fix DMA transfer direction (Vladis Dronov) [2129897]
- crypto: qat - fix default value of WDT timer (Vladis Dronov) [2129897]
- crypto: drivers - move from strlcpy with unused retval to strscpy (Vladis Dronov) [2129897]
- crypto: qat - add check to validate firmware images (Vladis Dronov) [2129897]
- Documentation: qat: rewrite description (Vladis Dronov) [2129897]
- Documentation: qat: Use code block for qat sysfs example (Vladis Dronov) [2129897]
- KVM: x86: Inject #UD on emulated XSETBV if XSAVES isn't enabled (Dr. David Alan Gilbert) [2079311]
- KVM: x86: Always enable legacy FP/SSE in allowed user XFEATURES (Dr. David Alan Gilbert) [2079311]
- KVM: x86: Reinstate kvm_vcpu_arch.guest_supported_xcr0 (Dr. David Alan Gilbert) [2079311]
- bonding: fix NULL deref in bond_rr_gen_slave_id (Jonathan Toppins) [2051778]
- tty: use new tty_insert_flip_string_and_push_buffer() in pty_write() (Rafael Aquini) [2078869] {CVE-2022-1462}
- tty: extract tty_flip_buffer_commit() from tty_flip_buffer_push() (Rafael Aquini) [2078869] {CVE-2022-1462}
- tty: drop tty_schedule_flip() (Rafael Aquini) [2078869] {CVE-2022-1462}
- tty: the rest, stop using tty_schedule_flip() (Rafael Aquini) [2078869] {CVE-2022-1462}
- tty: drivers/tty/, stop using tty_schedule_flip() (Rafael Aquini) [2078869] {CVE-2022-1462}
- vt: keyboard, use tty_insert_flip_string in puts_queue (Rafael Aquini) [2078869] {CVE-2022-1462}
- vt: use tty_insert_flip_string in respond_string (Rafael Aquini) [2078869] {CVE-2022-1462}

* Mon Oct 03 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-429.el8]
- intel_th: pci: Add Raptor Lake-S CPU support (Michael Petlan) [2040035]
- intel_th: pci: Add Raptor Lake-S PCH support (Michael Petlan) [2040035]
- virtio-net: support XDP when not more queues (Eugenio Pérez) [2122225]
- virtio_net: Don't process redirected XDP frames when XDP is disabled (Eugenio Pérez) [2122225]
- virtio_net: Fix not restoring real_num_rx_queues (Eugenio Pérez) [2122225]
- x86,config: Enable straight-line-speculation fix (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- x86/alternative: Relax text_poke_bp() constraint (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- perf/x86: Add support for perf text poke event for text_poke_bp_batch() callers (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- objtool: Add straight-line-speculation validation (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- objtool: Support conditional retpolines (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- objtool: Refactor sibling call detection logic (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- objtool: Change dead_end_function() to return boolean (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- x86/lib/atomic64_386_32: Rename things (Wander Lairson Costa) [2062175] {CVE-2021-26341}
- KVM: arm64: Fix debug architecture version (Gavin Shan) [2123587]
- thunderbolt: Add support for Intel Raptor Lake (Torez Smith) [2040037]
- iommu/vt-d: Fix compile error with CONFIG_PCI_ATS not set (Myron Stowe) [2118428 2122515 2127028]
- iommu/vt-d: Cure VF irqdomain hickup (Myron Stowe) [2118428 2122515 2127028]
- x86/pci: Set default irq domain in pcibios_add_device() (Myron Stowe) [2118428 2122515 2127028]
- iommm/amd: Store irq domain in struct device (Myron Stowe) [2118428 2122515 2127028]
- iommm/vt-d: Store irq domain in struct device (Myron Stowe) [2118428 2122515 2127028]
- PCI/MSI: Provide pci_dev_has_special_msi_domain() helper (Myron Stowe) [2118428 2122515 2127028]
- x86/msi: Consolidate MSI allocation (Myron Stowe) [2118428 2122515 2127028]
- PCI/MSI: Rework pci_msi_domain_calc_hwirq() (Myron Stowe) [2118428 2122515 2127028]
- x86/irq: Consolidate UV domain allocation (Myron Stowe) [2118428 2122515 2127028]
- x86/irq: Consolidate DMAR irq allocation (Myron Stowe) [2118428 2122515 2127028]
- x86_ioapic_Consolidate_IOAPIC_allocation (Myron Stowe) [2118428 2122515 2127028]
- x86/msi: Consolidate HPET allocation (Myron Stowe) [2118428 2122515 2127028]
- iommu/irq_remapping: Consolidate irq domain lookup (Myron Stowe) [2118428 2122515 2127028]
- iommu/amd: Consolidate irq domain getter (Myron Stowe) [2118428 2122515 2127028]
- iommu/vt-d: Consolidate irq domain getter (Myron Stowe) [2118428 2122515 2127028]
- x86/irq: Add allocation type for parent domain retrieval (Myron Stowe) [2118428 2122515 2127028]
- irqdomain: Export irq_domain_update_bus_token (Myron Stowe) [2118428 2122515 2127028]
- perf/x86/intel: Update the FRONTEND MSR mask on Sapphire Rapids (Michael Petlan) [2125349]
- perf/x86/intel/uncore: Fix invalid unit check (Michael Petlan) [2125349]

* Tue Sep 27 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-428.el8]
- KVM: s390: pv: don't present the ecall interrupt twice (Tobias Huschle) [2125236]
- s390/mm: do not trigger write fault when vma does not allow VM_WRITE (Tobias Huschle) [2125218]
- PCI: Print a debug message on PCI device release (Tobias Huschle) [2125216]
- s390/pci: fix leak of PCI device structure (Tobias Huschle) [2125216]
- s390/pci: refactor zpci_create_device() (Tobias Huschle) [2125216]
- s390/pci: remove superfluous zdev->zbus check (Tobias Huschle) [2125216]
- x86/boot/64: Add missing fixup_pointer() for next_early_pgt access (Rafael Aquini) [2082806]
- x86/boot/64: Fix crash if kernel image crosses page table boundary (Rafael Aquini) [2082806]
- mm/slab_common: fix possible double free of kmem_cache (Waiman Long) [2093781]
- mm/slab_common: Deleting kobject in kmem_cache_destroy() without holding slab_mutex/cpu_hotplug_lock (Waiman Long) [2093781]
- mm/slab_common: use WARN() if cache still has objects on destroy (Waiman Long) [2093781]
- slab: use __func__ to trace function name (Waiman Long) [2093781]
- s390/hugetlb: fix prepare_hugepage_range() check for 2 GB hugepages (Tobias Huschle) [2125215]
- platform/x86: intel/pmc: Add Alder Lake N support to PMC core driver (Prarit Bhargava) [2072654]
- crash_core: Increase crashkernel=auto size for x86_64, s390 and arm64 (Lichen Liu) [2122874]
- virtio-net: fix use-after-free in skb_gro_receive (Cindy Lu) [2069047]
- virtio-net: fix use-after-free in page_to_skb() (Cindy Lu) [2069047]
- virtio-net: restrict build_skb() use to some arches (Cindy Lu) [2069047]
- virtio-net: page_to_skb() use build_skb when there's sufficient tailroom (Cindy Lu) [2069047]
- sched/fair: Consider CPU affinity when allowing NUMA imbalance in find_idlest_group() (Phil Auld) [2110020]
- sched/numa: Adjust imb_numa_nr to a better approximation of memory channels (Phil Auld) [2110020]
- sched/numa: Apply imbalance limitations consistently (Phil Auld) [2110020]
- sched/numa: Do not swap tasks between nodes when spare capacity is available (Phil Auld) [2110020]
- sched/numa: Initialise numa_migrate_retry (Phil Auld) [2110020]
- cpufreq: intel_pstate: Handle no_turbo in frequency invariance (Phil Auld) [2100594]
- sched/fair: Introduce SIS_UTIL to search idle CPU based on sum of util_avg (Phil Auld) [2100594]
- i2c: piix4: Fix a memory leak in the EFCH MMIO support (Sudheesh Mavila) [2105160]
- assoc_array: Fix BUG_ON during garbage collect (Dave Wysochanski) [1920523]
- wait: Fix __wait_event_hrtimeout for RT/DL tasks (Derek Barbosa) [2125233]

* Wed Sep 21 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-427.el8]
- raid1: ensure write behind bio has less than BIO_MAX_VECS sectors (Nigel Croxon) [2116209]
- ceph: fix statfs for subdir mounts (Xiubo Li) [2120943]
- ceph: try to queue a writeback if revoking fails (Xiubo Li) [2120940]
- ceph: update the auth cap when the async create req is forwarded (Xiubo Li) [2120932]
- ceph: make change_auth_cap_ses a global symbol (Xiubo Li) [2120932]
- fs/dcache: export d_same_name() helper (Xiubo Li) [2120932]
- ceph: wait for the first reply of inflight async unlink (Xiubo Li) [2120932]
- redhat: Enable KASAN_VMALLOC (Nico Pache) [2108620]
- arm64: select KASAN_VMALLOC for SW/HW_TAGS modes (Nico Pache) [2108620]
- x86/crash: Fix crash_setup_memmap_entries() out-of-bounds access (Nico Pache) [2108620]
- mm: defer kmemleak object creation of module_alloc() (Nico Pache) [2108620]
- arm64: kaslr: keep modules inside module region when KASAN is enabled (Nico Pache) [2108620]
- kasan: arm64: fix pcpu_page_first_chunk crash with KASAN_VMALLOC (Nico Pache) [2108620]
- arm64: Kconfig: select KASAN_VMALLOC if KANSAN_GENERIC is enabled (Nico Pache) [2108620]
- arm64: kaslr: support randomized module area with KASAN_VMALLOC (Nico Pache) [2108620]
- arm64: Kconfig: support CONFIG_KASAN_VMALLOC (Nico Pache) [2108620]
- arm64: kasan: abstract _text and _end to KERNEL_START/END (Nico Pache) [2108620]
- arm64: kasan: don't populate vmalloc area for CONFIG_KASAN_VMALLOC (Nico Pache) [2108620]
- x86/kasan: support KASAN_VMALLOC (Nico Pache) [2108620]
- ath9k: htc: clean up statistics macros (Jose Ignacio Tornos Martinez) [2084598] {CVE-2022-1679}
- ath9k: hif_usb: simplify if-if to if-else (Jose Ignacio Tornos Martinez) [2084598] {CVE-2022-1679}
- ath9k: fix use-after-free in ath9k_hif_usb_rx_cb (Jose Ignacio Tornos Martinez) [2084598] {CVE-2022-1679}
- igmp: Add ip_mc_list lock in ip_check_mc_rcu (Hangbin Liu) [2114946] {CVE-2022-20141}
- scsi: zfcp: Fix missing auto port scan and thus missing target ports (Tobias Huschle) [2121089]
- vfio/type1: Unpin zero pages (Alex Williamson) [2123015]

* Wed Sep 14 2022 Lucas Zampieri <lzampier@redhat.com> [4.18.0-426.el8]
- iommu/vt-d: Make DMAR_UNITS_SUPPORTED default 1024 (Jerry Snitselaar) [2120412]
- Revert "iommu/vt-d: Make DMAR_UNITS_SUPPORTED a config setting" (Jerry Snitselaar) [2120412]
- ptrace: Check PTRACE_O_SUSPEND_SECCOMP permission on PTRACE_SEIZE (Oleg Nesterov) [2121269] {CVE-2022-30594}
- redhat: remove unused STAMP variable from genspec.sh (Herton R. Krzesinski)
- internal: Update RHEL_MINOR for the start of RHEL-8.8 development (Lucas Zampieri)