From 9a0a14abbb7b9e6e28056b9f80f759df76048ea1 Mon Sep 17 00:00:00 2001
From: Eng33 <eng33@waveshare.net>
Date: Fri, 8 Mar 2024 18:37:03 +0800
Subject: [PATCH 0953/1085] Dtoverlay:add waveshare 4inch dsi lcd (C) dtoverlay

Signed-off-by: Eng33 <eng33@waveshare.net>
---
 .../boot/dts/overlays/vc4-kms-dsi-waveshare-panel-overlay.dts  | 3 +++
 1 file changed, 3 insertions(+)

--- a/arch/arm/boot/dts/overlays/vc4-kms-dsi-waveshare-panel-overlay.dts
+++ b/arch/arm/boot/dts/overlays/vc4-kms-dsi-waveshare-panel-overlay.dts
@@ -112,6 +112,9 @@
 				   <&touch>, "touchscreen-size-y:0=1480",
 				   <&touch>, "touchscreen-inverted-x?",
 				   <&touch>, "touchscreen-swapped-x-y?";
+		4_0_inchC = <&panel>, "compatible=waveshare,4inch-panel",
+				   <&touch>, "touchscreen-size-x:0=720",
+				   <&touch>, "touchscreen-size-y:0=720";
 		i2c1 = <&i2c_frag>, "target:0=",<&i2c1>,
 		       <0>, "-3-4+5";
 		disable_touch = <&touch>, "status=disabled";
