* Mon May 27 2019 Fabian Arrotin <arrfab@centos.org> - 4.18.9-80.el8
- Rolled in CentOS secureboot cert
- Debranding patches

* Tue May 07 2019 CentOS Sources <bugs@centos.org> - 4.18.0-80.el8.centos
- Apply debranding changes

* Wed Mar 13 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-80.el8]
- [arm64] revert "arm64: tlb: Avoid synchronous TLBIs when freeing page tables" (Christoph von Recklinghausen) [1685697]

* Mon Mar 11 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-79.el8]
- [firmware] drivers/firmware: psci_checker: stash and use topology_core_cpumask for hotplug tests (Josh Poimboeuf) [1687101]
- [arm64] arm64: topology: re-introduce numa mask check for scheduler MC selection (Josh Poimboeuf) [1687101]
- [arm64] arm64: topology: rename llc_siblings to align with other struct members (Josh Poimboeuf) [1687101]
- [arm64] arm64: smp: remove cpu and numa topology information when hotplugging out CPU (Josh Poimboeuf) [1687101]
- [arm64] arm64: topology: restrict updating siblings_masks to online cpus only (Josh Poimboeuf) [1687101]
- [arm64] arm64: topology: add support to remove cpu topology sibling masks (Josh Poimboeuf) [1687101]
- [arm64] arm64: numa: separate out updates to percpu nodeid and NUMA node cpumap (Josh Poimboeuf) [1687101]
- [arm64] arm64: topology: refactor reset_cpu_topology to add support for removing topology (Josh Poimboeuf) [1687101]

* Sun Mar 10 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-78.el8]
- [fs] gfs2: Fix missed wakeups in find_insert_glock (Andreas Grunbacher) [1678907]

* Thu Mar 07 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-77.el8]
- [firmware] efi: Reduce the amount of memblock reservations for persistent allocations (Bhupesh Sharma) [1682988]
- [firmware] efi: Permit multiple entries in persistent memreserve data structure (Bhupesh Sharma) [1682988]
- [kernel] cpu/hotplug: Create SMT sysfs interface for all arches (Josh Poimboeuf) [1686068]
- [net] netfilter: nft_set_hash: bogus element self comparison from deactivation path (Florian Westphal) [1678574]
- [net] netfilter: nft_set_hash: fix lookups with fixed size hash on big endian (Florian Westphal) [1678574]

* Tue Mar 05 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-76.el8]
- [security] revert "Add a SysRq option to lift kernel lockdown" (Lenny Szubowicz) [1684348]
- [s390] s390/setup: fix boot crash for machine without EDAT-1 (Philipp Rudo) [1677357]
- [s390] s390/setup: fix early warning messages (Philipp Rudo) [1677357]

* Fri Mar 01 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-75.el8]
- [netdrv] net: hns3: add 8 BD limit for tx flow (Xiaojun Tan) [1676771]
- [netdrv] net: hns3: fix a SSU buffer checking bug (Xiaojun Tan) [1676771]
- [netdrv] net: hns3: aligning buffer size in SSU to 256 bytes (Xiaojun Tan) [1676771]
- [netdrv] net: hns3: getting tx and dv buffer size through firmware (Xiaojun Tan) [1676771]
- [net] netfilter: nf_nat_snmp_basic: add missing length checks in ASN.1 cbs (Florian Westphal) [1676602]
- [char] ipmi: fix use-after-free of user->release_barrier.rda (Xiaojun Tan) [1677550]
- [char] ipmi: Prevent use-after-free in deliver_response (Xiaojun Tan) [1677550]

* Wed Feb 27 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-74.el8]
- [x86] revert "cpu/hotplug: Add SMT policy options" (Josh Poimboeuf) [1683690]
- [crypto] net: crypto set sk to NULL when af_alg_release (Neil Horman) [1679450] {CVE-2019-8912}
- [drm] drm/i915/gvt: update force-to-nonpriv register whitelist (Paul Lai) [1643972]
- [kernel] MODSIGN: Also check platform keyring in mod_verify_sig() (Lenny Szubowicz) [1568532]
- [kernel] Fix for module sig verification (Lenny Szubowicz) [1568532]
- [security] efi: Lock down the kernel if booted in secure boot mode (Lenny Szubowicz) [1568532]
- [firmware] efi: Add an EFI_SECURE_BOOT flag to indicate secure boot mode (Lenny Szubowicz) [1568532]
- [x86] Copy secure_boot flag in boot params across kexec reboot (Lenny Szubowicz) [1568532]
- [fs] debugfs: Restrict debugfs when the kernel is locked down (Lenny Szubowicz) [1568532]
- [mm] x86/mmiotrace: Lock down the testmmiotrace module (Lenny Szubowicz) [1568532]
- [kernel] Lock down module params that specify hardware parameters (eg. ioport) (Lenny Szubowicz) [1568532]
- [tty] Lock down TIOCSSERIAL (Lenny Szubowicz) [1568532]
- [pcmcia] Prohibit PCMCIA CIS storage when the kernel is locked down (Lenny Szubowicz) [1568532]
- [acpi] acpi: Disable ACPI table override if the kernel is locked down (Lenny Szubowicz) [1568532]
- [acpi] acpi: Ignore acpi_rsdp kernel param when the kernel has been locked down (Lenny Szubowicz) [1568532]
- [acpi] ACPI: Limit access to custom_method when the kernel is locked down (Lenny Szubowicz) [1568532]
- [x86] x86/msr: Restrict MSR access when the kernel is locked down (Lenny Szubowicz) [1568532]
- [x86] x86: Lock down IO port access when the kernel is locked down (Lenny Szubowicz) [1568532]
- [pci] PCI: Lock down BAR access when the kernel is locked down (Lenny Szubowicz) [1568532]
- [kernel] uswsusp: Disable when the kernel is locked down (Lenny Szubowicz) [1568532]
- [kernel] hibernate: Disable when the kernel is locked down (Lenny Szubowicz) [1568532]
- [kernel] kexec_load: Disable at runtime if the kernel is locked down (Lenny Szubowicz) [1568532]
- [char] Restrict /dev/{mem, kmem, port} when the kernel is locked down (Lenny Szubowicz) [1568532]
- [kernel] MODSIGN: Enforce module signatures if the kernel is locked down (Lenny Szubowicz) [1568532]
- [security] Add a SysRq option to lift kernel lockdown (Lenny Szubowicz) [1568532]
- [security] Add the ability to lock down access to the running kernel image (Lenny Szubowicz) [1568532]

* Tue Feb 26 2019 Frantisek Hrbata <fhrbata@redhat.com> [4.18.0-73.el8]
- [net] tun: forbid iface creation with rtnl ops (Sabrina Dubroca) [1680969]
- [net] revert "bridge: do not add port to router list when receives query with source 0.0.0.0" (Hangbin Liu) [1679896]
- [net] sctp: walk the list of asoc safely (Marcelo Leitner) [1679920] {CVE-2019-8956}
- [net] netfilter: nf_nat: skip nat clash resolution for same-origin entries (Florian Westphal) [1677647]
- [net] netfilter: nf_conntrack: resolve clash for matching conntracks (Florian Westphal) [1677647]
- [net] netfilter: nf_tables: fix flush after rule deletion in the same batch (Phil Sutter) [1677672]
- [net] gro_cell: add napi_disable in gro_cells_destroy (Stefano Brivio) [1674408]
- [net] sctp: call gso_reset_checksum when computing checksum in sctp_gso_segment (Xin Long) [1669386]
- [net] ipvs: fix dependency on nf_defrag_ipv6 (Andrea Claudi) [1660808]
- [net] sctp: check and update stream->out_curr when allocating stream_out (Xin Long) [1651877]

* Mon Feb 25 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-72.el8]
- [x86] cpu/hotplug: Add SMT policy options (Josh Poimboeuf) [1677405]

* Fri Feb 22 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-71.el8]
- [pci] pci/quirks: Add quirk to reset nvgpu at boot for the Lenovo ThinkPad P50 (Lyude Paul) [1677022]
- [arm64] arm64, vmcoreinfo : Append 'MAX_USER_VA_BITS' to vmcoreinfo (Bhupesh Sharma) [1672962]
- [md] dm thin: fix bug where bio that overwrites thin block ignores FUA (Mike Snitzer) [1679211]
- [pci] PCI: Fix "try" semantics of bus and slot reset (Myron Stowe) [1662901]
- [acpi] acpi/nfit: Fix bus command validation (Jeff Moyer) [1673958]
- [pci] PCI/MSI: Return -ENOSPC from pci_alloc_irq_vectors_affinity() (Myron Stowe) [1667773]
- [fs] NFS: Don't use page_file_mapping after removing the page (Benjamin Coddington) [1664190]
- [fs] NFS: Fix up return value on fatal errors in nfs_page_async_flush() (Benjamin Coddington) [1664190]
- [md] md: fix raid10 hang issue caused by barrier (Xiao Ni) [1630921]
- [md] md/raid1: don't clear bitmap bits on interrupted recovery. (Xiao Ni) [1677360]
- [virt] kvm: fix kvm_ioctl_create_device() reference counting (CVE-2019-6974) (Paolo Bonzini) [1673843] {CVE-2019-6974}
- [block] blk-mq: fix a hung issue when fsync (Ming Lei) [1674399]
- [block] Revert "block: cover another queue enter recursion via BIO_QUEUE_ENTERED" (Ming Lei) [1673966]
- [tools] perf tools: Check for null when copying nsinfo. (Jiri Olsa) [1676451]
- [iommu] iommu/amd: Fix IOMMU page flush when detach device from a domain (Suravee Suthikulpanit) [1672476]

* Tue Feb 19 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-70.el8]
- [kernel] namespace: Add padding fix to user_table[] (Prarit Bhargava) [1677103]
- [x86] KVM: nVMX: unconditionally cancel preemption timer in free_nested (CVE-2019-7221) (Paolo Bonzini) [1673841] {CVE-2019-7221}
- [scsi] scsi: sd: fix entropy gathering for most rotational disks (Ewan Milne) [1676735]
- [scsi] scsi: sd: Contribute to randomness when running rotational device (Ewan Milne) [1676735]
- [rpmspec] Revert "Drop -doc subpackage" (Prarit Bhargava) [1657609]
- [net] svcrdma: Remove max_sge check at connect time (Don Dutile) [1638869]
- [net] svcrdma: Reduce max_send_sges (Don Dutile) [1638869]
- [arm64] arm64: mm: Introduce MAX_USER_VA_BITS definition (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlb: Rewrite stale comment in asm/tlbflush.h (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlb: Avoid synchronous TLBIs when freeing page tables (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlb: Remove redundant !CONFIG_HAVE_RCU_TABLE_FREE code (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlbflush: Allow stride to be specified for __flush_tlb_range() (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlb: Justify non-leaf invalidation in flush_tlb_range() (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlb: Add DSB ISHST prior to TLBI in __flush_tlb_[kernel_]pgtable() (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlb: Use last-level invalidation in flush_tlb_kernel_range() (Christoph von Recklinghausen) [1672997]
- [mm] arm64: mm: EXPORT vabits_user to modules (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: fix ARM64_USER_VA_BITS_52 builds (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: Kconfig: Re-jig CONFIG options for 52-bit VA (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: mm: Allow forcing all userspace addresses to 52-bit (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: mm: introduce 52-bit userspace support (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: mm: Prevent mismatched 52-bit VA support (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: mm: Offset TTBR1 to allow 52-bit PTRS_PER_PGD (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: mm: Define arch_get_mmap_end, arch_get_mmap_base (Christoph von Recklinghausen) [1672997]
- [firmware] arm64: mm: Introduce DEFAULT_MAP_WINDOW (Christoph von Recklinghausen) [1672997]
- [mm] mm: mmap: Allow for "high" userspace addresses (Christoph von Recklinghausen) [1672997]
- [mm] arm64: mm: apply r/o permissions of VM areas to its linear alias as well (Christoph von Recklinghausen) [1672997]
- [mm] arm64: mm: purge lazily unmapped vm regions before changing permissions (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: mm: Don't wait for completion of TLB invalidation when page aging (Christoph von Recklinghausen) [1672997]
- [mm] arm64: mm: Use __pa_symbol() for set_swapper_pgd() (Christoph von Recklinghausen) [1672997]
- [mm] arm64: mm: Drop the unused cpu parameter (Christoph von Recklinghausen) [1672997]
- [arm64] arm64/mm: move runtime pgds to rodata (Christoph von Recklinghausen) [1672997]
- [mm] arm64/mm: use fixmap to modify swapper_pg_dir (Christoph von Recklinghausen) [1672997]
- [arm64] arm64/mm: Separate boot-time page tables from swapper_pg_dir (Christoph von Recklinghausen) [1672997]
- [arm64] arm64/mm: Pass ttbr1 as a parameter to __enable_mmu() (Christoph von Recklinghausen) [1672997]
- [mm] arm64: fix erroneous warnings in page freeing functions (Christoph von Recklinghausen) [1672997]
- [mm] arm64: Implement page table free interfaces (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: tlbflush: Introduce __flush_tlb_kernel_pgtable (Christoph von Recklinghausen) [1672997]
- [lib] ioremap: Update pgtable free interfaces with addr (Christoph von Recklinghausen) [1672997]
- [mm] x86/mm: Disable ioremap free page handling on x86-PAE (Christoph von Recklinghausen) [1672997]
- [arm64] arm64: KVM: Enable Common Not Private translations (Christoph von Recklinghausen) [1504991]
- [arm64] arm64: mm: Support Common Not Private translations (Christoph von Recklinghausen) [1504991]
- [kernel] cpu/hotplug: Fix "SMT disabled by BIOS" detection for KVM (Igor Mammedov) [1668147]
- [tools] perf tools: Compile perf with -g instead of -ggdb3 to workaround gdb crash (Jiri Olsa) [1667109]

* Thu Feb 14 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-69.el8]
- [fs] Revert "gfs2: Fix loop in gfs2_rbm_find" (Andreas Grunbacher) [1658528]
- [net] bpf: fix sanitation of alu op with pointer / scalar type from different paths (Jiri Olsa) [1673631] {CVE-2019-7308}
- [net] bpf: prevent out of bounds speculation on pointer arithmetic (Jiri Olsa) [1673631] {CVE-2019-7308}
- [net] bpf: move {prev_,}insn_idx into verifier env (Jiri Olsa) [1673631] {CVE-2019-7308}
- [net] bpf/verifier: per-register parent pointers (Jiri Olsa) [1673631] {CVE-2019-7308}
- [net] bpf: restrict unknown scalars of mixed signed bounds for unprivileged (Jiri Olsa) [1673631] {CVE-2019-7308}
- [net] bpf: Simplify ptr_min_max_vals adjustment (Jiri Olsa) [1673631] {CVE-2019-7308}
- [net] bpf: fix inner map masking to prevent oob under speculation (Jiri Olsa) [1673631] {CVE-2019-7308}
- [include] KABI: struct class padding (Prarit Bhargava) [1670035]
- [include] KABI: struct timer_list padding (Prarit Bhargava) [1670035]
- [include] KABI: struct irq_domain padding (Prarit Bhargava) [1670035]
- [nvdimm] libnvdimm, pmem: Fix badblocks population for 'raw' namespaces (Jeff Moyer) [1672315]
- [netdrv] net/mlx5e: FPGA, fix Innova IPsec TX offload data path performance (Alaa Hleihel) [1648230]
- [kernel] exec: increase BINPRM_BUF_SIZE to 256 (Oleg Nesterov) [1447445]

* Wed Feb 13 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-68.el8]
- [include] KABI: struct kset padding (Prarit Bhargava) [1669796]
- [include] KABI: struct kobject and kobj_type padding (Prarit Bhargava) [1669796]
- [include] KABI: struct delayed_work padding (Prarit Bhargava) [1669796]
- [include] KABI: struct work_struct padding (Prarit Bhargava) [1669796]
- [include] KABI: struct hrtimer padding (Prarit Bhargava) [1669796]
- [include] KABI: struct user_namespace padding (Prarit Bhargava) [1669796]
- [include] KABI: struct resource padding (Prarit Bhargava) [1669796]
- [include] KABI: Protect device_driver struct (Prarit Bhargava) [1666316]
- [include] KABI: Protect radix functions (Prarit Bhargava) [1669079]
- [char] ipmi: msghandler: Fix potential Spectre v1 vulnerabilities (Tony Camuso) [1672582]
- [vhost] vhost: fix OOB in get_rx_bufs() (Jason Wang) [1668665] {CVE-2018-16880}

* Sat Feb 09 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-67.el8]
- [md] dm: don't use bio_trim() afterall (Mike Snitzer) [1673657]
- [md] dm: add memory barrier before waitqueue_active (Mike Snitzer) [1673110]
- [x86] x86: uaccess: Inhibit speculation past access_ok() in user_access_begin() (Joe Lawrence) [1670113] {CVE-2018-20669}
- [kernel] make 'user_access_begin()' do 'access_ok()' (Joe Lawrence) [1670113] {CVE-2018-20669}
- [drm] i915: fix missing user_access_end() in page fault exception case (Joe Lawrence) [1670113] {CVE-2018-20669}
- [drm] drm/i915: Force the slow path after a user-write error (Joe Lawrence) [1670113] {CVE-2018-20669}
- [x86] x86/microcode/amd: Don't falsely trick the late loading mechanism (David Arcari) [1654904]
- [fs] iomap: get/put the page in iomap_page_create/release() (Artem Savkov) [1664298]
- [scsi] scsi: qla2xxx: Add new FC-NVMe enable BIT to enable FC-NVMe feature (Himanshu Madhani) [1671569]
- [message] mptsas: pci-id table changes (Tomas Henzl) [1666730]
- [message] mptsas: Taint kernel if mptsas is loaded (Tomas Henzl) [1666730]
- [kernel] genirq/matrix: Improve target CPU selection for managed interrupts. (Gary Hook) [1669557]
- [kernel] irq/matrix: Spread managed interrupts on allocation (Gary Hook) [1669557]
- [kernel] irq/matrix: Split out the CPU selection code into a helper (Gary Hook) [1669557]
- [net] sit: check if IPv6 enabled before calling ip6_err_gen_icmpv6_unreach() (Stefano Brivio) [1671680]
- [net] geneve: should not call rt6_lookup() when ipv6 was disabled (Stefano Brivio) [1671680]
- [net] netfilter: physdev: relax br_netfilter dependency (Phil Sutter) [1650382]
- [net] netfilter: nf_tables: add NFTA_RULE_POSITION_ID to nla_policy (Phil Sutter) [1670563]
- [net] netfilter: nf_tables: Support RULE_ID reference in new rule (Phil Sutter) [1670563]
- [net] rtnetlink: fix incorrect handling of device stats passed to userspace (Ivan Vecera) [1668298]
- [net] netfilter: nf_tables: handle nft_object lookups via rhltable (Phil Sutter) [1659725]
- [net] netfilter: nf_tables: prepare nft_object for lookups via hashtable (Phil Sutter) [1659725]
- [net] netfilter: nf_tables: selective rule dump needs table to be specified (Phil Sutter) [1659725]
- [net] netfilter: nf_tables: Fix for endless loop when dumping ruleset (Phil Sutter) [1659725]
- [net] netfilter: nf_tables: Speed up selective rule dumps (Phil Sutter) [1659725]
- [net] exclude sock_reuseport from kABI protection (Paolo Abeni) [1665984]
- [include] KABI: struct device padding (Don Dutile) [1664445]
- [include] KABI: struct dma_map_ops padding (Don Dutile) [1664482]
- [kernel] swiotlb: clear io_tlb_start and io_tlb_end in swiotlb_exit (Don Dutile) [1664484]
- [kernel] dma-mapping: remove a few unused exports (Don Dutile) [1664484]
- [include] dma-mapping: properly stub out the DMA API for !CONFIG_HAS_DMA (Don Dutile) [1664484]
- [kernel] dma-mapping: remove dmam_{declare,release}_coherent_memory (Don Dutile) [1664484]
- [kernel] dma-mapping: implement dmam_alloc_coherent using dmam_alloc_attrs (Don Dutile) [1664484]
- [include] dma-mapping: implement dma_map_single_attrs using dma_map_page_attrs (Don Dutile) [1664484]
- [include] dma-mapping: fix flags in dma_alloc_wc (Don Dutile) [1664484]
- [include] dma-mapping: deprecate dma_zalloc_coherent (Don Dutile) [1664484]
- [arm64] arm64: default to the direct mapping in get_arch_dma_ops (Don Dutile) [1664484]
- [kernel] dma-mapping: fix inverted logic in dma_supported (Don Dutile) [1664484]
- [include] dma-mapping: bypass indirect calls for dma-direct (Don Dutile) [1664484]
- [kernel] dma-direct: merge swiotlb_dma_ops into the dma_direct code (Don Dutile) [1664484]
- [kernel] dma-direct: do not include SME mask in the DMA supported check (Don Dutile) [1664484]
- [kernel] dma-direct: use dma_direct_map_page to implement dma_direct_map_sg (Don Dutile) [1664484]
- [kernel] dma-direct: improve addressability error reporting (Don Dutile) [1664484]
- [kernel] dma-direct: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [xen] swiotlb: remove dma_mark_clean (Don Dutile) [1664484]
- [xen] swiotlb: remove SWIOTLB_MAP_ERROR (Don Dutile) [1664484]
- [xen] xen-swiotlb: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [kernel] swiotlb: Skip cache maintenance on map error (Don Dutile) [1664484]
- [kernel] swiotlb: add support for non-coherent DMA (Don Dutile) [1664484]
- [kernel] swiotlb: mark is_swiotlb_buffer static (Don Dutile) [1664484]
- [kernel] swiotlb: remove a pointless comment (Don Dutile) [1664484]
- [kernel] swiotlb: clean up reporting (Don Dutile) [1664484]
- [kernel] dma-direct: reject highmem pages from dma_alloc_from_contiguous (Don Dutile) [1664484]
- [kernel] dma-direct: provide page based alloc/free helpers (Don Dutile) [1664484]
- [include] dma-direct: Make DIRECT_MAPPING_ERROR viable for SWIOTLB (Don Dutile) [1664484]
- [kernel] dma-direct: respect DMA_ATTR_NO_WARN (Don Dutile) [1664484]
- [kernel] dma-direct: document the zone selection logic (Don Dutile) [1664484]
- [kernel] dma-direct: fix return value of dma_direct_supported (Don Dutile) [1664484]
- [kernel] dma-direct: always allow dma mask <= physiscal memory size (Don Dutile) [1664484]
- [kernel] dma-direct: implement complete bus_dma_mask handling (Don Dutile) [1664484]
- [kernel] dma-direct: refine dma_direct_alloc zone selection (Don Dutile) [1664484]
- [kernel] dma-direct: add an explicit dma_direct_get_required_mask (Don Dutile) [1664484]
- [kernel] kernel/dma/direct: take DMA offset into account in dma_direct_supported (Don Dutile) [1664484]
- [kernel] dma-mapping: factor out dummy DMA ops (Don Dutile) [1664484]
- [mm] arm64: dma-mapping: Fix FORCE_CONTIGUOUS buffer clearing (Don Dutile) [1664484]
- [iommu] iommu/dma-iommu: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [iommu] iommu/vt-d: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [iommu] iommu/intel: small map_page cleanup (Don Dutile) [1664484]
- [iommu] intel-iommu: mark intel_dma_ops static (Don Dutile) [1664484]
- [iommu] ia64: remove iommu_dma_supported (Don Dutile) [1664484]
- [iommu] iommu: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [iommu] iommu/dma: Use fast DMA domain lookup (Don Dutile) [1664484]
- [x86] x86/amd_gart: fix unmapping of non-GART mappings (Don Dutile) [1664484]
- [x86] x86/amd_gart: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [mm] arm64: remove the dummy_dma_ops mapping_error method (Don Dutile) [1664484]
- [powerpc] powerpc: Do not redefine NEED_DMA_MAP_STATE (Don Dutile) [1664484]
- [powerpc] powerpc/iommu: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [s390] s390: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [kernel] dma-mapping: always build the direct mapping code (Don Dutile) [1664484]
- [kernel] dma-mapping: move dma_cache_sync out of line (Don Dutile) [1664484]
- [kernel] dma-mapping: move various slow path functions out of line (Don Dutile) [1664484]
- [base] dma-mapping: move dma_get_required_mask to kernel/dma (Don Dutile) [1664484]
- [base] dma-mapping: move dma_default_get_required_mask under ifdef (Don Dutile) [1664484]
- [include] dma-mapping: merge dma_unmap_page_attrs and dma_unmap_single_attrs (Don Dutile) [1664484]
- [include] dma-mapping: simplify the dma_sync_single_range_for_{cpu,device} implementation (Don Dutile) [1664484]
- [include] dma-mapping: return an error code from dma_mapping_error (Don Dutile) [1664484]
- [pci] dma-mapping: remove the mapping_error dma_map_ops method (Don Dutile) [1664484]
- [include] dma-mapping: provide a generic DMA_MAPPING_ERROR (Don Dutile) [1664484]
- [kernel] dma-mapping: move the arm64 noncoherent alloc/free support to common code (Don Dutile) [1664484]
- [mm] arm64: fix warnings without CONFIG_IOMMU_DMA (Don Dutile) [1664484]
- [arm64] arm64: use the generic swiotlb_dma_ops (Don Dutile) [1664484]
- [kernel] swiotlb: don't dip into swiotlb pool for coherent allocations (Don Dutile) [1664484]
- [kernel] swiotlb: refactor swiotlb_map_page (Don Dutile) [1664484]
- [kernel] swiotlb: use swiotlb_map_page in swiotlb_map_sg_attrs (Don Dutile) [1664484]
- [kernel] swiotlb: merge swiotlb_unmap_page and unmap_single (Don Dutile) [1664484]
- [kernel] swiotlb: remove the overflow buffer (Don Dutile) [1664484]
- [kernel] swiotlb: do not panic on mapping failures (Don Dutile) [1664484]
- [mm] arm64/dma-mapping: Mildly optimise non-coherent IOMMU ops (Don Dutile) [1664484]
- [iommu] iommu: Add fast hook for getting DMA domains (Don Dutile) [1664484]
- [iommu] iommu: Remove the ->map_sg indirection (Don Dutile) [1664484]
- [iommu] kernel/dma: remove unsupported gfp_mask parameter from dma_alloc_from_contiguous() (Don Dutile) [1664484]
- [mm] mm/cma: remove unsupported gfp_mask parameter from cma_alloc() (Don Dutile) [1664484]
- [kernel] dma-mapping: move the remap helpers to a separate file (Don Dutile) [1664484]
- [include] dma-mapping: fix return type of dma_set_max_seg_size() (Don Dutile) [1664484]
- [include] dma-mapping: translate __GFP_NOFAIL to DMA_ATTR_NO_WARN (Don Dutile) [1664484]
- [include] dma-debug: Check for drivers mapping invalid addresses in dma_map_single() (Don Dutile) [1664484]
- [base] dma-mapping: make the get_required_mask method available unconditionally (Don Dutile) [1664484]
- [xen] dma-mapping: support non-coherent devices in dma_common_get_sgtable (Don Dutile) [1664484]
- [kernel] dma-mapping: consolidate the dma mmap implementations (Don Dutile) [1664484]
- [kernel] dma-mapping: merge direct and noncoherent ops (Don Dutile) [1664484]
- [include] dma-mapping: move the dma_coherent flag to struct device (Don Dutile) [1664484]
- [include] dma-mapping: remove dma_deconfigure (Don Dutile) [1664484]
- [base] dma-mapping: remove dma_configure (Don Dutile) [1664484]
- [include] dma-mapping: relax warning for per-device areas (Don Dutile) [1664484]
- [kernel] dma-mapping: add the missing ARCH_HAS_SYNC_DMA_FOR_CPU_ALL declaration (Don Dutile) [1664484]
- [kernel] dma-noncoherent: add a arch_sync_dma_for_cpu_all hook (Don Dutile) [1664484]
- [block] deprecate elevator= kernel parameter (Jeff Moyer) [1665295]
- [rpmspec] kernel.spec: disable kabi checks until RC (=?UTF-8?q?=C4=8Cestm=C3=ADr=20Kalina?=) [1671007]
- [iommu] iommu/amd: Unmap all mapped pages in error path of map_sg (Jerry Snitselaar) [1668448]
- [iommu] iommu/amd: Call free_iova_fast with pfn in map_sg (Jerry Snitselaar) [1668448]

* Thu Feb 07 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-66.el8]
- [arm64] arm64, vmcoreinfo : Append 'MAX_PHYSMEM_BITS' to vmcoreinfo (Bhupesh Sharma) [1666679]
- [kernel] sched/debug: Initialize sd_sysctl_cpus if !CONFIG_CPUMASK_OFFSTACK (Joe Lawrence) [1667840]
- [init] Small change to the message about certified hardware (Steve Best) [1671765]
- [x86] x86/kdump: make the behavior of crashkernel=X consistent with kaslr (Pingfan Liu) [1640799]
- [x86] Add back support for Intel processors (Steve Best) [1670529]
- [net] SUNRPC: Clean up initialisation of the struct rpc_rqst (Benjamin Coddington) [1650494]
- [x86] KABI, x86/paravirt: Protect paravirt ops structures (Waiman Long) [1669957]
- [include] KABI: struct module padding (Prarit Bhargava) [1669480]
- [include] KABI: struct stack_trace_struct padding (Prarit Bhargava) [1669480]
- [documentation] iommu: Fix passthrough option documentation (Gary Hook) [1658391]
- [iommu] iommu: Add config option to set passthrough as default (Gary Hook) [1658391]
- [kernel] redhat: kernel: clean up taint flags (Jiri Benc) [1654313]

* Wed Feb 06 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-65.el8]
- [scsi] scsi: qedi: Add the CRC size within iSCSI NVM image (Charles Rose) [1670186]
- [fs] iomap: don't search past page end in iomap_is_partially_uptodate (Eric Sandeen) [1657588]
- [netdrv] cxgb4: update supported DCB version (Arjun Vynipadath) [1668571]
- [x86] kexec, KEYS: Make use of platform keyring for signature verify (Kairui Song) [1640486]
- [security] integrity, KEYS: add a reference to platform keyring (Kairui Song) [1640486]
- [security] efi: Allow the "db" UEFI variable to be suppressed (Kairui Song) [1640486]
- [security] efi: Import certificates from UEFI Secure Boot (Kairui Song) [1640486]
- [security] efi: Add an EFI signature blob parser (Kairui Song) [1640486]
- [include] efi: Add EFI signature data types (Kairui Song) [1640486]
- [security] integrity: Load certs to the platform keyring (Kairui Song) [1640486]
- [security] integrity: Define a trusted platform keyring (Kairui Song) [1640486]
- [security] security/integrity: remove unnecessary 'init_keyring' variable (Kairui Song) [1640486]
- [x86] Fix kexec forbidding kernels signed with keys in the secondary keyring to boot (Kairui Song) [1640486]
- [crypto] Replace magic for trusting the secondary keyring with #define (Kairui Song) [1640486]
- [acpi] acpi/nfit: Fix command-supported detection (Jeff Moyer) [1665812]
- [acpi] acpi/nfit: Block function zero DSMs (Jeff Moyer) [1665812]
- [md] dm: add missing trace_block_split() to __split_and_process_bio() (Mike Snitzer) [1645283]
- [md] dm: fix dm_wq_work() to only use __split_and_process_bio() if appropriate (Mike Snitzer) [1645283]
- [md] dm: fix redundant IO accounting for bios that need splitting (Mike Snitzer) [1645283]
- [md] dm: fix clone_bio() to trigger blk_recount_segments() (Mike Snitzer) [1645283]
- [block] block: cover another queue enter recursion via BIO_QUEUE_ENTERED (Mike Snitzer) [1645283]
- [md] dm thin: fix passdown_double_checking_shared_status() (Mike Snitzer) [1668039]
- [tools] bpftool: Fix prog dump by tag (Jiri Olsa) [1667305]
- [arm64] arm64: ftrace: Fix to enable syscall events on arm64 (Don Dutile) [1668035]
- [arm64] arm64: implement syscall wrappers (Don Dutile) [1668035]
- [arm64] arm64: convert compat wrappers to C (Don Dutile) [1668035]
- [arm64] arm64: use SYSCALL_DEFINE6() for mmap (Don Dutile) [1668035]
- [arm64] arm64: use {COMPAT,}SYSCALL_DEFINE0 for sigreturn (Don Dutile) [1668035]
- [arm64] arm64: remove in-kernel call to sys_personality() (Don Dutile) [1668035]
- [include] kernel: add ksys_personality() (Don Dutile) [1668035]
- [arm64] arm64: drop alignment from syscall tables (Don Dutile) [1668035]
- [arm64] arm64: entry: remove unused register aliases (Don Dutile) [1668035]
- [arm64] arm64: convert native/compat syscall entry to C (Don Dutile) [1668035]
- [arm64] arm64: svc: Ensure hardirq tracing is updated before return (Don Dutile) [1668035]
- [arm64] arm64: convert syscall trace logic to C (Don Dutile) [1668035]
- [arm64] arm64: move sve_user_{enable,disable} to <asm/fpsimd.h> (Don Dutile) [1668035]
- [arm64] arm64: kill change_cpacr() (Don Dutile) [1668035]
- [arm64] arm64: convert raw syscall invocation to C (Don Dutile) [1668035]
- [arm64] arm64: introduce syscall_fn_t (Don Dutile) [1668035]
- [arm64] arm64: remove sigreturn wrappers (Don Dutile) [1668035]
- [arm64] arm64: rseq: Implement backend rseq calls and select HAVE_RSEQ (Don Dutile) [1668035]
- [sound] ALSA: usb-audio: Add vendor and product name for Dell WD19 Dock (Jaroslav Kysela) [1664249]
- [infiniband] IB/hfi1: Fix an out-of-bounds access in get_hw_stats (Alex Estrin) [1667104]
- [infiniband] IB/hfi1: Incorrect sizing of sge for PIO will OOPs (Alex Estrin) [1667095]
- [drm] drm/nouveau: register backlight on pascal and newer (Ben Skeggs) [1664899]
- [drm] drm/nouveau/disp/gm200-: enforce identity-mapped SOR assignment for LVDS/eDP panels (Ben Skeggs) [1664899]
- [drm] drm/nouveau/disp: move eDP panel power handling (Ben Skeggs) [1664899]
- [drm] drm/nouveau/devinit: don't fail when PMU/PRE_OS is missing from VBIOS (Ben Skeggs) [1664899]
- [kernel] locking/rwsem: Fix (possible) missed wakeup (Waiman Long) [1668014]
- [kernel] futex: Fix (possible) missed wakeup (Waiman Long) [1668014]
- [kernel] sched/wake_q: Fix wakeup ordering for wake_q (Waiman Long) [1668014]
- [kernel] sched/wake_q: Document wake_q_add() (Waiman Long) [1668014]
- [kernel] sched/wait: Fix rcuwait_wake_up() ordering (Waiman Long) [1668014]
- [kernel] sched/Documentation: Update wake_up() & co. memory-barrier guarantees (Waiman Long) [1668014]
- [kvm] KVM: PPC: Book3S HV: Flush guest mappings when turning dirty tracking on/off (Laurent Vivier) [1650386]
- [kvm] KVM: PPC: Book3S HV: Cleanups - constify memslots, fix comments (Laurent Vivier) [1650386]
- [kvm] KVM: PPC: Book3S HV: Map single pages when doing dirty page logging (Laurent Vivier) [1650386]
- [kvm] KVM: PPC: Pass change type down to memslot commit function (Laurent Vivier) [1650386]
- [vhost] vhost: log dirty page correctly (Jason Wang) [1657578]
- [netdrv] netxen: taint as unsupported in RHEL8 (Tony Camuso) [1654825]
- [hid] HID: hiddev: fix potential Spectre v1 (Benjamin Tissoires) [1664611]
- [net] resort to custom code for sk_buff padding (Paolo Abeni) [1665984]
- [net] add padding to cipher_context (Paolo Abeni) [1665984]
- [net] add padding to tls_crypto_context (Paolo Abeni) [1665984]
- [net] add padding to ipv4_devconf (Paolo Abeni) [1665984]
- [net] ip6mr: Fix potential Spectre v1 vulnerability (Stefano Brivio) [1663472]
- [net] ipv4: Fix potential Spectre v1 vulnerability (Stefano Brivio) [1663472]
- [include] add KABI padding to file_system_type (Eric Sandeen) [1665320 1650565]
- [include] add KABI padding to multiple fs ops vectors (Eric Sandeen) [1665320]
- [fs] add KABI padding to dentry structure (Eric Sandeen) [1665320]
- [fs] add KABI padding to inode structure (Eric Sandeen) [1665320]
- [include] add KABI padding to file_lock structure (Eric Sandeen) [1665320]
- [include] KABI: add an iopoll method to struct file_operations (Eric Sandeen) [1665320]
- [sound] ALSA: emux: Fix potential Spectre v1 vulnerabilities (Jaroslav Kysela) [1663477]
- [sound] ALSA: pcm: Fix potential Spectre v1 vulnerability (Jaroslav Kysela) [1663477]
- [sound] ALSA: rme9652: Fix potential Spectre v1 vulnerability (Jaroslav Kysela) [1663477]
- [sound] ALSA: emu10k1: Fix potential Spectre v1 vulnerabilities (Jaroslav Kysela) [1663477]
- [powerpc] powerpc/tm: Unset MSR[TS] if not recheckpointing (Gustavo Duarte) [1663853]
- [netdrv] r8152: Add support for MAC address pass through on RTL8153-BND (Perry Yuan) [1658433]
- [hid] HID: debug: fix the ring buffer implementation (Tony Camuso) [1669469] {CVE-2019-3819}

* Wed Jan 23 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-64.el8]
- [netdrv] net: hns: Fix WARNING when hns modules installed (Xiaojun Tan) [1662120]
- [netdrv] net: hns: Fix ping failed when use net bridge and send multicast (Xiaojun Tan) [1662120]
- [netdrv] net: hns: Add mac pcs config when enable|disable mac (Xiaojun Tan) [1662120]
- [netdrv] net: hns: Fix ntuple-filters status error. (Xiaojun Tan) [1662120]
- [netdrv] net: hns: Free irq when exit from abnormal branch (Xiaojun Tan) [1662120]
- [netdrv] net: hns: Clean rx fbd when ae stopped. (Xiaojun Tan) [1662120]
- [netdrv] net: hns: Some registers use wrong address according to the datasheet. (Xiaojun Tan) [1662120]
- [netdrv] net: hns: All ports can not work when insmod hns ko after rmmod. (Xiaojun Tan) [1662120]
- [netdrv] net: hns: Incorrect offset address used for some registers. (Xiaojun Tan) [1662120]
- [include] ipmi: RH_KABI macros to pad kabi exposed structs (Tony Camuso) [1658175]
- [scsi] reserve space in structures for KABI (Ewan Milne) [1664397]

* Sat Jan 19 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-63.el8]
- [include] PCI: Add reserved fields to 'struct hotplug_slot' (Myron Stowe) [1663534]
- [include] PCI: Add reserved fields to 'struct hotplug_slot_ops' (Myron Stowe) [1663534]
- [pci] PCI: Add reserved fields to 'struct pci_sriov' (Myron Stowe) [1663534]
- [include] PCI: Add reserved fields to 'struct pci_driver' (Myron Stowe) [1663534]
- [include] PCI: Add reserved fields to 'struct pci_bus' (Myron Stowe) [1663534]
- [include] PCI: Add reserved fields, and extension, to 'struct pci_dev' (Myron Stowe) [1663534]
- [pci] PCI: Add missing include to drivers/pci.h (Myron Stowe) [1663534]
- [pci] PCI/IOV: Use VF0 cached config space size for other VFs (Myron Stowe) [1663534]
- [include] PCI: always include 'p2pdma' in 'struct pci_dev' (Myron Stowe) [1663534]
- [ata] PCI: Remove pci_set_dma_max_seg_size() (Myron Stowe) [1663534]
- [pci] PCI: Remove pci_set_dma_seg_boundary() (Myron Stowe) [1663534]
- [include] PCI: Remove pci_unmap_addr() wrappers for DMA API (Myron Stowe) [1663534]
- [pci] PCI/AER: Abstract AER interrupt handling (Myron Stowe) [1663534]
- [pci] PCI: Uninline PCI bus accessors for better ftracing (Myron Stowe) [1663534]
- [pci] PCI/portdrv: Add runtime PM hooks for port service drivers (Myron Stowe) [1663534]
- [pci] PCI: Make link active reporting detection generic (Myron Stowe) [1663534]
- [block] block: don't lose track of REQ_INTEGRITY flag (Ming Lei) [1665684]
- [nvme] nvme-pci: fix nvme_setup_irqs() (Ming Lei) [1661439]
- [lib] sbitmap: Protect swap_lock from hardirq (Ming Lei) [1666192]
- [lib] sbitmap: Protect swap_lock from softirqs (Ming Lei) [1666192]
- [scsi] scsi: isci: initialize shost fully before calling scsi_add_host() (Ming Lei) [1664918]
- [nvme] nvmet-fc: Mark NVMe/FC target mode driver as unsupported (Ewan Milne) [1664838]
- [netdrv] bnx2x: Assign unique DMAE channel number for FW DMAE transactions. (Jonathan Toppins) [1638306]
- [fs] block: don't use un-ordered __set_current_state(TASK_UNINTERRUPTIBLE) (Ming Lei) [1664580]
- [netdrv] qed: Wait for ready indication before rereading the shmem (Chad Dupuis) [1652417]
- [netdrv] qed: Avoid sending mailbox commands when MFW is not responsive (Chad Dupuis) [1652417]
- [netdrv] qed: Wait for MCP halt and resume commands to take place (Chad Dupuis) [1652417]
- [netdrv] qed: Prevent a possible deadlock during driver load and unload (Chad Dupuis) [1652417]
- [fs] gfs2: Fix loop in gfs2_rbm_find (Andreas Grunbacher) [1658528]
- [fs] gfs2: Get rid of potential double-freeing in gfs2_create_inode (Andreas Grunbacher) [1658539]

* Thu Jan 17 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-62.el8]
- [vhost] vhost/vsock: fix vhost vsock cid hashing inconsistent (Stefan Hajnoczi) [1619848] {CVE-2018-14625}
- [vhost] vhost/vsock: fix use-after-free in network stack callers (Stefan Hajnoczi) [1619848] {CVE-2018-14625}
- [netdrv] bnx2x: Add VF spoof-checking configuration (Jonathan Toppins) [1646842]
- [netdrv] net-next: hinic: fix a problem in free_tx_poll() (Xiaojun Tan) [1642016]
- [netdrv] net: hns: fix for unmapping problem when SMMU is on (Xiaojun Tan) [1640526]
- [netdrv] net: hns: add netif_carrier_off before change speed and duplex (Xiaojun Tan) [1640526]
- [netdrv] net: hns: add the code for cleaning pkt in chip (Xiaojun Tan) [1640526]
- [netdrv] net: hns: modify variable type in hns_nic_reuse_page (Xiaojun Tan) [1640526]

* Wed Jan 16 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-61.el8]
- [irqchip] Mark GICv2 deprecated (Wei Huang) [1609391]
- [scsi] qla2xxx: Use correct number of vectors for online CPUs (Himanshu Madhani) [1644058]
- [scsi] megaraid_sas: mark Aero controllers as tech preview (Tomas Henzl) [1659972]
- [scsi] megaraid_sas: add retry logic in megasas_readl (Tomas Henzl) [1659972]
- [scsi] scsi: megaraid_sas: Introduce new Aero adapter type (Tomas Henzl) [1659972]
- [scsi] scsi: megaraid_sas: Fix Ventura series based checks (Tomas Henzl) [1659972]
- [scsi] scsi: libfc: retry PRLI if we cannot analyse the payload (Chris Leech) [1631843]
- [scsi] scsi: libfc: check fc_frame_payload_get() return value for null (Chris Leech) [1631843]
- [scsi] scsi: libfc: hold disc_mutex in fc_disc_stop_rports() (Chris Leech) [1631843]
- [scsi] scsi: libfc: fixup lockdep annotations (Chris Leech) [1631843]
- [scsi] scsi: libfc: fixup 'sleeping function called from invalid context' (Chris Leech) [1631843]
- [scsi] scsi: libfc: Add lockdep annotations (Chris Leech) [1631843]
- [md] dm crypt: fix parsing of extended IV arguments (Mike Snitzer) [1665290]
- [kernel] redhat: kabi: reserved padding for kernel sched data structures (Rafael Aquini) [1664858]
- [kernel] redhat: kabi: reserved padding for MM related data structures (Rafael Aquini) [1664858]
- [vfio] vfio/type1: Fix unmap overflow off-by-one (Alex Williamson) [1662291]
- [message] mptspi: pci-id table changes (Tomas Henzl) [1651803]
- [message] mptspi: Taint kernel if mptspi is loaded (Tomas Henzl) [1651803]
- [block] kabi: reserve space for public data structure (Ming Lei) [1551939]
- [block] kabi: reserve space for blk-mq related structure (Ming Lei) [1551939]
- [block] kabi: reserve space for bsg related structure (Ming Lei) [1551939]
- [block] kabi: reserve space for integrity related structure (Ming Lei) [1551939]
- [block] kabi: reserve space for CONFIG_BLK_DEV_ZONED (Ming Lei) [1551939]
- [ata] ata: Disable AHCI ALPM feature for Ampere Computing eMAG SATA (David Milburn) [1663347]
- [kvm] KVM: x86: Add CPUID support for new instruction WBNOINVD (Andrew Jones) [1659491]
- [x86] KVM: x86: Use jmp to invoke kvm_spurious_fault() from .fixup (Andrew Jones) [1659491]
- [virt] kvm: Change offset in kvm_write_guest_offset_cached to unsigned (Andrew Jones) [1659491]
- [virt] kvm: Disallow wraparound in kvm_gfn_to_hva_cache_init (Andrew Jones) [1659491]
- [kvm] KVM: x86: svm: report MSR_IA32_MCG_EXT_CTL as unsupported (Andrew Jones) [1659491]
- [virt] arm/arm64: KVM: Add ARM_EXCEPTION_IS_TRAP macro (Andrew Jones) [1659491]
- [arm64] arm64: KVM: Avoid setting the upper 32 bits of VTCR_EL2 to 1 (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: Fix unintended stage 2 PMD mappings (Andrew Jones) [1659491]
- [virt] arm/arm64: KVM: vgic: Force VM halt when changing the active state of GICv3 PPIs/SGIs (Andrew Jones) [1659491]
- [arm64] KVM: arm/arm64: Fixup the kvm_exit tracepoint (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: vgic: Consider priority and active state for pending irq (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: vgic: Fix off-by-one bug in vgic_get_irq() (Andrew Jones) [1659491]
- [kvm] KVM: X86: Fix NULL deref in vcpu_scan_ioapic (Andrew Jones) [1659491]
- [kvm] KVM: Fix UAF in nested posted interrupt processing (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: vgic: Cap SPIs to the VM-defined maximum (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: vgic: Do not cond_resched_lock() with IRQs disabled (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: vgic-v2: Set active_source to 0 when restoring state (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: Fix VMID alloc race by reverting to lock-less (Andrew Jones) [1659491]
- [kvm] KVM: nVMX: Free the VMREAD/VMWRITE bitmaps if alloc_kvm_area() fails (Andrew Jones) [1659491]
- [kvm] arm64: KVM: Install stage-2 translation before enabling traps (Andrew Jones) [1659491]
- [kvm] arm64: KVM: Make VHE Stage-2 TLB invalidation operations non-interruptible (Andrew Jones) [1659491]
- [arm64] arm64: entry: Remove confusing comment (Andrew Jones) [1659491]
- [kvm] arm64: entry: Place an SB sequence following an ERET instruction (Andrew Jones) [1659491]
- [arm64] arm64: Add support for SB barrier and patch in over DSB; ISB sequences (Andrew Jones) [1659491]
- [kvm] kvm: nVMX: Set VM instruction error for VMPTRLD of unbacked page (Andrew Jones) [1659491]
- [kvm] kvm: svm: Ensure an IBPB on all affected CPUs when freeing a vmcb (Andrew Jones) [1659491]
- [kvm] kvm: mmu: Fix race in emulated page table writes (Andrew Jones) [1659491]
- [kvm] KVM: nVMX/nSVM: Fix bug which sets vcpu->arch.tsc_offset to L1 tsc_offset (Andrew Jones) [1659491]
- [kvm] KVM: VMX: Update shared MSRs to be saved/restored on MSR_EFER.LMA changes (Andrew Jones) [1659491]
- [kvm] KVM: x86: Fix kernel info-leak in KVM_HC_CLOCK_PAIRING hypercall (Andrew Jones) [1659491]
- [kvm] svm: Add mutex_lock to protect apic_access_page_done on AMD systems (Andrew Jones) [1659491]
- [kvm] KVM/nVMX: Do not validate that posted_intr_desc_addr is page aligned (Andrew Jones) [1659491]
- [kvm] KVM: arm64: Safety check PSTATE when entering guest and handle IL (Andrew Jones) [1659491]
- [virt] KVM: arm64: Fix caching of host MDCR_EL2 value (Andrew Jones) [1659491]
- [kvm] x86/kvm/nVMX: allow bare VMXON state migration (Andrew Jones) [1659491]
- [kvm] x86/kvm/lapic: preserve gfn_to_hva_cache len on cache reinit (Andrew Jones) [1659491]
- [kvm] KVM: hyperv: define VP assist page helpers (Andrew Jones) [1659491]
- [kvm] KVM: nVMX: move check_vmentry_postreqs() call to nested_vmx_enter_non_root_mode() (Andrew Jones) [1659491]
- [kvm] KVM: nVMX: Always reflect #NM VM-exits to L1 (Andrew Jones) [1659491]
- [kvm] KVM: x86: hyperv: consistently use 'hv_vcpu' for 'struct kvm_vcpu_hv' variables (Andrew Jones) [1659491]
- [kvm] KVM: x86: hyperv: enforce vp_index < KVM_MAX_VCPUS (Andrew Jones) [1659491]
- [kvm] KVM: nVMX: restore host state in nested_vmx_vmexit for VMFail (Andrew Jones) [1659491]
- [kvm] KVM: nVMX: Clear reserved bits of #DB exit qualification (Andrew Jones) [1659491]
- [virt] KVM: arm/arm64: Ensure only THP is candidate for adjustment (Andrew Jones) [1659491]
- [kvm] x86: kvm: avoid unused variable warning (Andrew Jones) [1659491]
- [kvm] powerpc64/ftrace: Include ftrace.h needed for enable/disable calls (Andrew Jones) [1659491]
- [kvm] x86/kvm/vmx: Remove duplicate l1d flush definitions (Andrew Jones) [1659491]
- [tools] perf kvm: Fix subcommands on s390 (Andrew Jones) [1659491]
- [arm64] arm64: add PSR_AA32_* definitions (Andrew Jones) [1659491]
- [pci] PCI: hotplug: Document TODOs (Myron Stowe) [1664454]
- [pci] PCI: hotplug: Embed hotplug_slot (Myron Stowe) [1664454]
- [pci] PCI: hotplug: Drop hotplug_slot_info (Myron Stowe) [1664454]
- [pci] PCI: hotplug: Constify hotplug_slot_ops (Myron Stowe) [1664454]
- [pci] PCI: pciehp: Reshuffle controller struct for clarity (Myron Stowe) [1664454]
- [pci] PCI: pciehp: Rename controller struct members for clarity (Myron Stowe) [1664454]
- [pci] PCI: pciehp: Unify controller and slot structs (Myron Stowe) [1664454]
- [pci] PCI: pciehp: Tolerate Presence Detect hardwired to zero (Myron Stowe) [1664454]
- [pci] PCI: pciehp: Drop hotplug_slot_ops wrappers (Myron Stowe) [1664454]
- [pci] PCI: pciehp: Drop unnecessary includes (Myron Stowe) [1664454]
- [pci] PCI: pciehp: Differentiate between surprise and safe removal (Myron Stowe) [1664454]
- [pci] PCI: Simplify disconnected marking (Myron Stowe) [1664454]
- [tools] perf vendor events arm64: Revise core JSON events for eMAG (Jiri Olsa) [1663353]
- [tools] perf vendor events arm64: Enable JSON events for eMAG (Jiri Olsa) [1663353]
- [perf] drivers/perf: xgene: Add CPU hotplug support (Jiri Olsa) [1663349]
- [scsi] mpt3sas: mark Aero controllers as tech preview (Tomas Henzl) [1663281]
- [powerpc] KVM: PPC: Book3S HV: Keep rc bits in shadow pgtable in sync with host (Suraj Jitindar Singh) [1662029]
- [powerpc] KVM: PPC: Book3S HV: Introduce kvmhv_update_nest_rmap_rc_list() (Suraj Jitindar Singh) [1662029]
- [powerpc] KVM: PPC: Book3S HV: Apply combination of host and l1 pte rc for nested guest (Suraj Jitindar Singh) [1662029]
- [powerpc] KVM: PPC: Book3S HV: Align gfn to L1 page size when inserting nest-rmap entry (Suraj Jitindar Singh) [1662029]
- [powerpc] KVM: PPC: Book3S HV: Hold kvm->mmu_lock across updating nested pte rc bits (Suraj Jitindar Singh) [1662029]
- [tools] perf python: Do not force closing original perf descriptor in evlist.get_pollfd (Jiri Olsa) [1659445]
- [mm] mm: thp: relax __GFP_THISNODE for MADV_HUGEPAGE mappings (Andrea Arcangeli) [1613993]
- [rpmspec] spec: Add libperf-jvmti.so into perf debuginfo rpm (Jiri Olsa) [1653570]
- [scsi] scsi: hisi_sas: Fix spin lock management in slot_index_alloc_quirk_v2_hw() (Xiaojun Tan) [1642819]
- [scsi] scsi: hisi_sas: Update v3 hw AIP_LIMIT and CFG_AGING_TIME register values (Xiaojun Tan) [1642819]
- [scsi] scsi: hisi_sas: Use block layer tag instead for IPTT (Xiaojun Tan) [1642819]
- [scsi] scsi: hisi_sas: unmask interrupts ent72 and ent74 (Xiaojun Tan) [1642819]
- [scsi] scsi: hisi_sas: Free slot later in slot_complete_vx_hw() (Xiaojun Tan) [1642819]
- [scsi] scsi: hisi_sas: Fix the race between IO completion and timeout for SMP/internal IO (Xiaojun Tan) [1642819]
- [scsi] scsi: hisi_sas: Move evaluation of hisi_hba in hisi_sas_task_prep() (Xiaojun Tan) [1642819]
- [scsi] scsi: hisi_sas: Feed back linkrate(max/min) when re-attached (Xiaojun Tan) [1642819]
- [hwtracing] intel_th: pci: Add Ice Lake PCH support (Jiri Olsa) [1485529]

* Fri Jan 11 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-60.el8]
- [kernel] userns: also map extents in the reverse map to kernel IDs (Chris von Recklinghausen) [1652679] {CVE-2018-18955}
- [net] ipv6: route: Fix return value of ip6_neigh_lookup() on neigh_create() error (Stefano Brivio) [1662789]
- [net] ipv6: frags: Fix bogus skb->sk in reassembled packets (Herbert Xu) [1645839]
- [net] redhat: blacklist auto-loadable net modules in modules-extra (Marcelo Leitner) [1642795]
- [net] redhat: move sctp modules to kernel-modules-extra (Marcelo Leitner) [1642795]
- [net] add reserved fields to neighbour (Paolo Abeni) [1655084]
- [net] add reserved fields to rtnl_link_stats* (Paolo Abeni) [1655084]
- [net] reserve bits in netdev_features_t for future features (Paolo Abeni) [1655084]
- [net] add reserved fields to sk_buff (Paolo Abeni) [1655084]
- [net] add reserved fields to ipv6_devconf (Paolo Abeni) [1655084]
- [net] add reserved fields to fib_rule (Paolo Abeni) [1655084]
- [net] add reserved fields to sock (Paolo Abeni) [1655084]
- [net] add reserved fields to genl_family (Paolo Abeni) [1655084]
- [net] add reserved fields to proto_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to proto (Paolo Abeni) [1655084]
- [net] add reserved fields to genl_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to dst_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to dst_entry (Paolo Abeni) [1655084]
- [net] add reserved fields to lwtunnel_state (Paolo Abeni) [1655084]
- [net] add reserved fields to packet_type (Paolo Abeni) [1655084]
- [net] add reserved fields to napi_struct (Paolo Abeni) [1655084]
- [net] add reserved fields to net_device (Paolo Abeni) [1655084]
- [net] exclude wireless_dev from KABI protection (Paolo Abeni) [1655084]
- [net] add reserved fields to dcbnl_rtnl_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to xfrm_* (Paolo Abeni) [1655084]
- [net] add reserved fields to switchdev_obj (Paolo Abeni) [1655084]
- [net] add reserved fields to switchdev_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to l3mdev_ops (Paolo Abeni) [1655084]
- [net] exclude ndisc_ops from kABI protection (Paolo Abeni) [1655084]
- [net] add reserved fields to xfrmdev_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to tlsdev_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to netdev_rx_queue (Paolo Abeni) [1655084]
- [net] add reserved fields to netdev_queue (Paolo Abeni) [1655084]
- [net] add reserved fields to rtnl_link_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to ethtool_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to header_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to net_device_ops (Paolo Abeni) [1655084]
- [net] add reserved fields to flowi* structs (Paolo Abeni) [1655084]
- [arm64] KVM: arm64: Clarify explanation of STAGE2_PGTABLE_LEVELS (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] KVM: arm/arm64: Rename kvm_arm_config_vm to kvm_arm_setup_stage2 (Christoph von Recklinghausen) [1643586 1643522]
- [virt] KVM: arm64: Drop __cpu_init_stage2 on the VHE path (Christoph von Recklinghausen) [1643586 1643522]
- [kvm] kvm: arm64: Allow tuning the physical address size for VM (Christoph von Recklinghausen) [1643586 1643522]
- [kvm] kvm: arm64: Limit the minimum number of page table levels (Christoph von Recklinghausen) [1643586 1643522]
- [virt] kvm: arm64: Set a limit on the IPA size (Christoph von Recklinghausen) [1643586 1643522]
- [kvm] kvm: arm64: Add 52bit support for PAR to HPFAR conversoin (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] kvm: arm64: Switch to per VM IPA limit (Christoph von Recklinghausen) [1643586 1643522]
- [kvm] kvm: arm64: Configure VTCR_EL2.SL0 per VM (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] kvm: arm64: Dynamic configuration of VTTBR mask (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] kvm: arm64: Make stage2 page table layout dynamic (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] kvm: arm64: Prepare for dynamic stage2 page table layout (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] kvm: arm/arm64: Prepare for VM specific stage2 translations (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] kvm: arm64: Configure VTCR_EL2 per VM (Christoph von Recklinghausen) [1643586 1643522]
- [virt] kvm: arm/arm64: Allow arch specific configurations for VM (Christoph von Recklinghausen) [1643586 1643522]
- [kvm] kvm: arm64: Clean up VTCR_EL2 initialisation (Christoph von Recklinghausen) [1643586 1643522]
- [arm64] arm64: Add a helper for PARange to physical shift conversion (Christoph von Recklinghausen) [1643586 1643522]
- [kvm] kvm: arm64: Add helper for loading the stage2 setting for a VM (Christoph von Recklinghausen) [1643586 1643522]
- [virt] kvm: arm/arm64: Remove spurious WARN_ON (Christoph von Recklinghausen) [1643586 1643522]
- [virt] kvm: arm/arm64: Fix stage2_flush_memslot for 4 level page table (Christoph von Recklinghausen) [1643586 1643522]
- [hv] hv_balloon: avoid touching uninitialized struct page during tail onlining (Vitaly Kuznetsov) [1662277]
- [x86] Mark AMD EPYC guests as supported (David Arcari) [1663356]
- [netdrv] be2net: Disable queue dump in be_tx_timeout handler (Petr Oros) [1646838]
- [vhost] vhost: Fix Spectre V1 vulnerability (Jason Wang) [1663469]
- [mm] mm/hugetlb.c: teach follow_hugetlb_page() to handle FOLL_NOWAIT (Andrea Arcangeli) [1575028]
- [tools] cpupower: Fix AMD Family 0x17 msr_pstate size (Prarit Bhargava) [1659883]
- [tools] cpupower: Fix coredump on VMWare (Prarit Bhargava) [1659883]
- [scsi] scsi: csiostor: remove flush_scheduled_work() (Arjun Vynipadath) [1663973]
- [powerpc] KVM: PPC: Book3S HV: Fix race between kvm_unmap_hva_range and MMU mode switch (David Gibson) [1663225]
- [fs] userfaultfd: check VM_MAYWRITE was set after verifying the uffd is registered (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [mm] userfaultfd: shmem: UFFDIO_COPY: set the page dirty if VM_WRITE is not set (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [mm] userfaultfd: shmem: add i_size checks (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [mm] userfaultfd: shmem/hugetlbfs: only allow to register VM_MAYWRITE vmas (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [mm] userfaultfd: shmem: allocate anonymous memory for MAP_PRIVATE shmem (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [mm] userfaultfd: use ENOENT instead of EFAULT if the atomic copy user fails (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [mm] userfaultfd: allow get_mempolicy(MPOL_F_NODE|MPOL_F_ADDR) to trigger userfaults (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [fs] userfaultfd: clear flag if remap event not enabled (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [fs] userfaultfd: disable irqs when taking the waitqueue lock (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [fs] fs/userfaultfd.c: remove redundant pointer uwq (Andrea Arcangeli) [1657615] {CVE-2018-18397}
- [fs] NFS: nfs_compare_mount_options always compare auth flavors. (Steve Dickson) [1661619]
- [infiniband] RDMA/hns: Bugfix for RoCE loopback test (Xiaojun Tan) [1663359]
- [infiniband] RDMA/hns: Update posting & querying mailbox (Xiaojun Tan) [1663359]
- [infiniband] RDMA/hns: Fix the bug while use multi-hop of pbl (Xiaojun Tan) [1663359]
- [infiniband] RDMA/hns: Init qp context when modify qp from reset to init (Xiaojun Tan) [1663359]
- [infiniband] RDMA/hns: Bugfix pbl configuration for rereg mr (Xiaojun Tan) [1663359]
- [security] selinux: add support for RTM_NEWCHAIN, RTM_DELCHAIN, and RTM_GETCHAIN (Ondrej Mosnacek) [1660564]
- [scsi] scsi: megaraid_sas: driver version update (Tomas Henzl) [1656261]
- [scsi] scsi: megaraid_sas: Use 63-bit DMA addressing (Tomas Henzl) [1656261]
- [x86] x86/kvm: mark as TechPreview when running as a nested hypervisor (Vitaly Kuznetsov) [1519039]
- [rpmspec] kernel.spec: Fix kernel-tools files section logic (Prarit Bhargava) [1661247]
- [crypto] crypto: ccp - Make function sev_get_firmware() static (Gary Hook) [1632894]
- [crypto] crypto: ccp - Allow SEV firmware to be chosen based on Family and Model (Gary Hook) [1632894]
- [crypto] crypto: ccp - Fix static checker warning (Gary Hook) [1632894]
- [crypto] crypto: ccp - add timeout support in the SEV command (Gary Hook) [1632894]
- [nvdimm] nvdimm: Use namespace index data to reduce number of label reads needed (Jeff Moyer) [1634345]
- [nvdimm] nvdimm: Split label init out from the logic for getting config data (Jeff Moyer) [1634345]
- [nvdimm] nvdimm: Remove empty if statement (Jeff Moyer) [1634345]
- [nvdimm] nvdimm: Clarify comment in sizeof_namespace_index (Jeff Moyer) [1634345]
- [nvdimm] nvdimm: Sanity check labeloff (Jeff Moyer) [1634345]
- [nvdimm] libnvdimm, dimm: Maximize label transfer size (Jeff Moyer) [1634345]
- [mm] mm/page-writeback.c: fix range_cyclic writeback vs writepages deadlock (Brian Foster) [1659528]
- [input] Input: elantech - disable elan-i2c for P52 and P72 (Benjamin Tissoires) [1658602]
- [fs] cachefiles: avoid deprecated get_seconds() (David Howells) [1655613]
- [fs] fscache, cachefiles: remove redundant variable 'cache' (David Howells) [1655613]
- [fs] cachefiles: Explicitly cast enumerated type in put_object (David Howells) [1655613]
- [fs] fscache: fix race between enablement and dropping of object (David Howells) [1655613]
- [fs] cachefiles: Fix page leak in cachefiles_read_backing_file while vmscan is active (David Howells) [1655613]
- [fs] fscache: Fix race in fscache_op_complete() due to split atomic_sub & read (David Howells) [1655613]
- [fs] cachefiles: Fix an assertion failure when trying to update a failed object (David Howells) [1655613]
- [fs] fscache: Fix out of bound read in long cookie keys (David Howells) [1655613]
- [fs] fscache: Fix incomplete initialisation of inline key space (David Howells) [1655613]
- [fs] cachefiles: fix the race between cachefiles_bury_object() and rmdir(2) (David Howells) [1655613]
- [kernel] ebpf: record usage of eBPF (Jiri Benc) [1654279]
- [kernel] add rh_features to /proc (Jiri Benc) [1654279]
- [kernel] add support for rh_features (Jiri Benc) [1654279]
- [fs] fs/lock: show locks taken by processes from another pidns (Miklos Szeredi) [1616125]
- [iommu] iommu/arm-smmu: Support non-strict mode (Xiaojun Tan) [1643114]
- [iommu] iommu/io-pgtable-arm-v7s: Add support for non-strict mode (Xiaojun Tan) [1643114]
- [iommu] iommu/arm-smmu-v3: Add support for non-strict mode (Xiaojun Tan) [1643114]
- [iommu] iommu/io-pgtable-arm: Add support for non-strict mode (Xiaojun Tan) [1643114]
- [iommu] iommu: Add "iommu.strict" command line option (Xiaojun Tan) [1643114]
- [iommu] iommu/dma: Add support for non-strict mode (Xiaojun Tan) [1643114]
- [iommu] iommu/arm-smmu: Ensure that page-table updates are visible before TLBI (Xiaojun Tan) [1643114]
- [iommu] iommu/arm-smmu-v3: Implement flush_iotlb_all hook (Xiaojun Tan) [1643114]
- [iommu] iommu/arm-smmu-v3: Avoid back-to-back CMD_SYNC operations (Xiaojun Tan) [1643114]
- [iommu] iommu/arm-smmu-v3: Fix unexpected CMD_SYNC timeout (Xiaojun Tan) [1643114]
- [iommu] iommu/io-pgtable-arm: Fix race handling in split_blk_unmap() (Xiaojun Tan) [1643114]
- [infiniband] RDMA/hns: Update some attributes of the RoCE device (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Limit the size of extend sge of sq (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Bugfix for CM test (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Submit bad wr when post send wr exception (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Bugfix for reserved qp number (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Refactor the codes for setting transport opode (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Move all prints out of irq handle (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Fix an error code in hns_roce_v2_init_eq_table() (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Fix usage of bitmap allocation functions return values (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Support flush cqe for hip08 in kernel space (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Program the tclass and flow label into the hardware (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Use macro instead of magic number (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Modify qp will return errno when qp type is illegal (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Assign the value for vlan field of qp context (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Only assgin the fields of the av if IB_QP_AV bit is set (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Enable modify_cq for uverbs. (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Update the data type of immediate data (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Use delay instead of usleep (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Add illegal hop_num judgement (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Add 50GE type of hnae3 device match (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Do not overwrite the error code during error unwind in hns_roce_init (Xiaojun Tan) [1639578]
- [infiniband] hns: Remove a set-but-not-used variable (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Update the implementation of set_mac (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Update the implementation of set_gid (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Add TPQ link table support (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Add TSQ link table support (Xiaojun Tan) [1639578]
- [infiniband] RDMA/hns: Fix endian conversions and annotations (Xiaojun Tan) [1639578]
- [scsi] scsi: hisi_sas: Add SATA FIS check for v3 hw (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: add memory barrier in task delivery function (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Tidy hisi_sas_task_prep() (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Implement handlers of PCIe FLR for v3 hw (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: relocate some common code for v3 hw (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: tidy host controller reset function a bit (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Fix the failure of recovering PHY from STP link timeout (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: tidy channel interrupt handler for v3 hw (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Drop hisi_sas_slot_abort() (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Update a couple of register settings for v3 hw (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Add missing PHY spinlock init (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Pre-allocate slot DMA buffers (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Release all remaining resources in clear nexus ha (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Add a flag to filter PHY events during reset (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Adjust task reject period during host reset (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Fix the conflict between dev gone and host reset (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Only process broadcast change in phy_bcast_v3_hw() (Zhou Wang) [1639541]
- [scsi] scsi: hisi_sas: Use dmam_alloc_coherent() (Zhou Wang) [1639541]
- [netdrv] xen/netfront: fix waiting for xenbus state change (Petr Oros) [1638456]

* Thu Jan 10 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-59.el8]
- [x86] expand cpu feature/bug bits (David Arcari) [1662434]
- [x86] add kabi support for cpuinfo_x86 (David Arcari) [1662434]
- [init] Display a message about certified hardware (Steve Best) [1660523]
- [scsi] scsi: t10-pi: Return correct ref tag when queue has no integrity profile (Ming Lei) [1660719]
- [scsi] scsi: storvsc: Fix a race in sub-channel creation that can cause panic (Mohammed Gamal) [1650149]
- [uio] uio_hv_generic: set callbacks on open (Mohammed Gamal) [1650149]
- [hv] vmbus: fix subchannel removal (Mohammed Gamal) [1650149]
- [uio] uio_hv_generic: defer opening vmbus until first use (Mohammed Gamal) [1650149]
- [hv] vmbus: split ring buffer allocation from open (Mohammed Gamal) [1650149]
- [hv] vmbus: pass channel to hv_process_channel_removal (Mohammed Gamal) [1650149]
- [hv] Drivers: hv: vmbus: Reset the channel callback in vmbus_onoffer_rescind() (Mohammed Gamal) [1650149]
- [uio] hv_uio_generic: map ringbuffer phys addr (Mohammed Gamal) [1650149]
- [uio] uio: introduce UIO_MEM_IOVA (Mohammed Gamal) [1650149]
- [hv] vmbus: add driver_override support (Mohammed Gamal) [1650149]
- [hv] vmbus: keep pointer to ring buffer page (Mohammed Gamal) [1650149]
- [uio] uio_hv_generic: increase size of receive and send buffers (Mohammed Gamal) [1650149]
- [uio] uio: add SPDX license tags (Mohammed Gamal) [1650149]
- [fs] gfs2: take jdata unstuff into account in do_grow (Robert S Peterson) [1660519]
- [drm] drm/dp_mst: Check if primary mstb is null (Lyude Paul) [1658711]
- [tools] perf tests: Use shebangs in the shell scripts (Michael Petlan) [1613523]

* Mon Jan 07 2019 Herton R. Krzesinski <herton@redhat.com> [4.18.0-58.el8]
- [mm] mm: put_and_wait_on_page_locked() while page is migrated (Baoquan He) [1649214]
- [netdrv] i40e: define proper net_device::neigh_priv_len (Stefan Assmann) [1658743]
- [netdrv] i40e: fix VLAN.TCI == 0 RX HW offload (Stefan Assmann) [1658743]
- [netdrv] i40e: fix mac filter delete when setting mac address (Stefan Assmann) [1658743]
- [netdrv] i40e: prevent overlapping tx_timeout recover (Stefan Assmann) [1658743]
- [netdrv] i40e: Use correct shift for VLAN priority (Stefan Assmann) [1658743]
- [netdrv] i40e: always set ks->base.speed in i40e_get_settings_link_up (Stefan Assmann) [1658743]
- [netdrv] i40e: don't restart nway if autoneg not supported (Stefan Assmann) [1658743]
- [netdrv] i40e: enable NETIF_F_NTUPLE and NETIF_F_HW_TC at driver load (Stefan Assmann) [1658743]
- [netdrv] i40e: restore NETIF_F_GSO_IPXIP[46] to netdev features (Stefan Assmann) [1658743]
- [acpi] ACPI/APEI: Clear GHES block_status before panic() (David Arcari) [1662442]
- [misc] VMCI: Resource wildcard match fixed (Vitaly Kuznetsov) [1652868]
- [mm] mm/page_alloc.c: don't call kasan_free_pages() at deferred mem init (Waiman Long) [1655964]
- [block] block/bio: Do not zero user pages (Ming Lei) [1662502]
- [vhost] disable zerocopy by default (Jason Wang) [1582756]
- [block] kyber: use sbitmap add_wait_queue/list_del wait helpers (Ming Lei) [1661426]
- [lib] sbitmap: add helpers for add/del wait queue handling (Ming Lei) [1661426]
- [net] Revert "sunrpc: Ensure we always close the socket after a connection shuts down" (Dave Wysochanski) [1657449]
- [vhost] vhost/vsock: fix reset orphans race with close timeout (Stefan Hajnoczi) [1660445]
- [misc] genwqe: Fix size check (Steve Best) [1660126]
- [fs] aio: fix spectre gadget in lookup_ioctx (Jeff Moyer) [1660963]
- [block] block: save irq state in blkg_lookup_create() (Ming Lei) [1660299]
- [md] dm: don't reuse bio for flushes (Ming Lei) [1660401]
- [wireless] mac80211_hwsim: Fix possible Spectre-v1 for hwsim_world_regdom_custom (Stanislaw Gruszka) [1637113]
- [wireless] nl80211: Fix possible Spectre-v1 for NL80211_TXRATE_HT (Stanislaw Gruszka) [1637113]
- [wireless] nl80211: Fix possible Spectre-v1 for CQM RSSI thresholds (Stanislaw Gruszka) [1637113]
- [block] blk-mq: enable IO poll if .nr_queues of type poll > 0 (Ming Lei) [1660826]
- [powerpc] powerpc/rtas: Fix a potential race between CPU-Offline & Migration (Desnes Augusto Nunes do Rosario) [1639266]
- [x86] kvm: x86: Add AMD's EX_CFG to the list of ignored MSRs (Eduardo Habkost) [1625111]
- [scsi] scsi_sysfs: make unpriv_sgio queue attribute accessible for non-block devices (Paolo Bonzini) [1584504]
- [block] scsi_ioctl: introduce unpriv_sgio queue flag (Paolo Bonzini) [1584504]
- [block] scsi_ioctl: pass request_queue to blk_verify_command (Paolo Bonzini) [1584504]
- [fs] ext4: missing !bh check in ext4_xattr_inode_write() (Lukas Czerner) [1659481]
- [fs] ext4: fix buffer leak in __ext4_read_dirblock() on error path (Lukas Czerner) [1659481]
- [fs] ext4: fix buffer leak in ext4_expand_extra_isize_ea() on error path (Lukas Czerner) [1659481]
- [fs] ext4: fix buffer leak in ext4_xattr_move_to_block() on error path (Lukas Czerner) [1659481]
- [fs] ext4: release bs.bh before re-using in ext4_xattr_block_find() (Lukas Czerner) [1659481]
- [fs] ext4: fix buffer leak in ext4_xattr_get_block() on error path (Lukas Czerner) [1659481]
- [fs] ext4: fix possible leak of s_journal_flag_rwsem in error path (Lukas Czerner) [1659481]
- [fs] ext4: fix possible leak of sbi->s_group_desc_leak in error path (Lukas Czerner) [1659481]
- [fs] ext4: avoid possible double brelse() in add_new_gdb() on error path (Lukas Czerner) [1659481]
- [fs] ext4: avoid buffer leak in ext4_orphan_add() after prior errors (Lukas Czerner) [1659481]
- [fs] ext4: avoid buffer leak on shutdown in ext4_mark_iloc_dirty() (Lukas Czerner) [1659481]
- [fs] ext4: fix possible inode leak in the retry loop of ext4_resize_fs() (Lukas Czerner) [1659481]
- [fs] ext4: fix missing cleanup if ext4_alloc_flex_bg_array() fails while resizing (Lukas Czerner) [1659481]
- [fs] ext4: add missing brelse() update_backups()'s error path (Lukas Czerner) [1659481]
- [fs] ext4: add missing brelse() add_new_gdb_meta_bg()'s error path (Lukas Czerner) [1659481]
- [fs] ext4: add missing brelse() in set_flexbg_block_bitmap()'s error path (Lukas Czerner) [1659481]
- [fs] ext4: avoid potential extra brelse in setup_new_flex_group_blocks() (Lukas Czerner) [1659481]
- [scsi] scsi: lpfc: Enable Management features for IF_TYPE=6 (Dick Kennedy) [1658755]
- [scsi] scsi: mpt3sas: Update driver version to 27.101.00.00 (Tomas Henzl) [1659035]
- [scsi] scsi: mpt3sas: Replace readl with ioc->base_readl (Tomas Henzl) [1659035]
- [scsi] scsi: mpt3sas: Add separate function for aero doorbell reads (Tomas Henzl) [1659035]
- [scsi] scsi: mpt3sas: Introduce flag for aero based controllers (Tomas Henzl) [1659035]
- [md] dm: do not allow readahead to limit IO size (Mike Snitzer) [1658757]
- [md] dm raid: fix false -EBUSY when handling check/repair message (Mike Snitzer) [1658757]
- [block] blk-mq: change blk_mq_queue_busy() to blk_mq_queue_inflight() (Mike Snitzer) [1658757]
- [md] dm rq: cleanup leftover code from recently removed q->mq_ops branching (Mike Snitzer) [1658757]
- [md] dm verity: log the hash algorithm implementation (Mike Snitzer) [1658757]
- [md] dm crypt: log the encryption algorithm implementation (Mike Snitzer) [1658757]
- [md] dm integrity: fix spelling mistake in workqueue name (Mike Snitzer) [1658757]
- [md] dm flakey: Properly corrupt multi-page bios. (Mike Snitzer) [1658757]
- [md] dm: Check for device sector overflow if CONFIG_LBDAF is not set (Mike Snitzer) [1658757]
- [md] dm crypt: use u64 instead of sector_t to store iv_offset (Mike Snitzer) [1658757]
- [md] dm kcopyd: Fix bug causing workqueue stalls (Mike Snitzer) [1658757]
- [md] dm snapshot: Fix excessive memory usage and workqueue stalls (Mike Snitzer) [1658757]
- [md] dm bufio: update comment in dm-bufio.c (Mike Snitzer) [1658757]
- [md] dm writecache: fix typo in error msg for creating writecache_flush_thread (Mike Snitzer) [1658757]
- [md] dm: remove indirect calls from __send_changing_extent_only() (Mike Snitzer) [1658757]
- [md] dm mpath: only flush workqueue when needed (Mike Snitzer) [1658757]
- [md] dm: avoid indirect call in __dm_make_request (Mike Snitzer) [1658757]
- [md] dm thin: bump target version (Mike Snitzer) [1658757]
- [md] dm thin: send event about thin-pool state change _after_ making it (Mike Snitzer) [1658757]
- [md] dm cache metadata: verify cache has blocks in blocks_are_clean_separate_dirty() (Mike Snitzer) [1658757]
- [md] dm writecache: remove disabled code in memory_entry() (Mike Snitzer) [1658757]
- [md] dm raid: avoid bitmap with raid4/5/6 journal device (Mike Snitzer) [1658757]
- [md] dm crypt: make workqueue names device-specific (Mike Snitzer) [1658757]
- [md] dm: add dm_table_device_name() (Mike Snitzer) [1658757]
- [md] dm ioctl: harden copy_params()'s copy_from_user() from malicious users (Mike Snitzer) [1658757]
- [md] dm: remove unnecessary unlikely() around WARN_ON_ONCE() (Mike Snitzer) [1658757]
- [md] dm thin: use refcount_t for thin_c reference counting (Mike Snitzer) [1658757]
- [netdrv] nfp: provide a better warning when ring allocation fails (Pablo Cascon) [1645456]
- [netdrv] nfp: use kvcalloc() to allocate SW buffer descriptor arrays (Pablo Cascon) [1645456]
- [scsi] scsi: lpfc: rport port swap discovery issue. (Dick Kennedy) [1656635]
- [scsi] scsi: lpfc: Fix discovery failures during port failovers with lots of vports (Dick Kennedy) [1656635]
- [scsi] scsi: lpfc: refactor mailbox structure context fields (Dick Kennedy) [1656635]
- [scsi] scsi: lpfc: Correct loss of fc4 type on remote port address change (Dick Kennedy) [1656635]
- [hid] HID: multitouch: Add pointstick support for Cirque Touchpad (Perry Yuan) [1656673]
- [powerpc] KVM: PPC: Book3S HV: Fix handling for interrupted H_ENTER_NESTED (Suraj Jitindar Singh) [1649980]
- [powerpc] powerpc: Select CONFIG_SWIOTLB (Gustavo Duarte) [1648466]
- [fs] nfs: Fix a missed page unlock after pg_doio() (Benjamin Coddington) [1651287]
- [arm64] arm64: fix possible spectre-v1 write in ptrace_hbp_set_event() (Mark Salter) [1637585]
- [fs] fsnotify: Fix busy inodes during unmount (Lukas Czerner) [1650462]
- [tools] perf vendor events arm64: Update ThunderX2 implementation defined pmu core events (Robert Richter) [1501638]
- [tools] perf tools: Fix undefined symbol scnprintf in libperf-jvmti.so (Jiri Olsa) [1579484]

* Tue Dec 18 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-57.el8]
- [block] blk-mq: export hctx->type in debugfs instead of sysfs (Ming Lei) [1660040]
- [block] blk-mq: fix dispatch from sw queue (Ming Lei) [1660040]
- [block] blk-mq: skip zero-queue maps in blk_mq_map_swqueue (Ming Lei) [1660040]
- [nvme] nvme-pci: don't share queue maps (Ming Lei) [1660040]
- [block] blk-mq: only dispatch to non-defauly queue maps if they have queues (Ming Lei) [1660040]
- [x86] KVM: LAPIC: Fix pv ipis use-before-initialization (Paul Lai) [1657702]
- [fs] autofs: fix directory and symlink access (Ian Kent) [1611967]
- [infiniband] IB/iser: Fix possible NULL deref at iser_inv_desc() (Don Dutile) [1657574]
- [infiniband] RDMA/core: Fix unwinding flow in case of error to register device (Don Dutile) [1657574]
- [infiniband] IB/rxe: fix for duplicate request processing and ack psns (Don Dutile) [1657574]
- [infiniband] IB/ipoib: Clear IPCB before icmp_send (Don Dutile) [1657574]
- [infiniband] RDMA/core: Do not expose unsupported counters (Don Dutile) [1657574]
- [infiniband] IB/ucm: Fix Spectre v1 vulnerability (Don Dutile) [1657574]
- [infiniband] RDMA/ucma: Fix Spectre v1 vulnerability (Don Dutile) [1657574]
- [infiniband] RDMA/uverbs: Don't overwrite NULL pointer with ZERO_SIZE_PTR (Don Dutile) [1657574]
- [infiniband] RDMA/cma: Do not ignore net namespace for unbound cm_id (Don Dutile) [1657574]
- [net] xprtrdma: Reset credit grant properly after a disconnect (Don Dutile) [1657574]
- [input] Input: hyper-v - fix wakeup from suspend-to-idle (Vitaly Kuznetsov) [1588888]
- [kernel] kernel: hung_task.c: disable on suspend (Vitaly Kuznetsov) [1588888]
- [kernel] redhat: add a comment with warning about RH_KABI_EXCLUDE usage (Jiri Benc) [1656933]
- [rpmspec] Sign the aarch64 kernel (Jeremy Linton) [1659158]

* Mon Dec 17 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-56.el8]
- [netdrv] nfp: flower: add geneve option match offload (Pablo Cascon) [1655604]
- [netdrv] nfp: flower: add geneve option push action offload (Pablo Cascon) [1655604]
- [netdrv] nfp: flower: offload tos and tunnel flags for ipv4 udp tunnels (Pablo Cascon) [1655604]
- [netdrv] nfp: flower: set ip tunnel ttl from encap action (Pablo Cascon) [1655604]
- [netdrv] nfp: flower: extract ipv4 udp tunnel ttl from route (Pablo Cascon) [1655604]
- [net] sctp: hold transport before accessing its asoc in sctp_transport_get_next (Marcelo Leitner) [1656271]
- [net] sctp: fix the data size calculation in sctp_data_size (Marcelo Leitner) [1656271]
- [net] sctp: fix race on sctp_id2asoc (Marcelo Leitner) [1656271]
- [net] rtnetlink: ndo_dflt_fdb_dump() only work for ARPHRD_ETHER devices (Hangbin Liu) [1657120]
- [netdrv] mlx5e: fix csum adjustments caused by RXFCS (Hangbin Liu) [1657120]
- [net] drop skb on failure in ip_check_defrag() (Hangbin Liu) [1657120]
- [net] rtnl_configure_link: fix dev flags changes arg to __dev_notify_flags (Hangbin Liu) [1657120]
- [net] socket: fix a missing-check bug (Hangbin Liu) [1657120]
- [net] rtnetlink: Disallow FDB configuration for non-Ethernet device (Hangbin Liu) [1657120]
- [net] rtnetlink: Fail dump if target netnsid is invalid (Hangbin Liu) [1657120]
- [net] rtnetlink: fix rtnl_fdb_dump() for ndmsg header (Hangbin Liu) [1657120]
- [net] rtnl: limit IFLA_NUM_TX_QUEUES and IFLA_NUM_RX_QUEUES to 4096 (Hangbin Liu) [1657120]
- [net] socket: fix struct ifreq size in compat ioctl (Hangbin Liu) [1657120]
- [net] fix pskb_trim_rcsum_slow() with odd trim offset (Hangbin Liu) [1657120]
- [net] gso_segment: Reset skb->mac_len after modifying network header (Hangbin Liu) [1657120]
- [net] Use __kernel_clockid_t in uapi net_stamp.h (Davide Caratti) [1638022]
- [net] tun: Consistently configure generic netdev params via rtnetlink (Matteo Croce) [1657910]
- [net] tun: napi flags belong to tfile (Matteo Croce) [1657910]
- [net] tun: initialize napi_mutex unconditionally (Matteo Croce) [1657910]
- [net] tun: remove unused parameters (Matteo Croce) [1657910]
- [net] team: Forbid enslaving team device to itself (Matteo Croce) [1658725]
- [net] sched: Remove TCA_OPTIONS from policy (Davide Caratti) [1658516]
- [net] sched: cls_api: add missing validation of netlink attributes (Davide Caratti) [1658516]
- [net] sched: gred: pass the right attribute to gred_change_table_def() (Davide Caratti) [1658516]
- [net] sched: cls_u32: fix hnode refcounting (Davide Caratti) [1658516]
- [net] sched: Add policy validation for tc attributes (Davide Caratti) [1658516]
- [net] bpf: use __GFP_COMP while allocating page (Andrea Claudi) [1658231]
- [net] xsk: do not call synchronize_net() under RCU read lock (Andrea Claudi) [1658231]
- [net] bpf: fix partial copy of map_ptr when dst is scalar (Andrea Claudi) [1658231]
- [net] bpf: Fix bpf_msg_pull_data() (Andrea Claudi) [1658231]
- [net] bpf: fix shift upon scatterlist ring wrap-around in bpf_msg_pull_data (Andrea Claudi) [1658231]
- [net] bpf: fix sg shift repair start offset in bpf_msg_pull_data (Andrea Claudi) [1658231]
- [net] bpf: fix msg->data/data_end after sg shift repair in bpf_msg_pull_data (Andrea Claudi) [1658231]
- [net] bpf: fix several offset tests in bpf_msg_pull_data (Andrea Claudi) [1658231]
- [net] vlan: add support for tunnel offload (Andrea Claudi) [1656804]
- [net] 8021q: move vlan offload registrations into vlan_core (Hangbin Liu) [1657658]
- [net] ipv6/ndisc: Preserve IPv6 control buffer if protocol error handlers are called (Stefano Brivio) [1658010]
- [net] ipv6: Allow onlink routes to have a device mismatch if it is the default route (Stefano Brivio) [1658010]
- [net] ipv6: Fix index counter for unicast addresses in in6_dump_addrs (Stefano Brivio) [1658010]
- [net] ipv6: mcast: fix a use-after-free in inet6_mc_check (Stefano Brivio) [1658010]
- [net] ipv6: rate-limit probes for neighbourless routes (Stefano Brivio) [1658010]
- [net] ipv6: stop leaking percpu memory in fib6 info (Stefano Brivio) [1658010]
- [net] ipv6: Remove extra call to ip6_convert_metrics for multipath case (Stefano Brivio) [1658010]
- [net] ipv6: Display all addresses in output of /proc/net/if_inet6 (Stefano Brivio) [1658010]
- [net] ipv6: do not copy dst flags on rt init (Stefano Brivio) [1658010]
- [net] ipv6: Only update MTU metric if it set (Stefano Brivio) [1658010]
- [net] ipv6: don't get lwtstate twice in ip6_rt_copy_init() (Stefano Brivio) [1658010]
- [net] ipv6: Put lwtstate when destroying fib6_info (Stefano Brivio) [1658010]
- [net] ip6_tunnel: Fix encapsulation layout (Stefano Brivio) [1658008]
- [net] vxlan: fill ttl inherit info (Stefano Brivio) [1658008]
- [net] ip_tunnel: be careful when accessing the inner header (Stefano Brivio) [1658008]
- [net] vti6: remove !skb->ignore_df check from vti6_xmit() (Stefano Brivio) [1658008]
- [net] ip6_vti: fix a null pointer deference when destroy vti6 tunnel (Stefano Brivio) [1658008]
- [net] ip6_vti: fix creating fallback tunnel device for vti6 (Stefano Brivio) [1658008]
- [net] ip_vti: fix a null pointer deferrence when create vti fallback tunnel (Stefano Brivio) [1658008]
- [net] l2tp: use sk_dst_check() to avoid race on sk->sk_dst_cache (Stefano Brivio) [1658008]
- [net] macsec: let the administrator set UP state even if lowerdev is down (Sabrina Dubroca) [1645540]
- [net] macsec: update operstate when lower device changes (Sabrina Dubroca) [1645540]
- [net] tcp: do not restart timewait timer on rst reception (Paolo Abeni) [1657988]
- [net] tcp: really ignore MSG_ZEROCOPY if no SO_ZEROCOPY (Paolo Abeni) [1657988]
- [net] tcp, ulp: add alias for all ulp modules (Paolo Abeni) [1657988]
- [net] tcp, ulp: fix leftover icsk_ulp_ops preventing sock from reattach (Paolo Abeni) [1657988]
- [net] ipv4: tcp: send zero IPID for RST and ACK sent in SYN-RECV and TIME-WAIT state (Paolo Abeni) [1657988]
- [net] neighbour: Avoid writing before skb->head in neigh_hh_output() (Stefano Brivio) [1643336]
- [net] ipv6: Check available headroom in ip6_xmit() even without options (Stefano Brivio) [1643336]
- [net] ipv6: fix possible use-after-free in ip6_xmit() (Stefano Brivio) [1643336]
- [net] openvswitch: Fix push/pop ethernet validation (Hangbin Liu) [1657226]
- [net] cgroup, netclassid: add a preemption point to write_classid (Hangbin Liu) [1657226]
- [net] ethtool: fix a privilege escalation bug (Hangbin Liu) [1657226]
- [net] llc: set SOCK_RCU_FREE in llc_sap_add_socket() (Hangbin Liu) [1657226]
- [net] dcb: For wild-card lookups, use priority -1, not 0 (Hangbin Liu) [1657226]
- [net] packet: fix packet drop as of virtio gso (Hangbin Liu) [1657226]
- [net] netlabel: check for IPV4MASK in addrinfo_get (Hangbin Liu) [1657226]
- [net] netfilter: seqadj: re-load tcp header pointer after possible head reallocation (Florian Westphal) [1654259]
- [net] netfilter: nf_tables: avoid BUG_ON usage (Florian Westphal) [1654259]
- [net] netfilter: nf_tables: deactivate expressions in rule replecement routine (Florian Westphal) [1654259]
- [net] netfilter: nat: fix double register in masquerade modules (Florian Westphal) [1654259]
- [net] netfilter: add missing error handling code for register functions (Florian Westphal) [1654259]
- [net] netfilter: nf_tables: fix use-after-free when deleting compat expressions (Florian Westphal) [1654259]
- [net] netfilter: xt_RATEEST: remove netns exit routine (Florian Westphal) [1654259]
- [net] netfilter: nf_tables: don't use position attribute on rule replacement (Florian Westphal) [1654259]
- [net] revert "netfilter: nft_numgen: add map lookups for numgen random operations" (Florian Westphal) [1654259]
- [net] netfilter: xt_IDLETIMER: add sysfs filename checking routine (Florian Westphal) [1654259]
- [net] netfilter: conntrack: fix calculation of next bucket number in early_drop (Florian Westphal) [1654259]
- [net] netfilter: conntrack: get rid of double sizeof (Florian Westphal) [1654259]
- [net] netfilter: nft_set_rbtree: add missing rb_erase() in GC routine (Florian Westphal) [1654259]
- [net] netfilter: nfnetlink_queue: Solve the NFQUEUE/conntrack clash for NF_REPEAT (Florian Westphal) [1654259]
- [net] netfilter: nf_tables: release chain in flushing set (Florian Westphal) [1654259]
- [net] netfilter: xt_checksum: ignore gso skbs (Florian Westphal) [1654259]
- [net] netfilter: xt_cluster: add dependency on conntrack module (Florian Westphal) [1654259]
- [net] netfilter: fix memory leaks on netlink_dump_start error (Florian Westphal) [1654259]
- [net] netfilter: x_tables: do not fail xt_alloc_table_info too easilly (Florian Westphal) [1654259]
- [net] ipvs: fix race between ip_vs_conn_new() and ip_vs_del_dest() (Florian Westphal) [1654259]
- [net] netfilter: ip6t_rpfilter: set F_IFACE for linklocal addresses (Florian Westphal) [1654259]
- [net] xfrm: policy: use hlist rcu variants on insert (Sabrina Dubroca) [1657272]
- [net] xfrm: validate template mode (Sabrina Dubroca) [1657272]
- [net] xfrm: Fix NULL pointer dereference when skb_dst_force clears the dst_entry. (Sabrina Dubroca) [1657272]
- [net] xfrm: reset transport header back to network header after all input transforms ahave been applied (Sabrina Dubroca) [1657272]
- [net] xfrm: reset crypto_done when iterating over multiple input xfrms (Sabrina Dubroca) [1657272]
- [net] xfrm: Validate address prefix lengths in the xfrm selector. (Sabrina Dubroca) [1657272]
- [net] tls: fix currently broken MSG_PEEK behavior (Sabrina Dubroca) [1657225]
- [net] tls: zero the crypto information from tls_context before freeing (Sabrina Dubroca) [1657225]
- [net] tls: clear key material from kernel memory when do_tls_setsockopt_conf fails (Sabrina Dubroca) [1657225]
- [net] tls: don't copy the key out of tls12_crypto_info_aes_gcm_128 (Sabrina Dubroca) [1657225]
- [net] tls: Set count of SG entries if sk_alloc_sg returns -ENOSPC (Sabrina Dubroca) [1657225]
- [net] tls: possible hang when do_tcp_sendpages hits sndbuf is full case (Sabrina Dubroca) [1657225]
- [net] tls: Fix improper revert in zerocopy_from_iter (Sabrina Dubroca) [1657225]
- [net] tls: Fix zerocopy_from_iter iov handling (Sabrina Dubroca) [1657225]
- [net] netfilter: conntrack: reset tcp maxwin on re-register (Florian Westphal) [1647310]
- [net] configs: Enable CONFIG_IP_SET_HASH_IPMAC as a module (Stefano Brivio) [1655301]
- [net] udp: fix handling of CHECKSUM_COMPLETE packets (Paolo Abeni) [1655656]
- [net] udp: Unbreak modules that rely on external __skb_recv_udp() availability (Paolo Abeni) [1655656]
- [net] udp6: fix encap return code for resubmitting (Paolo Abeni) [1655656]
- [net] team: no need to do team_notify_peers or team_mcast_rejoin when disabling port (Hangbin Liu) [1653197]
- [net] sctp: not increase stream's incnt before sending addstrm_in request (Xin Long) [1651428]
- [net] sctp: not allow to set asoc prsctp_enable by sockopt (Xin Long) [1647272]
- [net] revert "sctp: remove sctp_transport_pmtu_check" (Xin Long) [1643330]
- [net] fix XPS static_key accounting (Ivan Vecera) [1651781]
- [net] restore call to netdev_queue_numa_node_write when resetting XPS (Ivan Vecera) [1651781]
- [net] allow fallback function to pass netdev (Ivan Vecera) [1651781]
- [net] allow ndo_select_queue to pass netdev (Ivan Vecera) [1651781]
- [net] Add generic ndo_select_queue functions (Ivan Vecera) [1651781]
- [net] Add support for subordinate traffic classes to netdev_pick_tx (Ivan Vecera) [1651781]
- [net] ixgbe: Add code to populate and use macvlan TC to Tx queue map (Ivan Vecera) [1651781]
- [net] Add support for subordinate device traffic classes (Ivan Vecera) [1651781]
- [net] net-sysfs: Drop support for XPS and traffic_class on single queue device (Ivan Vecera) [1651781]
- [net] Provide stub for __netif_set_xps_queue if there is no CONFIG_XPS (Ivan Vecera) [1651781]
- [net] allow to call netif_reset_xps_queues() under cpus_read_lock (Ivan Vecera) [1651781]
- [net] documentation: Add explanation for XPS using Rx-queue(s) map (Ivan Vecera) [1651781]
- [net] net-sysfs: Add interface for Rx queue(s) map per Tx queue (Ivan Vecera) [1651781]
- [net] Enable Tx queue selection based on Rx queues (Ivan Vecera) [1651781]
- [net] Record receive queue number for a connection (Ivan Vecera) [1651781]
- [net] sock: Change tx_queue_mapping in sock_common to unsigned short (Ivan Vecera) [1651781]
- [net] Use static_key for XPS maps (Ivan Vecera) [1651781]
- [net] Refactor XPS for CPUs and Rx queues (Ivan Vecera) [1651781]
- [net] devlink: Add helper function for safely copy string param (Ivan Vecera) [1647914]
- [net] devlink: Fix param cmode driverinit for string type (Ivan Vecera) [1647914]
- [net] devlink: Fix param set handling for string type (Ivan Vecera) [1647914]
- [net] devlink: Add Documentation/networking/devlink-params-bnxt.txt (Ivan Vecera) [1647914]
- [net] devlink: Add Documentation/networking/devlink-params.txt (Ivan Vecera) [1647914]
- [net] devlink: Add generic parameter msix_vec_per_pf_min (Ivan Vecera) [1647914]
- [net] devlink: Add generic parameter msix_vec_per_pf_max (Ivan Vecera) [1647914]
- [net] devlink: Add generic parameter ignore_ari (Ivan Vecera) [1647914]
- [net] devlink: double free in devlink_resource_fill() (Ivan Vecera) [1647914]
- [net] devlink: Add extack for eswitch operations (Ivan Vecera) [1647914]
- [net] devlink: Add generic parameters region_snapshot (Ivan Vecera) [1647914]
- [net] devlink: Add support for region snapshot read command (Ivan Vecera) [1647914]
- [net] devlink: Add support for region snapshot delete command (Ivan Vecera) [1647914]
- [net] devlink: Extend the support querying for region snapshot IDs (Ivan Vecera) [1647914]
- [net] devlink: Add support for region get command (Ivan Vecera) [1647914]
- [net] devlink: Add support for creating region snapshots (Ivan Vecera) [1647914]
- [net] devlink: Add callback to query for snapshot id before snapshot create (Ivan Vecera) [1647914]
- [net] devlink: Add support for creating and destroying regions (Ivan Vecera) [1647914]
- [net] devlink: fix incorrect return statement (Ivan Vecera) [1647914]
- [net] devlink: Add enable_sriov boolean generic parameter (Ivan Vecera) [1647914]
- [net] devlink: Add generic parameters internal_err_reset and max_macs (Ivan Vecera) [1647914]
- [net] devlink: Add devlink notifications support for params (Ivan Vecera) [1647914]
- [net] devlink: Add support for get/set driverinit value (Ivan Vecera) [1647914]
- [net] devlink: Add param set command (Ivan Vecera) [1647914]
- [net] devlink: Add param get command (Ivan Vecera) [1647914]
- [net] devlink: Add devlink_param register and unregister (Ivan Vecera) [1647914]
- [net] ipvs: call ip_vs_dst_notifier earlier than ipv6_dev_notf (Xin Long) [1645064]
- [net] ipv6: fix a dst leak when removing its exception (Xin Long) [1645064]
- [net] netfilter: ipset: list:set: Decrease refcount synchronously on deletion and replace (Stefano Brivio) [1649089]
- [net] bridge: remove ipv6 zero address check in mcast queries (Hangbin Liu) [1639666]
- [net] bridge: do not add port to router list when receives query with source 0.0.0.0 (Hangbin Liu) [1639666]
- [net] netfilter: ipv6: fix oops when defragmenting locally generated fragments (Florian Westphal) [1642341]
- [net] xfrm6: call kfree_skb when skb is toobig (Sabrina Dubroca) [1628851]
- [net] sched: act_police: fix memory leak in case of invalid control action (Ivan Vecera) [1638022]
- [net] sched: act_police: add missing spinlock initialization (Ivan Vecera) [1638022]
- [net] netfilter: xt_socket: check sk before checking for netns. (Ivan Vecera) [1638022]
- [net] sched: act_police: fix race condition on state variables (Ivan Vecera) [1638022]
- [net] sched: cls_flower: validate nested enc_opts_policy to avoid warning (Ivan Vecera) [1638022]
- [net] sched: act_pedit: fix memory leak when IDR allocation fails (Ivan Vecera) [1638022]
- [net] configs: disable CAKE, ETF & SKBPRIO qdisc in config (Ivan Vecera) [1638022]
- [net] tc-tests: test denial of 'goto chain' for exceed traffic in police.json (Ivan Vecera) [1638022]
- [net] tc-tests: test denial of 'goto chain' on 'random' traffic in gact.json (Ivan Vecera) [1638022]
- [net] sched: act_police: disallow 'goto chain' on fallback control action (Ivan Vecera) [1638022]
- [net] sched: act_gact: disallow 'goto chain' on fallback control action (Ivan Vecera) [1638022]
- [net] net_sched: fix a crash in tc_new_tfilter() (Ivan Vecera) [1638022]
- [net] core: make function ___gnet_stats_copy_basic() static (Ivan Vecera) [1638022]
- [net] net_sched: convert idrinfo->lock from spinlock to a mutex (Ivan Vecera) [1638022]
- [net] loopback: clear skb->tstamp before netif_rx() (Ivan Vecera) [1638022]
- [net] skbuff: preserve sock reference when scrubbing the skb. (Ivan Vecera) [1638022]
- [net] netfilter: check if the socket netns is correct. (Ivan Vecera) [1638022]
- [net] sched: make function qdisc_free_cb() static (Ivan Vecera) [1638022]
- [net] sched: use reference counting for tcf blocks on rules update (Ivan Vecera) [1638022]
- [net] sched: implement tcf_block_refcnt_{get|put}() (Ivan Vecera) [1638022]
- [net] sched: protect block idr with spinlock (Ivan Vecera) [1638022]
- [net] sched: implement functions to put and flush all chains (Ivan Vecera) [1638022]
- [net] sched: change tcf block reference counter type to refcount_t (Ivan Vecera) [1638022]
- [net] sched: use Qdisc rcu API instead of relying on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: add helper function to take reference to Qdisc (Ivan Vecera) [1638022]
- [net] sched: extend Qdisc with rcu (Ivan Vecera) [1638022]
- [net] sched: rename qdisc_destroy() to qdisc_put() (Ivan Vecera) [1638022]
- [net] core: netlink: add helper refcount dec and lock function (Ivan Vecera) [1638022]
- [net] sched: act_ipt: check for underflow in __tcf_ipt_init() (Ivan Vecera) [1638022]
- [net] sched: Add hardware specific counters to TC actions (Ivan Vecera) [1638022]
- [net] core: Add new basic hardware counter (Ivan Vecera) [1638022]
- [net] net_sched: change tcf_del_walker() to take idrinfo->lock (Ivan Vecera) [1638022]
- [net] sched: Use FIELD_SIZEOF directly instead of reimplementing its function (Ivan Vecera) [1638022]
- [net] sched: act_sample: fix NULL dereference in the data path (Ivan Vecera) [1638022]
- [net] sched: act_police: don't use spinlock in the data path (Ivan Vecera) [1638022]
- [net] sched: act_police: use per-cpu counters (Ivan Vecera) [1638022]
- [net] net_sched: notify filter deletion when deleting a chain (Ivan Vecera) [1638022]
- [net] htb: use anonymous union for simplicity (Ivan Vecera) [1638022]
- [net] net_sched: remove redundant qdisc lock classes (Ivan Vecera) [1638022]
- [net] sched: cls_flower: dump offload count value (Ivan Vecera) [1638022]
- [net] net_sched: properly cancel netlink dump on failure (Ivan Vecera) [1638022]
- [net] sched: fix memory leak in act_tunnel_key_init() (Ivan Vecera) [1638022]
- [net] sched: action_ife: take reference to meta module (Ivan Vecera) [1638022]
- [net] act_ife: fix a potential use-after-free (Ivan Vecera) [1638022]
- [net] sched: act_nat: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_skbedit: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: null actions array pointer before releasing action (Ivan Vecera) [1638022]
- [net] sched: fix type of htb statistics (Ivan Vecera) [1638022]
- [net] net_sched: add missing tcf_lock for act_connmark (Ivan Vecera) [1638022]
- [net] revert "net: sched: act: add extack for lookup callback" (Ivan Vecera) [1638022]
- [net] tc-testing: add test-cases for numeric and invalid control action (Ivan Vecera) [1638022]
- [net] net_sched: reject unknown tcfa_action values (Ivan Vecera) [1638022]
- [net] sched: act_pedit: fix dump of extended layered op (Ivan Vecera) [1638022]
- [net] sched: return -ENOENT when trying to remove filter from non-existent chain (Ivan Vecera) [1638022]
- [net] sched: fix extack error message when chain is failed to be created (Ivan Vecera) [1638022]
- [net] sched: Fix memory exposure from short TCA_U32_SEL (Ivan Vecera) [1638022]
- [net] net_sched: fix unused variable warning in stmmac (Ivan Vecera) [1638022]
- [net] sch_cake: Fix TC filter flow override and expand it to hosts as well (Ivan Vecera) [1638022]
- [net] sch_cake: Remove unused including <linux/version.h> (Ivan Vecera) [1638022]
- [net] act_ife: fix a potential deadlock (Ivan Vecera) [1638022]
- [net] act_ife: move tcfa_lock down to where necessary (Ivan Vecera) [1638022]
- [net] revert "net: sched: act_ife: disable bh when taking ife_mod_lock" (Ivan Vecera) [1638022]
- [net] net_sched: remove unused tcfa_capab (Ivan Vecera) [1638022]
- [net] net_sched: remove list_head from tc_action (Ivan Vecera) [1638022]
- [net] net_sched: remove unused tcf_idr_check() (Ivan Vecera) [1638022]
- [net] net_sched: remove unused parameter for tcf_action_delete() (Ivan Vecera) [1638022]
- [net] net_sched: remove unnecessary ops->delete() (Ivan Vecera) [1638022]
- [net] net_sched: improve and refactor tcf_action_put_many() (Ivan Vecera) [1638022]
- [net] sched: always disable bh when taking tcf_lock (Ivan Vecera) [1638022]
- [net] sched: act_ife: always release ife action on init error (Ivan Vecera) [1638022]
- [net] cls_matchall: fix tcf_unbind_filter missing (Ivan Vecera) [1638022]
- [net] sched: act_ife: disable bh when taking ife_mod_lock (Ivan Vecera) [1638022]
- [net] sched: act_mirred method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_vlan method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_skbmod method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_skbedit method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_simple method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_police method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_pedit method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_nat method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_ipt method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_gact method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_sum method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_bpf method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_connmark method rename for grep-ability and consistency (Ivan Vecera) [1638022]
- [net] sched: act_police: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] core: protect rate estimator statistics pointer with lock (Ivan Vecera) [1638022]
- [net] sched: act_mirred: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: extend action ops with put_dev callback (Ivan Vecera) [1638022]
- [net] sched: act_vlan: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_tunnel_key: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_skbmod: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_simple: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_sample: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_pedit: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_ipt: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_ife: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_gact: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_csum: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] sched: act_bpf: remove dependency on rtnl lock (Ivan Vecera) [1638022]
- [net] tc: Update README and add config (Ivan Vecera) [1638022]
- [net] sched: fix block->refcnt decrement (Ivan Vecera) [1638022]
- [net] tc-tests: initial version of nat action unit tests (Ivan Vecera) [1638022]
- [net] sched: allow flower to match tunnel options (Ivan Vecera) [1638022]
- [net] flow_dissector: allow dissection of tunnel options from metadata (Ivan Vecera) [1638022]
- [net] tc-testing: remove duplicate spaces in skbedit match patterns (Ivan Vecera) [1638022]
- [net] tc-testing: remove duplicate spaces in connmark match patterns (Ivan Vecera) [1638022]
- [net] tc-testing: flush gact actions on test teardown (Ivan Vecera) [1638022]
- [net] tc-testing: fix ip address in u32 test (Ivan Vecera) [1638022]
- [net] sched: cls_flower: Fix an error code in fl_tmplt_create() (Ivan Vecera) [1638022]
- [net] sched: fix flush on non-existing chain (Ivan Vecera) [1638022]
- [net] sched: make tcf_chain_{get, put}() static (Ivan Vecera) [1638022]
- [net] sched: fix notifications for action-held chains (Ivan Vecera) [1638022]
- [net] sched: change name of zombie chain to "held_by_acts_only" (Ivan Vecera) [1638022]
- [net] act_mirred: use TC_ACT_REINSERT when possible (Ivan Vecera) [1638022]
- [net] tc: introduce TC_ACT_REINSERT. (Ivan Vecera) [1638022]
- [net] tc/act: remove unneeded RCU lock in action callback (Ivan Vecera) [1638022]
- [net] sched: user-space can't set unknown tcfa_action values (Ivan Vecera) [1638022]
- [net] Add and use skb_mark_not_on_list(). (Ivan Vecera) [1638022]
- [net] sch_netem: Move private queue handler to generic location. (Ivan Vecera) [1638022]
- [net] sch_htb: Remove local SKB queue handling code. (Ivan Vecera) [1638022]
- [net] act_bpf: Use kmemdup instead of duplicating it in tcf_bpf_init_from_ops (Ivan Vecera) [1638022]
- [net] cls_bpf: Use kmemdup instead of duplicating it in cls_bpf_prog_from_ops (Ivan Vecera) [1638022]
- [net] act_pedit: remove unnecessary semicolon (Ivan Vecera) [1638022]
- [net] sched: don't dump chains only held by actions (Ivan Vecera) [1638022]
- [net] sch_cake: Make gso-splitting configurable from userspace (Ivan Vecera) [1638022]
- [net] sched: unmark chain as explicitly created on delete (Ivan Vecera) [1638022]
- [net] sched: cls_api: fix dead code in switch (Ivan Vecera) [1638022]
- [net] sched: cls_flower: Use correct inline function for assignment of vlan tpid (Ivan Vecera) [1638022]
- [net] sched: fix trailing whitespace (Ivan Vecera) [1638022]
- [net] cbs: Add support for the graft function (Ivan Vecera) [1638022]
- [net] sched: add skbprio scheduler (Ivan Vecera) [1638022]
- [net] selftests: forwarding: add tests for TC chain templates (Ivan Vecera) [1638022]
- [net] selftests: forwarding: add tests for TC chains creation adn destruction (Ivan Vecera) [1638022]
- [net] selftests: forwarding: move shblock tc support check to a separate helper (Ivan Vecera) [1638022]
- [net] sched: cls_flower: propagate chain teplate creation and destruction to drivers (Ivan Vecera) [1638022]
- [net] sched: cls_flower: implement chain templates (Ivan Vecera) [1638022]
- [net] sched: cls_flower: change fl_init_dissector to accept mask and dissector (Ivan Vecera) [1638022]
- [net] sched: cls_flower: move key/mask dumping into a separate function (Ivan Vecera) [1638022]
- [net] sched: introduce chain templates (Ivan Vecera) [1638022]
- [net] sched: introduce chain object to uapi (Ivan Vecera) [1638022]
- [net] sched: Avoid implicit chain 0 creation (Ivan Vecera) [1638022]
- [net] sched: push ops lookup bits into tcf_proto_lookup_ops() (Ivan Vecera) [1638022]
- [net] nfp: bring back support for offloading shared blocks (Ivan Vecera) [1638022]
- [net] sched: use PTR_ERR_OR_ZERO macro in tcf_block_cb_register (Ivan Vecera) [1638022]
- [net] tc-tests: initial version of fw filter unit tests (Ivan Vecera) [1638022]
- [net] sch_cake: Fix tin order when set through skb->priority (Ivan Vecera) [1638022]
- [net] sched: act_skbedit: don't use spinlock in the data path (Ivan Vecera) [1638022]
- [net] sched: skbedit: use per-cpu counters (Ivan Vecera) [1638022]
- [net] tc-testing: add geneve options in tunnel_key unit tests (Ivan Vecera) [1638022]
- [net] sched: fix unprotected access to rcu cookie pointer (Ivan Vecera) [1638022]
- [net] sched: act_ife: fix memory leak in ife init (Ivan Vecera) [1638022]
- [net] sched: refactor flower walk to iterate over idr (Ivan Vecera) [1638022]
- [net] sched: flower: Fix null pointer dereference when run tc vlan command (Ivan Vecera) [1638022]
- [net] sched: Fix warnings from xchg() on RCU'd cookie pointer. (Ivan Vecera) [1638022]
- [net] cls_flower: fix error values for commands not supported by drivers (Ivan Vecera) [1638022]
- [net] nfp: handle cls_flower command default case (Ivan Vecera) [1638022]
- [net] bnxt: simplify cls_flower command switch and handle default case (Ivan Vecera) [1638022]
- [net] sch_cake: Conditionally split GSO segments (Ivan Vecera) [1638022]
- [net] sch_cake: Add overhead compensation support to the rate shaper (Ivan Vecera) [1638022]
- [net] sch_cake: Add DiffServ handling (Ivan Vecera) [1638022]
- [net] sch_cake: Add NAT awareness to packet classifier (Ivan Vecera) [1638022]
- [net] netfilter: Add nf_ct_get_tuple_skb global lookup function (Ivan Vecera) [1638022]
- [net] sch_cake: Add optional ACK filter (Ivan Vecera) [1638022]
- [net] sch_cake: Add ingress mode (Ivan Vecera) [1638022]
- [net] sched: Add Common Applications Kept Enhanced (cake) qdisc (Ivan Vecera) [1638022]
- [net] Use __u32 in uapi net_stamp.h (Ivan Vecera) [1638022]
- [net] sched: flower: Add supprt for matching on QinQ vlan headers (Ivan Vecera) [1638022]
- [net] sched: flower: Dump the ethertype encapsulated in vlan (Ivan Vecera) [1638022]
- [net] flow_dissector: Add support for QinQ dissection (Ivan Vecera) [1638022]
- [net] sched: flower: Add support for matching on vlan ethertype (Ivan Vecera) [1638022]
- [net] flow_dissector: Save vlan ethertype from headers (Ivan Vecera) [1638022]
- [net] sched: change action API to use array of pointers to actions (Ivan Vecera) [1638022]
- [net] sched: atomically check-allocate action (Ivan Vecera) [1638022]
- [net] sched: use reference counting action init (Ivan Vecera) [1638022]
- [net] sched: don't release reference on action overwrite (Ivan Vecera) [1638022]
- [net] sched: implement reference counted action release (Ivan Vecera) [1638022]
- [net] sched: add 'delete' function to action ops (Ivan Vecera) [1638022]
- [net] sched: implement action API that deletes action by index (Ivan Vecera) [1638022]
- [net] sched: always take reference to action (Ivan Vecera) [1638022]
- [net] sched: implement unlocked action init API (Ivan Vecera) [1638022]
- [net] sched: change type of reference and bind counters (Ivan Vecera) [1638022]
- [net] sched: use rcu for action cookie update (Ivan Vecera) [1638022]
- [net] sched: Make etf report drops on error_queue (Ivan Vecera) [1638022]
- [net] sched: Add HW offloading capability to ETF (Ivan Vecera) [1638022]
- [net] sched: Introduce the ETF Qdisc (Ivan Vecera) [1638022]
- [net] sched: Allow creating a Qdisc watchdog with other clocks (Ivan Vecera) [1638022]
- [net] packet: Hook into time based transmission. (Ivan Vecera) [1638022]
- [net] ipv6: Hook into time based transmission (Ivan Vecera) [1638022]
- [net] ipv4: Hook into time based transmission (Ivan Vecera) [1638022]
- [net] Add a new socket option for a future transmit time. (Ivan Vecera) [1638022]
- [net] Clear skb->tstamp only on the forwarding path (Ivan Vecera) [1638022]
- [net] sched: act_pedit: fix possible memory leak in tcf_pedit_init() (Ivan Vecera) [1638022]
- [net] net sched actions: add extack messages in pedit action (Ivan Vecera) [1638022]
- [net] net:sched: add action inheritdsfield to skbedit (Ivan Vecera) [1638022]
- [net] tc-testing: initial version of tunnel_key unit tests (Ivan Vecera) [1638022]
- [net] net sched actions: avoid bitwise operation on signed value in pedit (Ivan Vecera) [1638022]
- [net] net sched actions: fix misleading text strings in pedit action (Ivan Vecera) [1638022]
- [net] net sched actions: use sizeof operator for buffer length (Ivan Vecera) [1638022]
- [net] net sched actions: fix sparse warning (Ivan Vecera) [1638022]
- [net] net sched actions: fix coding style in pedit headers (Ivan Vecera) [1638022]
- [net] net sched actions: fix coding style in pedit action (Ivan Vecera) [1638022]
- [net] netem: slotting with non-uniform distribution (Ivan Vecera) [1638022]
- [net] check tunnel option type in tunnel flags (Ivan Vecera) [1638022]
- [net] sched: act_tunnel_key: add extended ack support (Ivan Vecera) [1638022]
- [net] tc-tests: add an extreme-case csum action test (Ivan Vecera) [1638022]
- [net] net_sched: remove unused htb drop_list (Ivan Vecera) [1638022]

* Sun Dec 16 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-55.el8]
- [rpmspec] always run make with HOSTCFLAGS/HOSTLDFLAGS set (Jiri Olsa) [1624124]
- [rpmspec] Pass global build flags to tools build (Jiri Olsa) [1624124]
- [rpmspec] Pass global build flags to bpftool build (Jiri Olsa) [1624124]
- [kernel] kbuild: Use HOST*FLAGS options from the command line (Jiri Olsa) [1624124]
- [scripts] kbuild: Rename HOST_LOADLIBES to KBUILD_HOSTLDLIBS (Jiri Olsa) [1624124]
- [tools] kbuild: Rename HOSTLDFLAGS to KBUILD_HOSTLDFLAGS (Jiri Olsa) [1624124]
- [scripts] kbuild: Rename HOSTCXXFLAGS to KBUILD_HOSTCXXFLAGS (Jiri Olsa) [1624124]
- [tools] kbuild: Rename HOSTCFLAGS to KBUILD_HOSTCFLAGS (Jiri Olsa) [1624124]
- [tools] tools cpupower: Override CFLAGS assignments (Jiri Olsa) [1624124]
- [tools] tools cpupower debug: Allow to use outside build flags (Jiri Olsa) [1624124]
- [tools] perf tools: Pass build flags to traceevent build (Jiri Olsa) [1624124]
- [tools] tools lib traceevent: Use LDFLAGS in the build commands (Jiri Olsa) [1624124]
- [tools] perf tools: Link libperf-jvmti.so with LDFLAGS variable (Jiri Olsa) [1624124]
- [tools] bpftool: Allow add linker flags via EXTRA_LDFLAGS variable (Jiri Olsa) [1624124]
- [tools] bpftool: Allow to add compiler flags via EXTRA_CFLAGS variable (Jiri Olsa) [1624124]
- [block] blkcg: handle dying request_queue when associating a blkg (Ming Lei) [1655485]
- [block] block: deactivate blk_stat timer in wbt_disable_default() (Ming Lei) [1655485]
- [lib] sbitmap: flush deferred clears for resize and shallow gets (Ming Lei) [1655485]
- [md] dm: fix request-based dm's use of dm_wait_for_completion (Ming Lei) [1655485]
- [nvme] nvme: fix irq vs io_queue calculations (Ming Lei) [1655485]
- [md] dm: fix inflight IO check (Ming Lei) [1655485]
- [md] dm: remove the pending IO accounting (Ming Lei) [1655485]
- [block] block: return just one value from part_in_flight (Ming Lei) [1655485]
- [block] block: switch to per-cpu in-flight counters (Ming Lei) [1655485]
- [block] block: delete part_round_stats and switch to less precise counting (Ming Lei) [1655485]
- [block] block: stop passing 'cpu' to all percpu stats methods (Ming Lei) [1655485]
- [md] dm rq: leverage blk_mq_queue_busy() to check for outstanding IO (Ming Lei) [1655485]
- [md] dm: dont rewrite dm_disk(md)->part0.in_flight (Ming Lei) [1655485]
- [lib] sbitmap: silence bogus lockdep IRQ warning (Ming Lei) [1655485]
- [scsi] scsi: Fix a harmless double shift bug (Ming Lei) [1655485]
- [block] blk-mq: re-build queue map in case of kdump kernel (Ming Lei) [1655485]
- [block] blkcg: put back rcu lock in blkcg_bio_issue_check() (Ming Lei) [1655485]
- [block] block: convert io-latency to use rq_qos_wait (Ming Lei) [1655485]
- [block] block: convert wbt_wait() to use rq_qos_wait() (Ming Lei) [1655485]
- [block] block: add rq_qos_wait to rq_qos (Ming Lei) [1655485]
- [block] blkcg: rename blkg_try_get() to blkg_tryget() (Ming Lei) [1655485]
- [block] blkcg: change blkg reference counting to use percpu_ref (Ming Lei) [1655485]
- [block] blkcg: remove bio_disassociate_task() (Ming Lei) [1655485]
- [block] blkcg: remove additional reference to the css (Ming Lei) [1655485]
- [block] blkcg: remove bio->bi_css and instead use bio->bi_blkg (Ming Lei) [1655485]
- [block] blkcg: associate writeback bios with a blkg (Ming Lei) [1655485]
- [block] blkcg: associate a blkg for pages being evicted by swap (Ming Lei) [1655485]
- [block] blkcg: consolidate bio_issue_init() to be a part of core (Ming Lei) [1655485]
- [block] blkcg: associate blkg when associating a device (Ming Lei) [1655485]
- [block] dm: set the static flush bio device on demand (Ming Lei) [1655485]
- [block] blkcg: introduce common blkg association logic (Ming Lei) [1655485]
- [block] blkcg: convert blkg_lookup_create() to find closest blkg (Ming Lei) [1655485]
- [block] blkcg: update blkg_lookup_create() to do locking (Ming Lei) [1655485]
- [block] blkcg: fix ref count issue with bio_blkcg() using task_css (Ming Lei) [1655485]
- [block] blk-mq: remove QUEUE_FLAG_POLL from default MQ flags (Ming Lei) [1655485]
- [block] block: enable polling by default if a poll map is initalized (Ming Lei) [1655485]
- [block] block: only allow polling if a poll queue_map exists (Ming Lei) [1655485]
- [block] block: remove ->poll_fn (Ming Lei) [1655485]
- [nvme] nvme-mpath: remove I/O polling support (Ming Lei) [1655485]
- [nvme] nvme-rdma: remove I/O polling support (Ming Lei) [1655485]
- [nvme] nvme-pci: remove the CQ lock for interrupt driven queues (Ming Lei) [1655485]
- [nvme] nvme-pci: don't poll from irq context when deleting queues (Ming Lei) [1655485]
- [nvme] nvme-pci: refactor nvme_disable_io_queues (Ming Lei) [1655485]
- [nvme] nvme-pci: consolidate code for polling non-dedicated queues (Ming Lei) [1655485]
- [nvme] nvme-pci: only allow polling with separate poll queues (Ming Lei) [1655485]
- [nvme] nvme-pci: cleanup SQ allocation a bit (Ming Lei) [1655485]
- [nvme] nvme-pci: use atomic bitops to mark a queue enabled (Ming Lei) [1655485]
- [block] block: move queues types to the block layer (Ming Lei) [1655485]
- [fs] aio: clear IOCB_HIPRI (Ming Lei) [1655485]
- [lib] sbitmap: fix sbitmap_for_each_set() (Ming Lei) [1655485]
- [block] blk-mq: don't call ktime_get_ns() if we don't need it (Ming Lei) [1655485]
- [block] block: add cmd_flags to print_req_error (Ming Lei) [1655485]
- [lib] sbitmap: optimize wakeup check (Ming Lei) [1655485]
- [lib] sbitmap: ammortize cost of clearing bits (Ming Lei) [1655485]
- [block] block: avoid extra bio reference for async O_DIRECT (Ming Lei) [1655485]
- [lib] sbitmap: don't loop for find_next_zero_bit() for !round_robin (Ming Lei) [1655485]
- [block] blk-mq: use plug for devices that implement ->commits_rqs() (Ming Lei) [1655485]
- [block] blk-mq: use bd->last == true for list inserts (Ming Lei) [1655485]
- [block] ataflop: implement mq_ops->commit_rqs() hook (Ming Lei) [1655485]
- [block] virtio_blk: implement mq_ops->commit_rqs() hook (Ming Lei) [1655485]
- [nvme] nvme: implement mq_ops->commit_rqs() hook (Ming Lei) [1655485]
- [block] blk-mq: add mq_ops->commit_rqs() (Ming Lei) [1655485]
- [block] block: improve logic around when to sort a plug list (Ming Lei) [1655485]
- [block] blk-mq: Add a NULL check in blk_mq_free_map_and_requests() (Ming Lei) [1655485]
- [block] ataflop: fix error handling in atari_floppy_init() (Ming Lei) [1655485]
- [block] block: add io timeout to sysfs (Ming Lei) [1655485]
- [block] block: use rcu_work instead of call_rcu to avoid sleep in softirq (Ming Lei) [1655485]
- [block] blk-mq: fix failure to decrement plug count on single rq removal (Ming Lei) [1655485]
- [block] sunvdc: Do not spin in an infinite loop when vio_ldc_send() returns EAGAIN (Ming Lei) [1655485]
- [block] block: sum requests in the plug structure (Ming Lei) [1655485]
- [block] blk-mq: Simplify request completion state (Ming Lei) [1655485]
- [scsi] scsi: Do not rely on blk-mq for double completions (Ming Lei) [1655485]
- [block] blk-mq: Return true if request was completed (Ming Lei) [1655485]
- [block] blk-mq: never redirect polled IO completions (Ming Lei) [1655485]
- [block] blk-mq: ensure mq_ops ->poll() is entered at least once (Ming Lei) [1655485]
- [block] block: make blk_poll() take a parameter on whether to spin or not (Ming Lei) [1655485]
- [nvme] nvme: remove opportunistic polling from bdev target (Ming Lei) [1655485]
- [block] blk-mq: remove 'tag' parameter from mq_ops->poll() (Ming Lei) [1655485]
- [block] blk-mq: when polling for IO, look for any completion (Ming Lei) [1655485]
- [block] block: fix attempt to assign NULL io_context (Ming Lei) [1655485]
- [block] block: Initialize BIO I/O priority early (Ming Lei) [1655485]
- [block] block: prevent merging of requests with different priorities (Ming Lei) [1655485]
- [fs] aio: Fix fallback I/O priority value (Ming Lei) [1655485]
- [block] block: Introduce get_current_ioprio() (Ming Lei) [1655485]
- [block] block: Remove bio->bi_ioc (Ming Lei) [1655485]
- [fs] aio: Comment use of IOCB_FLAG_IOPRIO aio flag (Ming Lei) [1655485]
- [nvme] nvme-fc: remove ->poll implementation (Ming Lei) [1655485]
- [block] block: have ->poll_fn() return number of entries polled (Ming Lei) [1655485]
- [block] block: avoid ordered task state change for polled IO (Ming Lei) [1655485]
- [nvme] nvme: default to 0 poll queues (Ming Lei) [1655485]
- [block] floppy: remove now unused 'flags' variable (Ming Lei) [1655485]
- [mmc] mmc: stop abusing the request queue_lock pointer (Ming Lei) [1655485]
- [block] ide: don't acquire queue_lock in ide_complete_pm_rq (Ming Lei) [1655485]
- [block] ide: don't acquire queue lock in ide_pm_execute_rq (Ming Lei) [1655485]
- [block] pktcdvd: remove queue_lock around blk_queue_max_hw_sectors (Ming Lei) [1655485]
- [block] floppy: remove queue_lock around floppy_end_request (Ming Lei) [1655485]
- [block] block: remove the rq_alloc_data request_queue field (Ming Lei) [1655485]
- [block] block: don't plug for aio/O_DIRECT HIPRI IO (Ming Lei) [1655485]
- [block] block: for async O_DIRECT, mark us as polling if asked to (Ming Lei) [1655485]
- [block] block: add polled wakeup task helper (Ming Lei) [1655485]
- [block] blk-rq-qos: inline check for q->rq_qos functions (Ming Lei) [1655485]
- [block] block: add queue_is_mq() helper (Ming Lei) [1655485]
- [nvme] nvme: provide optimized poll function for separate poll queues (Ming Lei) [1655485]
- [block] ide: clear ide_req()->special for non-passthrough requests (Ming Lei) [1655485]
- [nvme] nvme: fix handling of EINVAL on pci_alloc_irq_vectors_affinity() (Ming Lei) [1655485]
- [block] block: add wbt_disable_default export for BFQ (Ming Lei) [1655485]
- [block] block: remove the queue_lock indirection (Ming Lei) [1655485]
- [block] block: remove the lock argument to blk_alloc_queue_node (Ming Lei) [1655485]
- [mmc] mmc: stop abusing the request queue_lock pointer (Ming Lei) [1655485]
- [mmc] mmc: simplify queue initialization (Ming Lei) [1655485]
- [block] umem: don't override the queue_lock (Ming Lei) [1655485]
- [block] drbd: don't override the queue_lock (Ming Lei) [1655485]
- [block] blk-cgroup: move locking into blkg_destroy_all (Ming Lei) [1655485]
- [block] blk-cgroup: consolidate error handling in blkcg_init_queue (Ming Lei) [1655485]
- [block] block: remove a few unused exports (Ming Lei) [1655485]
- [block] block: update a few comments for the legacy request removal (Ming Lei) [1655485]
- [block] block: remove the unused lock argument to rq_qos_throttle (Ming Lei) [1655485]
- [block] block: remove queue_lockdep_assert_held (Ming Lei) [1655485]
- [block] block: use atomic bitops for ->queue_flags (Ming Lei) [1655485]
- [block] block: don't hold the queue_lock over blk_abort_request (Ming Lei) [1655485]
- [block] block: remove deadline __deadline manipulation helpers (Ming Lei) [1655485]
- [block] block: remove QUEUE_FLAG_BYPASS and ->bypass (Ming Lei) [1655485]
- [nvme] nvmet-rdma: fix response use after free (Ming Lei) [1655485]
- [nvme] nvme: validate controller state before rescheduling keep alive (Ming Lei) [1655485]
- [block] block, bfq: fix decrement of num_active_groups (Ming Lei) [1655485]
- [ata] libata: whitelist all SAMSUNG MZ7KM* solid-state disks (Ming Lei) [1655485]
- [nvme] nvme-rdma: fix double freeing of async event data (Ming Lei) [1655485]
- [nvme] nvme-pci: fix surprise removal (Ming Lei) [1655485]
- [nvme] nvme: Free ctrl device name on init failure (Ming Lei) [1655485]
- [nvme] nvme-fc: resolve io failures during connect (Ming Lei) [1655485]
- [nvme] nvme: make sure ns head inherits underlying device limits (Ming Lei) [1655485]
- [nvme] nvmet: don't try to add ns to p2p map unless it actually uses it (Ming Lei) [1655485]
- [nvme] nvme-pci: fix conflicting p2p resource adds (Ming Lei) [1655485]
- [nvme] nvmet: Optionally use PCI P2P memory (Ming Lei) [1655485]
- [nvme] nvmet: Introduce helper functions to allocate and free request SGLs (Ming Lei) [1655485]
- [nvme] nvme-pci: Add support for P2P memory in requests (Ming Lei) [1655485]
- [nvme] nvme-pci: Use PCI p2pmem subsystem to manage the CMB (Ming Lei) [1655485]
- [infiniband] IB/core: Ensure we map P2P memory correctly in rdma_rw_ctx_[init|destroy]() (Ming Lei) [1655485]
- [block] block: Add PCI P2P flag for request queue (Ming Lei) [1655485]
- [documentation] PCI/P2PDMA: Add P2P DMA driver writer's documentation (Ming Lei) [1655485]
- [documentation] docs-rst: Add a new directory for PCI documentation (Ming Lei) [1655485]
- [pci] PCI/P2PDMA: Introduce configfs/sysfs enable attribute helpers (Ming Lei) [1655485]
- [pci] PCI/P2PDMA: Add PCI p2pmem DMA mappings to adjust the bus offset (Ming Lei) [1655485]
- [pci] PCI/P2PDMA: Add sysfs group to display p2pmem stats (Ming Lei) [1655485]
- [pci] PCI/P2PDMA: Support peer-to-peer memory (Ming Lei) [1655485]
- [nvme] nvmet-rdma: support max(16KB, PAGE_SIZE) inline data (Ming Lei) [1655485]
- [nvme] nvme-rdma: support up to 4 segments of inline data (Ming Lei) [1655485]
- [fs] aio: fix failure to put the file pointer (Ming Lei) [1655485]
- [lib] scsi: Remove percpu_ida (Ming Lei) [1655485]
- [scsi] scsi: target: Convert target drivers to use sbitmap (Ming Lei) [1655485]
- [scsi] scsi: target: Abstract tag freeing (Ming Lei) [1655485]
- [block] mmc: block: Fix unsupported parallel dispatch of requests (Ming Lei) [1655485]
- [scsi] scsi: target: sbitmap: add seq_file forward declaration (Ming Lei) [1655485]
- [mm] mm, memory_hotplug: do not clear numa_node association after hot_remove (Waiman Long) [1657422]
- [fs] iomap: partially revert 4721a601099 (simulated directio short read on EFAULT) (Brian Foster) [1654713]
- [fs] splice: don't read more than available pipe space (Brian Foster) [1654713]
- [fs] vfs: allow some remap flags to be passed to vfs_clone_file_range (Brian Foster) [1654713]
- [fs] xfs: fix inverted return from xfs_btree_sblock_verify_crc (Brian Foster) [1654713]
- [fs] xfs: fix PAGE_MASK usage in xfs_free_file_space (Brian Foster) [1654713]
- [fs] fs/xfs: fix f_ffree value for statfs when project quota is set (Brian Foster) [1654713]
- [fs] iomap: readpages doesn't zero page tail beyond EOF (Brian Foster) [1654713]
- [fs] vfs: vfs_dedupe_file_range() doesn't return EOPNOTSUPP (Brian Foster) [1654713]
- [fs] iomap: dio data corruption and spurious errors when pipes fill (Brian Foster) [1654713]
- [fs] iomap: sub-block dio needs to zeroout beyond EOF (Brian Foster) [1654713]
- [fs] iomap: FUA is wrong for DIO O_DSYNC writes into unwritten extents (Brian Foster) [1654713]
- [fs] xfs: delalloc -> unwritten COW fork allocation can go wrong (Brian Foster) [1654713]
- [fs] xfs: flush removing page cache in xfs_reflink_remap_prep (Brian Foster) [1654713]
- [fs] xfs: extent shifting doesn't fully invalidate page cache (Brian Foster) [1654713]
- [fs] xfs: finobt AG reserves don't consider last AG can be a runt (Brian Foster) [1654713]
- [fs] xfs: fix transient reference count error in xfs_buf_resubmit_failed_buffers (Brian Foster) [1654713]
- [fs] xfs: uncached buffer tracing needs to print bno (Brian Foster) [1654713]
- [fs] xfs: make xfs_file_remap_range() static (Brian Foster) [1654713]
- [fs] xfs: fix shared extent data corruption due to missing cow reservation (Brian Foster) [1654713]
- [fs] xfs: fix overflow in xfs_attr3_leaf_verify (Brian Foster) [1654713]
- [fs] xfs: print buffer offsets when dumping corrupt buffers (Brian Foster) [1654713]
- [fs] xfs: Fix error code in 'xfs_ioc_getbmap()' (Brian Foster) [1654713]
- [fs] xfs: cancel COW blocks before swapext (Brian Foster) [1654713]
- [fs] xfs: clear ail delwri queued bufs on unmount of shutdown fs (Brian Foster) [1654713]
- [fs] xfs: use offsetof() in place of offset macros for __xfsstats (Brian Foster) [1654713]
- [fs] xfs: Fix xqmstats offsets in /proc/fs/xfs/xqmstat (Brian Foster) [1654713]
- [fs] xfs: fix use-after-free race in xfs_buf_rele (Brian Foster) [1654713]
- [fs] xfs: Add attibute remove and helper functions (Brian Foster) [1654713]
- [fs] xfs: Add attibute set and helper functions (Brian Foster) [1654713]
- [fs] xfs: Add helper function xfs_attr_try_sf_addname (Brian Foster) [1654713]
- [fs] xfs: Move fs/xfs/xfs_attr.h to fs/xfs/libxfs/xfs_attr.h (Brian Foster) [1654713]
- [fs] xfs: issue log message on user force shutdown (Brian Foster) [1654713]
- [fs] xfs: fix buffer state management in xrep_findroot_block (Brian Foster) [1654713]
- [fs] xfs: always assign buffer verifiers when one is provided (Brian Foster) [1654713]
- [fs] xfs: xrep_findroot_block should reject root blocks with siblings (Brian Foster) [1654713]
- [fs] xfs: add a define for statfs magic to uapi (Brian Foster) [1654713]
- [fs] xfs: print dangling delalloc extents (Brian Foster) [1654713]
- [fs] xfs: fix fork selection in xfs_find_trim_cow_extent (Brian Foster) [1654713]
- [fs] xfs: remove the unused trimmed argument from xfs_reflink_trim_around_shared (Brian Foster) [1654713]
- [fs] xfs: remove the unused shared argument to xfs_reflink_reserve_cow (Brian Foster) [1654713]
- [fs] xfs: handle zeroing in xfs_file_iomap_begin_delay (Brian Foster) [1654713]
- [fs] xfs: remove suport for filesystems without unwritten extent flag (Brian Foster) [1654713]
- [fs] xfs: remove XFS_IO_INVALID (Brian Foster) [1654713]
- [fs] xfs: remove [cm]time update from reflink calls (Brian Foster) [1654713]
- [fs] xfs: remove xfs_reflink_remap_range (Brian Foster) [1654713]
- [fs] xfs: remove redundant remap partial EOF block checks (Brian Foster) [1654713]
- [fs] xfs: support returning partial reflink results (Brian Foster) [1654713]
- [fs] xfs: clean up xfs_reflink_remap_blocks call site (Brian Foster) [1654713]
- [fs] xfs: fix pagecache truncation prior to reflink (Brian Foster) [1654713]
- [fs] vfs: clean up generic_remap_file_range_prep return value (Brian Foster) [1654713]
- [fs] vfs: hide file range comparison function (Brian Foster) [1654713]
- [fs] vfs: enable remap callers that can handle short operations (Brian Foster) [1654713]
- [fs] vfs: plumb remap flags through the vfs dedupe functions (Brian Foster) [1654713]
- [fs] vfs: plumb remap flags through the vfs clone functions (Brian Foster) [1654713]
- [fs] vfs: make remap_file_range functions take and return bytes completed (Brian Foster) [1654713]
- [fs] vfs: remap helper should update destination inode metadata (Brian Foster) [1654713]
- [fs] vfs: pass remap flags to generic_remap_checks (Brian Foster) [1654713]
- [fs] vfs: pass remap flags to generic_remap_file_range_prep (Brian Foster) [1654713]
- [fs] vfs: combine the clone and dedupe into a single remap_file_range (Brian Foster) [1654713]
- [fs] vfs: rename clone_verify_area to remap_verify_area (Brian Foster) [1654713]
- [fs] vfs: rename vfs_clone_file_prep to be more descriptive (Brian Foster) [1654713]
- [fs] vfs: skip zero-length dedupe requests (Brian Foster) [1654713]
- [fs] vfs: avoid problematic remapping requests into partial EOF block (Brian Foster) [1654713]
- [fs] vfs: strengthen checking of file range inputs to generic_remap_checks (Brian Foster) [1654713]
- [fs] vfs: exit early from zero length remap operations (Brian Foster) [1654713]
- [fs] vfs: check file ranges before cloning files (Brian Foster) [1654713]
- [fs] vfs: vfs_clone_file_prep_inodes should return EINVAL for a clone from beyond EOF (Brian Foster) [1654713]
- [block] blk-mq: not embed .mq_kobj and ctx->kobj into queue instance (Ming Lei) [1653124]
- [fs] fs: fix lost error code in dio_complete (Ming Lei) [1655364]
- [iommu] iommu/iova: Optimise attempts to allocate iova from 32bit address range (Robert Richter) [1639202]

* Fri Dec 14 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-54.el8]
- [drm] drm/nouveau/drm/nouveau: Check rc from drm_dp_mst_topology_mgr_resume() (Lyude Paul) [1658810]
- [x86] Mark Intel Apollo Lake supported (David Arcari) [1653799]
- [infiniband] IB/mlx5: Fix implicit ODP interrupted page fault (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Improve ODP debugging messages (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Use multi threaded workqueue for page fault handling (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Return success for PAGE_FAULT_RESUME in internal error state (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Lock QP during page fault handling (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Enumerate page fault types (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Add interface to hold and release core resources (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Release resource on error flow (Alaa Hleihel) [1658085]
- [netdrv] net/mlx4_core: Correctly set PFC param if global pause is turned off. (Alaa Hleihel) [1658085]
- [netdrv] net/mlx4_en: Change min MTU size to ETH_MIN_MTU (Alaa Hleihel) [1658085]
- [netdrv] mlx5: fix get_ip_proto() (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Fix page fault handling for MW (Alaa Hleihel) [1658085]
- [infiniband] RDMA/mlx5: Initialize return variable in case pagefault was skipped (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Skip non-ODP MR when handling a page fault (Alaa Hleihel) [1658085]
- [net] net/dim: Update DIM start sample after each DIM iteration (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Avoid load failure due to unknown link width (Alaa Hleihel) [1658085]
- [infiniband] RDMA/mlx5: Fix fence type for IB_WR_LOCAL_INV WR (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Removed unnecessary warnings in FEC caps query (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Fix selftest for small MTUs (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: RX, verify received packet size in Linear Striding RQ (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Apply the correct check for supporting TC esw rules split (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Adjust to max number of channles when re-attaching (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Always use the match level enum when parsing TC rule match (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Claim TC hw offloads support only under a proper build config (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Don't match on vlan non-existence if ethertype is wildcarded (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: IPoIB, Reset QP after channels are closed (Alaa Hleihel) [1658085]
- [netdrv] net/mlx4: Fix UBSAN warning of signed integer overflow (Alaa Hleihel) [1658085]
- [netdrv] net/mlx4_core: Fix uninitialized variable compilation warning (Alaa Hleihel) [1658085]
- [netdrv] net/mlx4_core: Zero out lkey field in SW2HW_MPT fw command (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Fix MR cache initialization (Alaa Hleihel) [1658085]
- [infiniband] RDMA/mlx5: Remove extraneous error check (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Take only bit 24-26 of wqe.pftype_wq for page fault type (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Fix memory leak when setting fpga ipsec caps (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Unmap DMA addr from HCA before IOMMU (Alaa Hleihel) [1658085]
- [infiniband] RDMA/mlx5: Remove superfluous version print (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Allow transition of DCI QP to reset (Alaa Hleihel) [1658085]
- [infiniband] IB/mlx5: Don't hold spin lock while checking device state (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Move mlx5e_priv_flags into en_ethtool.c (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5: Fix atomic_mode enum values (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: Delete unneeded function argument (Alaa Hleihel) [1658085]
- [netdrv] net/mlx5e: RX, Prefetch the xdp_frame data area (Alaa Hleihel) [1658085]
- [drm] drm/i915: Synchronize hpd work in i915_hpd_storm_ctl_show() (Lyude Paul) [1658376]
- [drm] drm/i915: Add short HPD IRQ storm detection for non-MST systems (Lyude Paul) [1658376]
- [drm] drm/i915: Clarify flow for disabling IRQs on storms (Lyude Paul) [1658376]
- [drm] drm/i915: Fix threshold check in intel_hpd_irq_storm_detect() (Lyude Paul) [1658376]
- [drm] drm/i915: Fix NULL deref when re-enabling HPD IRQs on systems with MST (Lyude Paul) [1658376]
- [drm] drm/i915: Fix possible race in intel_dp_add_mst_connector() (Lyude Paul) [1658376]
- [x86] kvm: x86: bump KVM_(SOFT_)MAX_VCPUS to 384 (Radim Krcmar) [1635205]
- [block] blk-mq: punt failed direct issue to dispatch list (Ming Lei) [1656653]
- [block] blk-mq: fix corruption with direct issue (Ming Lei) [1656653]
- [pci] PCI: Add support for Immediate Readiness (Myron Stowe) [1483409]
- [x86] x86/PCI: Remove node-local allocation when initialising host controller (Myron Stowe) [1483409]
- [arm64] arm64: PCI: Remove node-local allocations when initialising host controller (Myron Stowe) [1483409]
- [cpufreq] cpufreq: intel_pstate: Add base_frequency attribute (Prarit Bhargava) [1648207]
- [acpi] ACPI / CPPC: Add support for guaranteed performance (Prarit Bhargava) [1648207]
- [block] block: fix single range discard merge (Ming Lei) [1654096]
- [scsi] SCSI: fix queue cleanup race before queue initialization is done (Ming Lei) [1642404]
- [netdrv] net: hinic: fix null pointer dereference on pointer hwdev (Xiaojun Tan) [1654207]
- [netdrv] net-next/hinic: fix a bug in rx data flow (Xiaojun Tan) [1654207]
- [netdrv] net-next/hinic:fix a bug in set mac address (Xiaojun Tan) [1654207]
- [netdrv] net-next/hinic:add rx checksum offload for HiNIC (Xiaojun Tan) [1654207]
- [netdrv] net-next/hinic:replace multiply and division operators (Xiaojun Tan) [1654207]
- [netdrv] hinic: Fix l4_type parameter in hinic_task_set_tunnel_l4 (Xiaojun Tan) [1654207]
- [netdrv] net-next/hinic: add checksum offload and TSO support (Xiaojun Tan) [1654207]
- [netdrv] cxgb4: Remove SGE_HOST_PAGE_SIZE dependency on page size (Arjun Vynipadath) [1651082]

* Thu Dec 13 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-53.el8]
- [x86] kvm: x86: Report STIBP on GET_SUPPORTED_CPUID (Eduardo Habkost) [1644870]
- [kernel] power: remove possible deadlock when unregistering power_supply (Benjamin Tissoires) [1657623]
- [md] dm: call blk_queue_split() to impose device limits on bios (Mike Snitzer) [1657340]
- [pinctrl] Revert "pinctrl: intel: Do pin translation when lock IRQ" (Benjamin Tissoires) [1658075]
- [pinctrl] pinctrl: cannonlake: Fix HOSTSW_OWN register offset of H variant (Benjamin Tissoires) [1658075]
- [pinctrl] pinctrl: intel: Do pin translation in other GPIO operations as well (Benjamin Tissoires) [1658075]
- [pinctrl] pinctrl: cannonlake: Fix gpio base for GPP-E (Benjamin Tissoires) [1658075]
- [pinctrl] pinctrl: intel: Don't shadow error code of gpiochip_lock_as_irq() (Benjamin Tissoires) [1658075]
- [pinctrl] pinctrl: cannonlake: Fix community ordering for H variant (Benjamin Tissoires) [1658075]
- [pinctrl] pinctrl: intel: Do pin translation when lock IRQ (Benjamin Tissoires) [1658075]
- [firmware] efi: Prevent GICv3 WARN() by mapping the memreserve table before first use (Bhupesh Sharma) [1638640]
- [firmware] efi: Permit calling efi_mem_reserve_persistent() from atomic context (Bhupesh Sharma) [1638640]
- [firmware] efi/arm: Defer persistent reservations until after paging_init() (Bhupesh Sharma) [1638640]
- [firmware] efi/arm: Revert deferred unmap of early memmap mapping (Bhupesh Sharma) [1638640]
- [arm64] arm64: memblock: don't permit memblock resizing until linear mapping is up (Bhupesh Sharma) [1638640]
- [arm64] arm64: Fix /proc/iomem for reserved but not memory regions (Bhupesh Sharma) [1638640]
- [tty] tty: wipe buffer. (Christoph von Recklinghausen) [1655051]
- [tty] tty: wipe buffer if not echoing data (Christoph von Recklinghausen) [1655051]

* Wed Dec 12 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-52.el8]
- [powerpc] powerpc/perf: Remove sched_task function defined for thread-imc (Steve Best) [1657153]
- [s390] Add reserved fields to mm_context_t (Philipp Rudo) [1656874]
- [s390] Add reserved fields to thread_struct (Philipp Rudo) [1656874]
- [documentation] kdump: correct crashkernel=auto threshold (Raghavendra Rao) [1656698]
- [fs] NFSv4.x: fix lock recovery during delegation recall (Steve Dickson) [1656410]
- [x86] x86/spec_ctrl: Synchronize RHEL8 percpu SPEC_CTRL MSR states with new STIBP logic (Waiman Long) [1655662]
- [x86] x86/speculation: Provide IBPB always command line options (Waiman Long) [1655662]
- [x86] x86/speculation: Add seccomp Spectre v2 user space protection mode (Waiman Long) [1655662]
- [x86] x86/speculation: Enable prctl mode for spectre_v2_user (Waiman Long) [1655662]
- [x86] x86/speculation: Add prctl() control for indirect branch speculation (Waiman Long) [1655662]
- [x86] x86/speculation: Prepare arch_smt_update() for PRCTL mode (Waiman Long) [1655662]
- [x86] x86/speculation: Prevent stale SPEC_CTRL msr content (Waiman Long) [1655662]
- [x86] x86/speculation: Split out TIF update (Waiman Long) [1655662]
- [x86] ptrace: Remove unused ptrace_may_access_sched() and MODE_IBRS (Waiman Long) [1655662]
- [x86] x86/speculation: Prepare for conditional IBPB in switch_mm() (Waiman Long) [1655662]
- [x86] x86/speculation: Avoid __switch_to_xtra() calls (Waiman Long) [1655662]
- [x86] x86/process: Consolidate and simplify switch_to_xtra() code (Waiman Long) [1655662]
- [x86] x86/speculation: Prepare for per task indirect branch speculation control (Waiman Long) [1655662]
- [x86] x86/speculation: Add command line control for indirect branch speculation (Waiman Long) [1655662]
- [x86] x86/speculation: Unify conditional spectre v2 print functions (Waiman Long) [1655662]
- [x86] x86/speculataion: Mark command line parser data __initdata (Waiman Long) [1655662]
- [x86] x86/speculation: Mark string arrays const correctly (Waiman Long) [1655662]
- [x86] x86/speculation: Reorder the spec_v2 code (Waiman Long) [1655662]
- [x86] x86/l1tf: Show actual SMT state (Waiman Long) [1655662]
- [x86] x86/speculation: Rework SMT state change (Waiman Long) [1655662]
- [x86] sched/smt: Expose sched_smt_present static key (Waiman Long) [1655662]
- [x86] x86/Kconfig: Select SCHED_SMT if SMP enabled (Waiman Long) [1655662]
- [x86] sched/smt: Make sched_smt_present track topology (Waiman Long) [1655662]
- [x86] x86/speculation: Reorganize speculation control MSRs update (Waiman Long) [1655662]
- [x86] x86/speculation: Rename SSBD update functions (Waiman Long) [1655662]
- [x86] x86/speculation: Disable STIBP when enhanced IBRS is in use (Waiman Long) [1655662]
- [x86] x86/speculation: Move STIPB/IBPB string conditionals out of cpu_show_common() (Waiman Long) [1655662]
- [x86] x86/speculation: Remove unnecessary ret variable in cpu_show_common() (Waiman Long) [1655662]
- [x86] x86/speculation: Clean up spectre_v2_parse_cmdline() (Waiman Long) [1655662]
- [x86] x86/speculation: Update the TIF_SSBD comment (Waiman Long) [1655662]
- [x86] x86/retpoline: Remove minimal retpoline support (Waiman Long) [1655662]
- [x86] x86/retpoline: Make CONFIG_RETPOLINE depend on compiler support (Waiman Long) [1655662]
- [x86] x86/spec_ctrl: Temporarily remove the IBRS code from process.c & bugs.c (Waiman Long) [1655662]
- [nvme] nvme: flush namespace scanning work just before removing namespaces (Ewan Milne) [1656028]
- [netdrv] i40e: Fix deletion of MAC filters (Stefan Assmann) [1646847]
- [scsi] mpt3sas: Display message on Configurable secure HBA (Tomas Henzl) [1649314]
- [scsi] scsi: mpt3sas: Add support for Aero controllers (Tomas Henzl) [1649314]
- [scsi] scsi: mpt3sas: Update MPI headers to support Aero controllers (Tomas Henzl) [1649314]
- [scsi] megaraid_sas: Add support for MegaRAID Aero controllers (Tomas Henzl) [1649384]
- [netdrv] nfp: flower: enabled offloading of Team LAG (Pablo Cascon) [1649876]
- [netdrv] net/mlx5: IPSec, Fix the SA context hash key (Alaa Hleihel) [1645857]
- [hwmon] hwmon/k10temp: Add support for AMD family 17h, model 30h CPUs (Gary Hook) [1640681]
- [x86] x86/amd_nb: Add PCI device IDs for family 17h, model 30h (Gary Hook) [1640681]
- [x86] x86/amd_nb: Add support for newer PCI topologies (Gary Hook) [1640681]
- [hwmon] hwmon/k10temp, x86/amd_nb: Consolidate shared device IDs (Gary Hook) [1640681]
- [net] tipc: fix info leak from kernel tipc_event (Jon Maloy) [1643279]
- [net] tipc: eliminate message disordering during binding table update (Jon Maloy) [1643279]
- [net] tipc: fix unsafe rcu locking when accessing publication list (Jon Maloy) [1643279]
- [net] tipc: queue socket protocol error messages into socket receive buffer (Jon Maloy) [1643279]
- [net] tipc: ignore STATE_MSG on wrong link session (Jon Maloy) [1643279]
- [net] tipc: fix failover problem (Jon Maloy) [1643279]
- [net] tipc: eliminate possible recursive locking detected by LOCKDEP (Jon Maloy) [1643279]
- [net] tipc: lock wakeup & inputq at tipc_link_reset() (Jon Maloy) [1643279]
- [net] tipc: reset bearer if device carrier not ok (Jon Maloy) [1643279]
- [net] tipc: fix flow control accounting for implicit connect (Jon Maloy) [1643279]
- [net] tipc: check return value of __tipc_dump_start() (Jon Maloy) [1643279]
- [net] tipc: call start and done ops directly in __tipc_nl_compat_dumpit() (Jon Maloy) [1643279]
- [net] tipc: orphan sock in tipc_release() (Jon Maloy) [1643279]
- [net] tipc: switch to rhashtable iterator (Jon Maloy) [1643279]
- [net] tipc: fix a missing rhashtable_walk_exit() (Jon Maloy) [1643279]
- [net] tipc: add missing dev_put() on error in tipc_enable_l2_media (Jon Maloy) [1643279]
- [net] tipc: initialize broadcast link stale counter correctly (Jon Maloy) [1643279]
- [net] tipc: set link tolerance correctly in broadcast link (Jon Maloy) [1643279]
- [net] tipc: extend link reset criteria for stale packet retransmission (Jon Maloy) [1643279]
- [crypto] crypto: ccp - Add support for new CCP/PSP device ID (Gary Hook) [1634201]
- [crypto] crypto: ccp - Support register differences between PSP devices (Gary Hook) [1634201]
- [crypto] crypto: ccp - Remove unused #defines (Gary Hook) [1634201]
- [crypto] crypto: ccp - Add psp enabled message when initialization succeeds (Gary Hook) [1634201]
- [crypto] crypto: ccp - Fix command completion detection race (Gary Hook) [1634201]
- [crypto] crypto: ccp - Check for NULL PSP pointer at module unload (Gary Hook) [1634201]
- [net] sctp: increase sk_wmem_alloc when head->truesize is increased (Xin Long) [1645419]
- [net] sctp: count sk_wmem_alloc by skb truesize in sctp_packet_transmit (Xin Long) [1645419]
- [net] ipv6: re-do dad when interface has IFF_NOARP flag change (Hangbin Liu) [1644594]
- [net] netfilter: nf_tables: don't skip inactive chains during update (Florian Westphal) [1643746]
- [net] inet: frags: better deal with smp races (Sabrina Dubroca) [1645397]
- [net] geneve, vxlan: Don't set exceptions if skb->len < mtu (Xin Long) [1642842]
- [net] geneve, vxlan: Don't check skb_dst() twice (Xin Long) [1642842]
- [net] sctp: fix strchange_flags name for Stream Change Event (Xin Long) [1641852]
- [net] sctp: update dst pmtu with the correct daddr (Xin Long) [1644478]
- [net] sctp: not free the new asoc when sctp_wait_for_connect returns err (Xin Long) [1644155]
- [net] l2tp: fix a sock refcnt leak in l2tp_tunnel_register (Xin Long) [1642749]
- [net] sctp: check policy more carefully when getting pr status (Xin Long) [1637786]
- [net] sctp: get pr_assoc and pr_stream all status with SCTP_PR_SCTP_ALL instead (Xin Long) [1637786]
- [net] ipv4/igmp: fix v1/v2 switchback timeout based on rfc3376, 8.12 (Hangbin Liu) [1638598]
- [net] netfilter: nft_compat: ebtables 'nat' table is normal chain type (Florian Westphal) [1645377]
- [net] sched: exclude TC from kABI guarantee (Ivan Vecera) [1628454]
- [net] netfilter: nft_set_rbtree: allow loose matching of closing element in interval (Phil Sutter) [1641993]
- [net] netfilter: xt_nat: fix DNAT target for shifted portmap ranges (Paolo Abeni) [1634258]
- [net] sched: Fix for duplicate class dump (Phil Sutter) [1631179]
- [x86] KVM: X86: Fix scan ioapic use-before-initialization (Bandan Das) [1653835] {CVE-2018-19407}

* Fri Dec 07 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-51.el8]
- [scsi] scsi: vmw_pscsi: Rearrange code to avoid multiple calls to free_irq during unload (Cathy Avery) [1590875]
- [netdrv] net/ibmvnic: Fix RTNL deadlock during device reset (Steve Best) [1656076]
- [s390] s390/qeth: fix length check in SNMP processing (Philipp Rudo) [1655612]
- [s390] s390/ism: clear dmbe_mask bit before SMC IRQ handling (Philipp Rudo) [1655611]
- [net] net/smc: use after free fix in smc_wr_tx_put_slot() (Philipp Rudo) [1655611]
- [net] net/smc: atomic SMCD cursor handling (Philipp Rudo) [1655611]
- [net] net/smc: add SMC-D shutdown signal (Philipp Rudo) [1655611]
- [net] net/smc: use queue pair number when matching link group (Philipp Rudo) [1655611]
- [net] net/smc: abort CLC connection in smc_release (Philipp Rudo) [1655611]
- [net] net/smc: unregister rkeys of unused buffer (Philipp Rudo) [1655611]
- [net] net/smc: add infrastructure to send delete rkey messages (Philipp Rudo) [1655611]
- [net] net/smc: avoid a delay by waiting for nothing (Philipp Rudo) [1655611]
- [net] net/smc: cleanup listen worker mutex unlocking (Philipp Rudo) [1655611]
- [net] net/smc: short wait for late smc_clc_wait_msg (Philipp Rudo) [1655611]
- [net] net/smc: no link delete for a never active link (Philipp Rudo) [1655611]
- [net] net/smc: allow fallback after clc timeouts (Philipp Rudo) [1655611]
- [net] net/smc: remove sock_error detour in clc-functions (Philipp Rudo) [1655611]
- [net] net/smc: make smc_lgr_free() static (Philipp Rudo) [1655611]
- [net] net/smc: cleanup tcp_listen_worker initialization (Philipp Rudo) [1655611]
- [net] net/smc: fix smc_buf_unuse to use the lgr pointer (Philipp Rudo) [1655611]
- [net] Revert "net: simplify sock_poll_wait" (Philipp Rudo) [1655611]
- [powerpc] powerpc/pseries: Fix unitialized timer reset on migration (Steve Best) [1655053]
- [powerpc] powerpc/pseries/mobility: Extend start/stop topology update scope (Steve Best) [1655053]
- [x86] Mark Intel Cascade Lake supported (Steve Best) [1641425]

* Wed Dec 05 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-50.el8]
- [x86] KVM: VMX: re-add ple_gap module parameter (Gary Hook) [1652953]
- [netdrv] tg3: Add PHY reset for 5717/5719/5720 in change ring and flow control paths (Steve Best) [1655515]
- [pci] PCI/ASPM: Do not initialize link state when aspm_disabled is set (Myron Stowe) [1655246]
- [pci] PCI/ACPI: Allow _OSC presence to be optional for PCI (Myron Stowe) [1655246]
- [pci] PCI/ACPI: Correct error message for ASPM disabling (Myron Stowe) [1655246]
- [pci] PCI/ASPM: Fix link_state teardown on device removal (Myron Stowe) [1655246]
- [netdrv] ice: Change req_speeds to be u16 (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix the bytecount sent to netdev_tx_sent_queue (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix tx_timeout in PF driver (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix napi delete calls for remove (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix typo in error message (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix flags for port VLAN (Jonathan Toppins) [1644403]
- [netdrv] ice: Remove duplicate addition of VLANs in replay path (Jonathan Toppins) [1644403]
- [netdrv] ice: Free VSI contexts during for unload (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix dead device link issue with flow control (Jonathan Toppins) [1644403]
- [netdrv] ice: Check for reset in progress during remove (Jonathan Toppins) [1644403]
- [netdrv] ice: Set carrier state and start/stop queues in rebuild (Jonathan Toppins) [1644403]
- [netdrv] virtchnl: Added support to exchange additional speed values (Jonathan Toppins) [1644403]
- [netdrv] ice: Poll for link status change (Jonathan Toppins) [1644403]
- [netdrv] ice: Allocate VF interrupts and set queue map (Jonathan Toppins) [1644403]
- [netdrv] ice: Introduce ice_dev_onetime_setup (Jonathan Toppins) [1644403]
- [netdrv] ice: Use capability count returned by the firmware (Jonathan Toppins) [1644403]
- [netdrv] ice: Update expected FW version (Jonathan Toppins) [1644403]
- [netdrv] ice: Change device ID define names to align with branding string (Jonathan Toppins) [1644403]
- [netdrv] ice: Make ice_msix_clean_rings static (Jonathan Toppins) [1644403]
- [netdrv] ice: Update version string (Jonathan Toppins) [1644403]
- [netdrv] ice: Use the right function to enable/disable VSI (Jonathan Toppins) [1644403]
- [netdrv] ice: Add more flexibility on how we assign an ITR index (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix potential null pointer issues (Jonathan Toppins) [1644403]
- [netdrv] ice: Add code to go from ICE_FWD_TO_VSI_LIST to ICE_FWD_TO_VSI (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix forward to queue group logic (Jonathan Toppins) [1644403]
- [netdrv] ice: Extend malicious operations detection logic (Jonathan Toppins) [1644403]
- [netdrv] ice: Notify VF of link status change (Jonathan Toppins) [1644403]
- [netdrv] ice: Implement virtchnl commands for AVF support (Jonathan Toppins) [1644403]
- [netdrv] ice: Add handlers for VF netdevice operations (Jonathan Toppins) [1644403]
- [netdrv] ice: Add support for VF reset events (Jonathan Toppins) [1644403]
- [netdrv] ice: Update VSI and queue management code to handle VF VSI (Jonathan Toppins) [1644403]
- [netdrv] ice: Add handler to configure SR-IOV (Jonathan Toppins) [1644403]
- [netdrv] ice: Add support to detect SR-IOV capability and mailbox queues (Jonathan Toppins) [1644403]
- [netdrv] ice: Fix error on driver remove (Jonathan Toppins) [1644403]
- [netdrv] ice: Add support for dynamic interrupt moderation (Jonathan Toppins) [1644403]
- [netdrv] ice: Align ice_reset_req enum values to hardware reset values (Jonathan Toppins) [1644403]
- [netdrv] ice: Implement ethtool hook for RSS switch (Jonathan Toppins) [1644403]
- [netdrv] ice: Split irq_tracker into sw_irq_tracker and hw_irq_tracker (Jonathan Toppins) [1644403]
- [netdrv] ice: Check for actual link state of port after reset (Jonathan Toppins) [1644403]
- [netdrv] ice: Implement VSI replay framework (Jonathan Toppins) [1644403]
- [netdrv] ice: Expand use of VSI handles part 2/2 (Jonathan Toppins) [1644403]
- [netdrv] ice: Expand use of VSI handles part 1/2 (Jonathan Toppins) [1644403]
- [netdrv] ice: Change pf state behavior to protect reset path (Jonathan Toppins) [1644403]
- [netdrv] ice: Move common functions out of ice_main.c part 7/7 (Jonathan Toppins) [1644403]
- [netdrv] ice: Move common functions out of ice_main.c part 6/7 (Jonathan Toppins) [1644403]
- [netdrv] ice: Move common functions out of ice_main.c part 5/7 (Jonathan Toppins) [1644403]
- [netdrv] ice: Move common functions out of ice_main.c part 4/7 (Jonathan Toppins) [1644403]
- [netdrv] ice: Move common functions out of ice_main.c part 3/7 (Jonathan Toppins) [1644403]
- [netdrv] ice: Move common functions out of ice_main.c part 2/7 (Jonathan Toppins) [1644403]
- [netdrv] ice: Move common functions out of ice_main.c part 1/7 (Jonathan Toppins) [1644403]
- [netdrv] ice: fix changing of ring descriptor size (ethtool -G) (Jonathan Toppins) [1644403]
- [netdrv] ice: Update to capabilities admin queue command (Jonathan Toppins) [1644403]
- [netdrv] ice: Query the Tx scheduler node before adding it (Jonathan Toppins) [1644403]
- [netdrv] ice: Update comment for ice_fltr_mgmt_list_entry (Jonathan Toppins) [1644403]
- [netdrv] ice: update fw version check logic (Jonathan Toppins) [1644403]
- [netdrv] ice: update branding strings and supported device ids (Jonathan Toppins) [1644403]
- [netdrv] ice: replace unnecessary memcpy with direct assignment (Jonathan Toppins) [1644403]
- [netdrv] ice: use [sr]q.count when checking if queue is initialized (Jonathan Toppins) [1644403]
- [netdrv] ice: remove ndo_poll_controller (Jonathan Toppins) [1644403]
- [fs] fanotify: fix handling of events on child sub-directory (Miklos Szeredi) [1652432]
- [fs] fsnotify: generalize handling of extra event flags (Miklos Szeredi) [1652432]
- [netdrv] net: hns3: add common validation in hclge_dcb (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: fix for multiple unmapping DMA problem (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: rename hns_nic_dma_unmap (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: add handling for big TX fragment (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: move DMA map into hns3_fill_desc (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: remove hns3_fill_desc_tso (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Resume promisc mode and vlan filter status after loopback test (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Resume promisc mode and vlan filter status after reset (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Enable promisc mode when mac vlan table is full (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for rx vlan id handle to support Rev 0x21 hardware (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Add egress/ingress vlan filter for revision 0x21 (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Optimize for unicast mac vlan table (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix loss of coal configuration while doing reset (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Modify hns3_get_max_available_channels (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Change return type of hclge_tm_schd_info_update() (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for netdev not up problem when setting mtu (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for packet buffer setting bug (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Set extra mac address of pause param for HW (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix speed/duplex information loss problem when executing ethtool ethx cmd of VF (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Add get_media_type ops support for VF (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Remove print messages for error packet (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Add nic state check before calling netif_tx_wake_queue (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Add handle for default case (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Unify the prefix of vf functions (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix tqp array traversal condition for vf (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix ets validate issue (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix parameter type for q_id in hclge_tm_q_to_qs_map_cfg() (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix client initialize state issue when roce client initialize failed (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Clear client pointer when initialize client failed or unintialize finished (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix cmdq registers initialization issue for vf (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for setting speed for phy failed problem (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Check hdev state when getting link status (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Set STATE_DOWN bit of hdev state when stopping net (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Remove packet statistics of public (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Remove tx budget to clean more TX descriptors in a napi (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Refine hns3_get_link_ksettings() (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Remove redundant codes of query advertised flow control abilitiy (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Change the dst mac addr of loopback packet (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Only update mac configuation when necessary (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Preserve vlan 0 in hardware table (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix ping exited problem when doing lp selftest (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for loopback selftest failed problem (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix error of checking used vlan id (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for multicast failure (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for vf vlan delete failed problem (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: modify variable type in hns3_nic_reuse_page (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Add vlan filter setting by ethtool command -K (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Set tx ring' tc info when netdev is up (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix desc num set to default when setting channel (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for information of phydev lost problem when down/up (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Add support for serdes loopback selftest (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Refine the MSIX allocation for PF (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix MSIX allocation issue for VF (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: fix return value error while hclge_cmd_csq_clean failed (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Modify inconsistent bit mask macros (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for using wrong mask and shift in hclge_get_ring_chain_from_mbx (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Correct reset event status register (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Prevent to request reset frequently (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Prevent sending command during global or core reset (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Add configure for mac minimal frame size (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for l4 checksum offload bug (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix for waterline not setting correctly (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: Fix tc setup when netdev is first up (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: modify hnae_ to hnae3_ (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: simplify hclge_cmd_csq_clean (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: remove some redundant assignments (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: remove back in struct hclge_hw (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: add unlikely for error check (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: add l4_type check for both ipv4 and ipv6 (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: add vector status check before free vector (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: rename the interface for init_client_instance and uninit_client_instance (Xiaojun Tan) [1640945]
- [netdrv] net: hns3: remove hclge_get_vector_index from hclge_bind_ring_with_vector (Xiaojun Tan) [1640945]
- [kernel] redhat: Enable -Werror for architectures (Laura Abbott) [1582754]
- [drm] drm/atomic_helper: Remove dangling variable (Laura Abbott) [1582754]
- [s390] s390/tools: fix gcc 8 stringop-truncation warnings (Laura Abbott) [1582754]
- [tty] kgdboc: Fix restrict error (Laura Abbott) [1582754]
- [misc] misc: kgdbts: Fix restrict error (Laura Abbott) [1582754]
- [scsi] scsi: ibmvscsis: Fix a stringop-overflow warning (Laura Abbott) [1582754]
- [s390] s390/extmem: fix gcc 8 stringop-overflow warning (Laura Abbott) [1582754]
- [s390] s390/perf: fix gcc 8 array-bounds warning (Laura Abbott) [1582754]
- [kernel] kdb: Use strscpy with destination buffer size (Laura Abbott) [1582754]
- [fs] configfs: replace strncpy with memcpy (Laura Abbott) [1582754]
- [fs] kernfs: Replace strncpy with memcpy (Laura Abbott) [1582754]
- [kernel] disable stringop truncation warnings for now (Laura Abbott) [1582754]
- [sound] ALSA: intel_hdmi: Use strlcpy() instead of strncpy() (Laura Abbott) [1582754]
- [sound] ALSA: trident: Suppress gcc string warning (Laura Abbott) [1582754]
- [lib] kobject: Replace strncpy with memcpy (Laura Abbott) [1582754]
- [tty] TTY: isdn: Replace strncpy with memcpy (Laura Abbott) [1582754]
- [target] scsi: target/iscsi: Make iscsit_ta_authentication() respect the output buffer size (Laura Abbott) [1582754]
- [fs] fuse: don't need GETATTR after every READ (Miklos Szeredi) [1650538]
- [fs] fuse: allow fine grained attr cache invaldation (Miklos Szeredi) [1650538]

* Tue Dec 04 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-49.el8]
- [mm] mm: mremap: properly flush TLB before releasing the page (Rafael Aquini) [1645122] {CVE-2018-18281}
- [x86] x86/spec_ctrl: Change default Skylake Spectre v2 mitigation to retpoline (Waiman Long) [1651806]
- [fs] gfs2: write revokes should traverse sd_ail1_list in reverse (Andreas Grunbacher) [1652763]
- [fs] gfs2: Fix marking bitmaps non-full (Andreas Grunbacher) [1652762]
- [fs] GFS2: Flush the GFS2 delete workqueue before stopping the kernel threads (Andreas Grunbacher) [1652761]
- [fs] gfs2: Don't leave s_fs_info pointing to freed memory in init_sbd (Andreas Grunbacher) [1652759]
- [fs] gfs2: Use fs_* functions instead of pr_* function where we can (Andreas Grunbacher) [1652757]
- [fs] gfs2: slow the deluge of io error messages (Andreas Grunbacher) [1652757]
- [fs] gfs2_meta: ->mount() can get NULL dev_name (Andreas Grunbacher) [1652754]
- [powerpc] powerpc/vdso: Correct call frame information (Steve Best) [1651281]
- [i2c] i2c: i801: Add support for Intel Ice Lake (David Arcari) [1637435]
- [usb] xhci: Add quirk to workaround the errata seen on Cavium Thunder-X2 Soc (Robert Richter) [1649829]
- [x86] x86: numa_emulation: fix uniform-split numa emulation (Rafael Aquini) [1620341]
- [x86] x86: numa_emulation: introduce uniform split capability (Rafael Aquini) [1620341]
- [kernel] perf/hw_breakpoint: Modify breakpoint even if the new attr has disabled set (Mark Salter) [1643174]
- [x86] KVM: vmx: hyper-v: don't pass EPT configuration info to vmx_hv_remote_flush_tlb() (Paolo Bonzini) [1636610]
- [x86] KVM: x86: support CONFIG_KVM_AMD=y with CONFIG_CRYPTO_DEV_CCP_DD=m (Paolo Bonzini) [1636610]
- [x86] kvm: nVMX: fix entry with pending interrupt if APICv is enabled (Paolo Bonzini) [1636610]
- [x86] KVM: VMX: hide flexpriority from guest when disabled at the module level (Paolo Bonzini) [1636610]
- [x86] KVM: VMX: check for existence of secondary exec controls before accessing (Paolo Bonzini) [1636610]
- [x86] KVM: x86: fix L1TF's MMIO GFN calculation (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: cut down decimal places in update interval dialog (Paolo Bonzini) [1636610]
- [x86] KVM: nVMX: Fix emulation of VM_ENTRY_LOAD_BNDCFGS (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Do not use kvm_x86_ops->mpx_supported() directly (Paolo Bonzini) [1636610]
- [x86] KVM: nVMX: Do not expose MPX VMX controls when guest MPX disabled (Paolo Bonzini) [1636610]
- [x86] KVM: x86: never trap MSR_KERNEL_GS_BASE (Paolo Bonzini) [1636610]
- [x86] KVM: LAPIC: Fix pv ipis out-of-bounds access (Paolo Bonzini) [1636610]
- [x86] KVM: nVMX: Fix loss of pending IRQ/NMI before entering L2 (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: re-animate display of dead guests (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: indicate dead guests as such (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: handle guest removals more gracefully (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: don't reset stats when setting PID filter for debugfs (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: fix updates for dead guests (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: fix handling of invalid paths in debugfs provider (Paolo Bonzini) [1636610]
- [tools] tools/kvm_stat: fix python3 issues (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Unexport x86_emulate_instruction() (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Rename emulate_instruction() to kvm_emulate_instruction() (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Do not re-{try, execute} after failed emulation in L2 (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Default to not allowing emulation retry in kvm_mmu_page_fault (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Merge EMULTYPE_RETRY and EMULTYPE_ALLOW_REEXECUTE (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Invert emulation re-execute behavior to make it opt-in (Paolo Bonzini) [1636610]
- [x86] KVM: x86: SVM: Set EMULTYPE_NO_REEXECUTE for RSM emulation (Paolo Bonzini) [1636610]
- [x86] KVM: VMX: Do not allow reexecute_instruction() when skipping MMIO instr (Paolo Bonzini) [1636610]
- [x86] KVM: SVM: remove unused variable dst_vaddr_end (Paolo Bonzini) [1636610]
- [x86] KVM: nVMX: avoid redundant double assignment of nested_run_pending (Paolo Bonzini) [1636610]
- [x86] KVM: nVMX: Fix bad cleanup on error of get/set nested state IOCTLs (Paolo Bonzini) [1636610]
- [tools] kvm: selftests: Add platform_info_test (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Control guest reads of MSR_PLATFORM_INFO (Paolo Bonzini) [1636610]
- [x86] KVM: x86: Turbo bits in MSR_PLATFORM_INFO (Paolo Bonzini) [1636610]
- [x86] nVMX x86: Check VPID value on vmentry of L2 guests (Paolo Bonzini) [1636610]
- [x86] nVMX x86: check posted-interrupt descriptor addresss on vmentry of L2 (Paolo Bonzini) [1636610]
- [x86] KVM: nVMX: Wake blocked vCPU in guest-mode if pending interrupt in virtual APICv (Paolo Bonzini) [1636610]
- [x86] KVM: VMX: check nested state and CR4.VMXE against SMM (Paolo Bonzini) [1636610]
- [x86] kvm: x86: make kvm_{load|put}_guest_fpu() static (Paolo Bonzini) [1636610]
- [x86] x86/hyper-v: rename ipi_arg_{ex, non_ex} structures (Paolo Bonzini) [1636610]
- [x86] KVM: VMX: use preemption timer to force immediate VMExit (Paolo Bonzini) [1636610]
- [x86] KVM: VMX: modify preemption timer bit only when arming timer (Paolo Bonzini) [1636610]
- [x86] KVM: VMX: immediately mark preemption timer expired only for zero value (Paolo Bonzini) [1636610]
- [x86] KVM: SVM: Switch to bitmap_zalloc() (Paolo Bonzini) [1636610]
- [lib] bitmap: Add bitmap_alloc(), bitmap_zalloc() and bitmap_free() (Paolo Bonzini) [1636610]
- [x86] KVM/MMU: Fix comment in walk_shadow_page_lockless_end() (Paolo Bonzini) [1636610]
- [tools] kvm: selftests: use -pthread instead of -lpthread (Paolo Bonzini) [1636610]
- [tools] kvm: selftest: add dirty logging test (Paolo Bonzini) [1636610]
- [tools] kvm: selftest: pass in extra memory when create vm (Paolo Bonzini) [1636610]
- [tools] kvm: selftest: include the tools headers (Paolo Bonzini) [1636610]
- [tools] kvm: selftest: unify the guest port macros (Paolo Bonzini) [1636610]
- [x86] KVM: x86: don't reset root in kvm_mmu_setup() (Paolo Bonzini) [1636610]
- [x86] kvm: mmu: Don't read PDPTEs when paging is not enabled (Paolo Bonzini) [1636610]
- [x86] x86/kvm/lapic: always disable MMIO interface in x2APIC mode (Paolo Bonzini) [1636610]
- [s390] KVM: s390: Make huge pages unavailable in ucontrol VMs (Paolo Bonzini) [1636610]
- [s390] s390/mm: Check for valid vma before zapping in gmap_discard (Paolo Bonzini) [1636610]
- [tools] selftests: add headers_install to lib.mk (Paolo Bonzini) [1636610]
- [tools] selftests: kselftest: Remove outdated comment (Paolo Bonzini) [1636610]
- [tools] selftests: android: move config up a level (Paolo Bonzini) [1636610]
- [md] md: Avoid namespace collision with bitmap API (Paolo Bonzini) [1636610]

* Fri Nov 30 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-48.el8]
- [cpufreq] cpufreq / CPPC: Add cpuinfo_cur_freq support for CPPC (Prarit Bhargava) [1654361]
- [netdrv] nfp: flower: add ipv6 set flow label and hop limit offload (Pablo Cascon) [1651639]
- [netdrv] nfp: flower: add ipv4 set ttl and tos offload (Pablo Cascon) [1651639]
- [netdrv] ibmvnic: Update driver queues after change in ring size support (Steve Best) [1651947]
- [netdrv] ibmvnic: Fix RX queue buffer cleanup (Steve Best) [1651947]
- [netdrv] net/ibmnvic: Fix deadlock problem in reset (Steve Best) [1651947]
- [netdrv] ibmvnic: fix accelerated VLAN handling (Steve Best) [1651947]
- [netdrv] ibmvnic: Add ethtool private flag for driver-defined queue limits (Steve Best) [1651947]
- [netdrv] ibmvnic: Introduce driver limits for ring sizes (Steve Best) [1651947]
- [netdrv] ibmvnic: Increase maximum queue size limit (Steve Best) [1651947]
- [netdrv] ibmvnic: remove ndo_poll_controller (Steve Best) [1651947]
- [powerpc] powerpc/powernv/npu: Remove atsd_threshold debugfs setting (Steve Best) [1653661]
- [powerpc] powerpc/powernv/npu: Use size-based ATSD invalidates (Steve Best) [1653661]
- [powerpc] powerpc/powernv/npu: Reduce eieio usage when issuing ATSD invalidates (Steve Best) [1653661]
- [powerpc] powerpc/powernv/npu: Add a debugfs setting to change ATSD threshold (Steve Best) [1653661]
- [net] libceph: fall back to sendmsg for slab pages (Ilya Dryomov) [1653395]
- [s390] s390/qeth: utilize virtual MAC for Layer2 OSD devices (Philipp Rudo) [1653246]
- [fs] vfs: fix FIGETBSZ ioctl on an overlayfs file (Miklos Szeredi) [1651362]
- [fs] ovl: fix decode of dir file handle with multi lower layers (Miklos Szeredi) [1651362]
- [fs] ovl: fix missing override creds in link of a metacopy upper (Miklos Szeredi) [1651362]
- [fs] ovl: automatically enable redirect_dir on metacopy=on (Miklos Szeredi) [1651362]
- [fs] ovl: check whiteout in ovl_create_over_whiteout() (Miklos Szeredi) [1651362]
- [fs] ovl: fix recursive oi->lock in ovl_link() (Miklos Szeredi) [1651362]
- [fs] ovl: fix error handling in ovl_verify_set_fh() (Miklos Szeredi) [1651362]
- [mm] mm, memory_hotplug: check zone_movable in has_unmovable_pages (Baoquan He) [1643839]
- [netdrv] hv_netvsc: fix vf serial matching with pci slot info (Vitaly Kuznetsov) [1637519]
- [netdrv] hv_netvsc: remove ndo_poll_controller (Vitaly Kuznetsov) [1637519]
- [netdrv] hv_netvsc: pair VF based on serial number (Vitaly Kuznetsov) [1637519]
- [netdrv] hv_netvsc: fix schedule in RCU context (Vitaly Kuznetsov) [1637519]
- [pci] PCI: hv: Fix return value check in hv_pci_assign_slots() (Vitaly Kuznetsov) [1637519]
- [pci] PCI: hv: support reporting serial number as slot information (Vitaly Kuznetsov) [1637519]
- [pci] PCI: hv: Replace GFP_ATOMIC with GFP_KERNEL in new_pcichild_device() (Vitaly Kuznetsov) [1637519]
- [char] ipmi: Fix timer race with module unload (Robert Richter) [1649812]
- [arm64] arm64: hugetlb: Avoid unnecessary clearing in huge_ptep_set_access_flags (Christoph von Recklinghausen) [1635192]
- [arm64] arm64: hugetlb: Fix handling of young ptes (Christoph von Recklinghausen) [1635192]
- [mm] mm: Preserve _PAGE_DEVMAP across mprotect() calls (Jeff Moyer) [1647647]

* Thu Nov 29 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-47.el8]
- [crypto] crypto: vmx - Fix sleep-in-atomic bugs (Steve Best) [1653662]
- [netdrv] net: ena: update driver version from 2.0.1 to 2.0.2 (John Linville) [1634044]
- [netdrv] net: ena: fix crash during ena_remove() (John Linville) [1634044]
- [netdrv] net: ena: fix crash during failed resume from hibernation (John Linville) [1634044]
- [netdrv] net: ena: enable CONFIG_ENA_ETHERNET for aarch64 (John Linville) [1634044]
- [netdrv] net: ena: enable Low Latency Queues (John Linville) [1634044]
- [netdrv] net: ena: Fix Kconfig dependency on X86 (John Linville) [1634044]
- [netdrv] net: ena: fix indentations in ena_defs for better readability (John Linville) [1634044]
- [netdrv] net: ena: update driver version to 2.0.1 (John Linville) [1634044]
- [netdrv] net: ena: remove redundant parameter in ena_com_admin_init() (John Linville) [1634044]
- [netdrv] net: ena: change rx copybreak default to reduce kernel memory pressure (John Linville) [1634044]
- [netdrv] net: ena: limit refill Rx threshold to 256 to avoid latency issues (John Linville) [1634044]
- [netdrv] net: ena: explicit casting and initialization, and clearer error handling (John Linville) [1634044]
- [netdrv] net: ena: use CSUM_CHECKED device indication to report skb's checksum status (John Linville) [1634044]
- [netdrv] net: ena: add functions for handling Low Latency Queues in ena_netdev (John Linville) [1634044]
- [netdrv] net: ena: add functions for handling Low Latency Queues in ena_com (John Linville) [1634044]
- [netdrv] net: ena: introduce Low Latency Queues data structures according to ENA spec (John Linville) [1634044]
- [netdrv] net: ena: complete host info to match latest ENA spec (John Linville) [1634044]
- [netdrv] net: ena: minor performance improvement (John Linville) [1634044]
- [netdrv] net: ena: fix auto casting to boolean (John Linville) [1634044]
- [netdrv] net: ena: fix NULL dereference due to untimely napi initialization (John Linville) [1634044]
- [netdrv] net: ena: fix rare bug when failed restart/resume is followed by driver removal (John Linville) [1634044]
- [netdrv] net: ena: fix warning in rmmod caused by double iounmap (John Linville) [1634044]
- [netdrv] net: ena: remove ndo_poll_controller (John Linville) [1634044]
- [netdrv] net: ena: fix incorrect usage of memory barriers (John Linville) [1634044]
- [netdrv] net: ena: fix missing calls to READ_ONCE (John Linville) [1634044]
- [netdrv] net: ena: fix missing lock during device destruction (John Linville) [1634044]
- [netdrv] net: ena: fix potential double ena_destroy_device() (John Linville) [1634044]
- [netdrv] net: ena: fix device destruction to gracefully free resources (John Linville) [1634044]
- [netdrv] net: ena: fix driver when PAGE_SIZE == 64kB (John Linville) [1634044]
- [netdrv] net: ena: fix surprise unplug NULL dereference kernel crash (John Linville) [1634044]
- [s390] s390/zcrypt: reinit ap queue state machine during device probe (Philipp Rudo) [1653668]
- [s390] s390/kdump: Make elfcorehdr size calculation ABI compliant (Philipp Rudo) [1653245]
- [s390] s390/kdump: Fix elfcorehdr size calculation (Philipp Rudo) [1653245]
- [block] block: fix 32 bit overflow in __blkdev_issue_discard() (Ming Lei) [1638826]
- [ata] libata: blacklist SAMSUNG MZ7TD256HAFV-000L9 SSD (Ming Lei) [1638826]
- [block] block: copy ioprio in __bio_clone_fast() and bounce (Ming Lei) [1638826]
- [trace] kyber: fix wrong strlcpy() size in trace_kyber_latency() (Ming Lei) [1638826]
- [block] floppy: fix race condition in __floppy_read_block_0() (Ming Lei) [1638826]
- [block] block: make blk_try_req_merge() static (Ming Lei) [1638826]
- [block] block: remove dead queue members (Ming Lei) [1638826]
- [block] block: clean up dead code that is now redundant (Ming Lei) [1638826]
- [nvme] nvme: fix boot hang with only being able to get one IRQ vector (Ming Lei) [1638826]
- [block] ide: don't clear special on ide_queue_rq() entry (Ming Lei) [1638826]
- [block] null_blk: remove unused nullb device (Ming Lei) [1638826]
- [block] ide: don't use req->special (Ming Lei) [1638826]
- [block] pd: replace ->special use with private data in the request (Ming Lei) [1638826]
- [block] aoe: replace ->special use with private data in the request (Ming Lei) [1638826]
- [block] skd_main: don't use req->special (Ming Lei) [1638826]
- [block] nullb: remove leftover legacy request code (Ming Lei) [1638826]
- [scsi] fnic: fix fnic_scsi_host_{start,end}_tag (Ming Lei) [1638826]
- [block] block: remove set but not used variable 'et' (Ming Lei) [1638826]
- [block] block: remove the BLKPREP_* values. (Ming Lei) [1638826]
- [scsi] scsi: return blk_status_t from device handler ->prep_fn (Ming Lei) [1638826]
- [scsi] scsi: return blk_status_t from scsi_init_io and ->init_command (Ming Lei) [1638826]
- [scsi] scsi: clean up error handling in scsi_init_io (Ming Lei) [1638826]
- [scsi] scsi: push blk_status_t up into scsi_setup_{fs,scsi}_cmnd (Ming Lei) [1638826]
- [scsi] scsi: simplify scsi_prep_state_check (Ming Lei) [1638826]
- [block] ide: cleanup ->prep_rq calling convention (Ming Lei) [1638826]
- [block] block: remove req->timeout_list (Ming Lei) [1638826]
- [block] blk-mq: provide a helper to check if a queue is busy (Ming Lei) [1638826]
- [block] blk-mq-tag: change busy_iter_fn to return whether to continue or not (Ming Lei) [1638826]
- [block] ms_block: remove unused pointer 'set' (Ming Lei) [1638826]
- [block] sunvdc: fix compiler warning (Ming Lei) [1638826]
- [nvme] nvme: add separate poll queue map (Ming Lei) [1638826]
- [block] block: add REQ_HIPRI and inherit it from IOCB_HIPRI (Ming Lei) [1638826]
- [nvme] nvme: utilize two queue maps, one for reads and one for writes (Ming Lei) [1638826]
- [block] blk-mq: initial support for multiple queue maps (Ming Lei) [1638826]
- [block] blk-mq: improve plug list sorting (Ming Lei) [1638826]
- [block] blk-mq: cleanup and improve list insertion (Ming Lei) [1638826]
- [block] blk-mq: cache request hardware queue mapping (Ming Lei) [1638826]
- [block] blk-mq: separate number of hardware queues from nr_cpu_ids (Ming Lei) [1638826]
- [block] blk-mq: support multiple hctx maps (Ming Lei) [1638826]
- [block] blk-mq: add 'type' attribute to the sysfs hctx directory (Ming Lei) [1638826]
- [block] blk-mq: allow software queue to map to multiple hardware queues (Ming Lei) [1638826]
- [block] blk-mq: pass in request/bio flags to queue mapping (Ming Lei) [1638826]
- [block] blk-mq: provide dummy blk_mq_map_queue_type() helper (Ming Lei) [1638826]
- [block] blk-mq: abstract out queue map (Ming Lei) [1638826]
- [block] blk-mq: kill q->mq_map (Ming Lei) [1638826]
- [kernel] genirq/affinity: Add support for allocating interrupt sets (Ming Lei) [1638826]
- [kernel] genirq/affinity: Pass first vector to __irq_build_affinity_masks() (Ming Lei) [1638826]
- [kernel] genirq/affinity: Move two stage affinity spreading into a helper function (Ming Lei) [1638826]
- [kernel] genirq/affinity: Spread IRQs to all available NUMA nodes (Ming Lei) [1638826]
- [block] block: kill request ->cpu member (Ming Lei) [1638826]
- [block] block: get rid of q->softirq_done_fn() (Ming Lei) [1638826]
- [block] block: get rid of blk_queued_rq() (Ming Lei) [1638826]
- [block] blk-merge: kill dead queue lock held check (Ming Lei) [1638826]
- [block] block: remove req_no_special_merge() from merging code (Ming Lei) [1638826]
- [block] block: kill request slab cache (Ming Lei) [1638826]
- [block] block: remove request_list code (Ming Lei) [1638826]
- [block] bsg: move bsg-lib parts outside of request queue (Ming Lei) [1638826]
- [block] block: kill legacy parts of timeout handling (Ming Lei) [1638826]
- [block] block: remove __blk_put_request() (Ming Lei) [1638826]
- [block] block: get rid of MQ scheduler ops union (Ming Lei) [1638826]
- [block] block: remove dead elevator code (Ming Lei) [1638826]
- [block] block: remove legacy IO schedulers (Ming Lei) [1638826]
- [block] block: cleanup kick/queued handling (Ming Lei) [1638826]
- [block] block: remove non mq parts from the flush code (Ming Lei) [1638826]
- [block] block: remove legacy rq tagging (Ming Lei) [1638826]
- [block] blk-cgroup: remove legacy queue bypassing (Ming Lei) [1638826]
- [block] blk-wbt: kill check for legacy queue type (Ming Lei) [1638826]
- [block] block: remove blk_complete_request() (Ming Lei) [1638826]
- [block] bsg: convert to use blk-mq (Ming Lei) [1638826]
- [block] bsg: provide bsg_remove_queue() helper (Ming Lei) [1638826]
- [block] bsg: pass in desired timeout handler (Ming Lei) [1638826]
- [s390] dasd: remove dead code (Ming Lei) [1638826]
- [block] block: remove q->lld_busy_fn() (Ming Lei) [1638826]
- [scsi] scsi: kill off the legacy IO path (Ming Lei) [1638826]
- [scsi] scsi: provide mq_ops->busy() hook (Ming Lei) [1638826]
- [block] blk-mq: provide mq_ops->busy() hook (Ming Lei) [1638826]
- [block] blk-mq: remove legacy check in queue blk_freeze_queue() (Ming Lei) [1638826]
- [block] blk-mq: remove the request_list usage (Ming Lei) [1638826]
- [block] ide: convert to blk-mq (Ming Lei) [1638826]
- [block] mspro_block: convert to blk-mq (Ming Lei) [1638826]
- [block] ms_block: convert to blk-mq (Ming Lei) [1638826]
- [block] sunvdc: convert to blk-mq (Ming Lei) [1638826]
- [block] null_blk: Add conventional zone configuration for zoned support (Ming Lei) [1638826]
- [ata] libata: Apply NOLPM quirk for SAMSUNG MZ7TD256HAFV-000L9 (Ming Lei) [1638826]
- [block] block, bfq: fix asymmetric scenarios detection (Ming Lei) [1638826]
- [cdrom] gdrom: fix mistake in assignment of error (Ming Lei) [1638826]
- [block] blk-mq: place trace_block_getrq() in correct place (Ming Lei) [1638826]
- [block] block: Introduce blk_revalidate_disk_zones() (Ming Lei) [1638826]
- [block] block: add a report_zones method (Ming Lei) [1638826]
- [block] block: Expose queue nr_zones in sysfs (Ming Lei) [1638826]
- [block] block: Improve zone reset execution (Ming Lei) [1638826]
- [block] block: Introduce BLKGETNRZONES ioctl (Ming Lei) [1638826]
- [block] block: Introduce BLKGETZONESZ ioctl (Ming Lei) [1638826]
- [block] block: Limit allocation of zone descriptors for report zones (Ming Lei) [1638826]
- [block] block: Introduce blkdev_nr_zones() helper (Ming Lei) [1638826]
- [scsi] scsi: sd_zbc: Fix sd_zbc_check_zones() error checks (Ming Lei) [1638826]
- [scsi] scsi: sd_zbc: Reduce boot device scan and revalidate time (Ming Lei) [1638826]
- [scsi] scsi: sd_zbc: Rearrange code (Ming Lei) [1638826]
- [scsi] scsi: sd_zbc: Remove an assignment from sd_zbc_setup_report_cmnd() (Ming Lei) [1638826]
- [scsi] scsi: sd: don't crash the host on invalid commands (Ming Lei) [1638826]
- [pci] PCI/MSI: Warn and return error if driver enables MSI/MSI-X twice (Ming Lei) [1638826]
- [fs] f2fs: remove request_list check in is_idle() (Ming Lei) [1638826]
- [scsi] scsi: osd: initiator should use mq variant of request ending (Ming Lei) [1638826]
- [scsi] scsi: fnic: replace gross legacy tag hack with blk-mq hack (Ming Lei) [1638826]
- [infiniband] ib_srp: Remove WARN_ON in srp_terminate_io() (Ming Lei) [1638826]
- [scsi] scsi: ufs: Disable blk-mq for now (Ming Lei) [1638826]
- [block] sx8: convert to blk-mq (Ming Lei) [1638826]
- [block] z2ram: convert to blk-mq (Ming Lei) [1638826]
- [cdrom] gdrom: convert to blk-mq (Ming Lei) [1638826]
- [block] floppy: convert to blk-mq (Ming Lei) [1638826]
- [block] ataflop: convert to blk-mq (Ming Lei) [1638826]
- [block] ataflop: fix error handling during setup (Ming Lei) [1638826]
- [block] ataflop: fold headers into C file (Ming Lei) [1638826]
- [block] amiflop: convert to blk-mq (Ming Lei) [1638826]
- [block] amiflop: clean up on errors during setup (Ming Lei) [1638826]
- [block] amiflop: fold headers into C file (Ming Lei) [1638826]
- [block] swim3: convert to blk-mq (Ming Lei) [1638826]
- [block] swim3: add real error handling in setup (Ming Lei) [1638826]
- [block] swim: convert to blk-mq (Ming Lei) [1638826]
- [block] swim: fix cleanup on setup error (Ming Lei) [1638826]
- [mtd] mtd_blkdevs: convert to blk-mq (Ming Lei) [1638826]
- [block] xsysace: convert to blk-mq (Ming Lei) [1638826]
- [block] paride: convert pf to blk-mq (Ming Lei) [1638826]
- [block] paride: convert pd to blk-mq (Ming Lei) [1638826]
- [block] paride: convert pcd to blk-mq (Ming Lei) [1638826]
- [block] ps3disk: convert to blk-mq (Ming Lei) [1638826]
- [block] blk-mq: provide helper for setting up an SQ queue and tag set (Ming Lei) [1638826]
- [block] null_blk: remove set but not used variable 'q' (Ming Lei) [1638826]
- [cdrom] cdrom: don't attempt to fiddle with cdo->capability (Ming Lei) [1638826]
- [block] block: remove bogus check for queue_lock assignment (Ming Lei) [1638826]
- [block] null_blk: remove legacy IO path (Ming Lei) [1638826]
- [block] um: Convert ubd driver to blk-mq (Ming Lei) [1638826]
- [block] skd: fixup usage of legacy IO API (Ming Lei) [1638826]
- [block] aoe: convert aoeblk to blk-mq (Ming Lei) [1638826]
- [block] ide: remove redundant variables queue_run_ms and left (Ming Lei) [1638826]
- [scsi] scsi: core: scsi_io_completion convert BUGs to WARNs (Ming Lei) [1638826]
- [scsi] scsi: core: scsi_io_completion hints on fastpath (Ming Lei) [1638826]
- [scsi] scsi: core: add scsi_io_completion_reprep helper (Ming Lei) [1638826]
- [scsi] scsi: core: add scsi_io_completion_action helper (Ming Lei) [1638826]
- [scsi] scsi: core: add scsi_io_completion_nz_result function (Ming Lei) [1638826]
- [scsi] scsi: core: scsi_io_completion: rename variables (Ming Lei) [1638826]
- [scsi] scsi: core: scsi_io_completion: comment on end_request return (Ming Lei) [1638826]
- [scsi] scsi: core: use blk_mq_run_hw_queues in scsi_kick_queue (Ming Lei) [1638826]
- [scsi] scsi: sg: remove bad blk_end_request_all() call (Ming Lei) [1638826]
- [block] blk-mq: complete req in softirq context in case of single queue (Ming Lei) [1638826]
- [block] block, bfq: improve asymmetric scenarios detection (Ming Lei) [1638826]
- [block] block: remove redundant 'default n' from Kconfig-s (Ming Lei) [1638826]
- [block] blk-mq-debugfs: Also show requests that have not yet been started (Ming Lei) [1638826]
- [block] block: Finish renaming REQ_DISCARD into REQ_OP_DISCARD (Ming Lei) [1638826]
- [block] kyber: fix integer overflow of latency targets on 32-bit (Ming Lei) [1638826]
- [block] kyber: add tracepoints (Ming Lei) [1638826]
- [block] kyber: implement improved heuristics (Ming Lei) [1638826]
- [block] kyber: don't make domain token sbitmap larger than necessary (Ming Lei) [1638826]
- [block] block: export blk_stat_enable_accounting() (Ming Lei) [1638826]
- [block] block: move call of scheduler's ->completed_request() hook (Ming Lei) [1638826]
- [block] blk-mq: Enable support for runtime power management (Ming Lei) [1638826]
- [block] block: Make blk_get_request() block for non-PM requests while suspended (Ming Lei) [1638826]
- [block] block: Allow unfreezing of a queue while requests are in progress (Ming Lei) [1638826]
- [lib] percpu-refcount: Introduce percpu_ref_resurrect() (Ming Lei) [1638826]
- [block] block: Schedule runtime resume earlier (Ming Lei) [1638826]
- [block] block: Split blk_pm_add_request() and blk_pm_put_request() (Ming Lei) [1638826]
- [block] block, scsi: Change the preempt-only flag into a counter (Ming Lei) [1638826]
- [block] block: Move power management code into a new source file (Ming Lei) [1638826]
- [block] Blk-throttle: update to use rbtree with leftmost node cached (Ming Lei) [1638826]
- [block] block: use bio_add_page in bio_iov_iter_get_pages (Ming Lei) [1638826]
- [block] blok, bfq: do not plug I/O if all queues are weight-raised (Ming Lei) [1638826]
- [block] block, bfq: inject other-queue I/O into seeky idle queues on NCQ flash (Ming Lei) [1638826]
- [block] block, bfq: correctly charge and reset entity service in all cases (Ming Lei) [1638826]

* Wed Nov 28 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-46.el8]
- [rpmspec] redhat: fix bpf_samples build (Jiri Benc) [1611579]
- [fs] mnt: fix __detach_mounts infinite loop (Benjamin Coddington) [1628736]
- [pci] pcie: Enable Broadom iProc PCIE and mark it is as tech preview (Mark Langsdorf) [1576958]
- [pci] PCI/ACPI: Add iProc PCIe MCFG quirk (Mark Langsdorf) [1576958]
- [pci] PCI: iproc: Add ACPI/ECAM support (Mark Langsdorf) [1576958]
- [pci] PCI: iproc: Remove PAXC slot check to allow VF support (Mark Langsdorf) [1576958]
- [pci] PCI: iproc: Reduce inbound/outbound mapping print level (Mark Langsdorf) [1576958]
- [pci] PCI: iproc: Reject unconfigured physical functions from PAXC (Mark Langsdorf) [1576958]
- [pci] PCI: iproc: Disable MSI parsing in certain PAXC blocks (Mark Langsdorf) [1576958]
- [pci] PCI: iproc: Fix up corrupted PAXC root complex config registers (Mark Langsdorf) [1576958]
- [pci] PCI: iproc: Activate PAXC bridge quirk for more devices (Mark Langsdorf) [1576958]

* Tue Nov 27 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-45.el8]
- [s390] s390/mm: fix mis-accounting of pgtable_bytes (Joe Lawrence) [1644481]
- [mm] mm: add mm_pxd_folded checks to pgtable_bytes accounting functions (Joe Lawrence) [1644481]
- [mm] mm: introduce mm_[p4d|pud|pmd]_folded (Joe Lawrence) [1644481]
- [mm] mm: make the __PAGETABLE_PxD_FOLDED defines non-empty (Joe Lawrence) [1644481]
- [x86] x86/cpu/vmware: Do not trace vmware_sched_clock() (Vitaly Kuznetsov) [1650273]
- [fs] fuse: fix possibly missed wake-up after abort (Lukas Czerner) [1649244]
- [fs] fuse: fix leaked notify reply (Lukas Czerner) [1649244]
- [fs] fuse: fix blocked_waitq wakeup (Lukas Czerner) [1649244]
- [fs] fuse: set FR_SENT while locked (Lukas Czerner) [1649244]
- [fs] fuse: Fix use-after-free in fuse_dev_do_write() (Lukas Czerner) [1649244]
- [fs] fuse: Fix use-after-free in fuse_dev_do_read() (Lukas Czerner) [1649244]
- [fs] fuse: Add missed unlock_page() to fuse_readpages_fill() (Lukas Czerner) [1649244]
- [fs] fuse: Don't access pipe->buffers without pipe_lock() (Lukas Czerner) [1649244]
- [fs] fuse: fix initial parallel dirops (Lukas Czerner) [1649244]
- [fs] fuse: Fix oops at process_init_reply() (Lukas Czerner) [1649244]
- [fs] fuse: umount should wait for all requests (Lukas Czerner) [1649244]
- [fs] fuse: fix unlocked access to processing queue (Lukas Czerner) [1649244]
- [fs] fuse: fix double request_end() (Lukas Czerner) [1649244]
- [fs] fuse: fix use-after-free in fuse_direct_IO() (Lukas Czerner) [1599195]

* Fri Nov 23 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-44.el8]
- [firmware] efi: Fix debugobjects warning on 'efi_rts_work' (Waiman Long) [1652190]
- [rpmspec] kernel.spec: Do not zip modules on noarch builds (Prarit Bhargava) [1646471]
- [iommu] iommu/amd: Clear memory encryption mask from physical address (Gary Hook) [1640384]

* Thu Nov 22 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-43.el8]
- [powerpc] powerpc/mm/radix: Only need the Nest MMU workaround for R -> RW transition (Steve Best) [1651276]
- [powerpc] powerpc/mm/books3s: Add new pte bit to mark pte temporarily invalid (Steve Best) [1651276]
- [powerpc] powerpc/tm: Fix HFSCR bit for no suspend case (Steve Best) [1651275]

* Wed Nov 21 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-42.el8]
- [powerpc] powerpc/powernv: Fix concurrency issue with npu->mmio_atsd_usage (Steve Best) [1651267]
- [tools] perf tools: Remove ext from struct kmod_path (Jiri Olsa) [1581390]
- [tools] perf tools: Add gzip_is_compressed function (Jiri Olsa) [1581390]
- [tools] perf tools: Add lzma_is_compressed function (Jiri Olsa) [1581390]
- [tools] perf tools: Add is_compressed callback to compressions array (Jiri Olsa) [1581390]
- [tools] perf tools: Move the temp file processing into decompress_kmodule (Jiri Olsa) [1581390]
- [tools] perf tools: Use compression id in decompress_kmodule() (Jiri Olsa) [1581390]
- [tools] perf tools: Store compression id into struct dso (Jiri Olsa) [1581390]
- [tools] perf tools: Add compression id into 'struct kmod_path' (Jiri Olsa) [1581390]
- [tools] perf tools: Make is_supported_compression() static (Jiri Olsa) [1581390]
- [tools] perf tools: Make decompress_to_file() function static (Jiri Olsa) [1581390]
- [tools] perf tools: Get rid of dso__needs_decompress() call in __open_dso() (Jiri Olsa) [1581390]
- [tools] perf tools: Get rid of dso__needs_decompress() call in symbol__disassemble() (Jiri Olsa) [1581390]
- [tools] perf tools: Get rid of dso__needs_decompress() call in read_object_code() (Jiri Olsa) [1581390]
- [rpmspec] redhat: Enable kernel-tools (for kvm_stat) on s390x, too (Thomas Huth) [1631222]

* Tue Nov 20 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-41.el8]
- [drm] drm/atomic_helper: Stop modesets on unregistered connectors harder (Lyude Paul) [1631575]
- [drm] drm/nouveau: Fix nv50_mstc->best_encoder() (Lyude Paul) [1631575]
- [drm] drm/atomic_helper: Allow DPMS On<->Off changes for unregistered connectors (Lyude Paul) [1631575]
- [drm] drm/i915: Fix intel_dp_mst_best_encoder() (Lyude Paul) [1631575]
- [drm] drm/i915: Skip vcpi allocation for MSTB ports that are gone (Lyude Paul) [1631575]
- [drm] drm/i915: Don't unset intel_connector->mst_port (Lyude Paul) [1631575]
- [drm] drm/atomic_helper: Disallow new modesets on unregistered connectors (Lyude Paul) [1631575]
- [s390] s390/qeth: fix HiperSockets sniffer (Philipp Rudo) [1649773]
- [s390] s390/qeth: report 25Gbit link speed (Philipp Rudo) [1649772]
- [s390] s390/qeth: sanitize strings in debug messages (Philipp Rudo) [1649770]
- [s390] s390/qeth: fix initial operstate (Philipp Rudo) [1649769]
- [s390] s390/qeth: unregister netdevice only when registered (Philipp Rudo) [1649769]
- [powerpc] powerpc/64s: consolidate MCE counter increment (Steve Best) [1633550]
- [powerpc] powerpc/64s: move machine check SLB flushing to mm/slb.c (Steve Best) [1633550]
- [powerpc] powernv/pseries: consolidate code for mce early handling (Steve Best) [1633550]
- [powerpc] powerpc/pseries: Dump the SLB contents on SLB MCE errors (Steve Best) [1633550]
- [powerpc] powerpc/pseries: Display machine check error details (Steve Best) [1633550]
- [powerpc] powerpc/pseries: Flush SLB contents on SLB MCE errors (Steve Best) [1633550]
- [powerpc] powerpc/pseries: Define MCE error event section (Steve Best) [1633550]
- [powerpc] powerpc/pseries: Avoid using the size greater than RTAS_ERROR_LOG_MAX (Steve Best) [1633550]
- [powerpc] powerpc/pseries: Defer the logging of rtas error to irq work queue (Steve Best) [1633550]
- [powerpc] powerpc/pseries: Fix endianness while restoring of r3 in MCE handler (Steve Best) [1633550]
- [cdrom] cdrom: fix improper type cast, which can leat to information leak (Maurizio Lombardi) [1650476]

* Thu Nov 15 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-40.el8]
- [drm] drm/amdgpu/pm: Fix potential Spectre v1 (Rob Clark) [1637115]
- [drm] drm/i915/kvmgt: Fix potential Spectre v1 (Rob Clark) [1637115]
- [fs] gfs2: Fix metadata read-ahead during truncate (2) (Andreas Grunbacher) [1647982]
- [block] block: make sure writesame bio is aligned with logical block size (Ming Lei) [1648750]
- [block] block: cleanup __blkdev_issue_discard() (Ming Lei) [1648750]
- [block] block: make sure discard bio is aligned with logical block size (Ming Lei) [1648750]
- [block] block: Clear kernel memory before copying to user (Ming Lei) [1648752]
- [block] block: respect virtual boundary mask in bvecs (Ming Lei) [1648756]
- [block] xen: don't include <xen/xen.h> from <asm/io.h> and <asm/dma-mapping.h> (Ming Lei) [1648756]
- [block] block: remove ARCH_BIOVEC_PHYS_MERGEABLE (Ming Lei) [1648756]
- [block] xen: provide a prototype for xen_biovec_phys_mergeable in xen.h (Ming Lei) [1648756]
- [block] xen: remove the xen_biovec_phys_mergeable export (Ming Lei) [1648756]
- [block] arm: remove the unused BIOVEC_MERGEABLE define (Ming Lei) [1648756]
- [block] block: don't include bug.h from bio.h (Ming Lei) [1648756]
- [block] block: don't include io.h from bio.h (Ming Lei) [1648756]
- [block] block: remove bvec_to_phys (Ming Lei) [1648756]
- [block] block: merge BIOVEC_SEG_BOUNDARY into biovec_phys_mergeable (Ming Lei) [1648756]
- [block] block: add a missing BIOVEC_SEG_BOUNDARY check in bio_add_pc_page (Ming Lei) [1648756]
- [block] block: simplify BIOVEC_PHYS_MERGEABLE (Ming Lei) [1648756]
- [block] block: move req_gap_back_merge to blk.h (Ming Lei) [1648756]
- [block] block: move req_gap_{back,front}_merge to blk-merge.c (Ming Lei) [1648756]
- [block] block: move integrity_req_gap_{back,front}_merge to blk.h (Ming Lei) [1648756]
- [fs] gfs2: Fix iomap buffer head reference counting bug (Andreas Grunbacher) [1647073]
- [scsi] qla2xxx: Update driver version to 10.00.00.07.08.0-k1 (Himanshu Madhani) [1615896]
- [scsi] scsi: qla2xxx: Initialize port speed to avoid setting lower speed (Himanshu Madhani) [1615896]
- [scsi] scsi: qla2xxx: Fix incorrect port speed being set for FC adapters (Himanshu Madhani) [1615896]
- [block] block: brd: associate with queue until adding disk (Ming Lei) [1644602]
- [block] block: call rq_qos_exit() after queue is frozen (Ming Lei) [1641558]
- [block] block: fix the DISCARD request merge (Ming Lei) [1646776]
- [block] blk-mq: fallback to previous nr_hw_queues when updating fails (Ming Lei) [1642218]
- [block] blk-mq: realloc hctx when hw queue is mapped to another node (Ming Lei) [1642218]
- [block] blk-mq: change gfp flags to GFP_NOIO in blk_mq_realloc_hw_ctxs (Ming Lei) [1642218]
- [block] blk-mq: adjust debugfs and sysfs register when updating nr_hw_queues (Ming Lei) [1642218]
- [block] block: remove bio_rewind_iter() (Ming Lei) [1642208]

* Wed Nov 14 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-39.el8]
- [fs] jbd2: fix use after free in jbd2_log_do_checkpoint() (Lukas Czerner) [1644694]
- [fs] ext4: initialize retries variable in ext4_da_write_inline_data_begin() (Lukas Czerner) [1644694]
- [fs] ext4: fix build error when DX_DEBUG is defined (Lukas Czerner) [1644694]

* Tue Nov 13 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-38.el8]
- [pinctrl] pinctrl: intel: Add Ice Lake PCH pin controller support (David Arcari) [1483413]
- [netdrv] nfp: flower: fix vlan match by checking both vlan id and vlan pcp (Pablo Cascon) [1645220]
- [netdrv] nfp: flower: reject tunnel encap with ipv6 outer headers for offloading (Pablo Cascon) [1646644]
- [netdrv] nfp: populate bus-info on representors (Pablo Cascon) [1643998]
- [powerpc] KVM: PPC: Validate TCEs against preregistered memory page sizes (David Gibson) [1625821]
- [powerpc] KVM: PPC: Inform the userspace about TCE update failures (David Gibson) [1625821]
- [powerpc] KVM: PPC: Book3S: Fix guest DMA when guest partially backed by THP pages (David Gibson) [1625821]

* Fri Nov 09 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-37.el8]
- [kernel] locking/lockdep: Fix debug_locks off performance problem (Waiman Long) [1647560]
- [kernel] locking/lockdep: Remove duplicated 'lock_class_ops' percpu array (Waiman Long) [1647560]
- [kernel] locking/lockdep: Make class->ops a percpu counter and move it under CONFIG_DEBUG_LOCKDEP=y (Waiman Long) [1647560]
- [kernel] locking/lockdep: Add a faster path in __lock_release() (Waiman Long) [1647560]
- [kernel] locking/lockdep: Eliminate redundant IRQs check in __lock_acquire() (Waiman Long) [1647560]
- [kernel] locking/lockdep: Remove add_chain_cache_classes() (Waiman Long) [1647560]
- [fs] gfs2: Put bitmap buffers in put_super (Andreas Grunbacher) [1647073]
- [scsi] scsi: hpsa: limit transfer length to 1MB, not 512kB (Joseph Szczypek) [1643956]
- [netdrv] nfp: report FW vNIC stats in interface stats (Pablo Cascon) [1645032]
- [rpmspec] spec: Add bpftool debuginfo package (Jiri Olsa) [1633018]
- [crypto] crypto: chelsio: Fix memory corruption in DMA Mapped buffers (Arjun Vynipadath) [1631750]
- [cdrom] cdrom: Fix info leak/OOB read in cdrom_ioctl_drive_status (Maurizio Lombardi) [1627732] {CVE-2018-16658}

* Wed Nov 07 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-36.el8]
- [kernel] srcu: Make early-boot call_srcu() reuse workqueue lists (Waiman Long) [1644375]
- [tools] rcutorture: Test early boot call_srcu() (Waiman Long) [1644375]
- [kernel] srcu: Make call_srcu() available during very early boot (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_state.ofl_lock to raw_spinlock_t (Waiman Long) [1644375]
- [kernel] rcu: Remove obsolete ->dynticks_fqs and ->cond_resched_completed (Waiman Long) [1644375]
- [kernel] rcu: Switch ->dynticks to rcu_data structure, remove rcu_dynticks (Waiman Long) [1644375]
- [kernel] rcu: Switch dyntick nesting counters to rcu_data structure (Waiman Long) [1644375]
- [kernel] rcu: Switch urgent quiescent-state requests to rcu_data structure (Waiman Long) [1644375]
- [kernel] rcu: Switch lazy counts to rcu_data structure (Waiman Long) [1644375]
- [kernel] rcu: Switch last accelerate/advance to rcu_data structure (Waiman Long) [1644375]
- [kernel] rcu: Switch ->tick_nohz_enabled_snap to rcu_data structure (Waiman Long) [1644375]
- [kernel] rcu: Merge rcu_dynticks structure into rcu_data structure (Waiman Long) [1644375]
- [kernel] rcu: Remove unused rcu_dynticks_snap() from Tiny RCU (Waiman Long) [1644375]
- [kernel] rcu: Convert "1UL << x" to "BIT(x)" (Waiman Long) [1644375]
- [kernel] rcu: Avoid resched_cpu() when rescheduling the current CPU (Waiman Long) [1644375]
- [kernel] rcu: More aggressively enlist scheduler aid for nohz_full CPUs (Waiman Long) [1644375]
- [kernel] rcu: Compute jiffies_till_sched_qs from other kernel parameters (Waiman Long) [1644375]
- [kernel] rcu: Provide functions for determining if call_rcu() has been invoked (Waiman Long) [1644375]
- [kernel] rcu: Eliminate ->rcu_qs_ctr from the rcu_dynticks structure (Waiman Long) [1644375]
- [kernel] rcu: Motivate Tiny RCU forward progress (Waiman Long) [1644375]
- [kernel] rcutorture: Dump reader protection sequence if failures or close calls (Waiman Long) [1644375]
- [kernel] rcu: Provide improved interrupt-from-idle check in rcu_check_callbacks() (Waiman Long) [1644375]
- [kernel] rcu: Make need_resched() respond to urgent RCU-QS needs (Waiman Long) [1644375]
- [kernel] rcu: Inline _rcu_barrier() into its sole remaining caller (Waiman Long) [1644375]
- [kernel] rcu: Define rcu_all_qs() only in !PREEMPT builds (Waiman Long) [1644375]
- [kernel] rcu: Remove !PREEMPT code from rcu_note_voluntary_context_switch() (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in update.c (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in tree_plugin.h (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in tree_exp.h (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in tree.c (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in tiny.c (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in srcutree.h (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in rcutorture.c (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in rcu.h (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in Kconfig (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in rcupdate_wait.h (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in rculist.h (Waiman Long) [1644375]
- [kernel] rcu: Clean up flavor-related definitions and comments in rcupdate.h (Waiman Long) [1644375]
- [kernel] rcu: Remove now-unused rcutorture APIs (Waiman Long) [1644375]
- [kernel] rcuperf: Remove the "rcu_bh" and "sched" torture types (Waiman Long) [1644375]
- [kernel] rcutorture: Remove the "rcu_bh" and "sched" torture types (Waiman Long) [1644375]
- [kernel] rcu: Stop testing RCU-bh and RCU-sched (Waiman Long) [1644375]
- [kernel] rcutorture: Add RCU-bh and RCU-sched support for extended readers (Waiman Long) [1644375]
- [kernel] rcu: Consolidate RCU-sched update-side function definitions (Waiman Long) [1644375]
- [kernel] rcu: Consolidate RCU-bh update-side function definitions (Waiman Long) [1644375]
- [kernel] rcu: Pull rcu_gp_kthread() FQS loop into separate function (Waiman Long) [1644375]
- [kernel] rcu: Inline increment_cpu_stall_ticks() into its sole caller (Waiman Long) [1644375]
- [kernel] rcu: Fix typo in force_qs_rnp()'s parameter's parameter (Waiman Long) [1644375]
- [kernel] rcu: Eliminate initialization-time use of rsp (Waiman Long) [1644375]
- [kernel] rcu: Eliminate RCU-barrier use of rsp (Waiman Long) [1644375]
- [kernel] rcu: Eliminate quiescent-state and grace-period-nonstart use of rsp (Waiman Long) [1644375]
- [kernel] rcu: Eliminate callback-invocation/invocation use of rsp (Waiman Long) [1644375]
- [kernel] rcu: Eliminate grace-period management code use of rsp (Waiman Long) [1644375]
- [kernel] rcu: Eliminate stall-warning use of rsp (Waiman Long) [1644375]
- [kernel] rcu: Restructure rcu_check_gp_kthread_starvation() (Waiman Long) [1644375]
- [kernel] rcu: Simplify rcutorture_get_gp_data() (Waiman Long) [1644375]
- [kernel] rcu: Remove for_each_rcu_flavor() flavor-traversal macro (Waiman Long) [1644375]
- [kernel] rcu: Remove last non-flavor-traversal rsp local variable from tree_plugin.h (Waiman Long) [1644375]
- [kernel] rcu: Remove rcu_data structure's ->rsp field (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_node tree accessor macros (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from expedited grace-period functions (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from no-CBs CPU functions (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from print_cpu_stall_info() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_spawn_one_boost_kthread() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from dump_blkd_tasks() and friend (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_print_detail_task_stall() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_init_one() and friends (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_boot_init_percpu_data() and friends (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from _rcu_barrier() and friends (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from __rcu_pending() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from __call_rcu() and friend (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from __rcu_process_callbacks() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_check_gp_start_stall() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from force-quiescent-state functions (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_do_batch() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from CPU hotplug functions (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_check_quiescent_state() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_gp_kthread() and friends (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_gp_slow() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from note_gp_changes() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from __note_gp_changes() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_advance_cbs() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_accelerate_cbs_unlocked() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_accelerate_cbs() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_gp_kthread_wake() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_future_gp_cleanup() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from check_cpu_stall() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from print_cpu_stall() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from print_other_cpu_stall() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_stall_kick_kthreads() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_dump_cpu_stacks() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_check_gp_kthread_starvation() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from record_gp_stall_check_time() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_get_root() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_gp_in_progress() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_report_qs_rdp() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_report_unblock_qs_rnp() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_report_qs_rsp() (Waiman Long) [1644375]
- [kernel] rcu: Remove rsp parameter from rcu_report_qs_rnp() (Waiman Long) [1644375]
- [kernel] rcu: Remove rcu_data_p pointer to default rcu_data structure (Waiman Long) [1644375]
- [kernel] rcu: Remove rcu_state_p pointer to default rcu_state structure (Waiman Long) [1644375]
- [kernel] rcu: Remove rcu_state structure's ->rda field (Waiman Long) [1644375]
- [kernel] rcu: Eliminate rcu_state structure's ->call field (Waiman Long) [1644375]
- [kernel] rcu: Remove RCU_STATE_INITIALIZER() (Waiman Long) [1644375]
- [kernel] rcu: Express Tiny RCU updates in terms of RCU rather than RCU-sched (Waiman Long) [1644375]
- [kernel] rcu: Define RCU-sched API in terms of RCU for Tree RCU PREEMPT builds (Waiman Long) [1644375]
- [kernel] rcu: Fix typo in rcu_get_gp_kthreads_prio() header comment (Waiman Long) [1644375]
- [kernel] rcu: Drop "wake" parameter from rcu_report_exp_rdp() (Waiman Long) [1644375]
- [kernel] rcu: Update comments and help text for no more RCU-bh updaters (Waiman Long) [1644375]
- [kernel] rcu: Define RCU-bh update API in terms of RCU (Waiman Long) [1644375]
- [kernel] rcu: Report expedited grace periods at context-switch time (Waiman Long) [1644375]
- [kernel] rcu: Apply RCU-bh QSes to RCU-sched and RCU-preempt when safe (Waiman Long) [1644375]
- [kernel] rcu: Add warning to detect half-interrupts (Waiman Long) [1644375]
- [kernel] rcu: Remove now-unused ->b.exp_need_qs field from the rcu_special union (Waiman Long) [1644375]
- [kernel] rcu: Allow processing deferred QSes for exiting RCU-preempt readers (Waiman Long) [1644375]
- [kernel] rcutorture: Test extended "rcu" read-side critical sections (Waiman Long) [1644375]
- [kernel] rcu: Defer reporting RCU-preempt quiescent states when disabled (Waiman Long) [1644375]
- [kernel] rcu: Refactor rcu_{nmi,irq}_{enter,exit}() (Waiman Long) [1644375]
- [documentation] doc: Fix broken HTML directive (Waiman Long) [1644375]
- [documentation] doc: Update removal of RCU-bh/sched update machinery (Waiman Long) [1644375]
- [kernel] rcutorture: Maintain self-propagating CB only during forward-progress test (Waiman Long) [1644375]
- [kernel] rcutorture: Check GP completion at stutter end (Waiman Long) [1644375]
- [kernel] rcutorture: Print forward-progress test interval on error (Waiman Long) [1644375]
- [kernel] rcutorture: Adjust number of reader kthreads per CPU-hotplug operations (Waiman Long) [1644375]
- [kernel] rcutorture: Reduce priority of forward-progress testing (Waiman Long) [1644375]
- [kernel] rcutorture: Limit reader duration if irq or bh disabled (Waiman Long) [1644375]
- [kernel] rcutorture: Increase rcu_read_delay() longdelay_ms (Waiman Long) [1644375]
- [kernel] rcutorture: Add self-propagating callback to forward-progress testing (Waiman Long) [1644375]
- [kernel] rcutorture: Vary forward-progress test interval (Waiman Long) [1644375]
- [kernel] rcutorture: Avoid no-test complaint if too few forward-progress tries (Waiman Long) [1644375]
- [kernel] rcutorture: Also use GP sequence to judge forward progress (Waiman Long) [1644375]
- [kernel] rcutorture: Add forward-progress tests for RCU grace periods (Waiman Long) [1644375]
- [tools] rcutorture: Remove TREE06 and TREE08 from the default test list (Waiman Long) [1644375]
- [kernel] rcuperf: Warn on bad perf type for built-in tests (Waiman Long) [1644375]
- [kernel] rcutorture: Warn on bad torture type for built-in tests (Waiman Long) [1644375]
- [kernel] rcutorture: Force occasional reader waits (Waiman Long) [1644375]
- [tools] torture: Stop overwriting Make.out file with obsolete version (Waiman Long) [1644375]
- [documentation] doc: Improve rcu_dynticks::dynticks documentation (Waiman Long) [1644375]
- [documentation] doc: Fix broken RCU-requirements link to LKML archive (Waiman Long) [1644375]
- [documentation] doc: Add design documentation on interruption of NMI handlers (Waiman Long) [1644375]
- [kernel] rcutorture: Fix rcu_barrier successes counter (Waiman Long) [1644375]
- [kernel] rcutorture: Add support to detect if boost kthread prio is too low (Waiman Long) [1644375]
- [kernel] rcutorture: Use monotonic timestamp for stall detection (Waiman Long) [1644375]
- [kernel] rcutorture: Make boost test more robust (Waiman Long) [1644375]
- [kernel] rcutorture: Disable RT throttling for boost tests (Waiman Long) [1644375]
- [kernel] rcutorture: Emphasize testing of single reader protection type (Waiman Long) [1644375]
- [kernel] rcutorture: Handle extended read-side critical sections (Waiman Long) [1644375]
- [kernel] rcutorture: Make rcu_torture_timer() use rcu_torture_one_read() (Waiman Long) [1644375]
- [kernel] rcutorture: Use per-CPU random state for rcu_torture_timer() (Waiman Long) [1644375]
- [kernel] rcutorture: Use atomic increment for n_rcu_torture_timers (Waiman Long) [1644375]
- [kernel] rcutorture: Extract common code from rcu_torture_reader() (Waiman Long) [1644375]
- [kernel] rcuperf: Remove unused torturing_tasks() function (Waiman Long) [1644375]
- [kernel] rcu: Remove rcutorture test version and sequence number (Waiman Long) [1644375]
- [kernel] rcutorture: Change units of onoff_interval to jiffies (Waiman Long) [1644375]
- [kernel] rcu: Assign higher prio to RCU threads if rcutorture is built-in (Waiman Long) [1644375]
- [documentation] rculist: Improve documentation for list_for_each_entry_from_rcu() (Waiman Long) [1644375]
- [kernel] srcu: Add grace-period number to rcutorture statistics printout (Waiman Long) [1644375]
- [kernel] rcu: Print stall-warning NMI dyntick state in hexadecimal (Waiman Long) [1644375]
- [maintainers] MAINTAINERS: Update RCU, SRCU, and TORTURE-TEST entries (Waiman Long) [1644375]
- [kernel] rcu: Make rcu_seq_diff() more exact (Waiman Long) [1644375]
- [documentation] doc: Update synchronize_rcu() definition in whatisRCU.txt (Waiman Long) [1644375]
- [kernel] rcu: Check the range of jiffies_till_{first, next}_fqs when setting them (Waiman Long) [1644375]
- [kernel] rcu: Add diagnostics for rcutorture writer stall warning (Waiman Long) [1644375]
- [kernel] rcu: Add comment to the last sleep in the rcu tasks loop (Waiman Long) [1644375]
- [kernel] rcu: Speed up calling of RCU tasks callbacks (Waiman Long) [1644375]
- [kernel] rcu: Add comment documenting how rcu_seq_snap works (Waiman Long) [1644375]
- [kernel] rcu: Use RCU CPU stall timeout for rcu_check_gp_start_stall() (Waiman Long) [1644375]
- [kernel] rcu: Remove __maybe_unused from rcu_cpu_has_callbacks() (Waiman Long) [1644375]
- [kernel] rcu: Remove "inline" from rcu_perf_print_module_parms() (Waiman Long) [1644375]
- [kernel] rcu: Remove "inline" from rcu_torture_print_module_parms() (Waiman Long) [1644375]
- [kernel] rcu: Remove "inline" from panic_on_rcu_stall() and rcu_blocking_is_gp() (Waiman Long) [1644375]
- [kernel] rcu: Remove unused local variable "cpu" (Waiman Long) [1644375]
- [kernel] rcu: Remove unused rcu_kick_nohz_cpu() function (Waiman Long) [1644375]
- [kernel] rcu: Clarify and correct the rcu_preempt_qs() header comment (Waiman Long) [1644375]
- [kernel] rcu: Inline rcu_dynticks_momentary_idle() into its sole caller (Waiman Long) [1644375]
- [kernel] rcu: Mark task as .need_qs less aggressively (Waiman Long) [1644375]
- [kernel] rcu: Improve RCU-tasks naming and comments (Waiman Long) [1644375]
- [kernel] rcu: Use pr_fmt to prefix "rcu: " to logging output (Waiman Long) [1644375]
- [kernel] rcu: rcupdate.h: Get rid of Sphinx warnings at rcu_pointer_handoff() (Waiman Long) [1644375]
- [kernel] rcu: Improve rcu_note_voluntary_context_switch() reporting (Waiman Long) [1644375]
- [kernel] rcu: Make rcu_read_unlock_special() static (Waiman Long) [1644375]
- [kernel] rcu: Add diagnostics for offline CPUs failing to report QS (Waiman Long) [1644375]
- [kernel] rcu: Record ->gp_state for both phases of grace-period initialization (Waiman Long) [1644375]
- [kernel] rcu: Add CPU online/offline state to dump_blkd_tasks() (Waiman Long) [1644375]
- [kernel] rcu: Add up-tree information to dump_blkd_tasks() diagnostics (Waiman Long) [1644375]
- [kernel] rcu: Remove CPU-hotplug failsafe from force-quiescent-state code path (Waiman Long) [1644375]
- [kernel] rcu: Remove failsafe check for lost quiescent state (Waiman Long) [1644375]
- [kernel] rcu: Move grace-period pre-init delay after pre-init (Waiman Long) [1644375]
- [kernel] rcu: Add RCU-preempt check for waiting on newly onlined CPU (Waiman Long) [1644375]
- [kernel] rcu: Fix grace-period hangs due to race with CPU offline (Waiman Long) [1644375]
- [kernel] rcu: Fix grace-period hangs from mid-init task resume (Waiman Long) [1644375]
- [kernel] rcu: Suppress false-positive splats from mid-init task resume (Waiman Long) [1644375]
- [kernel] rcu: Suppress more involved false-positive preempted-task splats (Waiman Long) [1644375]
- [kernel] rcu: Suppress false-positive preempted-task splats (Waiman Long) [1644375]
- [kernel] rcu: Suppress false-positive offline-CPU lockdep-RCU splat (Waiman Long) [1644375]
- [kernel] rcu: Prevent useless FQS scan after all CPUs have checked in (Waiman Long) [1644375]
- [kernel] rcu: Replace smp_wmb() with smp_store_release() for stall check (Waiman Long) [1644375]
- [kernel] rcu: Fix typo and add additional debug (Waiman Long) [1644375]
- [kernel] rcu: Make rcu_report_unblock_qs_rnp() warn on violated preconditions (Waiman Long) [1644375]
- [kernel] rcu: Make rcu_init_new_rnp() stop upon already-set bit (Waiman Long) [1644375]
- [kernel] rcu: Fix an obsolete ->qsmaskinit comment (Waiman Long) [1644375]
- [kernel] rcu: Clean up handling of tasks blocked across full-rcu_node offline (Waiman Long) [1644375]
- [kernel] rcu: Identify grace period is in progress as we advance up the tree (Waiman Long) [1644375]
- [kernel] rcu: Use better variable names in funnel locking loop (Waiman Long) [1644375]
- [kernel] rcu: Rename the grace-period-request variables and parameters (Waiman Long) [1644375]
- [kernel] rcu: Regularize resetting of rcu_data wrap indicator (Waiman Long) [1644375]
- [kernel] rcutorture: Correctly handle grace-period sequence wrap (Waiman Long) [1644375]
- [kernel] rcu: Make rcu_start_this_gp() check for grace period already started (Waiman Long) [1644375]
- [kernel] rcu: Fix cpustart tracepoint gp_seq number (Waiman Long) [1644375]
- [kernel] rcu: Produce last "CleanupMore" trace only if late-breaking request (Waiman Long) [1644375]
- [kernel] rcu: Don't funnel-lock above leaf node if GP in progress (Waiman Long) [1644375]
- [documentation] doc: Update RCU CPU stall-warning documentation (Waiman Long) [1644375]
- [documentation] doc: Update memory-ordering documentation for ->gp-seq (Waiman Long) [1644375]
- [documentation] doc: Update data-structure documentation for ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Make simple callback acceleration refer to rdp->gp_seq_needed (Waiman Long) [1644375]
- [kernel] rcu: Remove ->gpnum and ->completed (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_fqs tracepoint to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_quiescent_state_report tracepoint to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_unlock_preempted_task tracepoint to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_preempt_task tracepoint to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_grace_period_init tracepoint to gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_future_grace_period tracepoint to gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_grace_period tracepoint to gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Make rcu_nocb_wait_gp() check if GP already requested (Waiman Long) [1644375]
- [kernel] rcu: Move from ->need_future_gp[] to ->gp_seq_needed (Waiman Long) [1644375]
- [kernel] rcutorture: Convert rcutorture_get_gp_data() to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Make RCU CPU stall warnings use ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert grace-period requests to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert ->completedqs to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert ->rcu_iw_gpnum to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Move rcu_gp_in_progress() to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Move rcu_nocb_gp_get() to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Move rcu_try_advance_all_cbs() to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Move rcu_implicit_dynticks_qs() to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_gpnum_ovf() to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Move RCU's grace-period-change code to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert conditional grace-period primitives to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Make quiescent-state reporting use ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Convert rcu_check_gp_kthread_starvation() to GP sequence number (Waiman Long) [1644375]
- [kernel] rcu: Make rcutorture's batches-completed API use ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Move rcu_gp_slow() to ->gp_seq (Waiman Long) [1644375]
- [kernel] rcu: Introduce grace-period sequence numbers (Waiman Long) [1644375]
- [kernel] rcu: Make rcu_gp_cleanup() write only once to ->gp_flags (Waiman Long) [1644375]
- [kernel] rcu: Diagnostics for grace-period startup hangs (Waiman Long) [1644375]
- [kernel] rcu: Exclude near-simultaneous RCU CPU stall warnings (Waiman Long) [1644375]
- [kernel] rcu: Use the proper lockdep annotation in dump_blkd_tasks() (Waiman Long) [1644375]
- [kernel] rcu: Add debugging info to assertion (Waiman Long) [1644375]
- [kernel] torture: Keep old-school dmesg format (Waiman Long) [1644375]
- [kernel] torture: Make online/offline messages appear only for verbose=2 (Waiman Long) [1644375]
- [tools] rcutorture: Make kvm-find-errors.sh find close calls (Waiman Long) [1644375]
- [tools] rcutorture: Remove obsolete TREE08-T.boot file (Waiman Long) [1644375]
- [tools] torture: Use a single build directory for torture scenarios (Waiman Long) [1644375]
- [kernel] srcu: Introduce srcu_read_{un,}lock_notrace() (Waiman Long) [1644375]
- [kernel] srcu: Add address of first callback to rcutorture output (Waiman Long) [1644375]
- [kernel] srcu: Document that srcu_funnel_gp_start() implies srcu_funnel_exp_start() (Waiman Long) [1644375]
- [kernel] srcu: Fix typos in __call_srcu() header comment (Waiman Long) [1644375]
- [kernel] rcu: Make expedited grace period use direct call on last leaf (Waiman Long) [1644375]

* Tue Nov 06 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-35.el8]
- [netdrv] nfp: flower: use offsets provided by pedit instead of index for ipv6 (Pablo Cascon) [1645132]
- [netdrv] nfp: flower: fix multiple keys per pedit action (Pablo Cascon) [1645132]
- [netdrv] nfp: flower: fix pedit set actions for multiple partial masks (Pablo Cascon) [1645132]
- [netdrv] nfp: flower: ignore checksum actions when performing pedit actions (Pablo Cascon) [1644400]
- [kernel] sched/fair: Fix throttle_list starvation with low CFS quota (Phil Auld) [1638526]
- [net] tipc: fix the big/little endian issue in tipc_dest (Jon Maloy) [1640712]
- [rpmspec] kernel.spec: Include kernel-signing-ca.cer public key (Prarit Bhargava) [1638465]
- [block] block: don't deal with discard limit in blkdev_issue_discard() (Ming Lei) [1631255]
- [powerpc] powerpc/mm: Check memblock_add against MAX_PHYSMEM_BITS range (Gustavo Duarte) [1561402]
- [powerpc] powerpc/mm: Increase MAX_PHYSMEM_BITS to 128TB with SPARSEMEM_VMEMMAP config (Gustavo Duarte) [1561402]

* Tue Nov 06 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-34.el8]
- [s390] s390/crypto: Enhance paes cipher to accept variable length key material (Philipp Rudo) [1644387]
- [s390] s390/pkey: move pckmo subfunction available checks away from module init (Philipp Rudo) [1644387]
- [s390] s390/pkey: Load pkey kernel module automatically (Philipp Rudo) [1644387]
- [s390] s390/zcrypt: fix broken zcrypt_send_cprb in-kernel api function (Philipp Rudo) [1644387]
- [s390] s390/pkey: Introduce new API for transforming key blobs (Philipp Rudo) [1644387]
- [s390] s390/pkey: Introduce new API for random protected key verification (Philipp Rudo) [1644387]
- [s390] s390/pkey: Add sysfs attributes to emit secure key blobs (Philipp Rudo) [1644387]
- [s390] s390/pkey: Add sysfs attributes to emit protected key blobs (Philipp Rudo) [1644387]
- [s390] s390/pkey: Define protected key blob format (Philipp Rudo) [1644387]
- [s390] s390/pkey: Introduce new API for random protected key generation (Philipp Rudo) [1644387]
- [s390] s390/zcrypt: add ap_adapter_mask sysfs attribute (Philipp Rudo) [1644387]
- [s390] s390/zcrypt: provide apfs failure code on type 86 error reply (Philipp Rudo) [1644387]
- [s390] s390/zcrypt: zcrypt device driver cleanup (Philipp Rudo) [1644387]
- [s390] s390/zcrypt: multiple zcrypt device nodes support (Philipp Rudo) [1644387]
- [s390] s390/zcrypt: enable AP bus scan without a valid default domain (Philipp Rudo) [1644387]
- [s390] s390/zcrypt: Use kmemdup to replace kmalloc + memcpy (Philipp Rudo) [1644387]
- [s390] s390/qeth: add TSO support for L2 devices (Philipp Rudo) [1644381]
- [s390] s390/qeth: add support for IPv6 TSO (Philipp Rudo) [1644381]
- [s390] s390/qeth: enhance TSO control sequence (Philipp Rudo) [1644381]
- [s390] s390/qeth: make TSO controls protocol-agnostic (Philipp Rudo) [1644381]
- [s390] s390: qeth: Fix potential array overrun in cmd/rc lookup (Philipp Rudo) [1644381]
- [s390] s390: qeth_core_mpc: Use ARRAY_SIZE instead of reimplementing its function (Philipp Rudo) [1644381]
- [scsi] scsi: mpt3sas: Remove unnecessary parentheses and simplify null checks (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Use dma_pool_zalloc (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Remove unused macro MPT3SAS_FMT (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Convert logging uses with MPT3SAS_FMT without logging levels (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Remove KERN_WARNING from panic uses (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Convert logging uses with MPT3SAS_FMT and reply_q_name to s: (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Convert mlsleading uses of pr_<level> with MPT3SAS_FMT (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Convert uses of pr_<level> with MPT3SAS_FMT to ioc_<level> (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Add ioc_<level> logging macros (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Fix calltrace observed while running IO & reset (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Improve kernel-doc headers (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Split _base_reset_handler(), mpt3sas_scsih_reset_handler() and mpt3sas_ctl_reset_handler() (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Fix a race condition in mpt3sas_base_hard_reset_handler() (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Fix _transport_smp_handler() error path (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Introduce struct mpt3sas_nvme_cmd (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Annotate switch/case fall-through (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Remove set-but-not-used variables (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Fix indentation (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Update driver version "26.100.00.00" (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: As per MPI-spec, use combined reply queue for SAS3.5 controllers when HBA supports more than 16 MSI-x vectors (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Fix, False timeout prints for ioctl and other internal commands during controller reset (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Don't access the structure after decrementing it's instance reference count (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Incorrect command status was set/marked as not used (Tomas Henzl) [1638649]
- [scsi] scsi: mpt3sas: Don't abort I/Os issued to NVMe drives while processing Async Broadcast primitive event (Tomas Henzl) [1638649]
- [netdrv] net/mlx5e: Do not ignore netdevice TX/RX queues number (Alaa Hleihel) [1643103]
- [netdrv] net/mlx5e: Use non-delayed work for update stats (Alaa Hleihel) [1643103]
- [netdrv] net/mlx5e: Initialize all netdev common structures in one place (Alaa Hleihel) [1643103]
- [netdrv] net/mlx5e: Always initialize update stats delayed work (Alaa Hleihel) [1643103]
- [netdrv] net/mlx5e: Gather common netdev init/cleanup functionality in one place (Alaa Hleihel) [1643103]
- [infiniband] RDMA/netdev: Fix netlink support in IPoIB (Alaa Hleihel) [1643103]
- [infiniband] RDMA/netdev: Hoist alloc_netdev_mqs out of the driver (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Consolidate checking of the proposed child interface (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Maintain the child_intfs list from ndo_init/uninit (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Do not remove child devices from within the ndo_uninit (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Get rid of the sysfs_mutex (Alaa Hleihel) [1643103]
- [infiniband] RDMA/netdev: Use priv_destructor for netdev cleanup (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Move init code to ndo_init (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Move all uninit code into ndo_uninit (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Use cancel_delayed_work_sync for neigh-clean task (Alaa Hleihel) [1643103]
- [infiniband] IB/ipoib: Get rid of IPOIB_FLAG_GOING_DOWN (Alaa Hleihel) [1643103]
- [infiniband] RDMA/ipoib: Fix use of sizeof() (Alaa Hleihel) [1643103]
- [netdrv] net/mlx5e: Do not recycle RX pages in interface down flow (Alaa Hleihel) [1643103 1643047]
- [netdrv] net/mlx5e: Replace call to MPWQE free with dealloc in interface down flow (Alaa Hleihel) [1643103 1643047]
- [net] net/xdp: Fix suspicious RCU usage warning (Alaa Hleihel) [1643103 1643047]
- [netdrv] net/mlx5: WQ, fixes for fragmented WQ buffers API (Alaa Hleihel) [1643103 1636183]
- [netdrv] net/mlx4_en: Use minimal rx and tx ring sizes on kdump kernel (Alaa Hleihel) [1643103 1615267]
- [x86] mark coffeelake-s/h 8+2 as supported (David Arcari) [1575461 1575460]
- [x86] x86/spec_ctrl: Synchronize STIBP changes with RHEL IBRS code (Waiman Long) [1643233]
- [x86] x86/speculation: Propagate information about RSB filling mitigation to sysfs (Waiman Long) [1643233]
- [x86] x86/speculation: Enable cross-hyperthread spectre v2 STIBP mitigation (Waiman Long) [1643233]
- [x86] x86/speculation: Apply IBPB more strictly to avoid cross-process data leak (Waiman Long) [1643233]
- [x86] x86/speculation: Add RETPOLINE_AMD support to the inline asm CALL_NOSPEC variant (Waiman Long) [1643233]
- [x86] x86/CPU: Fix unused variable warning when !CONFIG_IA32_EMULATION (Waiman Long) [1643233]
- [x86] x86/pti/64: Remove the SYSCALL64 entry trampoline (Waiman Long) [1643233]
- [x86] x86/entry/64: Use the TSS sp2 slot for SYSCALL/SYSRET scratch space (Waiman Long) [1643233]
- [x86] x86/entry/64: Document idtentry (Waiman Long) [1643233]
- [x86] x86/asm-offsets: Move TSS_sp0 and TSS_sp1 to asm-offsets.c (Waiman Long) [1643233]
- [x86] x86: Add entry trampolines to kcore (Waiman Long) [1643233]
- [kernel] kallsyms, x86: Export addresses of PTI entry trampolines (Waiman Long) [1643233]
- [kernel] kallsyms: Simplify update_iter_mod() (Waiman Long) [1643233]
- [scsi] scsi: csiostor: fix incorrect port capabilities (Arjun Vynipadath) [1628866]
- [scsi] scsi: csiostor: add a check for NULL pointer after kmalloc() (Arjun Vynipadath) [1628866]
- [scsi] scsi: csiostor: update ingress pack and pad boundary value (Arjun Vynipadath) [1628866]

* Wed Oct 31 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-33.el8]
- [netdrv] nfp: flower: use host context count provided by firmware (Pablo Cascon) [1639609]
- [netdrv] nfp: flower: use stats array instead of storing stats per flow (Pablo Cascon) [1639609]
- [netdrv] nfp: flower: use rhashtable for flow caching (Pablo Cascon) [1639609]
- [netdrv] nfp: avoid soft lockups under control message storm (Pablo Cascon) [1639609]
- [kernel] sched: disable autogroups by default (Phil Auld) [1568166]
- [s390] s390/keyboard: sanitize array index in do_kdsk_ioctl (Steve Best) [1637591]
- [char] ipmi:ssif: Add support for multi-part transmit messages > 2 parts (Tony Camuso) [1622053]
- [scsi] scsi: libsas: fix a race condition when smp task timeout (Zhou Wang) [1640426]
- [scsi] scsi: libsas: check the ata device status by ata_dev_enabled() (Zhou Wang) [1640426]
- [scsi] scsi: libsas: always unregister the old device if going to discover new (Zhou Wang) [1640426]
- [scsi] scsi: libsas: dynamically allocate and free ata host (Zhou Wang) [1640426]
- [scsi] scsi: libsas: remove irq save in sas_ata_qc_issue() (Zhou Wang) [1640426]

* Sat Oct 27 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-32.el8]
- [video] fbdev: make FB_BACKLIGHT a tristate (Rob Clark) [1643333 1589158]
- [netdrv] Taint kernel if e1000 is loaded (Neil Horman) [1643617]
- [netdrv] iavf: fix a typo (Stefan Assmann) [1627882]
- [netdrv] i40evf: remove ndo_poll_controller (Stefan Assmann) [1627882]
- [netdrv] intel-ethernet: use correct module license (Stefan Assmann) [1627882]
- [netdrv] iavf: finish renaming files to iavf (Stefan Assmann) [1627882]
- [netdrv] iavf: rename most of i40e strings (Stefan Assmann) [1627882]
- [netdrv] iavf: tracing infrastructure rename (Stefan Assmann) [1627882]
- [netdrv] iavf: replace i40e_debug with iavf version (Stefan Assmann) [1627882]
- [netdrv] iavf: rename i40e_hw to iavf_hw (Stefan Assmann) [1627882]
- [netdrv] iavf: rename I40E_ADMINQ_DESC (Stefan Assmann) [1627882]
- [netdrv] iavf: rename device ID defines (Stefan Assmann) [1627882]
- [netdrv] iavf: remove references to old names (Stefan Assmann) [1627882]
- [netdrv] iavf: move i40evf files to new name (Stefan Assmann) [1627882]
- [netdrv] iavf: rename i40e_status to iavf_status (Stefan Assmann) [1627882]
- [netdrv] iavf: rename functions and structs to new name (Stefan Assmann) [1627882]
- [netdrv] iavf: diet and reformat (Stefan Assmann) [1627882]
- [netdrv] configs: enable CONFIG_IAVF=m (Stefan Assmann) [1627882]
- [netdrv] intel-ethernet: rename i40evf to iavf (Stefan Assmann) [1627882]
- [netdrv] i40e(vf): remove i40e_ethtool_stats.h header file (Stefan Assmann) [1627882]
- [netdrv] i40evf: cancel workqueue sync for adminq when a VF is removed (Stefan Assmann) [1627882]
- [netdrv] i40evf: Don't enable vlan stripping when rx offload is turned on (Stefan Assmann) [1627882]
- [netdrv] i40evf: set IFF_UNICAST_FLT flag for the VF (Stefan Assmann) [1627882]
- [netdrv] i40evf: Validate the number of queues a PF sends (Stefan Assmann) [1627882]
- [netdrv] i40evf: Change a VF mac without reloading the VF driver (Stefan Assmann) [1627882]
- [netdrv] i40evf: update ethtool stats code and use helper functions (Stefan Assmann) [1627882]
- [netdrv] i40e: Add AQ command for rearrange NVM structure (Stefan Assmann) [1627882]
- [netdrv] i40e: Add additional return code to i40e_asq_send_command (Stefan Assmann) [1627882]
- [netdrv] i40e/i40evf: remove redundant functions i40evf_aq_(set/get)_phy_register (Stefan Assmann) [1627882]
- [netdrv] cls_flower: fix error values for commands not supported by drivers (Stefan Assmann) [1627882]
- [init] init/main.c: Enable watchdog_thresh control from kernel line (Prarit Bhargava) [1643161]
- [s390] s390/purgatory: Remove duplicate variable definitions (Philipp Rudo) [1642447]
- [s390] s390/purgatory: Add missing FORCE to Makefile targets (Philipp Rudo) [1642447]
- [s390] s390/purgatory: Fix crash with expoline enabled (Philipp Rudo) [1642447]
- [s390] s390: disable asm code expolines if cc does not support it (Philipp Rudo) [1642447]
- [netdrv] Revert be2net: remove desc field from be_eq_obj (Ivan Vecera) [1639867]

* Tue Oct 23 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-31.el8]
- [rpmspec] redhat: add optional bpf_samples package (Jiri Benc) [1611579]
- [powerpc] powerpc/time: Fix clockevent_decrementer initalisation for PR KVM (Steve Best) [1641615]
- [net] ip: frags: fix crash in ip_do_fragment() (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ipfrag: let ip(6)frag_high_thresh in ns be higher than in init_net (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ipv6: discard IP frag queue on more errors (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ip: fail fast on IP defrag errors (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ip: process in-order fragments efficiently (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ip: add helpers to process in-order fragments faster (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ipv6: defrag: drop non-last frags smaller than min mtu (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ipv4: frags: precedence bug in ip_expire() (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ip: use rb trees for IP frag queue (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] modify skb_rbtree_purge to return the truesize of all purged skbs (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [net] ip: discard IPv4 datagrams with overlapping segments (Sabrina Dubroca) [1616058] {CVE-2018-5391}
- [fs] ovl: fix format of setxattr debug (Miklos Szeredi) [1636875]
- [fs] ovl: fix access beyond unterminated strings (Miklos Szeredi) [1636875]
- [fs] ovl: make symbol 'ovl_aops' static (Miklos Szeredi) [1636875]
- [fs] vfs: swap names of (do,vfs)_clone_file_range() (Miklos Szeredi) [1636875]
- [fs] ovl: fix freeze protection bypass in ovl_clone_file_range() (Miklos Szeredi) [1636875]
- [fs] ovl: fix freeze protection bypass in ovl_write_iter() (Miklos Szeredi) [1636875]
- [fs] ovl: fix memory leak on unlink of indexed file (Miklos Szeredi) [1636875]
- [fs] ovl: fix oopses in ovl_fill_super() failure paths (Miklos Szeredi) [1636875]
- [fs] ovl: add ovl_fadvise() (Miklos Szeredi) [1636875]
- [fs] vfs: implement readahead(2) using POSIX_FADV_WILLNEED (Miklos Szeredi) [1636875]
- [fs] vfs: add the fadvise() file operation (Miklos Szeredi) [1636875]
- [fs] Documentation/filesystems: update documentation of file_operations (Miklos Szeredi) [1636875]
- [fs] ovl: fix GPF in swapfile_activate of file from overlayfs over xfs (Miklos Szeredi) [1636875]
- [fs] ovl: respect FIEMAP_FLAG_SYNC flag (Miklos Szeredi) [1636875]
- [fs] ovl: Enable metadata only feature (Miklos Szeredi) [1636875]
- [fs] ovl: Do not do metacopy only for ioctl modifying file attr (Miklos Szeredi) [1636875]
- [fs] ovl: Do not do metadata only copy-up for truncate operation (Miklos Szeredi) [1636875]
- [fs] ovl: add helper to force data copy-up (Miklos Szeredi) [1636875]
- [fs] ovl: Check redirect on index as well (Miklos Szeredi) [1636875]
- [fs] ovl: Set redirect on upper inode when it is linked (Miklos Szeredi) [1636875]
- [fs] ovl: Set redirect on metacopy files upon rename (Miklos Szeredi) [1636875]
- [fs] ovl: Do not set dentry type ORIGIN for broken hardlinks (Miklos Szeredi) [1636875]
- [fs] ovl: Add an inode flag OVL_CONST_INO (Miklos Szeredi) [1636875]
- [fs] ovl: Treat metacopy dentries as type OVL_PATH_MERGE (Miklos Szeredi) [1636875]
- [fs] ovl: Check redirects for metacopy files (Miklos Szeredi) [1636875]
- [fs] ovl: Move some dir related ovl_lookup_single() code in else block (Miklos Szeredi) [1636875]
- [fs] ovl: Do not expose metacopy only dentry from d_real() (Miklos Szeredi) [1636875]
- [fs] ovl: Open file with data except for the case of fsync (Miklos Szeredi) [1636875]
- [fs] ovl: Add helper ovl_inode_realdata() (Miklos Szeredi) [1636875]
- [fs] ovl: Store lower data inode in ovl_inode (Miklos Szeredi) [1636875]
- [fs] ovl: Fix ovl_getattr() to get number of blocks from lower (Miklos Szeredi) [1636875]
- [fs] ovl: Add helper ovl_dentry_lowerdata() to get lower data dentry (Miklos Szeredi) [1636875]
- [fs] ovl: Copy up meta inode data from lowest data inode (Miklos Szeredi) [1636875]
- [fs] ovl: Modify ovl_lookup() and friends to lookup metacopy dentry (Miklos Szeredi) [1636875]
- [fs] ovl: Use out_err instead of out_nomem (Miklos Szeredi) [1636875]
- [fs] ovl: A new xattr OVL_XATTR_METACOPY for file on upper (Miklos Szeredi) [1636875]
- [fs] ovl: Add helper ovl_already_copied_up() (Miklos Szeredi) [1636875]
- [fs] ovl: Copy up only metadata during copy up where it makes sense (Miklos Szeredi) [1636875]
- [fs] ovl: During copy up, first copy up metadata and then data (Miklos Szeredi) [1636875]
- [fs] ovl: Provide a mount option metacopy=on/off for metadata copyup (Miklos Szeredi) [1636875]
- [fs] ovl: Move the copy up helpers to copy_up.c (Miklos Szeredi) [1636875]
- [fs] ovl: Initialize ovl_inode->redirect in ovl_get_inode() (Miklos Szeredi) [1636875]
- [fs] ovl: fix documentation of non-standard behavior (Miklos Szeredi) [1636875]
- [fs] ovl: obsolete "check_copy_up" module option (Miklos Szeredi) [1636875]
- [fs] vfs: remove open_flags from d_real() (Miklos Szeredi) [1636875]
- [fs] Revert "fsnotify: support overlayfs" (Miklos Szeredi) [1636875]
- [fs] Partially revert "locks: fix file locking on overlayfs" (Miklos Szeredi) [1636875]
- [fs] Revert "vfs: do get_write_access() on upper layer of overlayfs" (Miklos Szeredi) [1636875]
- [fs] Revert "vfs: add flags to d_real()" (Miklos Szeredi) [1636875]
- [fs] Revert "vfs: update ovl inode before relatime check" (Miklos Szeredi) [1636875]
- [fs] Revert "ovl: fix relatime for directories" (Miklos Szeredi) [1636875]
- [fs] vfs: fix freeze protection in mnt_want_write_file() for overlayfs (Miklos Szeredi) [1636875]
- [fs] Revert "ovl: don't allow writing ioctl on lower layer" (Miklos Szeredi) [1636875]
- [fs] Revert "ovl: fix may_write_real() for overlayfs directories" (Miklos Szeredi) [1636875]
- [fs] vfs: don't open real (Miklos Szeredi) [1636875]
- [fs] ovl: add reflink/copyfile/dedup support (Miklos Szeredi) [1636875]
- [fs] ovl: add O_DIRECT support (Miklos Szeredi) [1636875]
- [fs] ovl: add ovl_fiemap() (Miklos Szeredi) [1636875]
- [fs] ovl: add lsattr/chattr support (Miklos Szeredi) [1636875]
- [fs] ovl: add ovl_fallocate() (Miklos Szeredi) [1636875]
- [fs] ovl: add ovl_mmap() (Miklos Szeredi) [1636875]
- [fs] ovl: add ovl_fsync() (Miklos Szeredi) [1636875]
- [fs] ovl: add ovl_write_iter() (Miklos Szeredi) [1636875]
- [fs] ovl: add ovl_read_iter() (Miklos Szeredi) [1636875]
- [fs] ovl: add helper to return real file (Miklos Szeredi) [1636875]
- [fs] ovl: stack file ops (Miklos Szeredi) [1636875]
- [fs] ovl: deal with overlay files in ovl_d_real() (Miklos Szeredi) [1636875]
- [fs] ovl: copy up file size as well (Miklos Szeredi) [1636875]
- [fs] Revert "Revert "ovl: get_write_access() in truncate"" (Miklos Szeredi) [1636875]
- [fs] ovl: copy up inode flags (Miklos Szeredi) [1636875]
- [fs] ovl: copy up times (Miklos Szeredi) [1636875]
- [fs] vfs: export vfs_dedupe_file_range_one() to modules (Miklos Szeredi) [1636875]
- [fs] vfs: export vfs_ioctl() to modules (Miklos Szeredi) [1636875]
- [fs] vfs: make open_with_fake_path() not contribute to nr_files (Miklos Szeredi) [1636875]
- [fs] ovl: fix wrong use of impure dir cache in ovl_iterate() (Miklos Szeredi) [1636875]
- [fs] new helper: open_with_fake_path() (Miklos Szeredi) [1636875]
- [fs] now we can fold open_check_o_direct() into do_dentry_open() (Miklos Szeredi) [1636875]
- [fs] lift fput() on late failures into path_openat() (Miklos Szeredi) [1636875]
- [fs] fold put_filp() into fput() (Miklos Szeredi) [1636875]
- [fs] introduce FMODE_OPENED (Miklos Szeredi) [1636875]
- [fs] ->file_open(): lose cred argument (Miklos Szeredi) [1636875]
- [fs] security_file_open(): lose cred argument (Miklos Szeredi) [1636875]
- [fs] get rid of cred argument of vfs_open() and do_dentry_open() (Miklos Szeredi) [1636875]
- [fs] pass ->f_flags value to alloc_empty_file() (Miklos Szeredi) [1636875]
- [fs] pass creds to get_empty_filp(), make sure dentry_open() passes the right creds (Miklos Szeredi) [1636875]
- [fs] alloc_file(): switch to passing O_... flags instead of FMODE_... mode (Miklos Szeredi) [1636875]
- [fs] make sure do_dentry_open() won't return positive as an error (Miklos Szeredi) [1636875]
- [fs] create_pipe_files(): use fput() if allocation of the second file fails (Miklos Szeredi) [1636875]
- [fs] turn filp_clone_open() into inline wrapper for dentry_open() (Miklos Szeredi) [1636875]
- [fs] fold security_file_free() into file_free() (Miklos Szeredi) [1636875]
- [fs] vfs: dedupe: extract helper for a single dedup (Miklos Szeredi) [1636875]
- [fs] vfs: dedupe: rationalize args (Miklos Szeredi) [1636875]
- [fs] vfs: dedupe: return int (Miklos Szeredi) [1636875]
- [fs] vfs: limit size of dedupe (Miklos Szeredi) [1636875]
- [fs] ovl: set I_CREATING on inode being created (Miklos Szeredi) [1636875]

* Tue Oct 23 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-30.el8]
- [rpmspec] redhat spec: Add new perf tools file (Jiri Olsa) [1579484]
- [tools] perf tools: Fix use of alternatives to find JDIR (Jiri Olsa) [1579484]
- [net] net: sock_diag: Fix spectre v1 gadget in __sock_diag_cmd() (Paolo Abeni) [1637576]
- [thunderbolt] thunderbolt: Add Intel as copyright holder (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Convert rest of the driver files to use SPDX identifier (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Print connected devices (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Make the driver less verbose (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Remove a meaningless NULL pointer check before dma_pool_destroy (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Initialize after IOMMUs (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Do not handle ICM events after domain is stopped (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Add support for runtime PM (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Remove redundant variable 'approved' (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Use correct ICM commands in system suspend (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: No need to take tb->lock in domain suspend/complete (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Do not unnecessarily call ICM get route (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Use 64-bit DMA mask if supported by the platform (Jarod Wilson) [1588929]
- [thunderbolt] thunderbolt: Fix small typo in variable name (Jarod Wilson) [1588929]
- [mm] Revert x86/e820: put !E820_TYPE_RAM regions into memblock.reserved (Baoquan He) [1639450]
- [mm] mm: return zero_resv_unavail optimization (Baoquan He) [1639450]
- [mm] mm: zero remaining unavailable struct pages (Baoquan He) [1639450]
- [mm] mm: skip invalid pages block at a time in zero_resv_unresv() (Baoquan He) [1639450]
- [mm] docs/mm: memblock: update kernel-doc comments (Baoquan He) [1639450]
- [mm] mm/memblock: add a name for memblock flags enumeration (Baoquan He) [1639450]
- [block] blk-wbt: wake up all when we scale up, not down (Ming Lei) [1640035]

* Sat Oct 20 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-29.el8]
- [video] fbdev: make FB_BACKLIGHT a tristate (Rob Clark) [1589158]
- [kernel] EDAC: Raise the maximum number of memory controllers (Aristeu Rozanski) [1634077]
- [netdrv] i40e: disallow changing the number of descriptors when AF_XDP is on (Stefan Assmann) [1630760]
- [netdrv] i40e: clean zero-copy XDP Rx ring on shutdown/reset (Stefan Assmann) [1630760]
- [netdrv] i40e: clean zero-copy XDP Tx ring on shutdown/reset (Stefan Assmann) [1630760]
- [netdrv] i40e: Remove unused msglen parameter from virtchnl functions (Stefan Assmann) [1630760]
- [netdrv] i40e: fix double 'NIC Link is Down' messages (Stefan Assmann) [1630760]
- [netdrv] i40e: add a helper function to validate a VF based on the vf id (Stefan Assmann) [1630760]
- [netdrv] i40e: use declared variables for pf and hw (Stefan Assmann) [1630760]
- [netdrv] i40e: Unset promiscuous settings on VF reset (Stefan Assmann) [1630760]
- [netdrv] i40e: Fix VF's link state notification (Stefan Assmann) [1630760]
- [netdrv] intel-ethernet: use correct module license (Stefan Assmann) [1630760]
- [netdrv] i40e(vf): remove i40e_ethtool_stats.h header file (Stefan Assmann) [1630760]
- [netdrv] i40e: fix possible compiler warning in xsk TX path (Stefan Assmann) [1630760]
- [netdrv] i40e: add AF_XDP zero-copy Tx support (Stefan Assmann) [1630760]
- [netdrv] i40e: move common Tx functions to i40e_txrx_common.h (Stefan Assmann) [1630760]
- [netdrv] xsk: i40e: get rid of useless struct xdp_umem_props (Stefan Assmann) [1630760]
- [netdrv] i40e: add AF_XDP zero-copy Rx support (Stefan Assmann) [1630760]
- [netdrv] i40e: move common Rx functions to i40e_txrx_common.h (Stefan Assmann) [1630760]
- [netdrv] i40e: refactor Rx path for re-use (Stefan Assmann) [1630760]
- [netdrv] i40e: added queue pair disable/enable functions (Stefan Assmann) [1630760]
- [netdrv] i40e: Prevent deleting MAC address from VF when set by PF (Stefan Assmann) [1630760]
- [netdrv] i40e: hold the rtnl lock on clearing interrupt scheme (Stefan Assmann) [1630760]
- [netdrv] i40e: Check and correct speed values for link on open (Stefan Assmann) [1630760]
- [netdrv] i40e: report correct statistics when XDP is enabled (Stefan Assmann) [1630760]
- [netdrv] i40e: static analysis report from community (Stefan Assmann) [1630760]
- [netdrv] i40e: use correct length for strncpy (Stefan Assmann) [1630760]
- [netdrv] i40evf: Change a VF mac without reloading the VF driver (Stefan Assmann) [1630760]
- [netdrv] i40e: move ethtool stats boiler plate code to i40e_ethtool_stats.h (Stefan Assmann) [1630760]
- [netdrv] i40e: convert queue stats to i40e_stats array (Stefan Assmann) [1630760]
- [netdrv] i40e: fix condition of WARN_ONCE for stat strings (Stefan Assmann) [1630760]
- [netdrv] i40e_txrx: mark expected switch fall-through (Stefan Assmann) [1630760]
- [netdrv] i40e_main: mark expected switch fall-through (Stefan Assmann) [1630760]
- [netdrv] i40e: fix i40e_add_queue_stats data pointer update (Stefan Assmann) [1630760]
- [netdrv] i40e: Add AQ command for rearrange NVM structure (Stefan Assmann) [1630760]
- [netdrv] i40e: Add additional return code to i40e_asq_send_command (Stefan Assmann) [1630760]
- [netdrv] i40e: fix warning about shadowed ring parameter (Stefan Assmann) [1630760]
- [netdrv] i40e: remove unnecessary i variable causing -Wshadow warning (Stefan Assmann) [1630760]
- [netdrv] i40e: convert priority flow control stats to use helpers (Stefan Assmann) [1630760]
- [netdrv] i40e: convert VEB TC stats to use an i40e_stats array (Stefan Assmann) [1630760]
- [netdrv] i40e: Set fec_config when forcing link state (Stefan Assmann) [1630760]
- [netdrv] i40e: add helper to copy statistic values into ethtool buffer (Stefan Assmann) [1630760]
- [netdrv] i40e: add helper function for copying strings from stat arrays (Stefan Assmann) [1630760]
- [netdrv] i40e: Remove duplicated prepare call in i40e_shutdown (Stefan Assmann) [1630760]
- [netdrv] cls_flower: fix error values for commands not supported by drivers (Stefan Assmann) [1630760]
- [netdrv] net: drivers/net: Convert random_ether_addr to eth_random_addr (Stefan Assmann) [1630760]
- [net] ipv4: don't let PMTU updates increase route MTU (Sabrina Dubroca) [1638845]
- [net] ipv4: update fnhe_pmtu when first hop's MTU changes (Sabrina Dubroca) [1638845]
- [net] xsk: add a simple buffer reuse queue (Ivan Vecera) [1634774]
- [net] samples/bpf: add -c/--copy -z/--zero-copy flags to xdpsock (Ivan Vecera) [1634774]
- [net] add napi_if_scheduled_mark_missed (Ivan Vecera) [1634774]
- [net] xsk: expose xdp_umem_get_(data, dma) to drivers (Ivan Vecera) [1634774]
- [net] xdp: export xdp_rxq_info_unreg_mem_model (Ivan Vecera) [1634774]
- [net] xdp: implement convert_to_xdp_frame for MEM_TYPE_ZERO_COPY (Ivan Vecera) [1634774]
- [net] xdp: Helper function to clear kernel pointers in xdp_frame (Ivan Vecera) [1634774]
- [net] xsk: i40e: get rid of useless struct xdp_umem_props (Ivan Vecera) [1631809]
- [net] xdp: fix uninitialized 'err' variable (Ivan Vecera) [1631805]
- [tools] headers uapi: Update tools's copy of linux/if_link.h (Ivan Vecera) [1631805]
- [tools] selftests/bpf: add test for multiple programs (Ivan Vecera) [1631805]
- [net] netdevsim: add support for simultaneous driver and hw XDP (Ivan Vecera) [1631805]
- [net] xdp: support simultaneous driver and hw XDP attachment (Ivan Vecera) [1631805]
- [net] xdp: factor out common program/flags handling from drivers (Ivan Vecera) [1631805]
- [net] xdp: don't make drivers report attachment mode (Ivan Vecera) [1631805]
- [net] xdp: add per mode attributes for attached programs (Ivan Vecera) [1631805]
- [net] sched: cls_flower: set correct offload data in fl_reoffload (Ivan Vecera) [1631522]
- [net] sched: call reoffload op on block callback reg (Ivan Vecera) [1631522]
- [net] sched: cls_bpf: implement offload tcf_proto_op (Ivan Vecera) [1631522]
- [net] sched: cls_u32: implement offload tcf_proto_op (Ivan Vecera) [1631522]
- [net] sched: cls_matchall: implement offload tcf_proto_op (Ivan Vecera) [1631522]
- [net] sched: cls_flower: implement offload tcf_proto_op (Ivan Vecera) [1631522]
- [net] sched: add tcf_proto_op to offload a rule (Ivan Vecera) [1631522]
- [net] sched: pass extack pointer to block binds and cb registration (Ivan Vecera) [1631522]

* Fri Oct 19 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-28.el8]
- [rpmspec] kernel.spec: s390/zfcpdump: add -zfcpdump kernel variant (Philipp Rudo) [1567291]
- [kernel] rh_taint: correct loaddable module support dependencies (Philipp Rudo) [1567291]
- [powerpc] KVM: PPC: Book3S HV: Avoid crash from THP collapse during radix page fault (David Gibson) [1639555]
- [irqchip] irqchip/gic-v3-its: Allow use of LPI tables in reserved memory (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Register LPI tables with EFI config table (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Check that all RDs have the same property table (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Use pre-programmed redistributor tables with kdump kernels (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Allow use of pre-programmed LPI tables (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Keep track of property table's PA and VA (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Move pending table allocation to init time (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Split property table clearing from allocation (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Simplify LPI_PENDBASE_SZ usage (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Change initialization ordering for LPIs (Jeremy Linton) [1625746]
- [firmware] efi: add API to reserve memory persistently across kexec reboot (Jeremy Linton) [1625746]
- [firmware] efi/arm: libstub: add a root memreserve config table (Jeremy Linton) [1625746]
- [firmware] efi: honour memory reservations passed via a linux specific config table (Jeremy Linton) [1625746]
- [irqchip] irqchip/gic-v3-its: Cap lpi_id_bits to reduce memory footprint (Jeremy Linton) [1625746]
- [infiniband] RDMA/bnxt_re: Fix system crash during RDMA resource initialization (Selvin Xavier) [1637122]
- [infiniband] RDMA/bnxt_re: Fix couple of memory leaks that could lead to IOMMU call traces (Selvin Xavier) [1637120]
- [arm64] arm64: KVM: Sanitize PSTATE.M when being set from userspace (Wei Huang) [1635721] {CVE-2018-18021}
- [arm64] arm64: KVM: Tighten guest core register access from userspace (Wei Huang) [1635721] {CVE-2018-18021}
- [fs] fs/cifs: require sha512 (Leif Sahlberg) [1610619]
- [fs] smb3: simplify code by removing CONFIG_CIFS_SMB311 (Leif Sahlberg) [1610619]
- [fs] smb3: add support for statfs for smb3.1.1 posix extensions (Leif Sahlberg) [1610619]
- [fs] cifs: allow disabling insecure dialects in the config (Leif Sahlberg) [1610619]
- [fs] smb3: if server does not support posix do not allow posix mount option (Leif Sahlberg) [1610619]

* Tue Oct 16 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-27.el8]
- [security] cap_inode_getsecurity: use d_find_any_alias() instead of d_find_alias() (Joe Lawrence) [1638647]
- [powerpc] powerpc/cacheinfo: Report the correct shared_cpu_map on big-cores (Steve Best) [1639265]
- [powerpc] powerpc: Use cpu_smallcore_sibling_mask at SMT level on bigcores (Steve Best) [1639265]
- [powerpc] powerpc: Detect the presence of big-cores via ibm, thread-groups (Steve Best) [1639265]
- [x86] mark amd rome as unsupported (David Arcari) [1638506]
- [netdrv] qed: Add support for virtual link (Chad Dupuis) [1638013]
- [netdrv] qede: Add driver support for 20G link speed (Chad Dupuis) [1638013]
- [netdrv] qed: Add driver support for 20G link speed (Chad Dupuis) [1638013]
- [netdrv] qed: Fix shmem structure inconsistency between driver and the mfw (Chad Dupuis) [1638013]
- [netdrv] qed: Add missing device config for RoCE EDPM in UFP mode (Chad Dupuis) [1638013]
- [netdrv] qed: Add a flag which indicates if offload TC is set (Chad Dupuis) [1638013]
- [netdrv] qed: Do not add VLAN 0 tag to untagged frames in multi-function mode (Chad Dupuis) [1638013]
- [netdrv] qed: Fix populating the invalid stag value in multi function mode (Chad Dupuis) [1638013]
- [tools] perf python: Fix pyrf_evlist__read_on_cpu() interface (Jiri Olsa) [1628229]
- [tools] perf mmap: Store real cpu number in 'struct perf_mmap' (Jiri Olsa) [1628229]

* Tue Oct 16 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-26.el8]
- [fs] gfs2: Fix iomap buffered write support for journaled files (2) (Andreas Grunbacher) [1637944]
- [xen] xen/manage: don't complain about an empty value in control/sysrq node (Vitaly Kuznetsov) [1623344]
- [drm] drm/amdgpu: Silence harmless WARN_ON() during MST disable (Lyude Paul) [1638137]
- [netdrv] net: macb: Fix regression breaking non-MDIO fixed-link PHYs (Petr Oros) [1638259]
- [netdrv] net: macb: do not disable MDIO bus at open/close time (Petr Oros) [1638259]
- [fs] proc: restrict kernel stack dumps to root (Waiman Long) [1638044]
- [base] firmware: Always initialize the fw_priv list object (Waiman Long) [1638044]
- [base] firmware: Fix security issue with request_firmware_into_buf() (Waiman Long) [1638044]
- [fs] sysfs: Do not return POSIX ACL xattrs via listxattr (Waiman Long) [1638044]
- [fs] vfs: don't evict uninitialized inode (Waiman Long) [1638044]
- [fs] new primitive: discard_new_inode() (Waiman Long) [1638044]
- [arm64] arm64: jump_label.h: use asm_volatile_goto macro instead of "asm goto" (Waiman Long) [1638044]
- [kernel] sched/topology: Set correct NUMA topology type (Waiman Long) [1638044]
- [kernel] bpf: 32-bit RSH verification must truncate input before the ALU op (Waiman Long) [1638044]
- [mm] mm: madvise(MADV_DODUMP): allow hugetlbfs pages (Waiman Long) [1638044]
- [x86] x86/pti: Fix section mismatch warning/error (Waiman Long) [1638044]
- [kernel] uaccess: Fix is_source param for check_copy_size() in copy_to_iter_mcsafe() (Waiman Long) [1638044]
- [x86] x86/mm: Expand static page table for fixmap space (Waiman Long) [1638044]
- [fs] fs/lock: skip lock owner pid translation in case we are in init_pid_ns (Waiman Long) [1638044]
- [x86] perf/x86/intel/lbr: Fix incomplete LBR call stack (Waiman Long) [1638044]
- [kernel] perf/hw_breakpoint: Split attribute parse and commit (Waiman Long) [1638044]
- [kernel] bitfield: fix *_encode_bits() (Waiman Long) [1638044]
- [kernel] posix-timers: Sanitize overrun handling (Waiman Long) [1638044]
- [kernel] posix-timers: Make forward callback return s64 (Waiman Long) [1638044]
- [kernel] alarmtimer: Prevent overflow for relative nanosleep (Waiman Long) [1638044]
- [x86] x86/entry/64: Add two more instruction suffixes (Waiman Long) [1638044]
- [powerpc] powerpc/kdump: Handle crashkernel memory reservation failure (Waiman Long) [1638044]
- [s390] s390/mm: correct allocate_pgste proc_handler callback (Waiman Long) [1638044]
- [x86] x86/numa_emulation: Fix emulated-to-physical node mapping (Waiman Long) [1638044]
- [x86] x86/paravirt: Fix some warning messages (Waiman Long) [1638044]
- [kernel] sched/fair: Fix vruntime_normalized() for remote non-migration wakeup (Waiman Long) [1638044]
- [kernel] bpf/verifier: disallow pointer subtraction (Waiman Long) [1638044]
- [mm] mm: shmem.c: Correctly annotate new inodes for lockdep (Waiman Long) [1638044]
- [kernel] sched/core: Use smp_mb() in wake_woken_function() (Waiman Long) [1638044]
- [kernel] bpf: fix rcu annotations in compute_effective_progs() (Waiman Long) [1638044]
- [x86] x86/mm/pti: Add an overflow check to pti_clone_pmds() (Waiman Long) [1638044]
- [x86] x86/pti: Check the return value of pti_user_pagetable_walk_pmd() (Waiman Long) [1638044]
- [x86] x86/pti: Check the return value of pti_user_pagetable_walk_p4d() (Waiman Long) [1638044]
- [powerpc] powerpc/pseries/mm: call H_BLOCK_REMOVE (Steve Best) [1637116]
- [powerpc] powerpc/pseries/mm: factorize PTE slot computation (Steve Best) [1637116]
- [powerpc] powerpc/pseries/mm: Introducing FW_FEATURE_BLOCK_REMOVE (Steve Best) [1637116]
- [watchdog] watchdog/hpwdt: Disable PreTimeout when Timeout is smaller (Joseph Szczypek) [1632945]
- [watchdog] watchdog: hpwdt: Update Driver Documentation (Joseph Szczypek) [1632945]
- [watchdog] watchdog: hpwdt: Update version number (Joseph Szczypek) [1632945]
- [watchdog] watchdog: hpwdt: Module parameter alias (Joseph Szczypek) [1632945]
- [watchdog] watchdog: hpwdt: Display module parameters (Joseph Szczypek) [1632945]
- [watchdog] watchdog: hpwdt: Claim NMI from iLO (Joseph Szczypek) [1632945]
- [watchdog] watchdog: hpwdt: Initialize pretimeout from module parameter (Joseph Szczypek) [1632945]

* Sat Oct 13 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-25.el8]
- [mm] mm/sparse: delete old sparse_init and enable new one (Baoquan He) [1625105]
- [mm] mm/sparse: add new sparse_init_nid() and sparse_init() (Baoquan He) [1625105]
- [mm] mm/sparse: move buffer init/fini to the common place (Baoquan He) [1625105]
- [mm] mm/sparse: use the new sparse buffer functions in non-vmemmap (Baoquan He) [1625105]
- [mm] mm/sparse: abstract sparse buffer allocations (Baoquan He) [1625105]
- [mm] mm/sparse: optimize memmap allocation during sparse_init() (Baoquan He) [1625105]
- [mm] mm/sparse.c: add a new parameter 'data_unit_size' for alloc_usemap_and_memmap (Baoquan He) [1625105]
- [mm] mm/sparsemem.c: defer the ms->section_mem_map clearing (Baoquan He) [1625105]
- [mm] mm/sparse.c: add a static variable nr_present_sections (Baoquan He) [1625105]
- [mm] mm/sparse.c: make sparse_init_one_section void and remove check (Baoquan He) [1625105]
- [target] scsi: target: iscsi: cxgbit: fix csk leak (Arjun Vynipadath) [1628864]
- [target] scsi: target: iscsi: cxgbit: use pr_debug() instead of pr_info() (Arjun Vynipadath) [1628864]
- [infiniband] iw_cxgb4: only allow 1 flush on user qps (Arjun Vynipadath) [1628865]
- [infiniband] iw_cxgb4: pass window scale in flowc work request (Arjun Vynipadath) [1628865]
- [infiniband] iw_cxgb4: remove duplicate memcpy() in c4iw_create_listen() (Arjun Vynipadath) [1628865]
- [netdrv] mlxsw: spectrum_switchdev: Do not leak RIFs when removing bridge (Petr Oros) [1638268]
- [tty] tty: vt_ioctl: fix potential Spectre v1 (Prarit Bhargava) [1637123]
- [powerpc] powerpc/time: Add set_state_oneshot_stopped decrementer callback (Steve Best) [1638287]
- [powerpc] powerpc/time: Use clockevents_register_device(), fixing an issue with large decrementer (Steve Best) [1638287]
- [hwmon] hwmon: (nct6775) Fix potential Spectre v1 (Dean Nelson) [1637464]
- [vfio] vfio-pci: Disable binding to PFs with SR-IOV enabled (Alex Williamson) [1637871]
- [netdrv] net: hns3: fix page_offset overflow when CONFIG_ARM64_64K_PAGES (Petr Oros) [1638385]
- [netdrv] net: hns: fix skb->truesize underestimation (Petr Oros) [1638385]
- [netdrv] net: hns: fix length and page_offset overflow when CONFIG_ARM64_64K_PAGES (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix get_vector ops in hclgevf_main module (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix warning bug when doing lp selftest (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix for mac pause not disable in pfc mode (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix for mailbox message truncated problem (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix return value error in hns3_reset_notify_down_enet (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix for reset_level default assignment probelm (Petr Oros) [1638385]
- [netdrv] net: hns3: Reset net device with rtnl_lock (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix for phy link issue when using marvell phy driver (Petr Oros) [1638385]
- [netdrv] net: hns3: Fix for command format parsing error in hclge_is_all_function_id_zero (Petr Oros) [1638385]
- [net] xprtrdma: Fix disconnect regression (Don Dutile) [1635418]
- [infiniband] RDMA/uverbs: Fix validity check for modify QP (Don Dutile) [1635418]
- [infiniband] IB/srp: Avoid that sg_reset -d $srp_device triggers an infinite loop (Don Dutile) [1635418]
- [infiniband] ucma: fix a use-after-free in ucma_resolve_ip() (Don Dutile) [1635418]
- [infiniband] RDMA/uverbs: Atomically flush and mark closed the comp event queue (Don Dutile) [1635418]
- [infiniband] RDMA/mlx4: Ensure that maximal send/receive SGE less than supported by HW (Don Dutile) [1635418 1623100]
- [infiniband] RDMA/cma: Protect cma dev list with lock (Don Dutile) [1635418]
- [infiniband] IB/ipoib: Avoid a race condition between start_xmit and cm_rep_handler (Don Dutile) [1635418]
- [infiniband] RDMA/ucma: check fd type in ucma_migrate_id() (Don Dutile) [1635418]
- [infiniband] RDMA/rxe: Set wqe->status correctly if an unexpected response is received (Don Dutile) [1635418]
- [infiniband] IB/IPoIB: Set ah valid flag in multicast send flow (Don Dutile) [1635418]
- [infiniband] RDMA/core: Avoid holding lock while initializing fields on stack (Don Dutile) [1635418]
- [infiniband] IB/rxe: Drop QP0 silently (Don Dutile) [1635418]
- [infiniband] RDMA/umem: Don't hold mmap_sem for too long (Don Dutile) [1635418]
- [infiniband] IB/srpt: Fix srpt_cm_req_recv() error path (2/2) (Don Dutile) [1635418]
- [infiniband] IB/srpt: Fix srpt_cm_req_recv() error path (1/2) (Don Dutile) [1635418]
- [infiniband] RDMA: Fix storage of PortInfo CapabilityMask in the kernel (Don Dutile) [1635418]
- [infiniband] IB/core: type promotion bug in rdma_rw_init_one_mr() (Don Dutile) [1635418]
- [infiniband] RDMA/i40w: Hold read semaphore while looking after VMA (Don Dutile) [1635418]
- [infiniband] vmw_pvrdma: Release netdev when vmxnet3 module is removed (Don Dutile) [1635418]
- [infiniband] ib_srpt: Fix a use-after-free in __srpt_close_all_ch() (Don Dutile) [1635418]
- [infiniband] ib_srpt: Fix a use-after-free in srpt_close_ch() (Don Dutile) [1635418]
- [infiniband] IB/srpt: Support HCAs with more than two ports (Don Dutile) [1635418]
- [infiniband] IB/rxe: don't clear the tx queue on every transfer (Don Dutile) [1635418]
- [infiniband] IB/core: add max_send_sge and max_recv_sge attributes (Don Dutile) [1635418 1623100]
- [infiniband] IB/rxe: support for 802.1q VLAN on the listener (Don Dutile) [1635418]
- [netdrv] cxgb4: impose mandatory VLAN usage when non-zero TAG ID (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: when max_tx_rate is 0 disable tx rate limiting (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: do not return DUPLEX_UNKNOWN when link is down (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: expose stats fetched from firmware via debugfs (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: remove stats fetched from firmware (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: specify IQTYPE in fw_iq_cmd (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: Fix the condition to check if the card is T5 (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: Support ethtool private flags (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: Add support for FW_ETH_TX_PKT_VM_WR (Arjun Vynipadath) [1628863]
- [netdrv] cxgb4: Add flag tc_flower_initialized (Arjun Vynipadath) [1628863]
- [s390] s390/zcrypt: remove VLA usage from the AP bus (Philipp Rudo) [1637865]
- [s390] s390/ap_bus: replace PTR_RET with PTR_ERR_OR_ZERO (Philipp Rudo) [1637865]
- [s390] s390/crypto: fix gcc 8 stringop-truncation warning (Philipp Rudo) [1637865]
- [s390] s390/zcrypt: code beautify (Philipp Rudo) [1637865]
- [s390] s390/zcrypt: add copy_from_user length plausibility checks (Philipp Rudo) [1637865]
- [s390] s390/zcrypt: Show load of cards and queues in sysfs (Philipp Rudo) [1637865]
- [s390] s390/kvm: fix deadlock when killed by oom (Philipp Rudo) [1638264]
- [fs] xfs: fix data corruption w/ unaligned reflink ranges (Brian Foster) [1633476]
- [fs] xfs: fix data corruption w/ unaligned dedupe ranges (Brian Foster) [1633476]
- [fs] xfs: update ctime and remove suid before cloning files (Brian Foster) [1633476]
- [fs] xfs: zero posteof blocks when cloning above eof (Brian Foster) [1633476]
- [fs] xfs: refactor clonerange preparation into a separate helper (Brian Foster) [1633476]
- [netdrv] nfp: avoid buffer leak when FW communication fails (Petr Oros) [1638233]
- [netdrv] nfp: don't fail probe on pci_sriov_set_totalvfs() errors (Petr Oros) [1638233]
- [netdrv] nfp: wait for posted reconfigs when disabling the device (Petr Oros) [1638233]
- [netdrv] liquidio: fix hang when re-binding VF host drv after running DPDK VF driver (Petr Oros) [1638224]
- [netdrv] r8169: set RxConfig after tx/rx is enabled for RTL8169sb/8110sb devices (Petr Oros) [1638210]
- [netdrv] r8169: add support for NCube 8168 network card (Petr Oros) [1638210]
- [netdrv] r8169: don't use MSI-X on RTL8106e (Petr Oros) [1638210]
- [netdrv] r8169: don't use MSI-X on RTL8168g (Petr Oros) [1638210]
- [powerpc] KVM: PPC: Book3S HV: Fix guest r11 corruption with POWER9 TM workarounds (David Gibson) [1637766]
- [drm] drm/amdgpu: Suppress keypresses from ACPI_VIDEO events (Lyude Paul) [1631918]
- [infiniband] IB/hfi1: Remove race conditions in user_sdma send path (Alex Estrin) [1637068]
- [infiniband] IB/hfi1: Eliminate races in the SDMA send error path (Alex Estrin) [1637068]
- [infiniband] IB/hfi1: Fix destroy_qp hang after a link down (Alex Estrin) [1637068]
- [infiniband] IB/hfi1: Fix context recovery when PBC has an UnsupportedVL (Alex Estrin) [1637068]
- [infiniband] IB/hfi1: Invalid user input can result in crash (Alex Estrin) [1637068]
- [infiniband] IB/hfi1: Fix SL array bounds check (Alex Estrin) [1637068]
- [powerpc] powerpc/fadump: re-register firmware-assisted dump if already registered (Steve Best) [1637383]
- [powerpc] powerpc/fadump: cleanup crash memory ranges support (Steve Best) [1637383]
- [powerpc] powerpc/fadump: merge adjacent memory ranges to reduce PT_LOAD segements (Steve Best) [1637383]
- [powerpc] powerpc/fadump: handle crash memory ranges array index overflow (Steve Best) [1637383]
- [scsi] scsi: qedi: Initialize the stats mutex lock (Chad Dupuis) [1637245]
- [fs] gfs2: Fix iomap buffered write support for journaled files (Andreas Grunbacher) [1637944]
- [fs] gfs2: eliminate update_rgrp_lvb_unlinked (Andreas Grunbacher) [1637944]
- [fs] gfs2: Fix gfs2_testbit to use clone bitmaps (Andreas Grunbacher) [1637944]
- [fs] gfs2: Get rid of gfs2_ea_strlen (Andreas Grunbacher) [1637944]
- [fs] GFS2: rgrp free blocks used incorrectly (Andreas Grunbacher) [1637944]
- [fs] gfs2: remove redundant variable 'moved' (Andreas Grunbacher) [1637944]
- [fs] gfs2: use iomap_readpage for blocksize == PAGE_SIZE (Andreas Grunbacher) [1637944]
- [fs] gfs2: Use iomap for stuffed direct I/O reads (Andreas Grunbacher) [1637944]
- [fs] gfs2: fallocate_chunk: Always initialize struct iomap (Andreas Grunbacher) [1637944]
- [fs] gfs2: Remove gfs2_write_(begin,end) (Andreas Grunbacher) [1637944]
- [fs] gfs2: iomap direct I/O support (Andreas Grunbacher) [1637944]
- [fs] gfs2: gfs2_extent_length cleanup (Andreas Grunbacher) [1637944]
- [fs] gfs2: iomap buffered write support (Andreas Grunbacher) [1637944]
- [fs] gfs2: Further iomap cleanups (Andreas Grunbacher) [1637944]
- [fs] fs: gfs2: Adding new return type vm_fault_t (Andreas Grunbacher) [1637944]
- [fs] gfs2: using posix_acl_xattr_size instead of posix_acl_to_xattr (Andreas Grunbacher) [1637944]
- [fs] gfs2: Don't reject a supposedly full bitmap if we have blocks reserved (Andreas Grunbacher) [1637944]
- [fs] gfs2: Eliminate redundant ip->i_rgd (Andreas Grunbacher) [1637944]
- [fs] gfs2: Stop messing with ip->i_rgd in the rlist code (Andreas Grunbacher) [1637944]
- [fs] gfs2: call ktime_get_coarse_real_ts64() directly (Andreas Grunbacher) [1637944]
- [fs] gfs2: Minor clarification to __gfs2_punch_hole (Andreas Grunbacher) [1637944]
- [fs] gfs2: Don't withdraw under a spin lock (Andreas Grunbacher) [1637944]
- [fs] gfs2: eliminate rs_inum and reduce the size of gfs2 inodes (Andreas Grunbacher) [1637944]
- [drm] drm/nouveau/drm/nouveau: Grab runtime PM ref in nv50_mstc_detect() (Lyude Paul) [1628749]
- [drm] drm/nouveau/disp: fix DP disable race (Lyude Paul) [1628749]
- [drm] drm/nouveau/drm/nouveau: Don't forget to cancel hpd_work on suspend/unload (Lyude Paul) [1628749]
- [drm] drm/nouveau/drm/nouveau: Prevent handling ACPI HPD events too early (Lyude Paul) [1628749]
- [drm] drm/nouveau: Reset MST branching unit before enabling (Lyude Paul) [1628749]
- [drm] drm/nouveau: Only write DP_MSTM_CTRL when needed (Lyude Paul) [1628749]
- [drm] drm/nouveau: Remove useless poll_enable() call in drm_load() (Lyude Paul) [1628749]
- [drm] drm/nouveau: Remove useless poll_disable() call in switcheroo_set_state() (Lyude Paul) [1628749]
- [drm] drm/nouveau: Remove useless poll_enable() call in switcheroo_set_state() (Lyude Paul) [1628749]
- [drm] drm/nouveau: Fix deadlocks in nouveau_connector_detect() (Lyude Paul) [1628749]
- [drm] drm/nouveau/drm/nouveau: Use pm_runtime_get_noresume() in connector_detect() (Lyude Paul) [1628749]
- [drm] drm/nouveau/drm/nouveau: Fix deadlock with fb_helper with async RPM requests (Lyude Paul) [1628749]
- [drm] drm/nouveau: Remove duplicate poll_enable() in pmops_runtime_suspend() (Lyude Paul) [1628749]
- [drm] drm/nouveau/drm/nouveau: Fix bogus drm_kms_helper_poll_enable() placement (Lyude Paul) [1628749]
- [md] dm table: require that request-based DM be layered on blk-mq devices (Mike Snitzer) [1637682]
- [md] dm: rename DM_TYPE_MQ_REQUEST_BASED to DM_TYPE_REQUEST_BASED (Mike Snitzer) [1637682]
- [md] dm: remove legacy request-based IO path (Mike Snitzer) [1637682]
- [md] dm linear: fix linear_end_io conditional definition (Mike Snitzer) [1637682]
- [md] dm linear: eliminate linear_end_io call if CONFIG_DM_ZONED disabled (Mike Snitzer) [1637682]
- [md] dm: fix report zone remapping to account for partition offset (Mike Snitzer) [1637682]
- [md] dm cache: destroy migration_cache if cache target registration failed (Mike Snitzer) [1637682]
- [md] dm cache: fix resize crash if user doesn't reload cache table (Mike Snitzer) [1637682]
- [md] dm cache metadata: ignore hints array being too small during resize (Mike Snitzer) [1637682]
- [md] dm raid: remove bogus const from decipher_sync_action() return type (Mike Snitzer) [1637682]
- [md] dm mpath: fix attached_handler_name leak and dangling hw_handler_name pointer (Mike Snitzer) [1637682]
- [md] dm thin metadata: fix __udivdi3 undefined on 32-bit (Mike Snitzer) [1637682]
- [md] dm thin metadata: try to avoid ever aborting transactions (Mike Snitzer) [1637682]
- [md] dm raid: bump target version, update comments and documentation (Mike Snitzer) [1637682]
- [md] dm raid: fix RAID leg rebuild errors (Mike Snitzer) [1637682]
- [md] dm raid: fix rebuild of specific devices by updating superblock (Mike Snitzer) [1637682]
- [md] dm raid: fix stripe adding reshape deadlock (Mike Snitzer) [1637682]
- [md] dm raid: fix reshape race on small devices (Mike Snitzer) [1637682]
- [md] dm: disable CRYPTO_TFM_REQ_MAY_SLEEP to fix a GFP_KERNEL recursion deadlock (Mike Snitzer) [1637682]
- [md] dm verity: fix crash on bufio buffer that was allocated with vmalloc (Mike Snitzer) [1637682]
- [md] dm writecache: fix a crash due to reading past end of dirty_bitmap (Mike Snitzer) [1637682]
- [md] dm crypt: don't decrease device limits (Mike Snitzer) [1637682]
- [md] dm cache metadata: set dirty on all cache blocks after a crash (Mike Snitzer) [1637682]
- [md] dm snapshot: remove stale FIXME in snapshot_map() (Mike Snitzer) [1637682]
- [md] dm snapshot: improve performance by switching out_of_order_list to rbtree (Mike Snitzer) [1637682]
- [md] dm kcopyd: avoid softlockup in run_complete_job (Mike Snitzer) [1637682]
- [md] dm cache metadata: save in-core policy_hint_size to on-disk superblock (Mike Snitzer) [1637682]
- [md] dm thin: stop no_space_timeout worker when switching to write-mode (Mike Snitzer) [1637682]
- [md] dm kcopyd: return void from dm_kcopyd_copy() (Mike Snitzer) [1637682]
- [md] dm thin: include metadata_low_watermark threshold in pool status (Mike Snitzer) [1637682]
- [md] dm writecache: report start_sector in status line (Mike Snitzer) [1637682]
- [md] dm crypt: convert essiv from ahash to shash (Mike Snitzer) [1637682]
- [md] dm crypt: use wake_up_process() instead of a wait queue (Mike Snitzer) [1637682]
- [md] dm integrity: recalculate checksums on creation (Mike Snitzer) [1637682]
- [md] dm integrity: flush journal on suspend when using separate metadata device (Mike Snitzer) [1637682]
- [md] dm integrity: use version 2 for separate metadata (Mike Snitzer) [1637682]
- [md] dm integrity: allow separate metadata device (Mike Snitzer) [1637682]
- [md] dm integrity: add ic->start in get_data_sector() (Mike Snitzer) [1637682]
- [md] dm integrity: report provided data sectors in the status (Mike Snitzer) [1637682]
- [md] dm integrity: implement fair range locks (Mike Snitzer) [1637682]
- [md] dm integrity: decouple common code in dm_integrity_map_continue() (Mike Snitzer) [1637682]
- [md] dm integrity: change 'suspending' variable from bool to int (Mike Snitzer) [1637682]
- [md] dm delay: add flush as a third class of IO (Mike Snitzer) [1637682]
- [md] dm delay: refactor repetitive code (Mike Snitzer) [1637682]
- [md] dm cache: only allow a single io_mode cache feature to be requested (Mike Snitzer) [1637682]
- [md] dm thin: update stale "Status" Documentation (Mike Snitzer) [1637682]
- [pci] PCI: Reprogram bridge prefetch registers on resume (Myron Stowe) [1637155]
- [input] Input: xen-kbdfront - fix multi-touch XenStore node's locations (Benjamin Tissoires) [1637027]
- [input] Input: elantech - enable middle button of touchpad on ThinkPad P72 (Benjamin Tissoires) [1637027]
- [hid] HID: i2c-hid: Use devm to allocate i2c_hid struct (Benjamin Tissoires) [1637027]
- [hid] HID: input: fix leaking custom input node name (Benjamin Tissoires) [1637027]
- [hid] HID: core: fix grouping by application (Benjamin Tissoires) [1637027]
- [hid] HID: multitouch: fix Elan panels with 2 input modes declaration (Benjamin Tissoires) [1637027]
- [input] Input: do not use WARN() in input_alloc_absinfo() (Benjamin Tissoires) [1637027]
- [s390] s390: vfio-ap: setup APCB mask using KVM dedicated function (Cornelia Huck) [1508118]
- [s390] KVM: s390: Tracing APCB changes (Cornelia Huck) [1508118]
- [s390] KVM: s390: fix locking for crypto setting error path (Cornelia Huck) [1508118]
- [s390] s390: doc: detailed specifications for AP virtualization (Cornelia Huck) [1508118]
- [s390] KVM: s390: CPU model support for AP virtualization (Cornelia Huck) [1508118]
- [s390] KVM: s390: device attrs to enable/disable AP interpretation (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: allow guest FORMAT-0 CRYCB on host FORMAT-2 (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: allow guest FORMAT-1 CRYCB on host FORMAT-2 (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: allow guest FORMAT-0 CRYCB on host FORMAT-1 (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: allow CRYCB FORMAT-0 (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: allow CRYCB FORMAT-1 (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: Allow CRYCB FORMAT-2 (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: Make use of CRYCB FORMAT2 clear (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: Do the CRYCB validation first (Cornelia Huck) [1508118]
- [s390] KVM: s390: Clear Crypto Control Block when using vSIE (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: implement VFIO_DEVICE_RESET ioctl (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: zeroize the AP queues (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: implement VFIO_DEVICE_GET_INFO ioctl (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: implement mediated device open callback (Cornelia Huck) [1508118]
- [s390] KVM: s390: interface to clear CRYCB masks (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: sysfs interface to view matrix mdev matrix (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: sysfs interfaces to configure control domains (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: sysfs interfaces to configure domains (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: sysfs interfaces to configure adapters (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: register matrix device with VFIO mdev framework (Cornelia Huck) [1508118]
- [s390] s390: vfio-ap: base implementation of VFIO AP device driver (Cornelia Huck) [1508118]
- [s390] KVM: s390: refactor crypto initialization (Cornelia Huck) [1508118]
- [s390] KVM: s390: introduce and use KVM_REQ_VSIE_RESTART (Cornelia Huck) [1508118]
- [s390] KVM: s390: vsie: simulate VCPU SIE entry/exit (Cornelia Huck) [1508118]
- [s390] s390/zcrypt: hex string mask improvements for apmask and aqmask (Cornelia Huck) [1508118]
- [s390] s390/zcrypt: AP bus support for alternate driver(s) (Cornelia Huck) [1508118]
- [s390] s390/zcrypt: switch return type to bool for ap_instructions_available() (Cornelia Huck) [1508118]
- [s390] s390/zcrypt: fix ap_instructions_available() returncodes (Cornelia Huck) [1508118]
- [s390] s390/zcrypt: Integrate ap_asm.h into include/asm/ap.h (Cornelia Huck) [1508118]
- [s390] s390/zcrypt: Review inline assembler constraints (Cornelia Huck) [1508118]
- [s390] s390/zcrypt: Add ZAPQ inline function (Cornelia Huck) [1508118]
- [net] ipv6: use rt6_info members when dst is set in rt6_fill_node (Xin Long) [1625864 1625803 1625117]

* Thu Oct 11 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-24.el8]
- [netdrv] amd-xgbe: use dma_mapping_error to check map errors (David Arcari) [1637666]
- [crypto] crypto: qat - Fix KASAN stack-out-of-bounds bug in adf_probe() (Waiman Long) [1629547]
- [powerpc] powerpc: fix csum_ipv6_magic() on little endian platforms (Diego Domingos) [1625579]
- [net] smc: generic netlink family should be __ro_after_init (Philipp Rudo) [1632435]
- [net] net/smc: fix sizeof to int comparison (Philipp Rudo) [1632435]
- [net] net/smc: no urgent data check for listen sockets (Philipp Rudo) [1632435]
- [net] net/smc: enable fallback for connection abort in state INIT (Philipp Rudo) [1632435]
- [net] net/smc: remove duplicate mutex_unlock (Philipp Rudo) [1632435]
- [net] net/smc: fix non-blocking connect problem (Philipp Rudo) [1632435]
- [net] net/smc: send response to test link signal (Philipp Rudo) [1632435]
- [net] net: simplify sock_poll_wait (Philipp Rudo) [1632435]
- [net] net/smc: Simplify ib_post_(send|recv|srq_recv)() calls (Philipp Rudo) [1632435]
- [net] net/smc: Remove a WARN_ON() statement (Philipp Rudo) [1632435]
- [powerpc] KVM: PPC: Book3S HV: Add NO_HASH flag to GET_SMMU_INFO ioctl result (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Add a VM capability to enable nested virtualization (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Add nested shadow page tables to debugfs (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Allow HV module to load without hypervisor mode (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Handle differing endianness for H_ENTER_NESTED (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Sanitise hv_regs on nested guest entry (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Add one-reg interface to virtual PTCR register (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Don't access HFSCR, LPIDR or LPCR when running nested (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Invalidate TLB when nested vcpu moves physical cpu (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Use hypercalls for TLB invalidation when nested (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Implement H_TLB_INVALIDATE hcall (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Introduce rmap to track nested guest mappings (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Handle page fault for a nested guest (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Handle hypercalls correctly when nested (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Use XICS hypercalls when running as a nested hypervisor (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Nested guest entry via hypercall (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Framework and hcall stubs for nested virtualization (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Use kvmppc_unmap_pte() in kvm_unmap_radix() (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Refactor radix page fault handler (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Make kvmppc_mmu_radix_xlate process/partition table agnostic (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Clear partition table entry on vm teardown (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Use ccr field in pt_regs struct embedded in vcpu struct (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Add a debugfs file to dump radix mappings (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Handle hypervisor instruction faults better (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Streamlined guest entry/exit path on P9 for radix guests (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Call kvmppc_handle_exit_hv() with vcore unlocked (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S: Rework TM save/restore code and make it C-callable (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Simplify real-mode interrupt handling (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Extract PMU save/restore operations as C-callable functions (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Move interrupt delivery on guest entry to C code (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S HV: Remove left-over code in XICS-on-XIVE emulation (Suraj Jitindar Singh) [1505999]
- [powerpc] KVM: PPC: Book3S: Simplify external interrupt handling (Suraj Jitindar Singh) [1505999]
- [powerpc] powerpc: Turn off CPU_FTR_P9_TM_HV_ASSIST in non-hypervisor mode (Suraj Jitindar Singh) [1505999]
- [powerpc] powerpc/64s: Remove POWER9 DD1 support (Suraj Jitindar Singh) [1505999]
- [netdrv] net/mlx5: Add Fast teardown support (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Set vlan masks for all offloaded TC rules (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: E-Switch, Fix out of bound access when setting vport rate (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Avoid unbounded peer devices when unpairing TC hairpin rules (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Cache the system image guid (Alaa Hleihel) [1636554]
- [netdrv] mlx5: remove ndo_poll_controller (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Check for SQ and not RQ state when modifying hairpin SQ (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Fix read from coherent memory (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: don't set CHECKSUM_COMPLETE on SCTP packets (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Set ECN for received packets using CQE indication (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Fix possible deadlock from lockdep when adding fte to fg (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Check for error in mlx5_attach_interface (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Consider PCI domain in search for next dev (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Fix not releasing read lock when adding flow rules (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: E-Switch, Fix memory leak when creating switchdev mode FDB tables (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Use u16 for Work Queue buffer strides offset (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Use u16 for Work Queue buffer fragment size (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Fix debugfs cleanup in the device init/remove flow (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Fix use-after-free in self-healing flow (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Make function mlx5i_grp_sw_update_stats() static (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: IPoIB, Use priv stats in completion rx flow (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: IPoIB, Add ndo stats support for IPoIB child devices (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: IPoIB, Add ndo stats support for IPoIB netdevices (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: IPoIB, Initialize max_opened_tc in mlx5i_init flow (Alaa Hleihel) [1636554]
- [netdrv] IB/mlx5: Fix leaking stack memory to userspace (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Reorganize the makefile (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: clock.c depends on CONFIG_PTP_1588_CLOCK (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: vxlan.c depends on CONFIG_VXLAN (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Move flow steering declarations into en/fs.h (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add CONFIG_MLX5_EN_ARFS for accelerated flow steering support (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add CONFIG_MLX5_EN_RXNFC for ethtool rx nfc (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Ethtool steering, move ethtool callbacks (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Reduce command polling interval (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Use max_num_eqs for calculation of required MSIX vectors (Alaa Hleihel) [1636554]
- [netdrv] RDMA/mlx5: Fix shift overflow in mlx5_ib_create_wq (Alaa Hleihel) [1636554]
- [netdrv] overflow.h: Add arithmetic shift helper (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Fix uninitialized variable (Alaa Hleihel) [1636554]
- [netdrv] RDMA: Fix return code check in rdma_set_cq_moderation (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, move vxlan logic to core driver (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, add sync lock for add/del vxlan port (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, return values for add/del port (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, rename from mlx5e to mlx5 (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, rename struct mlx5e_vxlan to mlx5_vxlan_port (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, move netdev only logic to en_main.c (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, add direct delete function (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, cleanup an unused member in vxlan work (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, replace ports radix-tree with hash table (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, check maximum number of UDP ports (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Vxlan, reflect 4789 UDP port default addition to software database (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Move XDP related code into new XDP files (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Restrict the combination of large MTU and XDP (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Gather all XDP pre-requisite checks in a single function (Alaa Hleihel) [1636554]
- [netdrv] IB/mlx5: avoid excessive warning msgs when creating VFs on 2nd port (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Use PARTIAL_GSO for UDP segmentation (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Remove redundant WARN when we cannot find neigh entry (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Fix tristate and description for MLX5 module (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Better return types for CQE API (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Use ERR_CAST() instead of coding it (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Add missing SET_DRIVER_VERSION command translation (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: fix uaccess beyond "count" in debugfs read/write handlers (Alaa Hleihel) [1636554]
- [netdrv] IB/mlx5: Honor cnt_set_id_valid flag instead of set_id (Alaa Hleihel) [1636554]
- [infiniband] IB/mlx5: fix uaccess beyond "count" in debugfs read/write handlers (Alaa Hleihel) [1636554]
- [infiniband] IB/mlx5: Fix GRE flow specification (Alaa Hleihel) [1636554]
- [infiniband] IB/mlx5: Remove set-but-not-used variables (Alaa Hleihel) [1636554]
- [infiniband] RDMA/mlx5: Don't leak UARs in case of free fails (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Update NIC HW stats on demand only (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add counter for total num of NOP operations (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add counter for MPWQE filler strides (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add channel events counter (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add a counter for congested UMRs (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add NAPI statistics (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add XDP_TX completions statistics (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add TX completions statistics (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: RX, Use existing WQ local variable (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Convert large order kzalloc allocations to kvzalloc (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add UDP GSO remaining counter (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5e: Add UDP GSO support (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Rate limit errors in command interface (Alaa Hleihel) [1636554]
- [netdrv] net/mlx5: Prevent warns in dmesg upon firmware commands (Alaa Hleihel) [1636554]
- [netdrv] mlx4: remove ndo_poll_controller (Alaa Hleihel) [1636553]
- [netdrv] net/mlx4: Use cpumask_available for eq->affinity_mask (Alaa Hleihel) [1636553]
- [netdrv] net/mlx4/en_rx: Mark expected switch fall-throughs (Alaa Hleihel) [1636553]
- [netdrv] net/mlx4/mcg: Mark expected switch fall-throughs (Alaa Hleihel) [1636553]
- [infiniband] IB/mlx4: Use 4K pages for kernel QP's WQE buffer (Alaa Hleihel) [1636553]
- [netdrv] net/mlx4_core: Allow MTTs starting at any index (Alaa Hleihel) [1636553]
- [infiniband] IB/mlx4: Test port number before querying type (Alaa Hleihel) [1636553]
- [powerpc] powerpc/numa: Skip onlining a offline node in kdump path (Steve Best) [1637118]
- [netdrv] net: aquantia: Make function aq_fw1x_set_power() static (David Arcari) [1636533]
- [netdrv] net: aquantia: memory corruption on jumbo frames (David Arcari) [1636533 1630377]
- [netdrv] net: aquantia: bump driver version (David Arcari) [1636533]
- [netdrv] net: aquantia: renaming for better visibility (David Arcari) [1636533]
- [netdrv] net: aquantia: whitespace changes (David Arcari) [1636533]
- [netdrv] net: aquantia: implement EEE support (David Arcari) [1636533]
- [netdrv] net: aquantia: implement WOL support (David Arcari) [1636533]
- [netdrv] net: aquantia: definitions for WOL (David Arcari) [1636533]
- [netdrv] net: aquantia: fix hw_atl_utils_fw_upload_dwords (David Arcari) [1636533]
- [netdrv] net: aquantia: Make some functions static (David Arcari) [1636533]
- [netdrv] net: aquantia: bump driver version (David Arcari) [1636533]
- [netdrv] net: aquantia: Add renegotiate ethtool operation support (David Arcari) [1636533]
- [netdrv] net: aquantia: Implement rx/tx flow control ethtools callback (David Arcari) [1636533]
- [netdrv] net: aquantia: Improve adapter init/deinit logic (David Arcari) [1636533]
- [netdrv] net: aquantia: Ethtool based ring size configuration (David Arcari) [1636533]
- [wireless] ath10k: fix memory leak of tpc_stats (Petr Oros) [1637528]
- [wireless] ath10k: snoc: use correct bus-specific pointer in RX retry (Petr Oros) [1637528]
- [wireless] ath10k: fix incorrect size of dma_free_coherent in ath10k_ce_alloc_src_ring_64 (Petr Oros) [1637528]
- [wireless] brcmsmac: fix wrap around in conversion from constant to s16 (Petr Oros) [1637528]
- [wireless] mt76x2: fix mrr idx/count estimation in mt76x2_mac_fill_tx_status() (Petr Oros) [1637528]
- [wireless] ath10k: transmit queued frames after processing rx packets (Petr Oros) [1637528]
- [wireless] ath10k: protect ath10k_htt_rx_ring_free with rx_ring.lock (Petr Oros) [1637528]
- [wireless] ath10k: use locked skb_dequeue for rx completions (Petr Oros) [1637528]
- [wireless] ath10k: sdio: set skb len for all rx packets (Petr Oros) [1637528]
- [wireless] ath10k: sdio: use same endpoint id for all packets in a bundle (Petr Oros) [1637528]
- [wireless] iwlwifi: cancel the injective function between hw pointers to tfd entry index (Petr Oros) [1637528]
- [wireless] ath10k: disable bundle mgmt tx completion event support (Petr Oros) [1637528]
- [wireless] ath10k: prevent active scans on potential unusable channels (Petr Oros) [1637528]
- [wireless] ath9k_hw: fix channel maximum power level test (Petr Oros) [1637528]
- [wireless] ath9k: report tx status on EOSP (Petr Oros) [1637528]
- [wireless] iwlwifi: pcie: don't access periphery registers when not available (Petr Oros) [1637528]
- [wireless] brcmfmac: fix brcmf_wiphy_wowl_params() NULL pointer dereference (Petr Oros) [1637528]
- [netdrv] be2net: don't flip hw_features when VXLANs are added/deleted (Petr Oros) [1637133]
- [netdrv] be2net: Fix memory leak in be_cmd_get_profile_config() (Petr Oros) [1637133]
- [netdrv] be2net: Mark expected switch fall-through (Petr Oros) [1637133]
- [netdrv] be2net: fix spelling mistake "seqence" -> "sequence" (Petr Oros) [1637133]
- [netdrv] be2net: Update the driver version to 12.0.0.0 (Petr Oros) [1637133]
- [netdrv] be2net: gather debug info and reset adapter (only for Lancer) on a tx-timeout (Petr Oros) [1637133]
- [netdrv] be2net: move rss_flags field in rss_info to ensure proper alignment (Petr Oros) [1637133]
- [netdrv] be2net: re-order fields in be_error_recovert to avoid hole (Petr Oros) [1637133]
- [netdrv] be2net: remove unused tx_jiffies field from be_tx_stats (Petr Oros) [1637133]
- [netdrv] be2net: move txcp field in be_tx_obj to eliminate holes in the struct (Petr Oros) [1637133]
- [netdrv] be2net: reorder fields in be_eq_obj structure (Petr Oros) [1637133]
- [netdrv] be2net: remove desc field from be_eq_obj (Petr Oros) [1637133]
- [netdrv] be2net: remove unused old custom busy-poll fields (Petr Oros) [1637133]
- [netdrv] be2net: remove unused old AIC info (Petr Oros) [1637133]
- [x86] x86/spec_ctrl/compat: Call IBRS_ENTRY only after valid kernel stack (Waiman Long) [1636843]
- [acpi] ACPI/PPTT: Handle architecturally unknown cache types (Jeremy Linton) [1636567]
- [base] drivers: base: cacheinfo: Do not populate sysfs for unknown cache types (Jeremy Linton) [1636567]
- [fs] getxattr: use correct xattr length (Lukas Czerner) [1637049]
- [x86] Mark Intel Cascade Lake supported (Steve Best) [1636651]
- [x86] x86/boot: Fix kexec booting failure in the SEV bit detection code (Kairui Song) [1632514]
- [scsi] scsi: megaraid_sas: driver version upgrade (Tomas Henzl) [1635565]
- [scsi] scsi: megaraid_sas: Support FW provided TM timeout values (Tomas Henzl) [1635565]
- [scsi] scsi: megaraid_sas: Return immediately from wait_for_adapter_operational after kill adapter (Tomas Henzl) [1635565]
- [scsi] scsi: megaraid_sas: Update controller info during resume (Tomas Henzl) [1635565]
- [scsi] scsi: megaraid_sas: Do not do Kill adapter if GET_CTRL_INFO times out (Tomas Henzl) [1635565]
- [scsi] qla2xxx: Update driver version to 10.00.00.07.08.0-k (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Check for Register disconnect (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Fix driver hang when FC-NVMe LUNs are configured (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Fix re-using LoopID when handle is in use (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Fix duplicate switch database entries (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Fix NVMe session hang on unload (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Fix iIDMA error (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Fix stalled relogin (Himanshu Madhani) [1633373]
- [scsi] scsi: qla2xxx: Fix unintended Logout (Himanshu Madhani) [1633373]
- [powerpc] powerpc/pseries: Disable CPU hotplug across migrations (Steve Best) [1633587]
- [block] blk-mq: I/O and timer unplugs are inverted in blktrace (Ming Lei) [1634330]
- [block] block: fix deadline elevator drain for zoned block devices (Ming Lei) [1634333]
- [block] blk-mq: Allow blocking queue tag iter callbacks (Ming Lei) [1634328]
- [block] block: use nanosecond resolution for iostat (Ming Lei) [1634329]
- [block] null_blk: fix zoned support for non-rq based operation (Ming Lei) [1634324]
- [block] blk-cgroup: increase number of supported policies (Ming Lei) [1634335]
- [block] block: bfq: swap puts in bfqg_and_blkg_put (Ming Lei) [1634334]
- [block] block: don't warn when doing fsync on read-only devices (Ming Lei) [1634331]
- [block] blkcg: use tryget logic when associating a blkg with a bio (Ming Lei) [1634332]
- [block] blkcg: delay blkg destruction until after writeback has (Ming Lei) [1634332]
- [block] Revert "blk-throttle: fix race between (Ming Lei) [1634332]
- [block] blk-wbt: remove dead code (Ming Lei) [1634326]
- [block] blk-wbt: improve waking of tasks (Ming Lei) [1634326]
- [block] blk-wbt: abstract out end IO completion handler (Ming Lei) [1634326]

* Tue Oct 09 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-23.el8]
- [dma] driver/dma/ioat: Call del_timer_sync() without holding prep_lock (Waiman Long) [1607654]
- [netdrv] bnxt_en: Fix VF mac address regression (Jonathan Toppins) [1635846]
- [netdrv] bnxt_en: Do not adjust max_cp_rings by the ones used by RDMA (Jonathan Toppins) [1635846]
- [netdrv] bnxt_en: Clean up unused functions (Jonathan Toppins) [1635846]
- [fs] fsnotify: fix ignore mask logic in fsnotify() (Lukas Czerner) [1635537]
- [net] net/af_iucv: locate IUCV header via skb_network_header() (Philipp Rudo) [1635332]
- [net] net/af_iucv: drop inbound packets with invalid flags (Philipp Rudo) [1635332]
- [net] net/af_iucv: fix skb handling on HiperTransport xmit error (Philipp Rudo) [1635332]
- [hid] HID: i2c-hid: Fix flooded incomplete report after S3 on Rayd touchscreen (David Arcari) [1635746]
- [i2c] i2c: core: ACPI: Make acpi_gsb_i2c_read_bytes() check i2c_transfer return value (David Arcari) [1635746]
- [i2c] i2c: designware: Re-init controllers with pm_disabled set on resume (David Arcari) [1635746]
- [i2c] i2c: core: ACPI: Properly set status byte to 0 for multi-byte writes (David Arcari) [1635746]
- [fs] fs/quota: Fix spectre gadget in do_quotactl (Lukas Czerner) [1635521]
- [fs] xfs: fix error handling in xfs_bmap_extents_to_btree (Brian Foster) [1633171]
- [fs] xfs: remove invalid log recovery first/last cycle check (Brian Foster) [1633171]
- [fs] xfs: validate inode di_forkoff (Brian Foster) [1633171]
- [fs] xfs: skip delalloc COW blocks in xfs_reflink_end_cow (Brian Foster) [1633171]
- [fs] xfs: don't treat unknown di_flags2 as corruption in scrub (Brian Foster) [1633171]
- [fs] xfs: remove duplicated include from alloc.c (Brian Foster) [1633171]
- [fs] xfs: don't bring in extents in xfs_bmap_punch_delalloc_range (Brian Foster) [1633171]
- [fs] xfs: fix transaction leak in xfs_reflink_allocate_cow() (Brian Foster) [1633171]
- [fs] xfs: avoid lockdep false positives in xfs_trans_alloc (Brian Foster) [1633171]
- [fs] xfs: refactor xfs_buf_log_item reference count handling (Brian Foster) [1633171]
- [fs] xfs: clean up xfs_trans_brelse() (Brian Foster) [1633171]
- [fs] xfs: don't unlock invalidated buf on aborted tx commit (Brian Foster) [1633171]
- [fs] xfs: remove last of unnecessary xfs_defer_cancel() callers (Brian Foster) [1633171]
- [fs] xfs: don't crash the vfs on a garbage inline symlink (Brian Foster) [1633171]
- [fs] iomap: set page dirty after partial delalloc on mkwrite (Brian Foster) [1633171]
- [fs] xfs: sanity check ag header values in xrep_calc_ag_resblks (Brian Foster) [1633171]
- [fs] xfs: recalculate summary counters at mount time if icount is bad (Brian Foster) [1633171]
- [fs] xfs: fix a null pointer dereference in xfs_bmap_extents_to_btree (Brian Foster) [1633171]
- [fs] xfs: remove b_last_holder & associated macros (Brian Foster) [1633171]
- [fs] xfs: repair the AGI (Brian Foster) [1633171]
- [fs] xfs: repair the AGFL (Brian Foster) [1633171]
- [fs] xfs: repair the AGF (Brian Foster) [1633171]
- [fs] xfs: remove dead error handling code in xfs_dquot_disk_alloc() (Brian Foster) [1633171]
- [fs] xfs: use WRITE_ONCE to update if_seq (Brian Foster) [1633171]
- [fs] xfs: fix a comment in xfs_log_reserve (Brian Foster) [1633171]
- [fs] xfs: only validate summary counts on primary superblock (Brian Foster) [1633171]
- [fs] xfs: substitute spaces with tabs (Brian Foster) [1633171]
- [fs] xfs: fold dfops into the transaction (Brian Foster) [1633171]
- [fs] xfs: always defer agfl block frees (Brian Foster) [1633171]
- [fs] xfs: pass transaction to xfs_defer_add() (Brian Foster) [1633171]
- [fs] xfs: replace xfs_defer_ops ->dop_pending with on-stack list (Brian Foster) [1633171]
- [fs] xfs: cancel dfops on xfs_defer_finish() error (Brian Foster) [1633171]
- [fs] xfs: clean out superfluous dfops dop params/vars (Brian Foster) [1633171]
- [fs] xfs: drop dop param from xfs_defer_op_type ->finish_item() callback (Brian Foster) [1633171]
- [fs] xfs: automatic dfops inode relogging (Brian Foster) [1633171]
- [fs] xfs: automatic dfops buffer relogging (Brian Foster) [1633171]
- [fs] xfs: add missing defer ijoins for held inodes (Brian Foster) [1633171]
- [fs] xfs: replace dop_low with transaction flag (Brian Foster) [1633171]
- [fs] xfs: pass transaction to dfops reset/move helpers (Brian Foster) [1633171]
- [fs] xfs: remove unused __xfs_defer_cancel() internal helper (Brian Foster) [1633171]
- [fs] xfs: use transaction for intent recovery instead of raw dfops (Brian Foster) [1633171]
- [fs] xfs: refactor internal dfops initialization (Brian Foster) [1633171]
- [fs] xfs: check da node magic in _node_lookup_int (Brian Foster) [1633171]
- [fs] xfs: use a local variable for magic number in xfs_da3_node_lookup_int (Brian Foster) [1633171]
- [fs] xfs: refactor log recovery check (Brian Foster) [1633171]
- [fs] xfs: move extent busy tree initialization to xfs_initialize_perag (Brian Foster) [1633171]
- [fs] xfs: avoid COW fork extent lookups in writeback if the fork didn't change (Brian Foster) [1633171]
- [fs] xfs: maintain a sequence count for inode fork manipulations (Brian Foster) [1633171]
- [fs] xfs: check for unknown v5 feature bits in superblock write verifier (Brian Foster) [1633171]
- [fs] xfs: verify icount in superblock write (Brian Foster) [1633171]
- [fs] libxfs: add more bounds checking to sb sanity checks (Brian Foster) [1633171]
- [fs] xfs: refactor superblock verifiers (Brian Foster) [1633171]
- [fs] xfs: refactor the xrep_extent_list into xfs_bitmap (Brian Foster) [1633171]
- [fs] xfs: introduce a new xfs_inode_has_cow_data helper (Brian Foster) [1633171]
- [fs] xfs: remove the xfs_ifork_t typedef (Brian Foster) [1633171]
- [fs] xfs: simplify xfs_idata_realloc (Brian Foster) [1633171]
- [fs] xfs: remove if_real_bytes (Brian Foster) [1633171]
- [fs] xfs: move the repair extent list into its own file (Brian Foster) [1633171]
- [fs] xfs: pass transaction lock while setting up agresv on cyclic metadata (Brian Foster) [1633171]
- [fs] xfs: remove deprecated barrier/nobarrier mount (Brian Foster) [1633171]
- [fs] xfs: clean up IRELE/iput callsites (Brian Foster) [1633171]
- [fs] xfs: kill IHOLD (Brian Foster) [1633171]
- [fs] xfs: bypass final dfops roll in trans commit path (Brian Foster) [1633171]
- [fs] xfs: drop unnecessary xfs_defer_finish() dfops parameter (Brian Foster) [1633171]
- [fs] xfs: remove unnecessary dfops init calls in xattr code (Brian Foster) [1633171]
- [fs] xfs: remove all boilerplate defer init/finish code (Brian Foster) [1633171]
- [fs] xfs: use internal dfops during (b|c)ui recovery (Brian Foster) [1633171]
- [fs] xfs: use internal dfops in attr code (Brian Foster) [1633171]
- [fs] xfs: use internal dfops in cow blocks cancel (Brian Foster) [1633171]
- [fs] xfs: support embedded dfops in transaction (Brian Foster) [1633171]
- [fs] xfs: pack holes in xfs_defer_ops and xfs_trans (Brian Foster) [1633171]
- [fs] xfs: reset dfops to initial state after finish (Brian Foster) [1633171]
- [fs] xfs: remove unused deferred ops committed field (Brian Foster) [1633171]
- [fs] xfs: make deferred processing safe for embedded dfops (Brian Foster) [1633171]
- [fs] xfs: fix transaction leak on remote attr set/remove failure (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops in log recovery intent processing (Brian Foster) [1633171]
- [fs] xfs: pull up dfops from xfs_itruncate_extents() (Brian Foster) [1633171]
- [fs] xfs: force summary counter recalc at next mount (Brian Foster) [1633171]
- [fs] xfs: refactor unmount record write (Brian Foster) [1633171]
- [fs] xfs: detect and fix bad summary counts at mount (Brian Foster) [1633171]
- [fs] xfs: fix indentation and other whitespace problems in scrub/repair (Brian Foster) [1633171]
- [fs] xfs: shorten struct xfs_scrub_context to struct xfs_scrub (Brian Foster) [1633171]
- [fs] xfs: shorten xfs_repair_ prefix to xrep_ (Brian Foster) [1633171]
- [fs] xfs: shorten xfs_scrub_ prefix (Brian Foster) [1633171]
- [fs] xfs: clean up xfs_btree_del_cursor callers (Brian Foster) [1633171]
- [fs] xfs: trivial xfs_btree_del_cursor cleanups (Brian Foster) [1633171]
- [fs] xfs: return from _defer_finish with a clean transaction (Brian Foster) [1633171]
- [fs] xfs: check leaf attribute block freemap in verifier (Brian Foster) [1633171]
- [fs] libxfs: Fix a couple of sparse complaintis (Brian Foster) [1633171]
- [fs] xfs: use swap macro in xfs_dir2_leafn_rebalance (Brian Foster) [1633171]
- [fs] xfs_bmap_util: use swap macro (Brian Foster) [1633171]
- [fs] xfs_attr_leaf: use swap macro in xfs_attr3_leaf_rebalance (Brian Foster) [1633171]
- [fs] xfs: don't assume a left rmap when allocating a new rmap (Brian Foster) [1633171]
- [fs] xfs: kill __xfs_buf_submit_common() (Brian Foster) [1633171]
- [fs] xfs: combine (a)sync buffer submission apis (Brian Foster) [1633171]
- [fs] xfs: use sync buffer I/O for sync delwri queue submission (Brian Foster) [1633171]
- [fs] xfs: refactor buffer submission into a common helper (Brian Foster) [1633171]
- [fs] xfs: remove xfs_defer_init() firstblock param (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in inode inactivate (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in extent swap (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in reflink cow block cancel (Brian Foster) [1633171]
- [fs] xfs: replace no-op firstblock init with ->t_firstblock (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in dq alloc (Brian Foster) [1633171]
- [fs] xfs: remove xfs_alloc_arg firstblock field (Brian Foster) [1633171]
- [fs] xfs: remove xfs_btree_cur private firstblock field (Brian Foster) [1633171]
- [fs] xfs: remove bmap format helpers firstblock params (Brian Foster) [1633171]
- [fs] xfs: remove bmap extent add helper firstblock params (Brian Foster) [1633171]
- [fs] xfs: remove xfs_bmalloca firstblock field (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in bmap extent split (Brian Foster) [1633171]
- [fs] xfs: remove bmap insert/collapse firstblock param (Brian Foster) [1633171]
- [fs] xfs: remove xfs_bunmapi() firstblock param (Brian Foster) [1633171]
- [fs] xfs: remove xfs_bmapi_write() firstblock param (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in insert/collapse range (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in xfs_bmapi_remap() (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock for all xfs_bunmapi() callers (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock for all xfs_bmapi_write() callers (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in xattr ops (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in attrfork add (Brian Foster) [1633171]
- [fs] xfs: remove firstblock param from xfs dir ops (Brian Foster) [1633171]
- [fs] xfs: use ->t_firstblock in dir ops (Brian Foster) [1633171]
- [fs] xfs: add firstblock field to xfs_trans (Brian Foster) [1633171]
- [fs] xfs: allow null firstblock in xfs_bmapi_write() when tp is null (Brian Foster) [1633171]
- [fs] xfs: refactor dfops init to attach to transaction (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops in reflink cow recover path (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops in cancel cow blocks operation (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops for rmap extent swap operations (Brian Foster) [1633171]
- [fs] xfs: remove unused btree cursor bc_private.a.dfops field (Brian Foster) [1633171]
- [fs] xfs: remove xfs_btree_cur bmbt dfops field (Brian Foster) [1633171]
- [fs] xfs: remove dfops param from internal bmap extent helpers (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops for collapse/insert range operations (Brian Foster) [1633171]
- [fs] xfs: remove struct xfs_bmalloca dfops field (Brian Foster) [1633171]
- [fs] xfs: remove xfs_bmapi_remap() dfops param (Brian Foster) [1633171]
- [fs] xfs: remove xfs_bunmapi() dfops param (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops for all xfs_bunmapi() callers (Brian Foster) [1633171]
- [fs] xfs: remove xfs_bmapi_write() dfops param (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops for all xfs_bmapi_write() callers (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops in dqalloc transaction (Brian Foster) [1633171]
- [fs] xfs: replace xfs_da_args->dfops accesses with ->t_dfops and remove (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops in extent split tx and remove param (Brian Foster) [1633171]
- [fs] xfs: remove dfops param in attr fork add path (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops for attr set/remove operations (Brian Foster) [1633171]
- [fs] xfs: use ->t_dfops for recovery of (b|c)ui log items (Brian Foster) [1633171]
- [fs] xfs: remove dfops param from high level dirname calls (Brian Foster) [1633171]
- [fs] xfs: remove dfops parameter from ifree call stack (Brian Foster) [1633171]
- [fs] xfs: rename xfs_trans ->t_agfl_dfops to ->t_dfops (Brian Foster) [1633171]
- [fs] xfs: cow unwritten conversion uses uninitialized dfops (Brian Foster) [1633171]
- [fs] xfs: update my copyrights for the writeback and iomap code (Brian Foster) [1633171]
- [fs] xfs: add support for sub-pagesize writeback without buffer_heads (Brian Foster) [1633171]
- [fs] xfs: allow writeback on pages without buffer heads (Brian Foster) [1633171]
- [fs] xfs: refactor the tail of xfs_writepage_map (Brian Foster) [1633171]
- [fs] xfs: remove xfs_start_page_writeback (Brian Foster) [1633171]
- [fs] xfs: move all writeback buffer_head manipulation into xfs_map_at_offset (Brian Foster) [1633171]
- [fs] xfs: don't look at buffer heads in xfs_add_to_ioend (Brian Foster) [1633171]
- [fs] xfs: remove the imap_valid flag (Brian Foster) [1633171]
- [fs] xfs: simplify xfs_map_blocks by using xfs_iext_lookup_extent directly (Brian Foster) [1633171]
- [fs] xfs: remove xfs_reflink_find_cow_mapping (Brian Foster) [1633171]
- [fs] xfs: remove the now unused XFS_BMAPI_IGSTATE flag (Brian Foster) [1633171]
- [fs] xfs: make xfs_writepage_map extent map centric (Brian Foster) [1633171]
- [fs] xfs: rename the offset variable in xfs_writepage_map (Brian Foster) [1633171]
- [fs] xfs: remove xfs_map_cow (Brian Foster) [1633171]
- [fs] xfs: remove xfs_reflink_trim_irec_to_next_cow (Brian Foster) [1633171]
- [fs] xfs: don't use XFS_BMAPI_IGSTATE in xfs_map_blocks (Brian Foster) [1633171]
- [fs] xfs: don't clear imap_valid for a non-uptodate buffers (Brian Foster) [1633171]
- [fs] xfs: do not set the page uptodate in xfs_writepage_map (Brian Foster) [1633171]
- [fs] xfs: move locking into xfs_bmap_punch_delalloc_range (Brian Foster) [1633171]
- [fs] xfs: simplify xfs_aops_discard_page (Brian Foster) [1633171]
- [fs] xfs: use iomap for blocksize == PAGE_SIZE readpage and readpages (Brian Foster) [1633171]
- [fs] iomap: fix WARN_ON_ONCE on uninitialized variable (Brian Foster) [1633171]
- [fs] iomap: Switch to offset_in_page for clarity (Brian Foster) [1633171]
- [fs] iomap: add support for sub-pagesize buffered I/O without buffer heads (Brian Foster) [1633171]
- [fs] iomap: add inline data support to iomap_readpage_actor (Brian Foster) [1633171]
- [fs] iomap: support direct I/O to inline data (Brian Foster) [1633171]
- [fs] iomap: refactor iomap_dio_actor (Brian Foster) [1633171]
- [fs] iomap: add initial support for writes without buffer heads (Brian Foster) [1633171]
- [fs] iomap: add an iomap-based readpage and readpages implementation (Brian Foster) [1633171]
- [fs] iomap: add private pointer to struct iomap (Brian Foster) [1633171]
- [fs] iomap: add a page_done callback (Brian Foster) [1633171]
- [fs] iomap: generic inline data handling (Brian Foster) [1633171]
- [fs] iomap: complete partial direct I/O writes synchronously (Brian Foster) [1633171]
- [fs] iomap: mark newly allocated buffer heads as new (Brian Foster) [1633171]
- [fs] fs: factor out a __generic_write_end helper (Brian Foster) [1633171]
- [netdrv] amd-xgbe: mark driver as tech preview (David Arcari) [1633209]
- [fs] ext4, dax: set ext4_dax_aops for dax files (Lukas Czerner) [1633239]
- [fs] ext4, dax: add ext4_bmap to ext4_dax_aops (Lukas Czerner) [1633239]
- [fs] ext4: don't mark mmp buffer head dirty (Lukas Czerner) [1633239]
- [fs] ext4: show test_dummy_encryption mount option in /proc/mounts (Lukas Czerner) [1633239]
- [fs] ext4: fix online resizing for bigalloc file systems with a 1k block size (Lukas Czerner) [1633239]
- [fs] ext4: fix online resize's handling of a too-small final block group (Lukas Czerner) [1633239]
- [fs] ext4: recalucate superblock checksum after updating free blocks/inodes (Lukas Czerner) [1633239]
- [fs] ext4: avoid arithemetic overflow that can trigger a BUG (Lukas Czerner) [1633239]
- [fs] ext4: avoid divide by zero fault when deleting corrupted inline directories (Lukas Czerner) [1633239]
- [fs] ext4: check to make sure the rename(2)'s destination is not freed (Lukas Czerner) [1633239]
- [fs] ext4: remove unneeded variable "err" in ext4_mb_release_inode_pa() (Lukas Czerner) [1633239]
- [fs] ext4: fix spectre gadget in ext4_mb_regular_allocator() (Lukas Czerner) [1633239]
- [fs] ext4: check for NUL characters in extended attribute's name (Lukas Czerner) [1633239]
- [fs] ext4: use ext4_warning() for sb_getblk failure (Lukas Czerner) [1633239]
- [fs] ext4: fix race when setting the bitmap corrupted flag (Lukas Czerner) [1633239]
- [fs] ext4: reset error code in ext4_find_entry in fallback (Lukas Czerner) [1633239]
- [fs] ext4: check allocation failure when duplicating "data" in ext4_remount() (Lukas Czerner) [1633239]
- [fs] ext4: sysfs: print ext4_super_block fields as little-endian (Lukas Czerner) [1633239]
- [firmware] efi/x86: Handle page faults occurring while running EFI runtime services (Bhupesh Sharma) [1627557]
- [firmware] efi: Make efi_rts_work accessible to efi page fault handler (Bhupesh Sharma) [1627557]
- [firmware] efi: Remove the declaration of efi_late_init() as the function is unused (Bhupesh Sharma) [1627557]
- [firmware] efi: Use a work queue to invoke EFI Runtime Services (Bhupesh Sharma) [1627557]
- [firmware] efi/x86: Use non-blocking SetVariable() for efi_delete_dummy_variable() (Bhupesh Sharma) [1627557]
- [fs] gfs2: Special-case rindex for gfs2_grow (Robert S Peterson) [1628360]
- [fs] GFS2: Fix recovery issues for spectators (Robert S Peterson) [1628298]

* Fri Oct 05 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-22.el8]
- [powerpc] powerpc/pkeys: Fix reading of ibm, processor-storage-keys property (Steve Best) [1633551]
- [powerpc] powerpc/pseries: Remove unneeded uses of dlpar work queue (Steve Best) [1633544]
- [powerpc] powerpc/pseries: Remove prrn_work workqueue (Steve Best) [1633544]
- [pci] ACPI / hotplug / PCI: Don't scan for non-hotplug bridges if slot is not bridge (Myron Stowe) [1634816]
- [pci] PCI: Fix enabling of PASID on RC integrated endpoints (Myron Stowe) [1634816]
- [pci] IB/hfi1,PCI: Allow bus reset while probing (Myron Stowe) [1634816]
- [pci] PCI: Fix faulty logic in pci_reset_bus() (Myron Stowe) [1634816]
- [pci] PCI: pciehp: Fix hot-add vs powerfault detection order (Myron Stowe) [1634816]
- [pci] Revert "PCI: Add ACS quirk for Intel 300 series" (Myron Stowe) [1634816]
- [powerpc] powerpc/numa: Use associativity if VPHN hcall is successful (Steve Best) [1633569]
- [pci] PCI: vmd: White list for fast interrupt handlers (Myron Stowe) [1632816]
- [pci] PCI: Add function 1 DMA alias quirk for Marvell 88SS9183 (Myron Stowe) [1632816]
- [pci] PCI: Rename pci_try_reset_bus() to pci_reset_bus() (Myron Stowe) [1632816]
- [pci] PCI: Deprecate pci_reset_bus() and pci_reset_slot() functions (Myron Stowe) [1632816]
- [pci] PCI: Unify try slot and bus reset API (Myron Stowe) [1632816]
- [pci] PCI: Hide pci_reset_bridge_secondary_bus() from drivers (Myron Stowe) [1632816]
- [pci] IB/hfi1: Use pci_try_reset_bus() for initiating PCI Secondary Bus Reset (Myron Stowe) [1632816]
- [pci] PCI: Handle error return from pci_reset_bridge_secondary_bus() (Myron Stowe) [1632816]
- [pci] PCI/IOV: Tidy pci_sriov_set_totalvfs() (Myron Stowe) [1632816]
- [pci] PCI: Enable PASID only if entire path supports End-End TLP prefixes (Myron Stowe) [1632816]
- [pci] PCI: Expand documentation for pci_add_dma_alias() (Myron Stowe) [1632816]
- [pci] PCI: Add DMA alias quirk for Microsemi Switchtec NTB (Myron Stowe) [1632816]
- [pci] switchtec: Use generic PCI Vendor ID and Class Code (Myron Stowe) [1632816]
- [pci] PCI: Make pci_get_rom_size() static (Myron Stowe) [1632816]
- [pci] PCI: Add check code for last image indicator not set (Myron Stowe) [1632816]
- [pci] PCI: Avoid accessing memory outside the ROM BAR (Myron Stowe) [1632816]
- [pci] PCI: Make early dump functionality generic (Myron Stowe) [1632816]
- [pci] PCI: Cleanup PCI_REBAR_CTRL_BAR_SHIFT handling (Myron Stowe) [1632816]
- [pci] PCI: Restore resized BAR state on resume (Myron Stowe) [1632816]
- [pci] PCI: Clean up resource allocation in devm_of_pci_get_host_bridge_resources() (Myron Stowe) [1632816]
- [pci] PCI: Add ACS Redirect disable quirk for Intel Sunrise Point (Myron Stowe) [1632816]
- [pci] PCI: Add device-specific ACS Redirect disable infrastructure (Myron Stowe) [1632816]
- [pci] PCI: Convert device-specific ACS quirks from NULL termination to ARRAY_SIZE (Myron Stowe) [1632816]
- [pci] PCI: Add "pci=disable_acs_redir=" parameter for peer-to-peer support (Myron Stowe) [1632816]
- [pci] PCI: Allow specifying devices using a base bus and path of devfns (Myron Stowe) [1632816]
- [pci] PCI: Make specifying PCI devices in kernel parameters reusable (Myron Stowe) [1632816]
- [pci] PCI: Hide ACS quirk declarations inside PCI core (Myron Stowe) [1632816]
- [pci] PCI: Document ACPI description of PCI host bridges (Myron Stowe) [1632816]
- [pci] PCI/MSI: Set IRQCHIP_ONESHOT_SAFE for PCI-MSI irqchips (Myron Stowe) [1632816]
- [pci] PCI: Limit config space size for Netronome NFP5000 (Myron Stowe) [1632816]
- [pci] PCI: Add PCI_DEVICE_DATA() macro to fully describe device ID entry (Myron Stowe) [1632816]
- [pci] PCI: Unify PCI and normal DMA direction definitions (Myron Stowe) [1632816]
- [pci] PCI: Use IRQF_ONESHOT if pci_request_irq() called with no handler (Myron Stowe) [1632816]
- [pci] PCI: Call dma_debug_add_bus() for pci_bus_type from PCI core (Myron Stowe) [1632816]
- [pci] PCI: Mark fall-through switch cases before enabling -Wimplicit-fallthrough (Myron Stowe) [1632816]

* Thu Oct 04 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-21.el8]
- [s390] s390/sclp: Allow to request adapter reset (Philipp Rudo) [1635273]
- [char] ipmi: Fix NULL pointer dereference in ssif_probe (Tony Camuso) [1635366]
- [char] ipmi: Fix I2C client removal in the SSIF driver (Tony Camuso) [1635366]
- [char] ipmi: kcs_bmc: don't change device name (Tony Camuso) [1635366]
- [kernel] timers: Clear timer_base::must_forward_clk with timer_base::lock held (Waiman Long) [1632820]
- [pci] switchtec: Fix Spectre v1 vulnerability (Waiman Long) [1632820]
- [kernel] cpu/hotplug: Prevent state corruption on error rollback (Waiman Long) [1632820]
- [kernel] cpu/hotplug: Adjust misplaced smb() in cpuhp_thread_fun() (Waiman Long) [1632820]
- [base] memory_hotplug: fix kernel_panic on offline page processing (Waiman Long) [1632820]
- [mm] mm/hugetlb: filter out hugetlb pages if HUGEPAGE migration is not supported (Waiman Long) [1632820]
- [lib] debugobjects: Make stack check warning more informative (Waiman Long) [1632820]
- [fs] fs/dcache.c: fix kmemcheck splat at take_dentry_name_snapshot() (Waiman Long) [1632820]
- [x86] x86/process: Don't mix user/kernel regs in 64bit __show_regs() (Waiman Long) [1632820]
- [x86] x86/dumpstack: Don't dump kernel memory based on usermode RIP (Waiman Long) [1632820]
- [x86] x86: Avoid pr_cont() in show_opcodes() (Waiman Long) [1632820]
- [x86] x86/entry/64: Wipe KASAN stack shadow before rewind_stack_do_exit() (Waiman Long) [1632820]
- [x86] x86/speculation/l1tf: Increase l1tf memory limit for Nehalem+ (Waiman Long) [1632820]
- [x86] x86/spectre: Add missing family 6 check to microcode check (Waiman Long) [1632820]
- [x86] x86/nmi: Fix NMI uaccess race against CR3 switching (Waiman Long) [1632820]
- [x86] x86/vdso: Fix lsl operand order (Waiman Long) [1632820]
- [x86] x86/vdso: Fix vDSO build if a retpoline is emitted (Waiman Long) [1632820]
- [x86] x86/speculation/l1tf: Suggest what to do on systems with too much RAM (Waiman Long) [1632820]
- [x86] x86/speculation/l1tf: Fix off-by-one error when warning that system has too much RAM (Waiman Long) [1632820]
- [x86] x86/speculation/l1tf: Fix overflow in l1tf_pfn_limit() on 32bit (Waiman Long) [1632820]
- [x86] x86/speculation/l1tf: Exempt zeroed PTEs from inversion (Waiman Long) [1632820]
- [x86] x86/mm/pti: Clear Global bit more aggressively (Waiman Long) [1632820]
- [x86] x86/paravirt: Fix spectre-v2 mitigations for paravirt guests (Waiman Long) [1632820]
- [target] scsi: target: iscsi: Use bin2hex instead of a re-implementation (Maurizio Lombardi) [1632184] {CVE-2018-14633}
- [target] scsi: target: iscsi: Use hex2bin instead of a re-implementation (Maurizio Lombardi) [1632184] {CVE-2018-14633}

* Wed Oct 03 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-20.el8]
- [netdrv] ibmvnic: Include missing return code checks in reset function (Steve Best) [1633553]
- [netdrv] ibmvnic: Update firmware error reporting with cause string (Steve Best) [1633553]
- [netdrv] ibmvnic: Remove code to request error information (Steve Best) [1633553]
- [s390] s390/qeth: remove duplicated carrier state tracking (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: clean up drop conditions for received cmds (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: re-indent qeth_check_ipa_data() (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: consume local address events (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove various redundant code (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove CARD_FROM_CDEV helper (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: pass card pointer in iob callback (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: re-use qeth_notify_skbs() (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove additional skb refcount (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: replace open-coded skb_queue_walk() (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: on gdev release, reset drvdata (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: fix discipline unload after setup error (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: use DEFINE_MUTEX for qeth_mod_mutex (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: convert layer attribute to enum (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: reduce 0-initializing when building IPA cmds (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: fine-tune spinlocks (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: fix typo in return value (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: invoke softirqs after napi_schedule() (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: uninstall IRQ handler on device removal (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove qeth_hdr_chk_and_bounce() (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: speed up TSO transmission (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: prepare for copy-free TSO transmission (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: check size of required HW header cache object (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: fix up protocol headers early (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: limit csum offload erratum to L3 devices (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove qeth_get_elements_no() (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove unused L3 xmit code (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: run non-offload L3 traffic over common xmit path (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: move L2 xmit code to core module (Hendrik Brueckner) [1633841]
- [s390] s390/qdio: reset old sbal_state flags (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: don't dump past end of unknown HW header (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: use vzalloc for QUERY OAT buffer (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: switch on SG by default for IQD devices (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: indicate error when netdev allocation fails (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: use true and false for boolean values (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: don't restrict qeth_card to DMA memory (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: clean up card initialization (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: do basic setup for data channel (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: use qeth_setup_ccw() to set up all CCWs (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: reduce hard-coded access to ccw channels (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: extract helper for MPC protocol type (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: speed up L2 IQD xmit (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: add support for constrained HW headers (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: merge linearize-check into HW header construction (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: add statistics for consumed buffer elements (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: use core MTU range checking (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: simplify max MTU handling (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: don't cache HW port number (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: allocate netdevice early (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove redundant netif_carrier_ok() checks (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: reset layer2 attribute on layer switch (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: fix race in used-buffer accounting (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: speed-up IPv4 OSA xmit (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: speed-up L3 IQD xmit (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: add a L3 xmit wrapper (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: increase GSO max size for eligible L3 devices (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: clean up exported symbols (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: consolidate ccwgroup driver definition (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: clean up Output Queue selection (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: fine-tune RX modesetting (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: remove unused buffer->aob pointer (Hendrik Brueckner) [1633841]
- [s390] s390/qeth: various buffer management cleanups (Hendrik Brueckner) [1633841]
- [powerpc] powerpc: Avoid code patching freed init sections (Steve Best) [1633545]
- [powerpc] powerpc/tm: Fix userspace r13 corruption (Steve Best) [1633543]
- [powerpc] powerpc/tm: Avoid possible userspace r1 corruption on reclaim (Steve Best) [1633543]
- [drm] drm/i915/cfl: Add a new CFL PCI ID (Rob Clark) [1626883]
- [drm] drm/i915/aml: Introducing Amber Lake platform (Rob Clark) [1626883]
- [drm] drm/i915/whl: Introducing Whiskey Lake platform (Rob Clark) [1626883]
- [char] ipmi: Move BT capabilities detection to the detect call (Frank Ramsay) [1618774]
- [char] ipmi: Rework SMI registration failure (Frank Ramsay) [1618774]

* Tue Oct 02 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-19.el8]
- [s390] s390: detect etoken facility (Thomas Huth) [1634069]
- [s390] s390/lib: use expoline for all bcr instructions (Thomas Huth) [1634069]
- [documentation] vm.txt: Adding 'nr_hugepages_mempolicy' parameter description (Prashant Dhamdhere) [1626547]

* Mon Oct 01 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-18.el8]
- [scsi] scsi: ipr: System hung while dlpar adding primary ipr adapter back (Steve Best) [1633217]
- [target] scsi: iscsi: target: Don't use stack buffer for scatterlist (Maurizio Lombardi) [1631342]
- [rpmspec] Forward port weak-modules support from RHEL 7 to RHEL 8 ("Herton R. Krzesinski") [1596884]
- [fs] xfs: Close race between direct IO and xfs_break_layouts() (Eric Sandeen) [1622191]
- [fs] xfs: remove unused iolock arg from xfs_break_dax_layouts (Eric Sandeen) [1622191]
- [fs] ext4: Close race between direct IO and ext4_break_layouts() (Eric Sandeen) [1616303]
- [fs] ext4: handle layout changes to pinned DAX mappings (Eric Sandeen) [1614154]
- [fs] dax: dax_layout_busy_page() warn on !exceptional (Eric Sandeen) [1614154]
- [fs] dax: mark tech preview (Eric Sandeen) [1627455]
- [mm] usercopy: Allow boot cmdline disabling of hardening (Christoph von Recklinghausen) [1589928]

* Thu Sep 27 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-17.el8]
- [s390] s390/crypto: Fix return code checking in cbc_paes_crypt() (Philipp Rudo) [1633266]
- [drm] amd/display/dc/basics/logger.c: fix build error with CONFIG_FORTIFY_SOURCE=y ("Herton R. Krzesinski") [1548068]
- [acpi] ACPICA: AML Parser: skip opcodes that open a scope upon parse failure (Jeremy Linton) [1609885]
- [acpi] ACPICA: ACPICA: add status check for acpi_hw_read before assigning return value (Jeremy Linton) [1609885]
- [acpi] ACPICA: AML Parser: ignore all exceptions resulting from incorrect AML during table load (Jeremy Linton) [1609885]
- [rpmspec] spec: Add missing BuildRequires for bpftool (Jiri Olsa) [1632756]
- [powerpc] KVM: PPC: Avoid marking DMA-mapped pages dirty in real mode (David Gibson) [1628412]
- [powerpc] powerpc/powernv/ioda: Allocate indirect TCE levels on demand (David Gibson) [1628412]
- [powerpc] powerpc/powernv: Rework TCE level allocation (David Gibson) [1628412]
- [powerpc] powerpc/powernv: Add indirect levels to it_userspace (David Gibson) [1628412]
- [powerpc] KVM: PPC: Make iommu_table::it_userspace big endian (David Gibson) [1628412]
- [powerpc] powerpc/powernv: Move TCE manupulation code to its own file (David Gibson) [1628412]
- [net] net_sched: fix NULL pointer dereference when delete tcindex filter (Andrea Claudi) [1627648]
- [net] net_sched: Fix missing res info when create new tc_index filter (Andrea Claudi) [1627648]
- [samples] samples/bpf: xdpsock: order memory on AArch64 (Jesper Brouer) [1615959]
- [samples] samples/bpf: xdp_redirect_cpu load balance like Suricata (Jesper Brouer) [1615959]
- [samples] samples/bpf: add Paul Hsieh's (LGPL 2.1) hash function SuperFastHash (Jesper Brouer) [1615959]
- [samples] samples/bpf: xdp_redirect_cpu handle parsing of double VLAN tagged packets (Jesper Brouer) [1615959]
- [samples] samples/bpf: all XDP samples should unload xdp/bpf prog on SIGTERM (Jesper Brouer) [1615959]
- [samples] samples/bpf: xdp_rxq_info action XDP_TX must adjust MAC-addrs (Jesper Brouer) [1615959]
- [samples] samples/bpf: extend xdp_rxq_info to read packet payload (Jesper Brouer) [1615959]
- [powerpc] KVM: PPC: Book3S HV: Use correct pagesize in kvm_unmap_radix() (David Gibson) [1625498]
- [net] igmp: fix incorrect unsolicit report count after link down and up (Hangbin Liu) [1625538]
- [net] igmp: fix incorrect unsolicit report count when join group (Hangbin Liu) [1625538]
- [netdrv] cxgb4: update 1.20.8.0 as the latest firmware supported (Arjun Vynipadath) [1622555]
- [virt] svm: nested virt support off by default (Bandan Das) [1571993]

* Wed Sep 26 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-16.el8]
- [powerpc] KVM: PPC: Book3S HV: Don't use compound_order to determine host mapping size (David Gibson) [1625860]
- [virt] arm64: KVM: Remove pgd_lock (Wei Huang) [1627474]
- [virt] KVM: Remove obsolete kvm_unmap_hva notifier backend (Wei Huang) [1627474]
- [virt] arm64: KVM: Only force FPEXC32_EL2.EN if trapping FPSIMD (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Clean dcache to PoC when changing PTE due to CoW (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Skip updating PTE entry if no change (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Skip updating PMD entry if no change (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Move DEBUG_SPINLOCK_BUG_ON to vgic.h (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Do not use spin_lock_irqsave/restore with irq disabled (Wei Huang) [1627474]
- [virt] KVM: arm: vgic-v3: Add support for ICC_SGI0R and ICC_ASGI1R accesses (Wei Huang) [1627474]
- [virt] KVM: arm64: vgic-v3: Add support for ICC_SGI0R_EL1 and ICC_ASGI1R_EL1 accesses (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic-v3: Add core support for Group0 SGIs (Wei Huang) [1627474]
- [virt] KVM: arm64: Remove non-existent AArch32 ICC_SGI1R encoding (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Fix lost IRQs from emulated physcial timer when blocked (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Fix potential loss of ptimer interrupts (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Fix possible spectre-v1 write in vgic_mmio_write_apr() (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Update documentation of the GIC devices wrt IIDR (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Let userspace opt-in to writable v2 IGROUPR (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Allow configuration of interrupt groups (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Return error on incompatible uaccess GICD_IIDR writes (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Permit uaccess writes to return errors (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Signal IRQs using their configured group (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Add group field to struct irq (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: GICv2 IGROUPR should read as zero (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Keep track of implementation revision (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic: Define GICD_IIDR fields for GICv2 and GIv3 (Wei Huang) [1627474]
- [virt] arm64: KVM: Cleanup tpidr_el2 init on non-VHE (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: vgic-debug: Show LPI status (Wei Huang) [1627474]
- [virt] KVM: arm64: vgic-its: Remove VLA usage (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Fix vgic init race (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Enable adaptative WFE trapping (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Remove unnecessary CMOs when creating HYP page tables (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Stop using the kernel's (pmd, pud, pgd)_populate helpers (Wei Huang) [1627474]
- [virt] KVM: arm/arm64: Consolidate page-table accessors (Wei Huang) [1627474]
- [virt] arm64: KVM: Avoid marking pages as XN in Stage-2 if CTR_EL0.DIC is set (Wei Huang) [1627474]
- [tools] radix tree test suite: Enable ubsan (Waiman Long) [1630244]
- [tools] radix tree test suite: Fix compilation (Waiman Long) [1630244]
- [block] blk-wbt: don't maintain inflight counts if disabled (Ming Lei) [1622790]
- [block] blk-wbt: fix has-sleeper queueing check (Ming Lei) [1622790]
- [block] blk-wbt: use wq_has_sleeper() for wq active check (Ming Lei) [1622790]
- [block] blk-wbt: move disable check into get_limit() (Ming Lei) [1622790]
- [block] block/DAC960.c: make some arrays static const, shrinks object (Ming Lei) [1622790]
- [block] blk-mq: sync the update nr_hw_queues with (Ming Lei) [1617959]
- [block] blk-mq: init hctx sched after update ctx and hctx mapping (Ming Lei) [1617959]
- [block] block: remove duplicate initialization (Ming Lei) [1622790]
- [block] tracing/blktrace: Fix to allow setting same value (Ming Lei) [1622790]
- [block] pktcdvd: fix setting of 'ret' error return for a few cases (Ming Lei) [1622790]
- [block] block: change return type to bool (Ming Lei) [1622790]
- [block] block, bfq: return nbytes and not zero from struct cftype (Ming Lei) [1622790]
- [block] block, bfq: improve code of bfq_bfqq_charge_time (Ming Lei) [1622790]
- [block] block, bfq: reduce write overcharge (Ming Lei) [1622790]
- [block] block, bfq: always update the budget of an entity when needed (Ming Lei) [1622790]
- [block] block, bfq: readd missing reset of parent-entity service (Ming Lei) [1622790]
- [block] block: don't warn for flush on read-only device (Ming Lei) [1622809]

* Tue Sep 25 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-15.el8]
- [kernel] locking/rwsem: Make owner store task pointer of last owning reader (Waiman Long) [1631842]
- [kernel] locking/rwsem: Exit read lock slowpath if queue empty & no writer (Waiman Long) [1631842]
- [x86] x86/microcode: Update the new microcode revision unconditionally (Prarit Bhargava) [1630931]
- [x86] x86/microcode: Make sure boot_cpu_data.microcode is up-to-date (Prarit Bhargava) [1630931]
- [arm64] arm64: tlb: Provide forward declaration of tlb_flush() before including tlb.h (Waiman Long) [1630521]
- [x86] x86/mm: Only use tlb_remove_table() for paravirt (Waiman Long) [1630521]
- [mm] mm: mmu_notifier fix for tlb_end_vma (Waiman Long) [1630521]
- [mm] mm/tlb, x86/mm: Support invalidating TLB caches for RCU_TABLE_FREE (Waiman Long) [1630521]
- [mm] mm/tlb: Remove tlb_remove_table() non-concurrent condition (Waiman Long) [1630521]
- [mm] mm: move tlb_table_flush to tlb_flush_mmu_free (Waiman Long) [1630521]
- [kernel] clocksource: Revert Remove kthread (Waiman Long) [1628402]
- [cpuidle] cpuidle: menu: Retain tick when shallow state is selected (Waiman Long) [1628402]
- [cpufreq] cpufreq: governor: Avoid accessing invalid governor_data (Waiman Long) [1628402]
- [cpuidle] cpuidle: menu: Handle stopped tick more aggressively (Waiman Long) [1628402]
- [kernel] sched: idle: Avoid retaining the tick when it has been stopped (Waiman Long) [1628402]
- [net] netfilter: xt_hashlimit: do not crash when reading proc file (Florian Westphal) [1630131]
- [x86] x86/boot/KASLR: Skip specified number of 1GB huge pages when doing physical randomization (KASLR) (Baoquan He) [1564824]
- [x86] x86/boot/KASLR: Add two new functions for 1GB huge pages handling (Baoquan He) [1564824]
- [mfd] mfd: intel-lpss: Add Ice Lake PCI IDs (Gopal Tiwari) [1483477]
- [mmc] mmc: sdhci-pci: Add support for Intel ICP (Gopal Tiwari) [1483496]

* Mon Sep 24 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-14.el8]
- [mm] mm: get rid of vmacache_flush_all() entirely (Waiman Long) [1631297] {CVE-2018-17182}
- [mm] mm, vmacache: hash addresses based on pmd (Waiman Long) [1631297] {CVE-2018-17182}
- [mm] mm: Allocate the mm_cpumask (mm->cpu_bitmap) dynamically based on nr_cpu_ids (Waiman Long) [1631297] {CVE-2018-17182}
- [infiniband] IB/hfi1: Invalid NUMA node information can cause a divide by zero (Alex Estrin) [1622222]
- [nvdimm] libnvdimm: Export max available extent (Jeff Moyer) [1627874]
- [nvdimm] libnvdimm: Use max contiguous area for namespace size (Jeff Moyer) [1627874]
- [netdrv] ice: Fix and update driver version string (Jonathan Toppins) [1611786]
- [netdrv] ice: Introduce SERVICE_DIS flag and service routine functions (Jonathan Toppins) [1611786]
- [netdrv] ice: Enable VSI Rx/Tx pruning only when VLAN 0 is active (Jonathan Toppins) [1611786]
- [netdrv] ice: Enable firmware logging during device initialization (Jonathan Toppins) [1611786]
- [netdrv] ice: Implement ice_bridge_getlink and ice_bridge_setlink (Jonathan Toppins) [1611786]
- [netdrv] ice: Add support for Tx hang, Tx timeout and malicious driver detection (Jonathan Toppins) [1611786]
- [netdrv] ice: Clean up register file (Jonathan Toppins) [1611786]
- [netdrv] ice: Implement handlers for ethtool PHY/link operations (Jonathan Toppins) [1611786]
- [netdrv] ice: Refactor VSI allocation, deletion and rebuild flow (Jonathan Toppins) [1611786]
- [netdrv] ice: Refactor switch rule management structures and functions (Jonathan Toppins) [1611786]
- [netdrv] ice: Code optimization for ice_fill_sw_rule() (Jonathan Toppins) [1611786]
- [netdrv] ice: Prevent control queue operations during reset (Jonathan Toppins) [1611786]
- [netdrv] ice: Update request resource command to latest specification (Jonathan Toppins) [1611786]
- [netdrv] ice: Updates to Tx scheduler code (Jonathan Toppins) [1611786]
- [netdrv] ice: Rework flex descriptor programming (Jonathan Toppins) [1611786]
- [netdrv] net/mlx5: Fix SQ offset in QPs with small RQ (Alaa Hleihel) [1623367]
- [x86] x86/spec_ctrl: Make IBRS code work with SSBD mitigation (Waiman Long) [1565180]
- [x86] x86/spec_ctrl: Auto-enable IBRS on Skylake (Waiman Long) [1565180]
- [x86] x86/spec_ctrl: Extend spectre_v2 boot option to support IBRS (Waiman Long) [1565180]
- [x86] x86/spec_ctrl: Boot time IBRS initialization (Waiman Long) [1565180]
- [x86] x86/spec_ctrl: Add IBRS code to the 64-bit assembly entry code (Waiman Long) [1565180]
- [x86] x86/cpufeatures: Increase NCAPINTS for future extension (Waiman Long) [1565180]
- [netdrv] ice: Trivial formatting fixes (Jonathan Toppins) [1611783]
- [netdrv] ice: Change struct members from bool to u8 (Jonathan Toppins) [1611783]
- [netdrv] ice: Fix potential return of uninitialized value (Jonathan Toppins) [1611783]
- [netdrv] ice: Fix a few null pointer dereference issues (Jonathan Toppins) [1611783]
- [netdrv] ice: Update to interrupts enabled in OICR (Jonathan Toppins) [1611783]
- [netdrv] ice: Set VLAN flags correctly (Jonathan Toppins) [1611783]
- [netdrv] ice: Use order_base_2 to calculate higher power of 2 (Jonathan Toppins) [1611783]
- [netdrv] ice: Fix bugs in control queue processing (Jonathan Toppins) [1611783]
- [netdrv] ice: Clean control queues only when they are initialized (Jonathan Toppins) [1611783]
- [netdrv] ice: Report stats for allocated queues via ethtool stats (Jonathan Toppins) [1611783]
- [netdrv] ice: Cleanup magic number (Jonathan Toppins) [1611783]
- [netdrv] ice: Remove unnecessary node owner check (Jonathan Toppins) [1611783]
- [netdrv] ice: Fix multiple static analyser warnings (Jonathan Toppins) [1611783]
- [virt] KVM: VMX: fixes for vmentry_l1d_flush module parameter (Waiman Long) [1616248] {CVE-2018-15572}
- [virt] KVM: x86: SVM: Call x86_spec_ctrl_set_guest/host() with interrupts disabled (Waiman Long) [1616248] {CVE-2018-15572}
- [virt] x86/kvm/vmx: Fix coding style in vmx_setup_l1d_flush() (Waiman Long) [1616248] {CVE-2018-15572}
- [x86] x86/speculation: Support Enhanced IBRS on future CPUs (Waiman Long) [1614144]
- [x86] x86/speculation: Protect against userspace-userspace spectreRSB (Waiman Long) [1616248] {CVE-2018-15572}
- [x86] x86/speculation: Remove SPECTRE_V2_IBRS in enum spectre_v2_mitigation (Waiman Long) [1616248] {CVE-2018-15572}
- [cpufreq] cpufreq: Fix a circular lock dependency problem (Waiman Long) [1599154]
- [kernel] cpu/hotplug: Add a cpus_read_trylock() function (Waiman Long) [1599154]
- [virt] xen/spinlock: Don't use pvqspinlock if only 1 vCPU (Waiman Long) [1618486]

* Thu Sep 20 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-13.el8]
- [mailbox] mailbox: PCC: handle parse error (David Arcari) [1630382]
- [hv] vmbus: don't return values for uninitalized channels (Vitaly Kuznetsov) [1617954]
- [mm] kernel/memremap, kasan: make ZONE_DEVICE with work with KASAN (Bill O'Donnell) [1629578]
- [mm] mm: fix BUG_ON() in vmf_insert_pfn_pud() from VM_MIXEDMAP removal (Jeff Moyer) [1622171]
- [mm] dax: remove VM_MIXEDMAP for fsdax and device dax (Jeff Moyer) [1622171]

* Wed Sep 19 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-12.el8]
- [i2c] i2c: i801: fix DNV's SMBCTRL register offset (David Arcari) [1628861]
- [fs] ceph: avoid a use-after-free in ceph_destroy_options() (Ilya Dryomov) [1629884]
- [fs] ceph: fix incorrect use of strncpy (Ilya Dryomov) [1629884]
- [block] rbd: support cloning across namespaces (Ilya Dryomov) [1629884]
- [block] rbd: factor out get_parent_info() (Ilya Dryomov) [1629884]
- [block] rbd: support for images within namespaces (Ilya Dryomov) [1629884]
- [block] rbd: pass rbd_spec into parse_rbd_opts_token() (Ilya Dryomov) [1629884]
- [net] libceph: weaken sizeof check in ceph_x_verify_authorizer_reply() (Ilya Dryomov) [1629884]
- [net] libceph: check authorizer reply/challenge length before reading (Ilya Dryomov) [1629884]
- [net] libceph: implement CEPHX_V2 calculation mode (Ilya Dryomov) [1629884]
- [net] libceph: add authorizer challenge (Ilya Dryomov) [1629884]
- [net] libceph: factor out encrypt_authorizer() (Ilya Dryomov) [1629884]
- [net] libceph: factor out __ceph_x_decrypt() (Ilya Dryomov) [1629884]
- [net] libceph: factor out __prepare_write_connect() (Ilya Dryomov) [1629884]
- [net] libceph: store ceph_auth_handshake pointer in ceph_connection (Ilya Dryomov) [1629884]
- [pci] PCI: pciehp: Deduplicate presence check on probe & resume (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Avoid implicit fallthroughs in switch statements (Myron Stowe) [1583983]
- [pci] PCI: Whitelist Thunderbolt ports for runtime D3 (Myron Stowe) [1583983]
- [pci] PCI: Whitelist native hotplug ports for runtime D3 (Myron Stowe) [1583983]
- [pci] PCI: sysfs: Resume to D0 on function reset (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Resume parent to D0 on config space access (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Resume to D0 on enable/disable (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Support interrupts sent from D3hot (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Obey compulsory command delay after resume (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Clear spurious events earlier on resume (Myron Stowe) [1583983]
- [pci] PCI: portdrv: Deduplicate PM callback iterator (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Avoid slot access during reset (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Always enable occupied slot on probe (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Become resilient to missed events (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Tolerate initially unstable link (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Declare pciehp_enable/disable_slot() static (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Drop enable/disable lock (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Enable/disable exclusively from IRQ thread (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Track enable/disable status (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Publish to user space last on probe (Myron Stowe) [1583983]
- [pci] PCI: hotplug: Demidlayer registration with the core (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Drop slot workqueue (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Handle events synchronously (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Stop blinking on slot enable failure (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Convert to threaded polling (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Convert to threaded IRQ (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Document struct slot and struct controller (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Declare pciehp_unconfigure_device() void (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Drop unnecessary NULL pointer check (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Fix unprotected list iteration in IRQ handler (Myron Stowe) [1583983]
- [pci] PCI: pciehp: Fix use-after-free on unplug (Myron Stowe) [1583983]
- [pci] PCI: hotplug: Don't leak pci_slot on registration failure (Myron Stowe) [1583983]
- [pci] PCI: hotplug: Delete skeleton driver (Myron Stowe) [1583983]
- [netdrv] be2net: Use Kconfig flag to support for enabling/disabling adapters (Petr Oros) [1611768]
- [acpi] ACPICA: Reference Counts: increase max to 0x4000 for large servers (Frank Ramsay) [1618760]

* Tue Sep 18 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-11.el8]
- [net] udp6: add missing checks on edumux packet processing (Paolo Abeni) [1625954]
- [net] udp4: fix IP_CMSG_CHECKSUM for connected sockets (Paolo Abeni) [1625954]
- [s390] s390/pci: fix out of bounds access during irq setup (Hendrik Brueckner) [1627462]
- [nvdimm] libnvdimm: fix ars_status output length calculation (Jeff Moyer) [1616307]

* Mon Sep 17 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-10.el8]
- [scsi] scsi: lpfc: Correct MDS diag and nvmet configuration (Dick Kennedy) [1628323]
- [iommu] iommu/arm-smmu: workaround DMA mode issues (Mark Salter) [1624077]
- [x86] x86/microcode: Allow late microcode loading with SMT disabled (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] tools headers: Synchronise x86 cpufeatures.h for L1TF additions (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/mm/kmmio: Make the tracer robust against L1TF (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/mm/pat: Make set_memory_np() L1TF safe (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Make pmd/pud_mknotpresent() invert (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Invert all not present mappings (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Fix SMT supported evaluation (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] KVM: VMX: Tell the nested hypervisor to skip L1D flush on vmentry (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation: Use ARCH_CAPABILITIES to skip L1D flush on vmentry (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation: Simplify sysfs report of VMX L1TF vulnerability (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] Documentation/l1tf: Remove Yonah processors from not vulnerable list (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Don't set l1tf_flush_l1d from vmx_handle_external_intr() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/irq: Let interrupt handlers set kvm_cpu_l1tf_flush_l1d (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86: Don't include linux/irq.h from asm/hardirq.h (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Introduce per-host-cpu analogue of l1tf_flush_l1d (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/irq: Demote irq_cpustat_t::__softirq_pending to u16 (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Move the l1tf_flush_l1d test to vmx_l1d_flush() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Replace 'vmx_l1d_flush_always' with 'vmx_l1d_flush_cond' (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Don't set l1tf_flush_l1d to true from vmx_l1d_flush() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: detect SMT disabled by BIOS (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] Documentation/l1tf: Fix typos (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Initialize the vmx_l1d_flush_pages' content (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Unbreak !__HAVE_ARCH_PFN_MODIFY_ALLOWED architectures (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] Documentation: Add section about CPU vulnerabilities (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/bugs, kvm: Introduce boot-time control of L1TF mitigations (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Set CPU_SMT_NOT_SUPPORTED early (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Expose SMT control init function (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/kvm: Allow runtime control of L1D flush (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/kvm: Serialize L1D flush parameter setter (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/kvm: Add static key for flush always (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/kvm: Move l1tf setup function (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/l1tf: Handle EPT disabled state proper (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/kvm: Drop L1TF MSR list approach (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/litf: Introduce vmx status variable (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Online siblings when SMT control is turned on (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Use MSR save list for IA32_FLUSH_CMD if required (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Extend add_atomic_switch_msr() to allow VMENTER only MSRs (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Separate the VMX AUTOLOAD guest/host number accounting (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Add find_msr() helper function (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Split the VMX MSR LOAD structures to have an host/guest numbers (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Add L1D flush logic (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Add L1D MSR based flush (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Add L1D flush algorithm (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM/VMX: Add module argument for L1TF mitigation (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/KVM: Warn user if KVM is loaded SMT and L1TF CPU bug being present (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Boot HT siblings at least once (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] Revert "x86/apic: Ignore secondary threads if nosmt=force" (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Fix up pte->pfn conversion for PAE (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Protect PAE swap entries against L1TF (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/CPU/AMD: Move TOPOEXT reenablement before reading smp_num_siblings (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/cpufeatures: Add detection of L1D cache flush support (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Extend 64bit swap file size limit (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/apic: Ignore secondary threads if nosmt=force (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/cpu/AMD: Evaluate smp_num_siblings early (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/CPU/AMD: Do not check CPUID max ext level before parsing SMP info (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/cpu/intel: Evaluate smp_num_siblings early (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/cpu/topology: Provide detect_extended_topology_early() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/cpu/common: Provide detect_ht_early() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/cpu/AMD: Remove the pointless detect_ht() call (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/cpu: Remove the pointless CPU printout (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Provide knobs to control SMT (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Split do_cpu_down() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] cpu/hotplug: Make bringup/teardown of smp threads symmetric (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/topology: Provide topology_smt_supported() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/smp: Provide topology_is_primary_thread() (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] sched/smt: Update sched_smt_present at runtime (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/bugs: Move the l1tf function and define pr_fmt properly (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Limit swap file size to MAX_PA/2 (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Disallow non privileged high MMIO PROT_NONE mappings (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Add sysfs reporting for l1tf (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Make sure the first page is always reserved (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Protect PROT_NONE PTEs against speculation (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Protect swap entries against L1TF (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Change order of offset/type in swap entry (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}
- [x86] x86/speculation/l1tf: Increase 32bit PAE __PHYSICAL_PAGE_SHIFT (Waiman Long) [1616046] {CVE-2018-3620 CVE-2018-3646}

* Thu Sep 13 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-9.el8]
- [pci] PCI/DPC: Remove indirection waiting for inactive link (Myron Stowe) [1485556]
- [pci] PCI/DPC: Use threaded IRQ for bottom half handling (Myron Stowe) [1485556]
- [pci] PCI/DPC: Print AER status in DPC event handling (Myron Stowe) [1485556]
- [pci] PCI/DPC: Remove rp_pio_status from dpc struct (Myron Stowe) [1485556]
- [pci] PCI/DPC: Defer event handling to work queue (Myron Stowe) [1485556]
- [pci] PCI/DPC: Leave interrupts enabled while handling event (Myron Stowe) [1485556]
- [net] net/mlx5e: Offload TC matching on tos/ttl for ip tunnels (Erez Alfasi) [1615121]
- [net] net/mlx5e: Support setup of tos and ttl for tunnel key TC action offload (Erez Alfasi) [1615121]
- [net] net/mlx5e: Use ttl from route lookup on tc encap offload only if needed (Erez Alfasi) [1615121]
- [net] net/sched: cls_flower: Support matching on ip tos and ttl for tunnels (Erez Alfasi) [1615121]
- [net] flow_dissector: Dissect tos and ttl from the tunnel info (Erez Alfasi) [1615121]
- [net] net/sched: tunnel_key: Allow to set tos and ttl for tc based ip tunnels (Erez Alfasi) [1615121]
- [net] net/sched: act_tunnel_key: disambiguate metadata dst error cases (Erez Alfasi) [1615121]
- [net] net/sched: add tunnel option support to act_tunnel_key (Erez Alfasi) [1615121]
- [iommu] iommu/amd: Add support for IOMMU XT mode (Suravee Suthikulpanit) [1504485]
- [iommu] iommu/amd: Add support for higher 64-bit IOMMU Control Register (Suravee Suthikulpanit) [1504485]
- [x86] x86: irq_remapping: Move irq remapping mode enum (Suravee Suthikulpanit) [1504485]
- [firmware] dcdbas: Add support for WSMT ACPI table (Charles Rose) [1502286]

* Wed Sep 12 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-8.el8]
- [documentation] scsi: documentation: add scsi_mod.use_blk_mq to scsi-parameters (Ewan Milne) [1600014]
- [scsi] scsi: core: Update SCSI_MQ_DEFAULT help text to match default (Ewan Milne) [1600014]
- [scsi] scsi: core: switch to scsi-mq by default (Ewan Milne) [1600014]
- [pci] PCI: Match Root Port's MPS to endpoint's MPSS as necessary (Myron Stowe) [1502324]
- [pci] PCI: Skip MPS logic for Virtual Functions (VFs) (Myron Stowe) [1502324]
- [pci] PCI: Check for PCIe Link downtraining (Myron Stowe) [1502324]
- [pci] PCI: Workaround IDT switch ACS Source Validation erratum (Myron Stowe) [1502324]
- [of] OF: Don't set default coherent DMA mask (Mark Salter) [1581822]
- [acpi] ACPI/IORT: Don't set default coherent DMA mask (Mark Salter) [1581822]
- [iommu] iommu/dma: Respect bus DMA limit for IOVAs (Mark Salter) [1581822]
- [of] of/device: Set bus DMA mask as appropriate (Mark Salter) [1581822]
- [acpi] ACPI/IORT: Set bus DMA mask as appropriate (Mark Salter) [1581822]
- [kernel] dma-mapping: Generalise dma_32bit_limit flag (Mark Salter) [1581822]
- [acpi] ACPI/IORT: Support address size limit for root complexes (Mark Salter) [1581822]
- [of] of/platform: Initialise default DMA masks (Mark Salter) [1581822]
- [net] Bluetooth: hidp: buffer overflow in hidp_process_report (Gopal Tiwari) [1623073] {CVE-2018-9363}
- [irqchip] irqchip/gic-v3-its: Reduce minimum LPI allocation to 1 for PCI devices (Mark Salter) [1550500]
- [irqchip] irqchip/gic-v3-its: Honor hypervisor enforced LPI range (Mark Salter) [1550500]
- [irqchip] irqchip/gic-v3: Expose GICD_TYPER in the rdist structure (Mark Salter) [1550500]
- [irqchip] irqchip/gic-v3-its: Drop chunk allocation compatibility (Mark Salter) [1550500]
- [irqchip] irqchip/gic-v3-its: Move minimum LPI requirements to individual busses (Mark Salter) [1550500]
- [irqchip] irqchip/gic-v3-its: Use full range of LPIs (Mark Salter) [1550500]
- [irqchip] irqchip/gic-v3-its: Refactor LPI allocator (Mark Salter) [1550500]

* Tue Sep 11 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-7.el8]
- [netdrv] hv_netvsc: Fix a deadlock by getting rtnl lock earlier in netvsc_probe() (Vitaly Kuznetsov) [1625609]
- [netdrv] hv_netvsc: ignore devices that are not PCI (Vitaly Kuznetsov) [1625609]
- [netdrv] hv/netvsc: Fix NULL dereference at single queue mode fallback (Vitaly Kuznetsov) [1625609]
- [netdrv] hv_netvsc: Add per-cpu ethtool stats for netvsc (Vitaly Kuznetsov) [1625609]
- [pci] PCI: shpchp: Separate existence of SHPC and permission to use it (Steve Best) [1622953]
- [powerpc] KVM: PPC: Book3S HV: Don't truncate HPTE index in xlate function (David Gibson) [1625513]
- [kernel] rh_kabi: Add macros to size and extend structs (Prarit Bhargava) [1564570]
- [pci] PCI: Remove unnecessary include of <linux/pci-aspm.h> (Myron Stowe) [1622672]
- [wireless] iwlwifi: Remove unnecessary include of <linux/pci-aspm.h> (Myron Stowe) [1622672]
- [wireless] ath9k: Remove unnecessary include of <linux/pci-aspm.h> (Myron Stowe) [1622672]
- [netdrv] igb: Remove unnecessary include of <linux/pci-aspm.h> (Myron Stowe) [1622672]
- [pci] PCI/ASPM: Convert to use sysfs_match_string() helper (Myron Stowe) [1622672]
- [virt] KVM: s390: Properly lock mm context allow_gmap_hpage_1m setting (Thomas Huth) [1623513]
- [virt] KVM: s390: vsie: copy wrapping keys to right place (Thomas Huth) [1623513]
- [virt] KVM: s390: Fix pfmf and conditional skey emulation (Thomas Huth) [1623513]
- [virt] KVM: s390: Fix storage attributes migration with memory slots (Thomas Huth) [1623513]
- [virt] KVM: s390: a utility function for migration (Thomas Huth) [1623513]

* Mon Sep 10 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-6.el8]
- [lib] vsprintf: Add command line option debug_boot_weak_hash (Prarit Bhargava) [1625687]
- [netdrv] i40e: Fix for Tx timeouts when interface is brought up if DCB is enabled (Stefan Assmann) [1616147]
- [misc] ocxl: Fix page fault handler in case of fault on dying process (Steve Best) [1624644]
- [edac] EDAC, sb_edac: Add support for systems with segmented PCI buses (Aristeu Rozanski) [1621849]
- [netdrv] xen-netfront: fix warn message as irq device name has '/' (Vitaly Kuznetsov) [1576160]
- [arm64] arm64, kaslr: export offset in VMCOREINFO ELF notes (Bhupesh Sharma) [1624246]
- [rpmspec] redhat: Move gfs2 and dlm out of kernel-modules-extra (Andrew Price) [1623511]
- [powerpc] powerpc/topology: Get topology for shared processors at boot (Steve Best) [1620039]
- [fs] gfs2: Don't set GFS2_RDF_UPTODATE when the lvb is updated (Robert S Peterson) [1622057]
- [fs] gfs2: improve debug information when lvb mismatches are found (Robert S Peterson) [1622057]
- [fs] gfs2: cleanup: call gfs2_rgrp_ondisk2lvb from gfs2_rgrp_out (Robert S Peterson) [1622057]
- [x86] Fix x86 32-bit invalid cpu boot failure message (Prarit Bhargava) [1571456]
- [net] net/ipv6: init ip6 anycast rt->dst.input as ip6_input (Hangbin Liu) [1615671]
- [pci] PCI/AER: Don't clear AER bits if error handling is Firmware-First (Myron Stowe) [1621933]
- [pci] PCI/AER: Remove duplicate PCI_EXP_AER_FLAGS definition (Myron Stowe) [1621933]
- [pci] PCI/portdrv: Remove pcie_portdrv_err_handler.slot_reset (Myron Stowe) [1621933]
- [pci] PCI/AER: Clear device status bits during ERR_COR handling (Myron Stowe) [1621933]
- [pci] PCI/AER: Clear device status bits during ERR_FATAL and ERR_NONFATAL (Myron Stowe) [1621933]
- [pci] PCI/AER: Remove ERR_FATAL code from ERR_NONFATAL path (Myron Stowe) [1621933]
- [pci] PCI/AER: Factor out ERR_NONFATAL status bit clearing (Myron Stowe) [1621933]
- [pci] PCI/AER: Clear only ERR_NONFATAL bits during non-fatal recovery (Myron Stowe) [1621933]
- [pci] PCI/AER: Clear only ERR_FATAL status bits during fatal recovery (Myron Stowe) [1621933]
- [pci] PCI/AER: Honor "pcie_ports=native" even if HEST sets FIRMWARE_FIRST (Myron Stowe) [1621933]
- [pci] PCI/AER: Add sysfs attributes for rootport cumulative stats (Myron Stowe) [1621933]
- [pci] PCI/AER: Add sysfs attributes to provide AER stats and breakdown (Myron Stowe) [1621933]
- [pci] PCI/AER: Define aer_stats structure for AER capable devices (Myron Stowe) [1621933]
- [pci] PCI/AER: Move internal declarations to drivers/pci/pci.h (Myron Stowe) [1621933]
- [pci] PCI/AER: Adopt lspci names for AER error decoding (Myron Stowe) [1621933]
- [pci] PCI/AER: Expose internal API for obtaining AER information (Myron Stowe) [1621933]
- [kernel] rcu: Make expedited GPs handle CPU 0 being offline (Gustavo Duarte) [1610262]
- [rpmspec] Generate BootLoaderSpec config fragments ("Herton R. Krzesinski") [1619766]

* Wed Aug 29 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-5.el8]
- [net] erspan: set erspan_ver to 1 by default when adding an erspan dev (Xin Long) [1619118]
- [hv] x86/hyper-v: Fix wrong merge conflict resolution (Vitaly Kuznetsov) [1597652]
- [hv] x86/hyper-v: Check for VP_INVAL in hyperv_flush_tlb_others() (Vitaly Kuznetsov) [1597652]
- [hv] x86/hyper-v: Check cpumask_to_vpset() return value in hyperv_flush_tlb_others_ex() (Vitaly Kuznetsov) [1597652]
- [hv] x86/hyper-v: Trace PV IPI send (Vitaly Kuznetsov) [1597652]
- [hv] x86/hyper-v: Use cheaper HVCALL_SEND_IPI hypercall when possible (Vitaly Kuznetsov) [1597652]
- [hv] x86/hyper-v: Use 'fast' hypercall for HVCALL_SEND_IPI (Vitaly Kuznetsov) [1597652]
- [hv] x86/hyper-v: Implement hv_do_fast_hypercall16 (Vitaly Kuznetsov) [1597652]
- [hv] x86/hyper-v: Use cheaper HVCALL_FLUSH_VIRTUAL_ADDRESS_(LIST, SPACE) hypercalls when possible (Vitaly Kuznetsov) [1597652]
- [netdrv] xen-netfront: fix queue name setting (Vitaly Kuznetsov) [1576160]
- [scsi] lfpc: add Lancer FCoE to the removed devices (Tomas Henzl) [1602033]
- [scsi] megaraid_sas: add removed id table (Tomas Henzl) [1602033]
- [scsi] aacraid: add removed id table (Tomas Henzl) [1602033]
- [scsi] qla4xxx: add removed id table (Tomas Henzl) [1602033]
- [scsi] lpfc: add removed id table (Tomas Henzl) [1602033]
- [scsi] qla2xxx: add removed id table (Tomas Henzl) [1602033]
- [scsi] mpt3sas: add removed id table (Tomas Henzl) [1602033]
- [scsi] be2iscsi: add removed id table (Tomas Henzl) [1602033]
- [scsi] rh_taint, pci : add information about removed hardware (Tomas Henzl) [1602033]
- [kernel] kernel: add SUPPORT_REMOVED kernel taint (Tomas Henzl) [1602033]
- [net] sunrpc: Change rpc_print_iostats to rpc_clnt_show_stats and handle rpc_clnt clones (Dave Wysochanski) [1610373]
- [net] sunrpc: Add _add_rpc_iostats() to add rpc_iostats metrics (Dave Wysochanski) [1610373]
- [net] sunrpc: add _print_rpc_iostats() to output metrics for one RPC op (Dave Wysochanski) [1610373]

* Mon Aug 27 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-4.el8]
- [net] xdp: exclude XDP from kABI guarantee (Jiri Benc) [1568551]
- [kernel] rh_kabi: introduce RH_KABI_EXCLUDE (Jiri Benc) [1568551]
- [powerpc] powerpc/powernv/pci: Work around races in PCI bridge enabling (Steve Best) [1620035]
- [block] blk-wbt: fix IO hang in wbt_wait() (Ming Lei) [1614198]
- [block] blkcg: Make blkg_root_lookup() work for queues in bypass mode (Ming Lei) [1614198]
- [block] null_blk: add lock drop/acquire annotation (Ming Lei) [1614198]
- [block] Blk-throttle: reduce tail io latency when iops limit is (Ming Lei) [1614198]
- [block] block: paride: pd: mark expected switch fall-throughs (Ming Lei) [1614198]
- [block] block: Ensure that a request queue is dissociated from the (Ming Lei) [1614198]
- [block] block: Introduce blk_exit_queue() (Ming Lei) [1614198]
- [block] blkcg: Introduce blkg_root_lookup() (Ming Lei) [1614198]
- [block] block: Remove two superfluous #include directives (Ming Lei) [1614198]
- [block] blk-mq: count the hctx as active before allocating tag (Ming Lei) [1614198]
- [block] block: bvec_nr_vecs() returns value for wrong slab (Ming Lei) [1614198]
- [block] drivers/block/drbd: remove the null check for (Ming Lei) [1614198]
- [block] drivers/block/aoe/aoedev: NULL check is not needed for (Ming Lei) [1614198]
- [block] drivers/block/mtip32xx: remove the null check for (Ming Lei) [1614198]
- [block] cfq: Suppress compiler warnings about comparisons (Ming Lei) [1614198]
- [block] cfq: Annotate fall-through in a switch statement (Ming Lei) [1614198]
- [block] blk-wbt: Avoid lock contention and thundering herd issue in (Ming Lei) [1590363]
- [block] target/loop: depend on SCSI (Ming Lei) [1614198]
- [block] xen-blkfront: use true and false for boolean values (Ming Lei) [1614198]
- [block] lightnvm: remove minor version check for 2.0 (Ming Lei) [1614198]
- [block] scsi: Check sense buffer size at build time (Ming Lei) [1614198]
- [block] libata-scsi: Move sense buffers onto stack (Ming Lei) [1614198]
- [block] cdrom: Use struct scsi_sense_hdr internally (Ming Lei) [1614198]
- [block] ide-cd: Remove redundant sense buffer (Ming Lei) [1614198]
- [block] block: Switch struct packet_command to use struct (Ming Lei) [1614198]
- [block] target: don't depend on SCSI (Ming Lei) [1614198]
- [block] scsi: build scsi_common.o for all scsi passthrough request (Ming Lei) [1614198]
- [block] scsi: cxlflash: Drop unused sense buffers (Ming Lei) [1614198]
- [block] ide-cd: Drop unused sense buffers (Ming Lei) [1614198]
- [block] blk-mq: fix updating tags depth (Ming Lei) [1611900]
- [block] block: really disable runtime-pm for blk-mq (Ming Lei) [1611902]
- [block] aoe: mark expected switch fall-through (Ming Lei) [1614198]
- [block] block: make iolatency avg_lat exponentially decay (Ming Lei) [1614198]
- [block] blk-cgroup: clear the throttle queue on fork (Ming Lei) [1614198]
- [block] blk-cgroup: hold the queue ref during throttling (Ming Lei) [1614198]
- [block] blk-iolatency: fix blkg leak in timer_fn (Ming Lei) [1614198]
- [block] block/bsg-lib: use PTR_ERR_OR_ZERO to simplify the flow path (Ming Lei) [1614198]
- [block] t10-pi: provide empty t10_pi_complete() for (Ming Lei) [1614198]
- [block] block: blk_init_allocated_queue() set q->fq as NULL in the (Ming Lei) [1614198]
- [block] nvme: use blk API to remap ref tags for IOs with metadata (Ming Lei) [1614198]
- [block] block: move dif_prepare/dif_complete functions to block layer (Ming Lei) [1614198]
- [block] block: move ref_tag calculation func to the block layer (Ming Lei) [1614198]
- [block] block: don't account for split bio's size in cgroup stats (Ming Lei) [1614198]
- [block] pktcdvd: Fix possible Spectre-v1 for pkt_devs (Ming Lei) [1614198]
- [block] partitions/aix: append null character to print data from disk (Ming Lei) [1614198]
- [block] partitions/aix: fix usage of uninitialized lv_info and lvname (Ming Lei) [1614198]
- [block] readahead: stricter check for bdi io_pages (Ming Lei) [1614198]
- [block] scsi: virtio_scsi: fix pi_bytes(out, in) on 4 KiB block size (Ming Lei) [1614198]
- [block] block: move bio_integrity_(intervals, bytes) into blkdev.h (Ming Lei) [1614198]
- [block] xen/blkfront: remove unused macros (Ming Lei) [1614198]
- [block] block: allow max_discard_segments to be stacked (Ming Lei) [1614198]
- [block] block: unexport bio_clone_bioset (Ming Lei) [1614198]
- [block] md: remove a bogus comment (Ming Lei) [1614198]
- [block] block: remove bio_clone_kmalloc (Ming Lei) [1614198]
- [block] exofs: use bio_clone_fast in _write_mirror (Ming Lei) [1614198]
- [block] bcache: don't clone bio in bch_data_verify (Ming Lei) [1614198]
- [block] block: bio_set_pages_dirty can't see NULL bv_page in a valid (Ming Lei) [1614198]
- [block] block: simplify bio_check_pages_dirty (Ming Lei) [1614198]
- [block] block: Rename the null_blk_mod kernel module back into (Ming Lei) [1614198]
- [block] blk-mq: fail the request in case issue failure (Ming Lei) [1614305]
- [block] blk-rq-qos: make depth comparisons unsigned (Ming Lei) [1614198]
- [block] blkcg: Track DISCARD statistics and output them in cgroup (Ming Lei) [1614198]
- [block] block: Track DISCARD statistics and output them in stat and (Ming Lei) [1614198]
- [block] block: Add and use op_stat_group() for indexing disk_stat (Ming Lei) [1614198]
- [block] block: Define and use STAT_READ and STAT_WRITE (Ming Lei) [1614198]
- [block] block: Add part_stat_read_accum to read across field entries (Ming Lei) [1614198]
- [block] block: make bdev_ops->rw_page() take a REQ_OP instead of bool (Ming Lei) [1614198]
- [block] pktcdvd: remove assignment in if condition (Ming Lei) [1614198]
- [block] blk-mq: issue directly if hw queue isn't busy in case of (Ming Lei) [1614305]
- [block] blk-iolatency: truncate our current time (Ming Lei) [1614198]
- [block] blk-iolatency: don't change the latency window (Ming Lei) [1614198]
- [block] block: remove blkdev_entry_to_request() macro (Ming Lei) [1614198]
- [block] block: skd: Use pad printk format for dma_addr_t values (Ming Lei) [1614198]
- [block] bsg: remove read/write support (Ming Lei) [1614198]
- [block] blk-iolatency: fix max_depth comparisons (Ming Lei) [1614198]
- [block] block: iolatency: avoid 64-bit division (Ming Lei) [1614198]
- [block] block/DAC960.c: fix defined but not used build warnings (Ming Lei) [1614198]
- [block] null_blk: add zone support (Ming Lei) [1614198]
- [block] null_blk: move shared definitions to header file (Ming Lei) [1614198]
- [block] block: Add default switch case to blk_pm_allow_request() to (Ming Lei) [1614198]
- [block] block: fix infinite loop if the device loses discard (Ming Lei) [1614198]
- [block] block, mm: remove unnecessary __GFP_HIGH flag (Ming Lei) [1614198]
- [block] null_blk: remove NULLB_DEV_FL_CONFIGURED on turning off nullb (Ming Lei) [1614198]
- [block] mm: skip readahead if the cgroup is congested (Ming Lei) [1614198]
- [block] Documentation: add a doc for blk-iolatency (Ming Lei) [1614198]
- [block] block: introduce blk-iolatency io controller (Ming Lei) [1614198]
- [block] rq-qos: introduce dio_bio callback (Ming Lei) [1614198]
- [block] block: remove external dependency on wbt_flags (Ming Lei) [1614198]
- [block] blk-rq-qos: refactor out common elements of blk-wbt (Ming Lei) [1614198]
- [block] blk-stat: export helpers for modifying blk_rq_stat (Ming Lei) [1614198]
- [block] memcontrol: schedule throttling if we are congested (Ming Lei) [1614198]
- [block] blkcg: add generic throttling mechanism (Ming Lei) [1614198]
- [block] swap, blkcg: issue swap io with the appropriate context (Ming Lei) [1614198]
- [block] blk: introduce REQ_SWAP (Ming Lei) [1614198]
- [block] blk-cgroup: allow controllers to output their own stats (Ming Lei) [1614198]
- [block] block: introduce bio_issue_as_root_blkg (Ming Lei) [1614198]
- [block] block: add bi_blkg to the bio for cgroups (Ming Lei) [1614198]
- [block] blk-mq: dequeue request one by one from sw queue if hctx is (Ming Lei) [1614305]
- [block] block/loop: mark expected switch fall-through (Ming Lei) [1614198]
- [block] drbd: mark expected switch fall-throughs (Ming Lei) [1614198]
- [block] blk-mq: only attempt to merge bio if there is rq in sw queue (Ming Lei) [1614305]
- [block] blk-mq: use list_splice_tail_init() to insert requests (Ming Lei) [1614305]
- [block] blk-mq: fix typo in a function comment (Ming Lei) [1614198]
- [block] blk-mq: code clean-up by adding an API to clear set->mq_map (Ming Lei) [1614198]
- [block] paride: remove redundant variable n (Ming Lei) [1614198]
- [block] partitions/ldm: remove redundant pointer dgrp (Ming Lei) [1614198]
- [block] loop: remove redundant pointer inode (Ming Lei) [1614198]
- [block] block/floppy: remove redundant variable dflags (Ming Lei) [1614198]
- [block] Block: blk-throttle: set low_valid immediately once one (Ming Lei) [1614198]
- [block] Blktrace: bail out early if block debugfs is not configured (Ming Lei) [1614198]
- [block] block: Document how blk_update_request() handles (Ming Lei) [1614198]
- [block] drbd: Do not redefine __must_hold() (Ming Lei) [1614198]
- [block] blk-mq: avoid to synchronize rcu inside blk_cleanup_queue() (Ming Lei) [1597067]
- [block] blk-mq: remove synchronize_rcu() from (Ming Lei) [1597067]
- [block] blk-mq: introduce new lock for protecting hctx->dispatch_wait (Ming Lei) [1597067]
- [block] blk-mq: don't pass **hctx to blk_mq_mark_tag_wait() (Ming Lei) [1597067]
- [block] blk-mq: cleanup blk_mq_get_driver_tag() (Ming Lei) [1597067]
- [block] block, bfq: give a better name to bfq_bfqq_may_idle (Ming Lei) [1614198]
- [block] block, bfq: fix service being wrongly set to zero in case of (Ming Lei) [1614198]
- [block] block, bfq: do not expire a queue that will deserve dispatch (Ming Lei) [1614198]
- [block] block, bfq: add/remove entity weights correctly (Ming Lei) [1614198]
- [block] block: Make struct request_queue smaller for (Ming Lei) [1614198]
- [block] block: Inline blk_queue_nr_zones() (Ming Lei) [1614198]
- [block] block: Remove bdev_nr_zones() (Ming Lei) [1614198]
- [block] include/uapi/linux/blkzoned.h: Remove a superfluous __packed (Ming Lei) [1614198]
- [block] block: Remove a superfluous cast from blkdev_report_zones() (Ming Lei) [1614198]

* Fri Aug 24 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-3.el8]
- [net] tls: mark as Tech Preview (Sabrina Dubroca) [1570255]
- [pci] PCI/VPD: Check for VPD access completion before checking for timeout (Myron Stowe) [1618820]
- [rpmspec] redhat: remove bootwrapper subpackage (Gustavo Duarte) [1578399]
- [virt] kvm: x86: Set highest physical address bits in non-present/reserved SPTEs (Paolo Bonzini) [1614808]
- [virt] KVM/x86: Use CC_SET()/CC_OUT in arch/x86/kvm/vmx.c (Paolo Bonzini) [1614808]
- [virt] KVM: X86: Implement PV IPIs in linux guest (Paolo Bonzini) [1614808]
- [virt] KVM: X86: Add kvm hypervisor init time platform setup callback (Paolo Bonzini) [1614808]
- [virt] KVM: X86: Implement "send IPI" hypercall (Paolo Bonzini) [1614808]
- [virt] KVM/x86: Move X86_CR4_OSXSAVE check into kvm_valid_sregs() (Paolo Bonzini) [1614808]
- [virt] KVM: x86: Skip pae_root shadow allocation if tdp enabled (Paolo Bonzini) [1614808]
- [virt] KVM/MMU: Combine flushing remote tlb in mmu_set_spte() (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: skip VMWRITE of HOST_(FS, GS)_BASE when possible (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: skip VMWRITE of HOST_(FS, GS)_SEL when possible (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: always initialize HOST_(FS, GS)_BASE to zero during setup (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: move struct host_state usage to struct loaded_vmcs (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: compute need to reload FS/GS/LDT on demand (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: remove a misleading comment regarding vmcs02 fields (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: rename __vmx_load_host_state() and vmx_save_host_state() (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: add dedicated utility to access guest's kernel_gs_base (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: track host_state.loaded using a loaded_vmcs pointer (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: refactor segmentation code in vmx_save_host_state() (Paolo Bonzini) [1614808]
- [virt] kvm: nVMX: Fix fault priority for VMX operations (Paolo Bonzini) [1614808]
- [virt] kvm: nVMX: Fix fault vector for VMX operation at CPL > 0 (Paolo Bonzini) [1614808]
- [virt] KVM: try __get_user_pages_fast even if not in atomic context (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: Add tlb_remote_flush callback support (Paolo Bonzini) [1614808]
- [virt] KVM: x86: Add tlb remote flush callback in kvm_x86_ops (Paolo Bonzini) [1614808]
- [virt] X86/Hyper-V: Add hyperv_nested_flush_guest_mapping ftrace support (Paolo Bonzini) [1614808]
- [virt] X86/Hyper-V: Add flush HvFlushGuestPhysicalAddressSpace hypercall support (Paolo Bonzini) [1614808]
- [virt] x86/kvm: Don't use pvqspinlock code if only 1 vCPU (Paolo Bonzini) [1614808]
- [virt] KVM/MMU: Simplify __kvm_sync_page() function (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Remove CR3_PCID_INVD flag (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Add multi-entry LRU cache for previous CR3s (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Flush only affected TLB entries in kvm_mmu_invlpg* (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Skip shadow page resync on CR3 switch when indicated by guest (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Support selectively freeing either current or previous MMU root (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Add a root_hpa parameter to kvm_mmu->invlpg() (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Skip TLB flush on fast CR3 switch when indicated by guest (Paolo Bonzini) [1614808]
- [virt] kvm: vmx: Support INVPCID in shadow paging mode (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Propagate guest PCIDs to host PCIDs (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Add ability to skip TLB flush when switching CR3 (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Use fast CR3 switch for nested VMX (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Support resetting the MMU context without resetting roots (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Add support for fast CR3 switch across different MMU modes (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Introduce KVM_REQ_LOAD_CR3 (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Introduce kvm_mmu_calc_root_page_role() (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Add fast CR3 switch code path (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Avoid taking MMU lock in kvm_mmu_sync_roots if no sync is needed (Paolo Bonzini) [1614808]
- [virt] kvm: x86: Make sync_page() flush remote TLBs once only (Paolo Bonzini) [1614808]
- [virt] KVM: MMU: drop vcpu param in gpte_access (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Separate logic allocating shadow vmcs to a function (Paolo Bonzini) [1614808]
- [virt] KVM: VMX: Mark vmcs header as shadow in case alloc_vmcs_cpu() allocate shadow vmcs (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Expose VMCS shadowing to L1 guest (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Do not forward VMREAD/VMWRITE VMExits to L1 if required so by vmcs12 vmread/vmwrite bitmaps (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: vmread/vmwrite: Use shadow vmcs12 if running L2 (Paolo Bonzini) [1614808]
- [virt] KVM: selftests: add tests for shadow VMCS save/restore (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: include shadow vmcs12 in nested state (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Cache shadow vmcs12 on VMEntry and flush to memory on VMExit (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Verify VMCS shadowing VMCS link pointer (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Verify VMCS shadowing controls (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Introduce nested_cpu_has_shadow_vmcs() (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Fail VMLAUNCH and VMRESUME on shadow VMCS (Paolo Bonzini) [1614808]
- [virt] KVM: nVMX: Allow VMPTRLD for shadow VMCS if vCPU supports VMCS shadowing (Paolo Bonzini) [1614808]
- [virt] KVM: VMX: Change vmcs12(read, write)_any() to receive vmcs12 as parameter (Paolo Bonzini) [1614808]
- [virt] KVM: VMX: Create struct for VMCS header (Paolo Bonzini) [1614808]
- [virt] kvm: selftests: add test for nested state save/restore (Paolo Bonzini) [1614808]
- [virt] kvm: nVMX: Introduce KVM_CAP_NESTED_STATE (Paolo Bonzini) [1614808]
- [virt] KVM: x86: do not load vmcs12 pages while still in SMM (Paolo Bonzini) [1614808]
- [virt] kvm: selftests: add basic test for state save and restore (Paolo Bonzini) [1614808]
- [virt] kvm: selftests: ensure vcpu file is released (Paolo Bonzini) [1614808]
- [virt] kvm: selftests: actually use all of lib/vmx.c (Paolo Bonzini) [1614808]
- [virt] kvm: selftests: create a GDT and TSS (Paolo Bonzini) [1614808]
- [virt] KVM: x86: ensure all MSRs can always be KVM_GET/SET_MSR'd (Paolo Bonzini) [1614808]
- [virt] KVM: vmx: remove save/restore of host BNDCGFS MSR (Paolo Bonzini) [1614808]
- [virt] KVM: Switch 'requests' to be 64-bit (explicitly) (Paolo Bonzini) [1614808]
- [virt] kvm: selftests: add cr4_cpuid_sync_test (Paolo Bonzini) [1614808]
- [virt] KVM: PPC: Book3S HV: Read kvm->arch.emul_smt_mode under kvm->lock (Paolo Bonzini) [1614808]
- [virt] KVM: PPC: Book3S HV: Allow creating max number of VCPUs on POWER9 (Paolo Bonzini) [1614808]
- [virt] KVM: PPC: Book3S HV: Pack VCORE IDs to access full VCPU ID space (Paolo Bonzini) [1614808]
- [virt] KVM: PPC: Book3S HV: Fix constant size warning (Paolo Bonzini) [1614808]
- [virt] KVM: PPC: Book3S HV: Add of_node_put() in success path (Paolo Bonzini) [1614808]
- [virt] KVM: PPC: Book3S: Fix matching of hardware and emulated TCE tables (Paolo Bonzini) [1614808]
- [virt] KVM: PPC: Remove mmio_vsx_tx_sx_enabled in KVM MMIO emulation (Paolo Bonzini) [1614808]

* Fri Aug 17 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-2.el8]
- [net] tcp: Add tcp_clamp_rto_to_user_timeout() helper to improve accuracy (Michael Cambria) [1605024]
- [net] tcp: Add tcp_retransmit_stamp() helper routine (Michael Cambria) [1605024]
- [net] tcp: convert icsk_user_timeout from jiffies to msecs (Michael Cambria) [1605024]
- [kernel] Revert sched/fair: Consider SD_NUMA when selecting the most idle group to schedule on (Lauro Ramos Venancio) [1585746]
- [kernel] redhat: makefile: adjust KBUILD_CFLAGS to reflect kernel.spec for powerpc builds (Gustavo Duarte) [1582568]
- [rpmspec] redhat: spec: build ppc64le kernel with -O3 (Gustavo Duarte) [1582568]
- [scsi] scsi: csiostor: update csio_get_flash_params() (Arjun Vynipadath) [1503574]
- [scsi] csiostor: Add a soft dep on cxgb4 driver (Arjun Vynipadath) [1503574]
- [firmware] dell_rbu: make firmware payload memory uncachable (Charles Rose) [1584401]

* Mon Aug 13 2018 Herton R. Krzesinski <herton@redhat.com> [4.18.0-1.el8]
- [scsi] scsi: lpfc: update driver version to 12.0.0.6 (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: Remove lpfc_enable_pbde as module parameter (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: Correct LCB ACCept payload (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: Limit tracking of tgt queue depth in fast path (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: Fix driver crash when re-registering NVME rports (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: Fix list corruption on the completion queue (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: Fix sysfs Speed value on CNA ports (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: Fix ELS abort on SLI-3 adapters (Dick Kennedy) [1613913]
- [scsi] scsi: lpfc: remove null check on nvmebuf (Dick Kennedy) [1613913]
- [arm64] arm64: fix ACPI dependencies (Bhupesh Sharma) [1556832]
- [arm64] arm64: acpi: fix alignment fault in accessing ACPI (Bhupesh Sharma) [1556832]
- [firmware] efi/arm: map UEFI memory map even w/o runtime services enabled (Bhupesh Sharma) [1556832]
- [firmware] efi/arm: preserve early mapping of UEFI memory map longer for BGRT (Bhupesh Sharma) [1556832]
- [acpi] drivers: acpi: add dependency of EFI for arm64 (Bhupesh Sharma) [1556832]
- [arm64] arm64: export memblock_reserve()d regions via /proc/iomem (Bhupesh Sharma) [1556832]
- [arm64] arm64: kconfig: Ensure spinlock fastpaths are inlined if !PREEMPT (Waiman Long) [1607924]
- [arm64] arm64: locking: Replace ticket lock implementation with qspinlock (Waiman Long) [1607924]
- [arm64] arm64: barrier: Implement smp_cond_load_relaxed (Waiman Long) [1607924]
- [scsi] scsi: lpfc: Revise copyright for new company language (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: update driver version to 12.0.0.5 (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: devloss timeout race condition caused null pointer reference (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: Fix NVME Target crash in defer rcv logic (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: Support duration field in Link Cable Beacon V1 command (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: Make PBDE optimizations configurable (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: Fix abort error path for NVMET (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: Fix panic if driver unloaded when port is offline (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: Fix driver not setting dpp bits correctly in doorbell word (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: Add Buffer overflow check, when nvme_info larger than PAGE_SIZE (Dick Kennedy) [1600946]
- [scsi] scsi: lpfc: use monotonic timestamps for statistics (Dick Kennedy) [1600946]
- [x86] mark intel knights landing and knights mill unsupported (David Arcari) [1610493]
- [netdrv] igb: Remove superfluous reset to PHY and page 0 selection (Corinna Vinschen) [1612824]
- [tools] selftests/powerpc: Fix ptrace-pkey for default execute permission change (Steve Best) [1498799]
- [tools] selftests/powerpc: Fix core-pkey for default execute permission change (Steve Best) [1498799]
- [powerpc] powerpc/pkeys: make protection key 0 less special (Steve Best) [1498799]
- [powerpc] powerpc/pkeys: Preallocate execute-only key (Steve Best) [1498799]
- [powerpc] powerpc/pkeys: Fix calculation of total pkeys (Steve Best) [1498799]
- [powerpc] powerpc/pkeys: Save the pkey registers before fork (Steve Best) [1498799]
- [powerpc] powerpc/pkeys: key allocation/deallocation must not change pkey registers (Steve Best) [1498799]
- [powerpc] powerpc/pkeys: Deny read/write/execute by default (Steve Best) [1498799]
- [powerpc] powerpc/pkeys: Give all threads control of their key permissions (Steve Best) [1498799]
- [s390] KVM: s390: Add huge page enablement control (David Hildenbrand) [1508102]
- [s390] s390/mm: Add huge page gmap linking support (David Hildenbrand) [1508102]
- [s390] s390/mm: hugetlb pages within a gmap can not be freed (David Hildenbrand) [1508102]
- [s390] KVM: s390: Beautify skey enable check (David Hildenbrand) [1508102]
- [s390] KVM: s390: Add skey emulation fault handling (David Hildenbrand) [1508102]
- [s390] s390/mm: Add huge pmd storage key handling (David Hildenbrand) [1508102]
- [s390] s390/mm: Clear skeys for newly mapped huge guest pmds (David Hildenbrand) [1508102]
- [s390] s390/mm: Clear huge page storage keys on enable_skey (David Hildenbrand) [1508102]
- [s390] s390/mm: Add huge page dirty sync support (David Hildenbrand) [1508102]
- [s390] s390/mm: Add gmap pmd invalidation and clearing (David Hildenbrand) [1508102]
- [s390] s390/mm: Add gmap pmd notification bit setting (David Hildenbrand) [1508102]
- [s390] s390/mm: Add gmap pmd linking (David Hildenbrand) [1508102]
- [s390] s390/mm: Abstract gmap notify bit setting (David Hildenbrand) [1508102]
- [s390] s390/mm: Make gmap_protect_range more modular (David Hildenbrand) [1508102]
- [s390] KVM: s390: Replace clear_user with kvm_clear_guest (David Hildenbrand) [1508102]
- [hwmon] hwmon: (ibmpowernv) Add attributes to enable/disable sensor groups (Steve Best) [1524684]
- [powerpc] powerpc/powernv: Add support to enable sensor groups (Steve Best) [1524684]
- [net] net/smc: improve delete link processing (Hendrik Brueckner) [1548452]
- [net] net/smc: provide fallback reason code (Hendrik Brueckner) [1548452]
- [net] net/smc: use correct vlan gid of RoCE device (Hendrik Brueckner) [1548452]
- [net] net/smc: fewer parameters for smc_llc_send_confirm_link() (Hendrik Brueckner) [1548452]
- [net] net/smc: remove local variable page in smc_rx_splice() (Hendrik Brueckner) [1548452]
- [net] net/smc: use DECLARE_BITMAP for rtokens_used_mask (Hendrik Brueckner) [1548452]
- [net] net/smc: add function to get link group from link (Hendrik Brueckner) [1548452]
- [net] net/smc: eliminate cursor read and write calls (Hendrik Brueckner) [1548452]
- [net] net/smc: provide smc mode in smc_diag.c (Hendrik Brueckner) [1548452]
- [s390] s390/ism: add device driver for internal shared memory (Hendrik Brueckner) [1548452]
- [net] net/smc: add SMC-D diag support (Hendrik Brueckner) [1548452]
- [net] net/smc: add SMC-D support in af_smc (Hendrik Brueckner) [1548452]
- [net] net/smc: add SMC-D support in data transfer (Hendrik Brueckner) [1548452]
- [net] net/smc: add SMC-D support in CLC messages (Hendrik Brueckner) [1548452]
- [net] net/smc: add pnetid support for SMC-D and ISM (Hendrik Brueckner) [1548452]
- [net] net/smc: add base infrastructure for SMC-D and ISM (Hendrik Brueckner) [1548452]
- [net] net/smc: add pnetid support (Hendrik Brueckner) [1548452]
- [net] net/smc: determine port attributes independent from pnet table (Hendrik Brueckner) [1548452]
- [x86] mark whiskey-lake processor supported (David Arcari) [1609604]
- [s390] KVM: s390: add etoken support for guests (Thomas Huth) [1612110]
- [char] ipmi: do not configure ipmi for HPE m400 (Tony Camuso) [1583537]
- [scsi] scsi: ipr: Format HCAM overlay ID 0x41 (Steve Best) [1498222]
- [x86] x86/stacktrace: Enable HAVE_RELIABLE_STACKTRACE for the ORC unwinder (Joe Lawrence) [1587952]
- [x86] x86/unwind/orc: Detect the end of the stack (Joe Lawrence) [1587952]
- [x86] x86/stacktrace: Do not fail for ORC with regs on stack (Joe Lawrence) [1587952]
- [x86] x86/stacktrace: Clarify the reliable success paths (Joe Lawrence) [1587952]
- [x86] x86/stacktrace: Remove STACKTRACE_DUMP_ONCE (Joe Lawrence) [1587952]
- [x86] x86/stacktrace: Do not unwind after user regs (Joe Lawrence) [1587952]
- [infiniband] IB/rxe: Mark Soft-RoCE Transport driver as tech-preview (Don Dutile) [1605216]
- [scsi] scsi: smartpqi: bump driver version to 1.1.4-130 (Don Brace) [1503736]
- [scsi] scsi: smartpqi: fix critical ARM issue reading PQI index registers (Don Brace) [1503736]
- [scsi] scsi: smartpqi: add inspur advantech ids (Don Brace) [1503736]
- [scsi] scsi: smartpqi: improve error checking for sync requests (Don Brace) [1503736]
- [scsi] scsi: smartpqi: improve handling for sync requests (Don Brace) [1503736]
- [netdrv] ice: mark driver as tech-preview (Jonathan Toppins) [1495347]
- [init] init/Kconfig: remove EXPERT from CHECKPOINT_RESTORE (Adrian Reber) [1568995 1557617 1525389]
- [scsi] be2iscsi: remove BE3 family support (Maurizio Lombardi) [1598366]
- [x86] update rh_check_supported processor list (David Arcari) [1595918]
- [kernel] kABI: Add generic kABI macros to use for kABI workarounds (Myron Stowe) [1546831]
- [pci] add pci_hw_vendor_status() (Maurizio Lombardi) [1590829]
- [ata] ahci: thunderx2: Fix for errata that affects stop engine (Robert Richter) [1563590]
- [pci] Vulcan: AHCI PCI bar fix for Broadcom Vulcan early silicon (Robert Richter) [1563590]
- [kernel] bpf: set default values for bpf_jit_harden and bpf_jit_kallsyms (Eugene Syromiatnikov) [1569061]
- [kernel] bpf: Add tech preview taint for syscall (Eugene Syromiatnikov) [1559877]
- [kernel] bpf: set unprivileged_bpf_disabled to 1 by default, add a boot parameter (Eugene Syromiatnikov) [1561171]
- [kernel] add Red Hat-specific taint flags (Eugene Syromiatnikov) [1559877]
- [tools] perf tests: Add Python 3 support to attr.py ("Herton R. Krzesinski") [1561505]
- [tools] perf scripts python: Add Python 3 support to stat-cpi.py ("Herton R. Krzesinski") [1561505]
- [kernel] kdump: fix a grammar issue in a kernel message (Dave Young) [1507353]
- [scripts] tags.sh: Ignore redhat/rpm (Prarit Bhargava) [1582586]
- [kernel] put RHEL info into generated headers (Prarit Bhargava) [1544999]
- [kernel] kdump: add support for crashkernel=auto (Dave Young) [1507353]
- [kernel] kdump: round up the total memory size to 128M for crashkernel reservation (Dave Young) [1507353]
- [arm64] acpi: prefer booting with ACPI over DTS (Mark Salter) [1576869]
- [acpi] aarch64: acpi scan: Fix regression related to X-Gene UARTs (Mark Salter) [1519554]
- [acpi] ACPI / irq: Workaround firmware issue on X-Gene based m400 (Mark Salter) [1519554]
- [x86] add rh_check_supported (David Arcari) [1565717]
- [scsi] qla2xxx: Remove PCI IDs of deprecated adapter (Himanshu Madhani) [1572233]
- [scsi] be2iscsi: remove unsupported device IDs (Chris Leech) [1574502]
- [scsi] Removing Obsolete hba pci-ids from rhel8 (Dick Kennedy) [1572321]
- [scsi] hpsa: modify hpsa driver version (Joseph Szczypek) [1471185]
- [scsi] hpsa: remove old cciss-based smartarray pci ids (Joseph Szczypek) [1471185]
- [kernel] rh_taint: add support for marking driver as unsupported (Jonathan Toppins) [1565704]
- [kernel] rh_taint: add support (David Arcari) [1565704]
- [scsi] qla4xxx: Remove deprecated PCI IDs from RHEL 8 (Chad Dupuis) [1518874]
- [scsi] aacraid: Remove depreciated device and vendor PCI id's (Raghava Aditya Renukunta) [1495307]
- [scsi] megaraid_sas: remove deprecated pci-ids (Tomas Henzl) [1509329]
- [scsi] mpt*: remove certain deprecated pci-ids (Tomas Henzl) [1511953]
- [kernel] modules: add rhelversion MODULE_INFO tag (Prarit Bhargava) [1544999]
- [acpi] ACPI: APEI: arm64: Ignore broken HPE moonshot APEI support (Al Stone) [1518076]
- [rpmspec] compute content hash for kernel-headers (Rafael Aquini) [1613003]
- [rpmspec] compress modules on all architectures ("Herton R. Krzesinski") [1614556]
- [rpmspec] add gcov rpm packaging support (Jan Stancek) [1601733]
- [rpmspec] don't ship spdxcheck.py (Jakub Racek)
- [rpmspec] clean stray bpf files (Jakub Racek) [1593309]
- [rpmspec] Copy symvers.gz to /lib/modules (Eugene Syromiatnikov) [1609695]
- [rpmspec] Add kabi-dup related code into specfile (Petr Oros) [1585672]
- [rpmspec] kernel spec: Add and enable kabi check (Petr Oros) [1585672]
- [rpmspec] Enable warning checks for configs in rpm build (Prarit Bhargava) [1589858]
- [rpmspec] remove workaround for rst2man-3 from python3-docutils ("Herton R. Krzesinski") [1602148]
- [rpmspec] fix dist tag used for hardlink in kernel-devel post ("Herton R. Krzesinski") [1596397]
- [scripts] get_maintainer.pl: Add optional .get_maintainer.MAINTAINERS override (Prarit Bhargava) [1595727]
- [rpmspec] drop kernel package dependency on python2 ("Herton R. Krzesinski") [1561505]
- [kernel] Makefile: Move RHEL definitions down (Jakub Racek) [1576568]
- [rpmspec] eBPF: Add bpftool package to spec file (Jerome Marchand) [1559607]
- [rpmspec] fix conflicts with COPYING file while installing newer 4.17 kernel ("Herton R. Krzesinski") [1579563]
- [rpmspec] do not build kernel meta-package on noarch ("Herton R. Krzesinski") [1579512]
- [rpmspec] kernel spec: remove copy of arch/x86/purgatory/sha256.* ("Herton R. Krzesinski")
- [rpmspec] spec: Add new arch/powerpc/kernel/module.lds file to kernel-devel rpm (Steve Best) [1572553]
- [rpmspec] kernel spec: fix recent build errors from brp-mangle-shebangs ("Herton R. Krzesinski") [1575966]
- [rpmspec] Add i386 to ExclusiveArch to fix noarch package build ("Herton R. Krzesinski") [1575152]
- [rpmspec] Build kernel-abi-whitelists package (Petr Oros) [1571189]
- [rpmspec] kernel spec: build bzImage for s390 (Hendrik Brueckner) [1570041]
- [rpmspec] kernel spec: arm64: package module.lds in kernel-devel (Mark Salter) [1569014]
- [rpmspec] Re-enable debuginfo packages and fix build with current dist tag ("Herton R. Krzesinski") [1568901]
- [rpmspec] kernel spec: build kernel-debug on all architectures ("Herton R. Krzesinski") [1567367]
- [rpmspec] don't build kernel meta-package if we are only building kernel headers ("Herton R. Krzesinski")
- [rpmspec] remove use_vdso macro ("Herton R. Krzesinski")
- [rpmspec] build perf and tools man pages instead of relying on a separate tarball ("Herton R. Krzesinski")
- [rpmspec] disable debug build if arch is in nobuildarches list ("Herton R. Krzesinski")
- [rpmspec] remove fedora changelog from spec file ("Herton R. Krzesinski")
- [rpmspec] only support ppc64le builds ("Herton R. Krzesinski")
- [rpmspec] remove x86 32-bit package support ("Herton R. Krzesinski")
- [rpmspec] remove arm 32-bit package support ("Herton R. Krzesinski")
- [rpmspec] remove configuration generation support from kernel spec file ("Herton R. Krzesinski")
- [rpmspec] remove broken out patches from kernel spec file ("Herton R. Krzesinski")
- [rpmspec] import kernel spec from rhel8 bootstrap dist-git ("Herton R. Krzesinski")